
EUTRA-RRC-Definitions DEFINITIONS AUTOMATIC TAGS ::=

BEGIN


BCCH-BCH-Message ::= SEQUENCE {
	message					BCCH-BCH-MessageType
}

BCCH-BCH-MessageType ::=						MasterInformationBlock


BCCH-BCH-Message-MBMS::= SEQUENCE {
	message					BCCH-BCH-MessageType-MBMS-r14
}

BCCH-BCH-MessageType-MBMS-r14 ::=					MasterInformationBlock-MBMS-r14


BCCH-DL-SCH-Message ::= SEQUENCE {
	message					BCCH-DL-SCH-MessageType
}

BCCH-DL-SCH-MessageType ::= CHOICE {
	c1						CHOICE {
		systemInformation						SystemInformation,
		systemInformationBlockType1				SystemInformationBlockType1
	},
	messageClassExtension	SEQUENCE {}
}


BCCH-DL-SCH-Message-BR ::= SEQUENCE {
	message					BCCH-DL-SCH-MessageType-BR-r13
}

BCCH-DL-SCH-MessageType-BR-r13 ::= CHOICE {
	c1						CHOICE {
		systemInformation-BR-r13				SystemInformation-BR-r13,
		systemInformationBlockType1-BR-r13		SystemInformationBlockType1-BR-r13
	},
	messageClassExtension	SEQUENCE {}
}


BCCH-DL-SCH-Message-MBMS ::= SEQUENCE {
	message						BCCH-DL-SCH-MessageType-MBMS-r14
}

BCCH-DL-SCH-MessageType-MBMS-r14 ::= CHOICE {
	c1						CHOICE {
		systemInformation-MBMS-r14						SystemInformation-MBMS-r14,
		systemInformationBlockType1-MBMS-r14				SystemInformationBlockType1-MBMS-r14
	},
	messageClassExtension	SEQUENCE {}
}


MCCH-Message ::=		SEQUENCE {
	message					MCCH-MessageType
}

MCCH-MessageType ::= CHOICE {
	c1							CHOICE {
		mbsfnAreaConfiguration-r9		MBSFNAreaConfiguration-r9
	},
	later						CHOICE {
		c2								CHOICE{
			mbmsCountingRequest-r10			MBMSCountingRequest-r10
		},
		messageClassExtension	SEQUENCE {}
	}
}


PCCH-Message ::= SEQUENCE {
	message					PCCH-MessageType
}

PCCH-MessageType ::= CHOICE {
	c1						CHOICE {
		paging									Paging
	},
	messageClassExtension	SEQUENCE {}
}


DL-CCCH-Message ::= SEQUENCE {
	message					DL-CCCH-MessageType
}

DL-CCCH-MessageType ::= CHOICE {
	c1						CHOICE {
		rrcConnectionReestablishment			RRCConnectionReestablishment,
		rrcConnectionReestablishmentReject		RRCConnectionReestablishmentReject,
		rrcConnectionReject						RRCConnectionReject,
		rrcConnectionSetup						RRCConnectionSetup
	},
	messageClassExtension	SEQUENCE {}
}


DL-DCCH-Message ::= SEQUENCE {
	message					DL-DCCH-MessageType
}

DL-DCCH-MessageType ::= CHOICE {
	c1						CHOICE {
		csfbParametersResponseCDMA2000			CSFBParametersResponseCDMA2000,
		dlInformationTransfer					DLInformationTransfer,
		handoverFromEUTRAPreparationRequest		HandoverFromEUTRAPreparationRequest,
		mobilityFromEUTRACommand				MobilityFromEUTRACommand,
		rrcConnectionReconfiguration			RRCConnectionReconfiguration,
		rrcConnectionRelease					RRCConnectionRelease,
		securityModeCommand						SecurityModeCommand,
		ueCapabilityEnquiry						UECapabilityEnquiry,
		counterCheck							CounterCheck,
		ueInformationRequest-r9					UEInformationRequest-r9,
		loggedMeasurementConfiguration-r10		LoggedMeasurementConfiguration-r10,
		rnReconfiguration-r10					RNReconfiguration-r10,
		rrcConnectionResume-r13					RRCConnectionResume-r13,
		spare3 NULL, spare2 NULL, spare1 NULL
	},
	messageClassExtension	SEQUENCE {}
}


UL-CCCH-Message ::= SEQUENCE {
	message					UL-CCCH-MessageType
}

UL-CCCH-MessageType ::= CHOICE {
	c1						CHOICE {
		rrcConnectionReestablishmentRequest		RRCConnectionReestablishmentRequest,
		rrcConnectionRequest					RRCConnectionRequest
	},
	messageClassExtension	CHOICE {
		c2						CHOICE {
			rrcConnectionResumeRequest-r13			RRCConnectionResumeRequest-r13
		},
		messageClassExtensionFuture-r13	SEQUENCE {}
		}
}


UL-DCCH-Message ::= SEQUENCE {
	message			UL-DCCH-MessageType
}

UL-DCCH-MessageType ::= CHOICE {
	c1						CHOICE {
		csfbParametersRequestCDMA2000				CSFBParametersRequestCDMA2000,
		measurementReport							MeasurementReport,
		rrcConnectionReconfigurationComplete		RRCConnectionReconfigurationComplete,
		rrcConnectionReestablishmentComplete		RRCConnectionReestablishmentComplete,
		rrcConnectionSetupComplete				RRCConnectionSetupComplete,
		securityModeComplete						SecurityModeComplete,
		securityModeFailure						SecurityModeFailure,
		ueCapabilityInformation					UECapabilityInformation,
		ulHandoverPreparationTransfer				ULHandoverPreparationTransfer,
		ulInformationTransfer						ULInformationTransfer,
		counterCheckResponse						CounterCheckResponse,
		ueInformationResponse-r9					UEInformationResponse-r9,
		proximityIndication-r9					ProximityIndication-r9,
		rnReconfigurationComplete-r10				RNReconfigurationComplete-r10,
		mbmsCountingResponse-r10					MBMSCountingResponse-r10,
		interFreqRSTDMeasurementIndication-r10	InterFreqRSTDMeasurementIndication-r10
	},
	messageClassExtension	CHOICE {
		c2							CHOICE {
			ueAssistanceInformation-r11			UEAssistanceInformation-r11,
			inDeviceCoexIndication-r11			InDeviceCoexIndication-r11,
			mbmsInterestIndication-r11			MBMSInterestIndication-r11,
			scgFailureInformation-r12				SCGFailureInformation-r12,
			sidelinkUEInformation-r12				SidelinkUEInformation-r12,
			wlanConnectionStatusReport-r13		WLANConnectionStatusReport-r13,
			rrcConnectionResumeComplete-r13		RRCConnectionResumeComplete-r13,
			spare9 NULL, spare8 NULL, spare7 NULL,
			spare6 NULL, spare5 NULL, spare4 NULL,
			spare3 NULL, spare2 NULL, spare1 NULL
		},
		messageClassExtensionFuture-r11	SEQUENCE {}
	}
}


SC-MCCH-Message-r13 ::= SEQUENCE {
	message					SC-MCCH-MessageType-r13
}


SC-MCCH-MessageType-r13 ::= CHOICE {
	c1						CHOICE {
		scptmConfiguration-r13						SCPTMConfiguration-r13
	},
	messageClassExtension	CHOICE {
		c2							CHOICE {
			scptmConfiguration-BR-r14				SCPTMConfiguration-BR-r14,
			spare									NULL
		},
		messageClassExtensionFuture-r14	SEQUENCE {}
	}
}


CounterCheck ::=			SEQUENCE {
	rrc-TransactionIdentifier			RRC-TransactionIdentifier,
	criticalExtensions					CHOICE {
		c1									CHOICE {
			counterCheck-r8						CounterCheck-r8-IEs,
			spare3 NULL, spare2 NULL, spare1 NULL
		},
		criticalExtensionsFuture			SEQUENCE {}
	}
}

CounterCheck-r8-IEs ::=	SEQUENCE {
	drb-CountMSB-InfoList				DRB-CountMSB-InfoList,
	nonCriticalExtension				CounterCheck-v8a0-IEs				OPTIONAL
}

CounterCheck-v8a0-IEs ::= SEQUENCE {
	lateNonCriticalExtension			OCTET STRING						OPTIONAL,
	nonCriticalExtension				SEQUENCE {}							OPTIONAL
}

DRB-CountMSB-InfoList ::=		SEQUENCE (SIZE (1..maxDRB)) OF DRB-CountMSB-Info

DRB-CountMSB-Info ::=	SEQUENCE {
	drb-Identity					DRB-Identity,
	countMSB-Uplink					INTEGER(0..33554431),
	countMSB-Downlink				INTEGER(0..33554431)
}


CounterCheckResponse ::=			SEQUENCE {
	rrc-TransactionIdentifier			RRC-TransactionIdentifier,
	criticalExtensions					CHOICE {
		counterCheckResponse-r8				CounterCheckResponse-r8-IEs,
		criticalExtensionsFuture			SEQUENCE {}
	}
}

CounterCheckResponse-r8-IEs ::=	SEQUENCE {
	drb-CountInfoList					DRB-CountInfoList,
	nonCriticalExtension				CounterCheckResponse-v8a0-IEs		OPTIONAL
}

CounterCheckResponse-v8a0-IEs ::= SEQUENCE {
	lateNonCriticalExtension			OCTET STRING						OPTIONAL,
	nonCriticalExtension				SEQUENCE {}							OPTIONAL
}

DRB-CountInfoList ::=			SEQUENCE (SIZE (0..maxDRB)) OF DRB-CountInfo

DRB-CountInfo ::=	SEQUENCE {
	drb-Identity					DRB-Identity,
	count-Uplink					INTEGER(0..4294967295),
	count-Downlink					INTEGER(0..4294967295)
}


CSFBParametersRequestCDMA2000 ::= SEQUENCE {
	criticalExtensions					CHOICE {
		csfbParametersRequestCDMA2000-r8	CSFBParametersRequestCDMA2000-r8-IEs,
		criticalExtensionsFuture			SEQUENCE {}
	}
}

CSFBParametersRequestCDMA2000-r8-IEs ::= SEQUENCE {
	nonCriticalExtension				CSFBParametersRequestCDMA2000-v8a0-IEs	OPTIONAL
}

CSFBParametersRequestCDMA2000-v8a0-IEs ::= SEQUENCE {
	lateNonCriticalExtension			OCTET STRING						OPTIONAL,
	nonCriticalExtension				SEQUENCE {}							OPTIONAL
}


CSFBParametersResponseCDMA2000 ::= SEQUENCE {
	rrc-TransactionIdentifier			RRC-TransactionIdentifier,
	criticalExtensions						CHOICE {
		csfbParametersResponseCDMA2000-r8		CSFBParametersResponseCDMA2000-r8-IEs,
		criticalExtensionsFuture				SEQUENCE {}
	}
}

CSFBParametersResponseCDMA2000-r8-IEs ::= SEQUENCE {
	rand								RAND-CDMA2000,
	mobilityParameters					MobilityParametersCDMA2000,
	nonCriticalExtension				CSFBParametersResponseCDMA2000-v8a0-IEs	OPTIONAL
}

CSFBParametersResponseCDMA2000-v8a0-IEs ::= SEQUENCE {
	lateNonCriticalExtension			OCTET STRING						OPTIONAL,
	nonCriticalExtension				SEQUENCE {}							OPTIONAL
}


DLInformationTransfer ::=			SEQUENCE {
	rrc-TransactionIdentifier			RRC-TransactionIdentifier,
	criticalExtensions					CHOICE {
		c1									CHOICE {
			dlInformationTransfer-r8			DLInformationTransfer-r8-IEs,
			spare3 NULL, spare2 NULL, spare1 NULL
		},
		criticalExtensionsFuture			SEQUENCE {}
	}
}

DLInformationTransfer-r8-IEs ::=	SEQUENCE {
	dedicatedInfoType					CHOICE {
		dedicatedInfoNAS					DedicatedInfoNAS,
		dedicatedInfoCDMA2000-1XRTT			DedicatedInfoCDMA2000,
		dedicatedInfoCDMA2000-HRPD			DedicatedInfoCDMA2000
	},
	nonCriticalExtension				DLInformationTransfer-v8a0-IEs		OPTIONAL
}

DLInformationTransfer-v8a0-IEs ::= SEQUENCE {
	lateNonCriticalExtension			OCTET STRING						OPTIONAL,
	nonCriticalExtension				SEQUENCE {}							OPTIONAL
}


HandoverFromEUTRAPreparationRequest ::= SEQUENCE {
	rrc-TransactionIdentifier		RRC-TransactionIdentifier,
	criticalExtensions					CHOICE {
		c1									CHOICE {
			handoverFromEUTRAPreparationRequest-r8
												HandoverFromEUTRAPreparationRequest-r8-IEs,
			spare3 NULL, spare2 NULL, spare1 NULL
		},
		criticalExtensionsFuture			SEQUENCE {}
	}
}

HandoverFromEUTRAPreparationRequest-r8-IEs ::= SEQUENCE {
	cdma2000-Type					CDMA2000-Type,
	rand							RAND-CDMA2000				OPTIONAL,	-- Cond cdma2000-Type
	mobilityParameters				MobilityParametersCDMA2000	OPTIONAL,	-- Cond cdma2000-Type
	nonCriticalExtension			HandoverFromEUTRAPreparationRequest-v890-IEs	OPTIONAL
}

HandoverFromEUTRAPreparationRequest-v890-IEs ::= SEQUENCE {
	lateNonCriticalExtension		OCTET STRING				OPTIONAL,
	nonCriticalExtension			HandoverFromEUTRAPreparationRequest-v920-IEs	OPTIONAL
}

HandoverFromEUTRAPreparationRequest-v920-IEs ::= SEQUENCE {
	concurrPrepCDMA2000-HRPD-r9		BOOLEAN					OPTIONAL,	-- Cond cdma2000-Type
	nonCriticalExtension			HandoverFromEUTRAPreparationRequest-v1020-IEs	OPTIONAL
}

HandoverFromEUTRAPreparationRequest-v1020-IEs ::= SEQUENCE {
	dualRxTxRedirectIndicator-r10		ENUMERATED {true}		OPTIONAL,	-- Cond cdma2000-1XRTT
	redirectCarrierCDMA2000-1XRTT-r10	CarrierFreqCDMA2000		OPTIONAL,	-- Cond dualRxTxRedirect
	nonCriticalExtension				SEQUENCE {}				OPTIONAL
}


InDeviceCoexIndication-r11 ::=		SEQUENCE {
	criticalExtensions					CHOICE {
		c1									CHOICE {
			inDeviceCoexIndication-r11				InDeviceCoexIndication-r11-IEs,
			spare3 NULL, spare2 NULL, spare1 NULL
		},
		criticalExtensionsFuture			SEQUENCE {}
	}
}

InDeviceCoexIndication-r11-IEs ::=	SEQUENCE {
	affectedCarrierFreqList-r11			AffectedCarrierFreqList-r11					OPTIONAL,
	tdm-AssistanceInfo-r11				TDM-AssistanceInfo-r11						OPTIONAL,
	lateNonCriticalExtension			OCTET STRING								OPTIONAL,
	nonCriticalExtension				InDeviceCoexIndication-v11d0-IEs			OPTIONAL
}

InDeviceCoexIndication-v11d0-IEs ::=	SEQUENCE {
	ul-CA-AssistanceInfo-r11			SEQUENCE {
		affectedCarrierFreqCombList-r11	AffectedCarrierFreqCombList-r11			OPTIONAL,
		victimSystemType-r11				VictimSystemType-r11
	}																			OPTIONAL,
	nonCriticalExtension				InDeviceCoexIndication-v1310-IEs								OPTIONAL
}

InDeviceCoexIndication-v1310-IEs ::=	SEQUENCE {
	affectedCarrierFreqList-v1310		AffectedCarrierFreqList-v1310		OPTIONAL,
	affectedCarrierFreqCombList-r13		AffectedCarrierFreqCombList-r13		OPTIONAL,
	nonCriticalExtension					InDeviceCoexIndication-v1360-IEs		OPTIONAL
}

InDeviceCoexIndication-v1360-IEs ::=	SEQUENCE {
	hardwareSharingProblem-r13		ENUMERATED {true}						OPTIONAL,
	nonCriticalExtension				SEQUENCE {}							OPTIONAL
}

AffectedCarrierFreqList-r11 ::=	SEQUENCE (SIZE (1..maxFreqIDC-r11)) OF AffectedCarrierFreq-r11

AffectedCarrierFreqList-v1310 ::= SEQUENCE (SIZE (1..maxFreqIDC-r11)) OF AffectedCarrierFreq-v1310

AffectedCarrierFreq-r11 ::=	SEQUENCE {
	carrierFreq-r11				MeasObjectId,
	interferenceDirection-r11	ENUMERATED {eutra, other, both, spare}
}

AffectedCarrierFreq-v1310 ::=	SEQUENCE {
	carrierFreq-v1310				MeasObjectId-v1310								OPTIONAL
}

AffectedCarrierFreqCombList-r11 ::=	SEQUENCE (SIZE (1..maxCombIDC-r11)) OF AffectedCarrierFreqComb-r11

AffectedCarrierFreqCombList-r13 ::= SEQUENCE (SIZE (1..maxCombIDC-r11)) OF AffectedCarrierFreqComb-r13

AffectedCarrierFreqComb-r11 ::=	SEQUENCE (SIZE (2..maxServCell-r10)) OF MeasObjectId

AffectedCarrierFreqComb-r13 ::= SEQUENCE (SIZE (2..maxServCell-r13)) OF MeasObjectId-r13

TDM-AssistanceInfo-r11 ::=	CHOICE {
	drx-AssistanceInfo-r11				SEQUENCE {
		drx-CycleLength-r11					ENUMERATED {sf40, sf64, sf80, sf128, sf160,
												sf256, spare2, spare1},
		drx-Offset-r11						INTEGER (0..255)	OPTIONAL,
		drx-ActiveTime-r11					ENUMERATED {sf20, sf30, sf40, sf60, sf80,
												sf100, spare2, spare1}
	},
	idc-SubframePatternList-r11			IDC-SubframePatternList-r11,
	...
}

IDC-SubframePatternList-r11 ::=	SEQUENCE (SIZE (1..maxSubframePatternIDC-r11)) OF IDC-SubframePattern-r11

IDC-SubframePattern-r11 ::= CHOICE {
	subframePatternFDD-r11				BIT STRING (SIZE (4)),
	subframePatternTDD-r11				CHOICE {
		subframeConfig0-r11					BIT STRING (SIZE (70)),
		subframeConfig1-5-r11				BIT STRING (SIZE (10)),
		subframeConfig6-r11					BIT STRING (SIZE (60))
	},
	...
}

VictimSystemType-r11 ::= SEQUENCE {
	gps-r11							ENUMERATED {true}				OPTIONAL,
	glonass-r11							ENUMERATED {true}				OPTIONAL,
	bds-r11								ENUMERATED {true}				OPTIONAL,
	galileo-r11						ENUMERATED {true}				OPTIONAL,
	wlan-r11							ENUMERATED {true}				OPTIONAL,
	bluetooth-r11						ENUMERATED {true}				OPTIONAL
}


InterFreqRSTDMeasurementIndication-r10 ::=			SEQUENCE {
	criticalExtensions					CHOICE {
		c1									CHOICE {
			interFreqRSTDMeasurementIndication-r10	InterFreqRSTDMeasurementIndication-r10-IEs,
			spare3 NULL, spare2 NULL, spare1 NULL
		},
		criticalExtensionsFuture			SEQUENCE {}
	}
}

InterFreqRSTDMeasurementIndication-r10-IEs ::=		SEQUENCE {
	rstd-InterFreqIndication-r10		CHOICE {
		start								SEQUENCE {
			rstd-InterFreqInfoList-r10				RSTD-InterFreqInfoList-r10
		},
		stop								NULL
	},
	lateNonCriticalExtension			OCTET STRING						OPTIONAL,
	nonCriticalExtension				SEQUENCE {}							OPTIONAL
}

RSTD-InterFreqInfoList-r10 ::=	SEQUENCE (SIZE(1..maxRSTD-Freq-r10)) OF RSTD-InterFreqInfo-r10

RSTD-InterFreqInfo-r10 ::=		SEQUENCE {
	carrierFreq-r10					ARFCN-ValueEUTRA,
	measPRS-Offset-r10				INTEGER (0..39),
	...,
	[[	carrierFreq-v1090			ARFCN-ValueEUTRA-v9e0				OPTIONAL
	]]
}


LoggedMeasurementConfiguration-r10 ::=	SEQUENCE {
	criticalExtensions					CHOICE {
		c1									CHOICE {
			loggedMeasurementConfiguration-r10		LoggedMeasurementConfiguration-r10-IEs,
			spare3 NULL, spare2 NULL, spare1 NULL
		},
		criticalExtensionsFuture				SEQUENCE {}
	}
}


LoggedMeasurementConfiguration-r10-IEs ::= SEQUENCE {
	traceReference-r10				TraceReference-r10,
	traceRecordingSessionRef-r10	OCTET STRING (SIZE (2)),
	tce-Id-r10						OCTET STRING (SIZE (1)),
	absoluteTimeInfo-r10			AbsoluteTimeInfo-r10,
	areaConfiguration-r10			AreaConfiguration-r10		OPTIONAL,	-- Need OR
	loggingDuration-r10				LoggingDuration-r10,
	loggingInterval-r10				LoggingInterval-r10,
	nonCriticalExtension			LoggedMeasurementConfiguration-v1080-IEs	OPTIONAL
}

LoggedMeasurementConfiguration-v1080-IEs ::= SEQUENCE {
	lateNonCriticalExtension-r10	OCTET STRING						OPTIONAL,
	nonCriticalExtension			LoggedMeasurementConfiguration-v1130-IEs	OPTIONAL
}

LoggedMeasurementConfiguration-v1130-IEs ::= SEQUENCE {
	plmn-IdentityList-r11			PLMN-IdentityList3-r11		OPTIONAL,	-- Need OR
	areaConfiguration-v1130			AreaConfiguration-v1130		OPTIONAL,	-- Need OR
	nonCriticalExtension			LoggedMeasurementConfiguration-v1250-IEs	OPTIONAL
}

LoggedMeasurementConfiguration-v1250-IEs ::= SEQUENCE {
	targetMBSFN-AreaList-r12	TargetMBSFN-AreaList-r12		OPTIONAL,	-- Need OP
	nonCriticalExtension			SEQUENCE {}					OPTIONAL
}

TargetMBSFN-AreaList-r12 ::=			SEQUENCE (SIZE (0..maxMBSFN-Area)) OF TargetMBSFN-Area-r12

TargetMBSFN-Area-r12 ::=				SEQUENCE {
	mbsfn-AreaId-r12					MBSFN-AreaId-r12		OPTIONAL,	-- Need OR
	carrierFreq-r12						ARFCN-ValueEUTRA-r9,
	...
}


MasterInformationBlock ::=			SEQUENCE {
	dl-Bandwidth						ENUMERATED {
											n6, n15, n25, n50, n75, n100},
	phich-Config						PHICH-Config,
	systemFrameNumber					BIT STRING (SIZE (8)),
	schedulingInfoSIB1-BR-r13			INTEGER (0..31),
	spare								BIT STRING (SIZE (5))
}



MasterInformationBlock-MBMS-r14 ::=			SEQUENCE {
	dl-Bandwidth-MBMS-r14						ENUMERATED {
											n6, n15, n25, n50, n75, n100},
	systemFrameNumber-r14					BIT STRING (SIZE (6)),
	additionalNonMBSFNSubframes-r14		INTEGER (0..3),
	spare									BIT STRING (SIZE (13))
}


MBMSCountingRequest-r10 ::=		SEQUENCE {
	countingRequestList-r10			CountingRequestList-r10,
	lateNonCriticalExtension		OCTET STRING						OPTIONAL,
	nonCriticalExtension			SEQUENCE {}							OPTIONAL
}

CountingRequestList-r10 ::=	SEQUENCE (SIZE (1..maxServiceCount)) OF CountingRequestInfo-r10

CountingRequestInfo-r10 ::=		SEQUENCE {
	tmgi-r10							TMGI-r9,
	...
}


MBMSCountingResponse-r10 ::=			SEQUENCE {
	criticalExtensions					CHOICE {
		c1									CHOICE {
			countingResponse-r10				MBMSCountingResponse-r10-IEs,
			spare3 NULL, spare2 NULL, spare1 NULL
		},
		criticalExtensionsFuture			SEQUENCE {}
	}
}

MBMSCountingResponse-r10-IEs ::=	SEQUENCE {
	mbsfn-AreaIndex-r10				INTEGER (0..maxMBSFN-Area-1)						OPTIONAL,
	countingResponseList-r10		CountingResponseList-r10			OPTIONAL,
	lateNonCriticalExtension		OCTET STRING						OPTIONAL,
	nonCriticalExtension			SEQUENCE {}							OPTIONAL
}

CountingResponseList-r10 ::=		SEQUENCE (SIZE (1..maxServiceCount)) OF CountingResponseInfo-r10

CountingResponseInfo-r10 ::=		SEQUENCE {
	countingResponseService-r10	INTEGER (0..maxServiceCount-1),
	...
}


MBMSInterestIndication-r11 ::=		SEQUENCE {
	criticalExtensions					CHOICE {
		c1									CHOICE {
			interestIndication-r11				MBMSInterestIndication-r11-IEs,
			spare3 NULL, spare2 NULL, spare1 NULL
		},
		criticalExtensionsFuture			SEQUENCE {}
	}
}

MBMSInterestIndication-r11-IEs ::=	SEQUENCE {
	mbms-FreqList-r11					CarrierFreqListMBMS-r11			OPTIONAL,
	mbms-Priority-r11					ENUMERATED {true}				OPTIONAL,
	lateNonCriticalExtension			OCTET STRING					OPTIONAL,
	nonCriticalExtension				MBMSInterestIndication-v1310-IEs	OPTIONAL
}

MBMSInterestIndication-v1310-IEs ::=	SEQUENCE {
	mbms-Services-r13					MBMS-ServiceList-r13				OPTIONAL,
	nonCriticalExtension				SEQUENCE {}						OPTIONAL
}


MBSFNAreaConfiguration-r9 ::=		SEQUENCE {
	commonSF-Alloc-r9					CommonSF-AllocPatternList-r9,
	commonSF-AllocPeriod-r9				ENUMERATED {
												rf4, rf8, rf16, rf32, rf64, rf128, rf256},
	pmch-InfoList-r9					PMCH-InfoList-r9,
	nonCriticalExtension				MBSFNAreaConfiguration-v930-IEs	OPTIONAL
}

MBSFNAreaConfiguration-v930-IEs ::= SEQUENCE {
	lateNonCriticalExtension			OCTET STRING						OPTIONAL,
	nonCriticalExtension				MBSFNAreaConfiguration-v1250-IEs	OPTIONAL
}

MBSFNAreaConfiguration-v1250-IEs ::= SEQUENCE {
	pmch-InfoListExt-r12				PMCH-InfoListExt-r12				OPTIONAL,	-- Need OR
	nonCriticalExtension				MBSFNAreaConfiguration-v1430-IEs	OPTIONAL
}

MBSFNAreaConfiguration-v1430-IEs ::= SEQUENCE {
	commonSF-Alloc-r14					CommonSF-AllocPatternList-r14,
	nonCriticalExtension				SEQUENCE {}							OPTIONAL
}

CommonSF-AllocPatternList-r9 ::=	SEQUENCE (SIZE (1..maxMBSFN-Allocations)) OF MBSFN-SubframeConfig

CommonSF-AllocPatternList-r14 ::=	SEQUENCE (SIZE (1..maxMBSFN-Allocations)) OF MBSFN-SubframeConfig-v1430


MeasurementReport ::=				SEQUENCE {
	criticalExtensions					CHOICE {
		c1									CHOICE{
			measurementReport-r8				MeasurementReport-r8-IEs,
			spare7 NULL,
			spare6 NULL, spare5 NULL, spare4 NULL,
			spare3 NULL, spare2 NULL, spare1 NULL
		},
		criticalExtensionsFuture			SEQUENCE {}
	}
}

MeasurementReport-r8-IEs ::=		SEQUENCE {
	measResults							MeasResults,
	nonCriticalExtension				MeasurementReport-v8a0-IEs							OPTIONAL
}

MeasurementReport-v8a0-IEs ::= SEQUENCE {
	lateNonCriticalExtension			OCTET STRING						OPTIONAL,
	nonCriticalExtension				SEQUENCE {}							OPTIONAL
}


MobilityFromEUTRACommand ::=		SEQUENCE {
	rrc-TransactionIdentifier			RRC-TransactionIdentifier,
	criticalExtensions					CHOICE {
		c1									CHOICE{
			mobilityFromEUTRACommand-r8		MobilityFromEUTRACommand-r8-IEs,
			mobilityFromEUTRACommand-r9		MobilityFromEUTRACommand-r9-IEs,
			spare2 NULL, spare1	NULL
		},
		criticalExtensionsFuture			SEQUENCE {}
	}
}

MobilityFromEUTRACommand-r8-IEs ::=	SEQUENCE {
	cs-FallbackIndicator				BOOLEAN,
	purpose								CHOICE{
		handover							Handover,
		cellChangeOrder						CellChangeOrder
	},
	nonCriticalExtension				MobilityFromEUTRACommand-v8a0-IEs	OPTIONAL
}

MobilityFromEUTRACommand-v8a0-IEs ::= SEQUENCE {
	lateNonCriticalExtension			OCTET STRING						OPTIONAL,
	nonCriticalExtension				MobilityFromEUTRACommand-v8d0-IEs	OPTIONAL
}

MobilityFromEUTRACommand-v8d0-IEs ::= SEQUENCE {
	bandIndicator						BandIndicatorGERAN			OPTIONAL,	-- Cond GERAN
	nonCriticalExtension				SEQUENCE {}					OPTIONAL
}

MobilityFromEUTRACommand-r9-IEs ::=	SEQUENCE {
	cs-FallbackIndicator				BOOLEAN,
	purpose								CHOICE{
		handover							Handover,
		cellChangeOrder						CellChangeOrder,
		e-CSFB-r9							E-CSFB-r9,
		...
	},
	nonCriticalExtension				MobilityFromEUTRACommand-v930-IEs	OPTIONAL
}

MobilityFromEUTRACommand-v930-IEs ::= SEQUENCE {
	lateNonCriticalExtension			OCTET STRING						OPTIONAL,
	nonCriticalExtension				MobilityFromEUTRACommand-v960-IEs	OPTIONAL
}

MobilityFromEUTRACommand-v960-IEs ::= SEQUENCE {
	bandIndicator						BandIndicatorGERAN			OPTIONAL,	-- Cond GERAN
	nonCriticalExtension				SEQUENCE {}					OPTIONAL
}

Handover ::=						SEQUENCE {
	targetRAT-Type						ENUMERATED {
											utra, geran, cdma2000-1XRTT, cdma2000-HRPD,
											spare4,	spare3, spare2, spare1, ...},
	targetRAT-MessageContainer			OCTET STRING,
	nas-SecurityParamFromEUTRA			OCTET STRING (SIZE (1))	OPTIONAL,	-- Cond UTRAGERAN
	systemInformation					SI-OrPSI-GERAN				OPTIONAL	-- Cond PSHO
}

CellChangeOrder ::=				SEQUENCE {
	t304								ENUMERATED {
											ms100, ms200, ms500, ms1000,
											ms2000, ms4000, ms8000, ms10000-v1310},
	targetRAT-Type						CHOICE {
			geran							SEQUENCE {
				physCellId						PhysCellIdGERAN,
				carrierFreq						CarrierFreqGERAN,
				networkControlOrder				BIT STRING (SIZE (2))		OPTIONAL,	-- Need OP
				systemInformation				SI-OrPSI-GERAN				OPTIONAL	-- Need OP
			},
			...
	}
}

SI-OrPSI-GERAN ::=					CHOICE {
	si									SystemInfoListGERAN,
	psi									SystemInfoListGERAN
}

E-CSFB-r9 ::=						SEQUENCE {
	messageContCDMA2000-1XRTT-r9		OCTET STRING		OPTIONAL,	-- Need ON
	mobilityCDMA2000-HRPD-r9			ENUMERATED {
											handover, redirection
										}					OPTIONAL,	-- Need OP
	messageContCDMA2000-HRPD-r9		OCTET STRING		OPTIONAL,	-- Cond concHO
	redirectCarrierCDMA2000-HRPD-r9	CarrierFreqCDMA2000	OPTIONAL	-- Cond concRedir
}


Paging ::=					SEQUENCE {
	pagingRecordList				PagingRecordList					OPTIONAL,	-- Need ON
	systemInfoModification			ENUMERATED {true}					OPTIONAL,	-- Need ON
	etws-Indication					ENUMERATED {true}					OPTIONAL,	-- Need ON
	nonCriticalExtension			Paging-v890-IEs						OPTIONAL
}

Paging-v890-IEs ::=			SEQUENCE {
	lateNonCriticalExtension		OCTET STRING							OPTIONAL,
	nonCriticalExtension			Paging-v920-IEs							OPTIONAL
}

Paging-v920-IEs ::=			SEQUENCE {
	cmas-Indication-r9				ENUMERATED {true}					OPTIONAL,	-- Need ON
	nonCriticalExtension				Paging-v1130-IEs				OPTIONAL
}

Paging-v1130-IEs ::=			SEQUENCE {
	eab-ParamModification-r11		ENUMERATED {true}					OPTIONAL,	-- Need ON
	nonCriticalExtension			Paging-v1310-IEs					OPTIONAL
}

Paging-v1310-IEs ::=			SEQUENCE {
	redistributionIndication-r13	ENUMERATED {true}					OPTIONAL,	--Need ON
	systemInfoModification-eDRX-r13	ENUMERATED {true}					OPTIONAL,	-- Need ON
	nonCriticalExtension			SEQUENCE {}							OPTIONAL
}

PagingRecordList ::=				SEQUENCE (SIZE (1..maxPageRec)) OF PagingRecord

PagingRecord ::=					SEQUENCE {
	ue-Identity							PagingUE-Identity,
	cn-Domain							ENUMERATED	{ps, cs},
	...
}

PagingUE-Identity ::=				CHOICE {
	s-TMSI								S-TMSI,
	imsi								IMSI,
	...
}

IMSI ::=							SEQUENCE (SIZE (6..21)) OF IMSI-Digit

IMSI-Digit ::=						INTEGER (0..9)


ProximityIndication-r9 ::= SEQUENCE {
	criticalExtensions					CHOICE {
		c1									CHOICE {
			proximityIndication-r9				ProximityIndication-r9-IEs,
			spare3 NULL, spare2 NULL, spare1 NULL
			},
		criticalExtensionsFuture			SEQUENCE {}
	}
}

ProximityIndication-r9-IEs ::= SEQUENCE {
	type-r9								ENUMERATED {entering, leaving},
	carrierFreq-r9						CHOICE {
		eutra-r9							ARFCN-ValueEUTRA,
		utra-r9								ARFCN-ValueUTRA,
		...,
		eutra2-v9e0							ARFCN-ValueEUTRA-v9e0
	},
	nonCriticalExtension				ProximityIndication-v930-IEs							OPTIONAL
}

ProximityIndication-v930-IEs ::= SEQUENCE {
	lateNonCriticalExtension			OCTET STRING						OPTIONAL,
	nonCriticalExtension				SEQUENCE {}							OPTIONAL
}


RNReconfiguration-r10 ::=		SEQUENCE {
	rrc-TransactionIdentifier		RRC-TransactionIdentifier,
	criticalExtensions				CHOICE {
		c1								CHOICE {
			rnReconfiguration-r10		RNReconfiguration-r10-IEs,
			spare3 NULL, spare2 NULL, spare1 NULL
		},
		criticalExtensionsFuture		SEQUENCE {}
	}
}

RNReconfiguration-r10-IEs ::=		SEQUENCE {
	rn-SystemInfo-r10					RN-SystemInfo-r10			OPTIONAL,	-- Need ON
	rn-SubframeConfig-r10				RN-SubframeConfig-r10			OPTIONAL,	-- Need ON
	lateNonCriticalExtension			OCTET STRING					OPTIONAL,
	nonCriticalExtension				SEQUENCE {}						OPTIONAL
}

RN-SystemInfo-r10 ::=			SEQUENCE {
	systemInformationBlockType1-r10		OCTET STRING (CONTAINING SystemInformationBlockType1)	OPTIONAL,	-- Need ON
	systemInformationBlockType2-r10		SystemInformationBlockType2		OPTIONAL,	-- Need ON
	...
}


RNReconfigurationComplete-r10 ::=		SEQUENCE {
	rrc-TransactionIdentifier				RRC-TransactionIdentifier,
	criticalExtensions						CHOICE {
		c1										CHOICE{
			rnReconfigurationComplete-r10			RNReconfigurationComplete-r10-IEs,
			spare3 NULL, spare2 NULL, spare1 NULL
		},
		criticalExtensionsFuture				SEQUENCE {}
	}
}

RNReconfigurationComplete-r10-IEs ::=	SEQUENCE {
	lateNonCriticalExtension				OCTET STRING				OPTIONAL,
	nonCriticalExtension					SEQUENCE {}					OPTIONAL
}


RRCConnectionReconfiguration ::=	SEQUENCE {
	rrc-TransactionIdentifier			RRC-TransactionIdentifier,
	criticalExtensions					CHOICE {
		c1									CHOICE{
			rrcConnectionReconfiguration-r8		RRCConnectionReconfiguration-r8-IEs,
			spare7 NULL,
			spare6 NULL, spare5 NULL, spare4 NULL,
			spare3 NULL, spare2 NULL, spare1 NULL
		},
		criticalExtensionsFuture			SEQUENCE {}
	}
}

RRCConnectionReconfiguration-r8-IEs ::= SEQUENCE {
	measConfig							MeasConfig						OPTIONAL,	-- Need ON
	mobilityControlInfo					MobilityControlInfo				OPTIONAL,	-- Cond HO
	dedicatedInfoNASList				SEQUENCE (SIZE(1..maxDRB)) OF
											DedicatedInfoNAS			OPTIONAL,	-- Cond nonHO
	radioResourceConfigDedicated		RadioResourceConfigDedicated	OPTIONAL, -- Cond HO-toEUTRA
	securityConfigHO					SecurityConfigHO				OPTIONAL,	-- Cond HO
	nonCriticalExtension				RRCConnectionReconfiguration-v890-IEs	OPTIONAL
}

RRCConnectionReconfiguration-v890-IEs ::= SEQUENCE {
	lateNonCriticalExtension			OCTET STRING (CONTAINING RRCConnectionReconfiguration-v8m0-IEs)	OPTIONAL,
	nonCriticalExtension				RRCConnectionReconfiguration-v920-IEs	OPTIONAL
}

-- Late non-critical extensions:
RRCConnectionReconfiguration-v8m0-IEs ::= SEQUENCE {
	-- Following field is only for pre REL-10 late non-critical extensions
	lateNonCriticalExtension			OCTET STRING								OPTIONAL,
	nonCriticalExtension				RRCConnectionReconfiguration-v10i0-IEs	OPTIONAL
}

RRCConnectionReconfiguration-v10i0-IEs ::= SEQUENCE {
	antennaInfoDedicatedPCell-v10i0	AntennaInfoDedicated-v10i0		OPTIONAL,	-- Need ON
	nonCriticalExtension				RRCConnectionReconfiguration-v10l0-IEs		OPTIONAL
}

RRCConnectionReconfiguration-v10l0-IEs ::= SEQUENCE {
	mobilityControlInfo-v10l0			MobilityControlInfo-v10l0			OPTIONAL,
	sCellToAddModList-v10l0			SCellToAddModList-v10l0			OPTIONAL,	-- Need ON
	-- Following field is only for late non-critical extensions from REL-10 to REL-11
	lateNonCriticalExtension			OCTET STRING						OPTIONAL,
	nonCriticalExtension				RRCConnectionReconfiguration-v12f0-IEs		OPTIONAL
}

RRCConnectionReconfiguration-v12f0-IEs ::= SEQUENCE {
	scg-Configuration-v12f0			SCG-Configuration-v12f0		OPTIONAL,	-- Cond nonFullConfig
	-- Following field is only for late non-critical extensions from REL-12
	lateNonCriticalExtension			OCTET STRING					OPTIONAL,
	nonCriticalExtension				RRCConnectionReconfiguration-v1370-IEs		OPTIONAL
}

RRCConnectionReconfiguration-v1370-IEs ::= SEQUENCE {
	radioResourceConfigDedicated-v1370	RadioResourceConfigDedicated-v1370	OPTIONAL, -- Need ON
	sCellToAddModListExt-v1370			SCellToAddModListExt-v1370	OPTIONAL,	-- Need ON
	-- Following field is only for late non-critical extensions from REL-13 onwards
	nonCriticalExtension					SEQUENCE {}					OPTIONAL
}

-- Regular non-critical extensions:
RRCConnectionReconfiguration-v920-IEs ::= SEQUENCE {
	otherConfig-r9						OtherConfig-r9				OPTIONAL,	-- Need ON
	fullConfig-r9						ENUMERATED {true}			OPTIONAL,	-- Cond HO-Reestab
	nonCriticalExtension				RRCConnectionReconfiguration-v1020-IEs	OPTIONAL
}

RRCConnectionReconfiguration-v1020-IEs ::= SEQUENCE {
	sCellToReleaseList-r10			SCellToReleaseList-r10			OPTIONAL,	-- Need ON
	sCellToAddModList-r10				SCellToAddModList-r10				OPTIONAL,	-- Need ON
	nonCriticalExtension				RRCConnectionReconfiguration-v1130-IEs	OPTIONAL
}

RRCConnectionReconfiguration-v1130-IEs ::= SEQUENCE {
	systemInformationBlockType1Dedicated-r11	OCTET STRING (CONTAINING SystemInformationBlockType1)																			OPTIONAL,	-- Need ON
	nonCriticalExtension				RRCConnectionReconfiguration-v1250-IEs	OPTIONAL
}

RRCConnectionReconfiguration-v1250-IEs ::= SEQUENCE {
	wlan-OffloadInfo-r12				CHOICE {
		release								NULL,
		setup									SEQUENCE {
			wlan-OffloadConfigDedicated-r12		WLAN-OffloadConfig-r12,
			t350-r12								ENUMERATED {min5, min10, min20, min30, min60,
												min120, min180, spare1}	OPTIONAL	-- Need OR
		}
	}																	OPTIONAL,		-- Need ON
	scg-Configuration-r12				SCG-Configuration-r12		OPTIONAL,	-- Cond nonFullConfig
	sl-SyncTxControl-r12				SL-SyncTxControl-r12			OPTIONAL,	-- Need ON
	sl-DiscConfig-r12					SL-DiscConfig-r12				OPTIONAL,	-- Need ON
	sl-CommConfig-r12					SL-CommConfig-r12				OPTIONAL,	-- Need ON
	nonCriticalExtension				RRCConnectionReconfiguration-v1310-IEs	OPTIONAL
}

RRCConnectionReconfiguration-v1310-IEs ::= SEQUENCE {
	sCellToReleaseListExt-r13			SCellToReleaseListExt-r13		OPTIONAL,	-- Need ON
	sCellToAddModListExt-r13			SCellToAddModListExt-r13		OPTIONAL,	-- Need ON
	lwa-Configuration-r13				LWA-Configuration-r13			OPTIONAL,	-- Need ON
	lwip-Configuration-r13				LWIP-Configuration-r13			OPTIONAL,	-- Need ON
	rclwi-Configuration-r13				RCLWI-Configuration-r13			OPTIONAL,	-- Need ON
	nonCriticalExtension				RRCConnectionReconfiguration-v1430-IEs						OPTIONAL
}

RRCConnectionReconfiguration-v1430-IEs ::= SEQUENCE {
	sl-V2X-ConfigDedicated-r14		SL-V2X-ConfigDedicated-r14		OPTIONAL,	-- Need ON
	sCellToAddModListExt-v1430		SCellToAddModListExt-v1430		OPTIONAL,	-- Need ON
	perCC-GapIndicationRequest-r14	ENUMERATED{true}					OPTIONAL,	-- Need ON
	systemInformationBlockType2Dedicated-r14	OCTET STRING (CONTAINING SystemInformationBlockType2)											OPTIONAL,	-- Cond nonHO
	nonCriticalExtension			SEQUENCE {}							OPTIONAL
}

SL-SyncTxControl-r12 ::=			SEQUENCE {
	networkControlledSyncTx-r12				ENUMERATED {on, off}		OPTIONAL	-- Need OP
}

PSCellToAddMod-r12 ::=				SEQUENCE {
	sCellIndex-r12						SCellIndex-r10,
	cellIdentification-r12				SEQUENCE {
		physCellId-r12						PhysCellId,
		dl-CarrierFreq-r12					ARFCN-ValueEUTRA-r9
	}																	OPTIONAL,	-- Cond SCellAdd
	radioResourceConfigCommonPSCell-r12		RadioResourceConfigCommonPSCell-r12	OPTIONAL,	-- Cond SCellAdd
	radioResourceConfigDedicatedPSCell-r12	RadioResourceConfigDedicatedPSCell-r12	OPTIONAL,	-- Cond SCellAdd2
	...,
	[[	antennaInfoDedicatedPSCell-v1280		AntennaInfoDedicated-v10i0	OPTIONAL	-- Need ON
	]],
	[[	sCellIndex-r13					SCellIndex-r13	OPTIONAL		-- Need ON
	]],
	[[	radioResourceConfigDedicatedPSCell-v1370	RadioResourceConfigDedicatedPSCell-v1370	OPTIONAL	-- Need ON
	]]
}

PSCellToAddMod-v12f0 ::=				SEQUENCE {
	radioResourceConfigCommonPSCell-r12		RadioResourceConfigCommonPSCell-v12f0	OPTIONAL
}

PSCellToAddMod-v1440 ::=				SEQUENCE {
	radioResourceConfigCommonPSCell-r14		RadioResourceConfigCommonPSCell-v1440	OPTIONAL
}

PowerCoordinationInfo-r12 ::= SEQUENCE {
	p-MeNB-r12							INTEGER (1..16),
	p-SeNB-r12							INTEGER (1..16),
	powerControlMode-r12				INTEGER (1..2)
}

SCellToAddModList-r10 ::=		SEQUENCE (SIZE (1..maxSCell-r10)) OF SCellToAddMod-r10

SCellToAddModList-v10l0 ::=		SEQUENCE (SIZE (1..maxSCell-r10)) OF SCellToAddMod-v10l0

SCellToAddModListExt-r13 ::=	SEQUENCE (SIZE (1..maxSCell-r13)) OF SCellToAddModExt-r13

SCellToAddModListExt-v1370 ::=	SEQUENCE (SIZE (1..maxSCell-r13)) OF SCellToAddModExt-v1370

SCellToAddModListExt-v1430 ::=	SEQUENCE (SIZE (1..maxSCell-r13)) OF SCellToAddModExt-v1430

SCellToAddMod-r10 ::=			SEQUENCE {
	sCellIndex-r10						SCellIndex-r10,
	cellIdentification-r10				SEQUENCE {
		physCellId-r10						PhysCellId,
		dl-CarrierFreq-r10					ARFCN-ValueEUTRA
	}																OPTIONAL,	-- Cond SCellAdd
	radioResourceConfigCommonSCell-r10		RadioResourceConfigCommonSCell-r10	OPTIONAL,	-- Cond SCellAdd
	radioResourceConfigDedicatedSCell-r10	RadioResourceConfigDedicatedSCell-r10	OPTIONAL,	-- Cond SCellAdd2
	...,
	[[	dl-CarrierFreq-v1090				ARFCN-ValueEUTRA-v9e0	OPTIONAL	-- Cond EARFCN-max
	]],
	[[	antennaInfoDedicatedSCell-v10i0		AntennaInfoDedicated-v10i0	OPTIONAL	-- Need ON
	]],
	[[	srs-SwitchFromServCellIndex-r14		INTEGER (0.. 31) OPTIONAL	-- Need ON
	]]
}

SCellToAddMod-v10l0 ::=			SEQUENCE {
	radioResourceConfigCommonSCell-v10l0		RadioResourceConfigCommonSCell-v10l0	OPTIONAL
}

SCellToAddModExt-r13 ::=			SEQUENCE {
	sCellIndex-r13						SCellIndex-r13,
	cellIdentification-r13				SEQUENCE {
		physCellId-r13						PhysCellId,
		dl-CarrierFreq-r13					ARFCN-ValueEUTRA-r9
	}																OPTIONAL,	-- Cond SCellAdd
	radioResourceConfigCommonSCell-r13		RadioResourceConfigCommonSCell-r10	OPTIONAL,	-- Cond SCellAdd
	radioResourceConfigDedicatedSCell-r13	RadioResourceConfigDedicatedSCell-r10	OPTIONAL,	-- Cond SCellAdd2
	antennaInfoDedicatedSCell-r13			AntennaInfoDedicated-v10i0		OPTIONAL	-- Need ON
}

SCellToAddModExt-v1370 ::=			SEQUENCE {
	radioResourceConfigCommonSCell-v1370		RadioResourceConfigCommonSCell-v10l0	OPTIONAL
}

SCellToAddModExt-v1430 ::=			SEQUENCE {
	srs-SwitchFromServCellIndex-r14			INTEGER (0.. 31)			OPTIONAL,	-- Need ON
	...
}

SCellToReleaseList-r10 ::=			SEQUENCE (SIZE (1..maxSCell-r10)) OF SCellIndex-r10

SCellToReleaseListExt-r13 ::=			SEQUENCE (SIZE (1..maxSCell-r13)) OF SCellIndex-r13

SCG-Configuration-r12 ::=			CHOICE {
	release								NULL,
	setup								SEQUENCE {
		scg-ConfigPartMCG-r12				SEQUENCE {
			scg-Counter-r12						INTEGER (0.. 65535)			OPTIONAL,	-- Need ON
			powerCoordinationInfo-r12			PowerCoordinationInfo-r12	OPTIONAL,	-- Need ON
			...
		}																OPTIONAL,	-- Need ON
		scg-ConfigPartSCG-r12				SCG-ConfigPartSCG-r12		OPTIONAL	-- Need ON
	}
}

SCG-Configuration-v12f0 ::=			CHOICE {
	release								NULL,
	setup								SEQUENCE {
		scg-ConfigPartSCG-v12f0				SCG-ConfigPartSCG-v12f0		OPTIONAL	-- Need ON
	}
}

SCG-ConfigPartSCG-r12 ::=			SEQUENCE {
	radioResourceConfigDedicatedSCG-r12	RadioResourceConfigDedicatedSCG-r12	OPTIONAL,	-- Need ON
	sCellToReleaseListSCG-r12			SCellToReleaseList-r10		OPTIONAL,	-- Need ON
	pSCellToAddMod-r12					PSCellToAddMod-r12			OPTIONAL,	-- Need ON
	sCellToAddModListSCG-r12			SCellToAddModList-r10		OPTIONAL,	-- Need ON
	mobilityControlInfoSCG-r12			MobilityControlInfoSCG-r12	OPTIONAL,	-- Need ON
	...,
	[[
	sCellToReleaseListSCG-Ext-r13			SCellToReleaseListExt-r13		OPTIONAL,	-- Need ON
	sCellToAddModListSCG-Ext-r13				SCellToAddModListExt-r13	OPTIONAL	-- Need ON
	]],
	[[
	sCellToAddModListSCG-Ext-v1370		SCellToAddModListExt-v1370	OPTIONAL	-- Need ON
	]],
	[[
	pSCellToAddMod-v1440				PSCellToAddMod-v1440		OPTIONAL	-- Need ON
	]]
}

SCG-ConfigPartSCG-v12f0 ::=			SEQUENCE {
	pSCellToAddMod-v12f0				PSCellToAddMod-v12f0			OPTIONAL,	-- Need ON
	sCellToAddModListSCG-v12f0		SCellToAddModList-v10l0		OPTIONAL	-- Need ON
}

SecurityConfigHO ::=				SEQUENCE {
	handoverType						CHOICE {
		intraLTE							SEQUENCE {
			securityAlgorithmConfig			SecurityAlgorithmConfig		OPTIONAL,	-- Cond fullConfig
			keyChangeIndicator					BOOLEAN,
			nextHopChainingCount				NextHopChainingCount
		},
		interRAT							SEQUENCE {
			securityAlgorithmConfig			SecurityAlgorithmConfig,
			nas-SecurityParamToEUTRA			OCTET STRING (SIZE(6))
		}
	},
	...
}



RRCConnectionReconfigurationComplete ::= SEQUENCE {
	rrc-TransactionIdentifier			RRC-TransactionIdentifier,
	criticalExtensions					CHOICE {
		rrcConnectionReconfigurationComplete-r8
											RRCConnectionReconfigurationComplete-r8-IEs,
		criticalExtensionsFuture			SEQUENCE {}
	}
}

RRCConnectionReconfigurationComplete-r8-IEs ::= SEQUENCE {
	nonCriticalExtension				RRCConnectionReconfigurationComplete-v8a0-IEs	OPTIONAL
}

RRCConnectionReconfigurationComplete-v8a0-IEs ::= SEQUENCE {
	lateNonCriticalExtension			OCTET STRING						OPTIONAL,
	nonCriticalExtension				RRCConnectionReconfigurationComplete-v1020-IEs	OPTIONAL
}

RRCConnectionReconfigurationComplete-v1020-IEs ::= SEQUENCE {
	rlf-InfoAvailable-r10				ENUMERATED {true}				OPTIONAL,
	logMeasAvailable-r10				ENUMERATED {true}				OPTIONAL,
	nonCriticalExtension				RRCConnectionReconfigurationComplete-v1130-IEs	OPTIONAL
}

RRCConnectionReconfigurationComplete-v1130-IEs ::= SEQUENCE {
	connEstFailInfoAvailable-r11		ENUMERATED {true}				OPTIONAL,
	nonCriticalExtension				RRCConnectionReconfigurationComplete-v1250-IEs	OPTIONAL
}

RRCConnectionReconfigurationComplete-v1250-IEs ::= SEQUENCE {
	logMeasAvailableMBSFN-r12			ENUMERATED {true}				OPTIONAL,
	nonCriticalExtension				RRCConnectionReconfigurationComplete-v1430-IEs						OPTIONAL
}

RRCConnectionReconfigurationComplete-v1430-IEs ::= SEQUENCE {
	perCC-GapIndicationList-r14			PerCC-GapIndicationList-r14		OPTIONAL,
	numFreqEffective-r14				INTEGER (1..12)					OPTIONAL,
	numFreqEffectiveReduced-r14			INTEGER (1..12)					OPTIONAL,
	nonCriticalExtension				SEQUENCE {}						OPTIONAL
}


RRCConnectionReestablishment ::=	SEQUENCE {
	rrc-TransactionIdentifier			RRC-TransactionIdentifier,
	criticalExtensions					CHOICE {
		c1									CHOICE{
			rrcConnectionReestablishment-r8		RRCConnectionReestablishment-r8-IEs,
			spare7 NULL,
			spare6 NULL, spare5 NULL, spare4	NULL,
			spare3 NULL, spare2 NULL, spare1	NULL
		},
		criticalExtensionsFuture			SEQUENCE {}
	}
}

RRCConnectionReestablishment-r8-IEs ::= SEQUENCE {
	radioResourceConfigDedicated		RadioResourceConfigDedicated,
	nextHopChainingCount				NextHopChainingCount,
	nonCriticalExtension				RRCConnectionReestablishment-v8a0-IEs	OPTIONAL
}

RRCConnectionReestablishment-v8a0-IEs ::= SEQUENCE {
	lateNonCriticalExtension			OCTET STRING						OPTIONAL,
	nonCriticalExtension				SEQUENCE {}							OPTIONAL
}


RRCConnectionReestablishmentComplete ::= SEQUENCE {
	rrc-TransactionIdentifier			RRC-TransactionIdentifier,
	criticalExtensions					CHOICE {
		rrcConnectionReestablishmentComplete-r8
											RRCConnectionReestablishmentComplete-r8-IEs,
		criticalExtensionsFuture			SEQUENCE {}
	}
}

RRCConnectionReestablishmentComplete-r8-IEs ::= SEQUENCE {
	nonCriticalExtension				RRCConnectionReestablishmentComplete-v920-IEs	OPTIONAL
}

RRCConnectionReestablishmentComplete-v920-IEs ::= SEQUENCE {
	rlf-InfoAvailable-r9				ENUMERATED {true}				OPTIONAL,
	nonCriticalExtension				RRCConnectionReestablishmentComplete-v8a0-IEs	OPTIONAL
}

RRCConnectionReestablishmentComplete-v8a0-IEs ::= SEQUENCE {
	lateNonCriticalExtension			OCTET STRING						OPTIONAL,
	nonCriticalExtension				RRCConnectionReestablishmentComplete-v1020-IEs	OPTIONAL
}

RRCConnectionReestablishmentComplete-v1020-IEs ::= SEQUENCE {
	logMeasAvailable-r10				ENUMERATED {true}				OPTIONAL,
	nonCriticalExtension				RRCConnectionReestablishmentComplete-v1130-IEs	OPTIONAL
}

RRCConnectionReestablishmentComplete-v1130-IEs ::= SEQUENCE {
	connEstFailInfoAvailable-r11		ENUMERATED {true}				OPTIONAL,
	nonCriticalExtension				RRCConnectionReestablishmentComplete-v1250-IEs	OPTIONAL
}

RRCConnectionReestablishmentComplete-v1250-IEs ::= SEQUENCE {
	logMeasAvailableMBSFN-r12			ENUMERATED {true}				OPTIONAL,
	nonCriticalExtension				SEQUENCE {}						OPTIONAL
}


RRCConnectionReestablishmentReject ::= SEQUENCE {
	criticalExtensions					CHOICE {
		rrcConnectionReestablishmentReject-r8
											RRCConnectionReestablishmentReject-r8-IEs,
		criticalExtensionsFuture			SEQUENCE {}
	}
}

RRCConnectionReestablishmentReject-r8-IEs ::= SEQUENCE {
	nonCriticalExtension				RRCConnectionReestablishmentReject-v8a0-IEs	OPTIONAL
}

RRCConnectionReestablishmentReject-v8a0-IEs ::= SEQUENCE {
	lateNonCriticalExtension			OCTET STRING						OPTIONAL,
	nonCriticalExtension				SEQUENCE {}							OPTIONAL
}


RRCConnectionReestablishmentRequest ::= SEQUENCE {
	criticalExtensions					CHOICE {
		rrcConnectionReestablishmentRequest-r8
											RRCConnectionReestablishmentRequest-r8-IEs,
		criticalExtensionsFuture			SEQUENCE {}
	}
}

RRCConnectionReestablishmentRequest-r8-IEs ::= SEQUENCE {
	ue-Identity							ReestabUE-Identity,
	reestablishmentCause				ReestablishmentCause,
	spare								BIT STRING (SIZE (2))
}

ReestabUE-Identity ::=				SEQUENCE {
	c-RNTI								C-RNTI,
	physCellId							PhysCellId,
	shortMAC-I							ShortMAC-I
}

ReestablishmentCause ::=			ENUMERATED {
										reconfigurationFailure, handoverFailure,
										otherFailure, spare1}


RRCConnectionReject ::=				SEQUENCE {
	criticalExtensions					CHOICE {
		c1									CHOICE {
			rrcConnectionReject-r8				RRCConnectionReject-r8-IEs,
			spare3 NULL, spare2 NULL, spare1 NULL
		},
		criticalExtensionsFuture			SEQUENCE {}
	}
}

RRCConnectionReject-r8-IEs ::=		SEQUENCE {
	waitTime							INTEGER (1..16),
	nonCriticalExtension				RRCConnectionReject-v8a0-IEs		OPTIONAL
}

RRCConnectionReject-v8a0-IEs ::= SEQUENCE {
	lateNonCriticalExtension			OCTET STRING						OPTIONAL,
	nonCriticalExtension				RRCConnectionReject-v1020-IEs		OPTIONAL
}

RRCConnectionReject-v1020-IEs ::=	SEQUENCE {
	extendedWaitTime-r10				INTEGER (1..1800)					OPTIONAL,	-- Need ON
	nonCriticalExtension				RRCConnectionReject-v1130-IEs		OPTIONAL
}

RRCConnectionReject-v1130-IEs ::=	SEQUENCE {
	deprioritisationReq-r11				SEQUENCE {
		deprioritisationType-r11			ENUMERATED {frequency, e-utra},
		deprioritisationTimer-r11			ENUMERATED {min5, min10, min15, min30}
	}																		OPTIONAL,	-- Need ON
	nonCriticalExtension				RRCConnectionReject-v1320-IEs							OPTIONAL
}

RRCConnectionReject-v1320-IEs ::=	SEQUENCE {
	rrc-SuspendIndication-r13				ENUMERATED {true}				OPTIONAL,	--	Need ON
	nonCriticalExtension					SEQUENCE {}						OPTIONAL
}


RRCConnectionRelease ::=			SEQUENCE {
	rrc-TransactionIdentifier			RRC-TransactionIdentifier,
	criticalExtensions					CHOICE {
		c1									CHOICE {
			rrcConnectionRelease-r8				RRCConnectionRelease-r8-IEs,
			spare3 NULL, spare2 NULL, spare1 NULL
		},
		criticalExtensionsFuture			SEQUENCE {}
	}
}

RRCConnectionRelease-r8-IEs ::=		SEQUENCE {
	releaseCause						ReleaseCause,
	redirectedCarrierInfo				RedirectedCarrierInfo				OPTIONAL,	-- Need ON
	idleModeMobilityControlInfo			IdleModeMobilityControlInfo			OPTIONAL,	-- Need OP
	nonCriticalExtension				RRCConnectionRelease-v890-IEs		OPTIONAL
}

RRCConnectionRelease-v890-IEs ::=	SEQUENCE {
	lateNonCriticalExtension			OCTET STRING (CONTAINING RRCConnectionRelease-v9e0-IEs)	OPTIONAL,
	nonCriticalExtension				RRCConnectionRelease-v920-IEs		OPTIONAL
}

-- Late non critical extensions
RRCConnectionRelease-v9e0-IEs ::= SEQUENCE {
	redirectedCarrierInfo-v9e0			RedirectedCarrierInfo-v9e0			OPTIONAL,	-- Cond NoRedirect-r8
	idleModeMobilityControlInfo-v9e0	IdleModeMobilityControlInfo-v9e0	OPTIONAL,	-- Cond IdleInfoEUTRA
	nonCriticalExtension				SEQUENCE {}							OPTIONAL
}

-- Regular non critical extensions
RRCConnectionRelease-v920-IEs ::=	SEQUENCE {
	cellInfoList-r9					CHOICE {
		geran-r9						CellInfoListGERAN-r9,
		utra-FDD-r9						CellInfoListUTRA-FDD-r9,
		utra-TDD-r9						CellInfoListUTRA-TDD-r9,
		...,
		utra-TDD-r10					CellInfoListUTRA-TDD-r10
	}															OPTIONAL,	-- Cond Redirection
	nonCriticalExtension			RRCConnectionRelease-v1020-IEs		OPTIONAL
}

RRCConnectionRelease-v1020-IEs ::=	SEQUENCE {
	extendedWaitTime-r10				INTEGER (1..1800)		OPTIONAL,	-- Need ON
	nonCriticalExtension			RRCConnectionRelease-v1320-IEs				OPTIONAL
}

RRCConnectionRelease-v1320-IEs::=	SEQUENCE {
	resumeIdentity-r13					ResumeIdentity-r13				OPTIONAL,	-- Need OR
	nonCriticalExtension				SEQUENCE {}						OPTIONAL
}

ReleaseCause ::=				ENUMERATED {loadBalancingTAUrequired,
											other, cs-FallbackHighPriority-v1020, rrc-Suspend-v1320}

RedirectedCarrierInfo ::=			CHOICE {
	eutra								ARFCN-ValueEUTRA,
	geran								CarrierFreqsGERAN,
	utra-FDD							ARFCN-ValueUTRA,
	utra-TDD							ARFCN-ValueUTRA,
	cdma2000-HRPD						CarrierFreqCDMA2000,
	cdma2000-1xRTT						CarrierFreqCDMA2000,
	...,
	utra-TDD-r10						CarrierFreqListUTRA-TDD-r10
}

RedirectedCarrierInfo-v9e0 ::=			SEQUENCE {
	eutra-v9e0								ARFCN-ValueEUTRA-v9e0
}

CarrierFreqListUTRA-TDD-r10 ::=			SEQUENCE (SIZE (1..maxFreqUTRA-TDD-r10)) OF ARFCN-ValueUTRA

IdleModeMobilityControlInfo ::=		SEQUENCE {
	freqPriorityListEUTRA				FreqPriorityListEUTRA			OPTIONAL,		-- Need ON
	freqPriorityListGERAN				FreqsPriorityListGERAN			OPTIONAL,		-- Need ON
	freqPriorityListUTRA-FDD			FreqPriorityListUTRA-FDD		OPTIONAL,		-- Need ON
	freqPriorityListUTRA-TDD			FreqPriorityListUTRA-TDD		OPTIONAL,		-- Need ON
	bandClassPriorityListHRPD			BandClassPriorityListHRPD		OPTIONAL,		-- Need ON
	bandClassPriorityList1XRTT			BandClassPriorityList1XRTT		OPTIONAL,		-- Need ON
	t320								ENUMERATED {
											min5, min10, min20, min30, min60, min120, min180,
											spare1}						OPTIONAL,		-- Need OR
	...,
	[[	freqPriorityListExtEUTRA-r12		FreqPriorityListExtEUTRA-r12		OPTIONAL		-- Need ON
	]],
	[[	freqPriorityListEUTRA-v1310			FreqPriorityListEUTRA-v1310			OPTIONAL,		-- Need ON
		freqPriorityListExtEUTRA-v1310		FreqPriorityListExtEUTRA-v1310		OPTIONAL		-- Need ON
	]]
}

IdleModeMobilityControlInfo-v9e0 ::=	SEQUENCE {
	freqPriorityListEUTRA-v9e0			SEQUENCE (SIZE (1..maxFreq)) OF FreqPriorityEUTRA-v9e0
}

FreqPriorityListEUTRA ::=			SEQUENCE (SIZE (1..maxFreq)) OF FreqPriorityEUTRA

FreqPriorityListExtEUTRA-r12 ::=		SEQUENCE (SIZE (1..maxFreq)) OF FreqPriorityEUTRA-r12

FreqPriorityListEUTRA-v1310 ::=			SEQUENCE (SIZE (1..maxFreq)) OF FreqPriorityEUTRA-v1310

FreqPriorityListExtEUTRA-v1310 ::=		SEQUENCE (SIZE (1..maxFreq)) OF FreqPriorityEUTRA-v1310

FreqPriorityEUTRA ::=				SEQUENCE {
	carrierFreq							ARFCN-ValueEUTRA,
	cellReselectionPriority				CellReselectionPriority
}

FreqPriorityEUTRA-v9e0 ::=			SEQUENCE {
	carrierFreq-v9e0					ARFCN-ValueEUTRA-v9e0		OPTIONAL	-- Cond EARFCN-max
}

FreqPriorityEUTRA-r12 ::=				SEQUENCE {
	carrierFreq-r12							ARFCN-ValueEUTRA-r9,
	cellReselectionPriority-r12				CellReselectionPriority
}

FreqPriorityEUTRA-v1310 ::=				SEQUENCE {
	cellReselectionSubPriority-r13				CellReselectionSubPriority-r13		OPTIONAL		-- Need ON
}

FreqsPriorityListGERAN ::=			SEQUENCE (SIZE (1..maxGNFG)) OF FreqsPriorityGERAN

FreqsPriorityGERAN ::=				SEQUENCE {
	carrierFreqs						CarrierFreqsGERAN,
	cellReselectionPriority				CellReselectionPriority
}

FreqPriorityListUTRA-FDD ::=		SEQUENCE (SIZE (1..maxUTRA-FDD-Carrier)) OF FreqPriorityUTRA-FDD

FreqPriorityUTRA-FDD ::=			SEQUENCE {
	carrierFreq							ARFCN-ValueUTRA,
	cellReselectionPriority				CellReselectionPriority
}

FreqPriorityListUTRA-TDD ::=		SEQUENCE (SIZE (1..maxUTRA-TDD-Carrier)) OF FreqPriorityUTRA-TDD

FreqPriorityUTRA-TDD ::=			SEQUENCE {
	carrierFreq							ARFCN-ValueUTRA,
	cellReselectionPriority				CellReselectionPriority
}

BandClassPriorityListHRPD ::=		SEQUENCE (SIZE (1..maxCDMA-BandClass)) OF BandClassPriorityHRPD

BandClassPriorityHRPD ::=			SEQUENCE {
	bandClass							BandclassCDMA2000,
	cellReselectionPriority				CellReselectionPriority
}

BandClassPriorityList1XRTT ::=	SEQUENCE (SIZE (1..maxCDMA-BandClass)) OF BandClassPriority1XRTT

BandClassPriority1XRTT ::=			SEQUENCE {
	bandClass							BandclassCDMA2000,
	cellReselectionPriority				CellReselectionPriority
}

CellInfoListGERAN-r9 ::=		SEQUENCE (SIZE (1..maxCellInfoGERAN-r9)) OF CellInfoGERAN-r9

CellInfoGERAN-r9 ::=				SEQUENCE {
	physCellId-r9						PhysCellIdGERAN,
	carrierFreq-r9						CarrierFreqGERAN,
	systemInformation-r9				SystemInfoListGERAN
}

CellInfoListUTRA-FDD-r9 ::=			SEQUENCE (SIZE (1..maxCellInfoUTRA-r9)) OF CellInfoUTRA-FDD-r9

CellInfoUTRA-FDD-r9 ::=				SEQUENCE {
	physCellId-r9						PhysCellIdUTRA-FDD,
	utra-BCCH-Container-r9				OCTET STRING
}

CellInfoListUTRA-TDD-r9 ::=			SEQUENCE (SIZE (1..maxCellInfoUTRA-r9)) OF CellInfoUTRA-TDD-r9

CellInfoUTRA-TDD-r9 ::=				SEQUENCE {
	physCellId-r9						PhysCellIdUTRA-TDD,
	utra-BCCH-Container-r9				OCTET STRING
}

CellInfoListUTRA-TDD-r10 ::=		SEQUENCE (SIZE (1..maxCellInfoUTRA-r9)) OF CellInfoUTRA-TDD-r10

CellInfoUTRA-TDD-r10 ::=			SEQUENCE {
	physCellId-r10						PhysCellIdUTRA-TDD,
	carrierFreq-r10						ARFCN-ValueUTRA,
	utra-BCCH-Container-r10				OCTET STRING
}


RRCConnectionRequest ::=			SEQUENCE {
	criticalExtensions					CHOICE {
		rrcConnectionRequest-r8				RRCConnectionRequest-r8-IEs,
		criticalExtensionsFuture			SEQUENCE {}
	}
}

RRCConnectionRequest-r8-IEs ::=		SEQUENCE {
	ue-Identity							InitialUE-Identity,
	establishmentCause					EstablishmentCause,
	spare								BIT STRING (SIZE (1))
}

InitialUE-Identity ::=				CHOICE {
	s-TMSI								S-TMSI,
	randomValue							BIT STRING (SIZE (40))
}

EstablishmentCause ::=				ENUMERATED {
										emergency, highPriorityAccess, mt-Access, mo-Signalling,
										mo-Data, delayTolerantAccess-v1020, mo-VoiceCall-v1280, spare1}


RRCConnectionResume-r13 ::=		SEQUENCE {
	rrc-TransactionIdentifier			RRC-TransactionIdentifier,
	criticalExtensions					CHOICE {
		c1									CHOICE {
			rrcConnectionResume-r13				RRCConnectionResume-r13-IEs,
			spare3								NULL,
			spare2								NULL,
			spare1								NULL
		},
		criticalExtensionsFuture			SEQUENCE {}
	}
}

RRCConnectionResume-r13-IEs ::=		SEQUENCE {
	radioResourceConfigDedicated-r13		RadioResourceConfigDedicated	OPTIONAL,	-- Need ON
	nextHopChainingCount-r13				NextHopChainingCount,
	measConfig-r13							MeasConfig						OPTIONAL,	-- Need ON
	antennaInfoDedicatedPCell-r13			AntennaInfoDedicated-v10i0		OPTIONAL,	-- Need ON
	drb-ContinueROHC-r13					ENUMERATED {true}				OPTIONAL,	-- Need OP
	lateNonCriticalExtension				OCTET STRING					OPTIONAL,
	rrcConnectionResume-v1430-IEs			RRCConnectionResume-v1430-IEs	OPTIONAL
}

RRCConnectionResume-v1430-IEs ::= SEQUENCE {
	otherConfig-r14				OtherConfig-r9				OPTIONAL,			-- Need ON
	nonCriticalExtension		SEQUENCE {}					OPTIONAL
}


RRCConnectionResumeComplete-r13 ::= SEQUENCE {
	rrc-TransactionIdentifier				RRC-TransactionIdentifier,
	criticalExtensions							CHOICE {
		rrcConnectionResumeComplete-r13				RRCConnectionResumeComplete-r13-IEs,
		criticalExtensionsFuture					SEQUENCE {}
	}
}

RRCConnectionResumeComplete-r13-IEs ::= SEQUENCE {
	selectedPLMN-Identity-r13			INTEGER (1..maxPLMN-r11)				OPTIONAL,
	dedicatedInfoNAS-r13				DedicatedInfoNAS						OPTIONAL,
	rlf-InfoAvailable-r13				ENUMERATED {true}						OPTIONAL,
	logMeasAvailable-r13				ENUMERATED {true}						OPTIONAL,
	connEstFailInfoAvailable-r13		ENUMERATED {true}						OPTIONAL,
	mobilityState-r13					ENUMERATED {normal, medium, high, spare}	OPTIONAL,
	mobilityHistoryAvail-r13			ENUMERATED {true}						OPTIONAL,
	logMeasAvailableMBSFN-r13			ENUMERATED {true}						OPTIONAL,
	lateNonCriticalExtension			OCTET STRING					OPTIONAL,
	nonCriticalExtension				SEQUENCE {}						OPTIONAL
}


RRCConnectionResumeRequest-r13 ::=	SEQUENCE {
	criticalExtensions						CHOICE {
		rrcConnectionResumeRequest-r13			RRCConnectionResumeRequest-r13-IEs,
		criticalExtensionsFuture				SEQUENCE {}
	}
}

RRCConnectionResumeRequest-r13-IEs ::=		SEQUENCE {
	resumeIdentity-r13								CHOICE {
		resumeID-r13									ResumeIdentity-r13,
		truncatedResumeID-r13							BIT STRING (SIZE (24))
	},
	shortResumeMAC-I-r13								BIT STRING (SIZE (16)),
	resumeCause-r13									ResumeCause,
	spare											BIT STRING (SIZE (1))
}

ResumeCause ::=				ENUMERATED {
										emergency, highPriorityAccess, mt-Access, mo-Signalling,
										mo-Data, delayTolerantAccess-v1020, mo-VoiceCall-v1280, spare1}



RRCConnectionSetup ::=				SEQUENCE {
	rrc-TransactionIdentifier			RRC-TransactionIdentifier,
	criticalExtensions					CHOICE {
		c1									CHOICE {
			rrcConnectionSetup-r8				RRCConnectionSetup-r8-IEs,
			spare7 NULL,
			spare6 NULL, spare5 NULL, spare4 NULL,
			spare3 NULL, spare2 NULL, spare1 NULL
		},
		criticalExtensionsFuture			SEQUENCE {}
	}
}

RRCConnectionSetup-r8-IEs ::=		SEQUENCE {
	radioResourceConfigDedicated		RadioResourceConfigDedicated,
	nonCriticalExtension				RRCConnectionSetup-v8a0-IEs			OPTIONAL
}

RRCConnectionSetup-v8a0-IEs ::= SEQUENCE {
	lateNonCriticalExtension			OCTET STRING						OPTIONAL,
	nonCriticalExtension				SEQUENCE {}							OPTIONAL
}


RRCConnectionSetupComplete ::=		SEQUENCE {
	rrc-TransactionIdentifier			RRC-TransactionIdentifier,
	criticalExtensions					CHOICE {
		c1									CHOICE{
			rrcConnectionSetupComplete-r8		RRCConnectionSetupComplete-r8-IEs,
			spare3 NULL, spare2 NULL, spare1 NULL
		},
		criticalExtensionsFuture			SEQUENCE {}
	}
}

RRCConnectionSetupComplete-r8-IEs ::= SEQUENCE {
	selectedPLMN-Identity				INTEGER (1..maxPLMN-r11),
	registeredMME						RegisteredMME						OPTIONAL,
	dedicatedInfoNAS					DedicatedInfoNAS,
	nonCriticalExtension				RRCConnectionSetupComplete-v8a0-IEs	OPTIONAL
}

RRCConnectionSetupComplete-v8a0-IEs ::= SEQUENCE {
	lateNonCriticalExtension			OCTET STRING						OPTIONAL,
	nonCriticalExtension				RRCConnectionSetupComplete-v1020-IEs	OPTIONAL
}

RRCConnectionSetupComplete-v1020-IEs ::= SEQUENCE {
	gummei-Type-r10						ENUMERATED {native, mapped}			OPTIONAL,
	rlf-InfoAvailable-r10				ENUMERATED {true}					OPTIONAL,
	logMeasAvailable-r10				ENUMERATED {true}					OPTIONAL,
	rn-SubframeConfigReq-r10			ENUMERATED {required, notRequired}	OPTIONAL,
	nonCriticalExtension				RRCConnectionSetupComplete-v1130-IEs	OPTIONAL
}

RRCConnectionSetupComplete-v1130-IEs ::= SEQUENCE {
	connEstFailInfoAvailable-r11		ENUMERATED {true}				OPTIONAL,
	nonCriticalExtension				RRCConnectionSetupComplete-v1250-IEs		OPTIONAL
}

RRCConnectionSetupComplete-v1250-IEs ::= SEQUENCE {
	mobilityState-r12					ENUMERATED {normal, medium, high, spare}	OPTIONAL,
	mobilityHistoryAvail-r12			ENUMERATED {true}				OPTIONAL,
	logMeasAvailableMBSFN-r12			ENUMERATED {true}				OPTIONAL,
	nonCriticalExtension				RRCConnectionSetupComplete-v1320-IEs						OPTIONAL
}

RRCConnectionSetupComplete-v1320-IEs ::= SEQUENCE {
	ce-ModeB-r13						ENUMERATED {supported}						OPTIONAL,
	s-TMSI-r13							S-TMSI										OPTIONAL,
	attachWithoutPDN-Connectivity-r13	ENUMERATED {true}							OPTIONAL,
	up-CIoT-EPS-Optimisation-r13		ENUMERATED {true}							OPTIONAL,
	cp-CIoT-EPS-Optimisation-r13		ENUMERATED {true}							OPTIONAL,
	nonCriticalExtension				RRCConnectionSetupComplete-v1330-IEs		OPTIONAL
}

RRCConnectionSetupComplete-v1330-IEs ::= SEQUENCE {
	ue-CE-NeedULGaps-r13					ENUMERATED {true}				OPTIONAL,
	nonCriticalExtension				RRCConnectionSetupComplete-v1430-IEs		OPTIONAL
}

RRCConnectionSetupComplete-v1430-IEs ::= SEQUENCE {
	dcn-ID-r14							INTEGER (0..65535)				OPTIONAL,
	nonCriticalExtension				SEQUENCE {}						OPTIONAL
}

RegisteredMME ::=					SEQUENCE {
	plmn-Identity						PLMN-Identity						OPTIONAL,
	mmegi								BIT STRING (SIZE (16)),
	mmec								MMEC
}


SCGFailureInformation-r12 ::=		SEQUENCE {
	criticalExtensions					CHOICE {
		c1									CHOICE {
			scgFailureInformation-r12			SCGFailureInformation-r12-IEs,
			spare3 NULL, spare2 NULL, spare1 NULL
		},
		criticalExtensionsFuture			SEQUENCE {}
	}
}

SCGFailureInformation-r12-IEs ::=	SEQUENCE {
	failureReportSCG-r12				FailureReportSCG-r12			OPTIONAL,
	nonCriticalExtension				SCGFailureInformation-v1310-IEs	OPTIONAL
}

SCGFailureInformation-v1310-IEs ::= SEQUENCE {
	lateNonCriticalExtension			OCTET STRING (CONTAINING SCGFailureInformation-v12d0-IEs)						OPTIONAL,
	nonCriticalExtension				SEQUENCE {}							OPTIONAL
}

-- Late non-critical extensions:
SCGFailureInformation-v12d0-IEs ::= SEQUENCE {
	failureReportSCG-v12d0				FailureReportSCG-v12d0				OPTIONAL,	nonCriticalExtension				SEQUENCE {}							OPTIONAL
}

-- Regular non-critical extensions:
FailureReportSCG-r12 ::=			SEQUENCE {
	failureType-r12						ENUMERATED {t313-Expiry, randomAccessProblem,
												rlc-MaxNumRetx, scg-ChangeFailure },
	measResultServFreqList-r12			MeasResultServFreqList-r10		OPTIONAL,
	measResultNeighCells-r12			MeasResultList2EUTRA-r9			OPTIONAL,
	...,
	[[	failureType-v1290				ENUMERATED {maxUL-TimingDiff-v1290}	OPTIONAL
	]],
	[[	measResultServFreqListExt-r13	MeasResultServFreqListExt-r13		OPTIONAL
	]]
}

FailureReportSCG-v12d0 ::= SEQUENCE {
	measResultNeighCells-v12d0			MeasResultList2EUTRA-v9e0			OPTIONAL
}


SCPTMConfiguration-r13 ::=		SEQUENCE {
	sc-mtch-InfoList-r13			SC-MTCH-InfoList-r13,
	scptm-NeighbourCellList-r13		SCPTM-NeighbourCellList-r13			OPTIONAL,	-- Need OP
	lateNonCriticalExtension		OCTET STRING						OPTIONAL,
	nonCriticalExtension			SCPTMConfiguration-v1340							OPTIONAL
}

SCPTMConfiguration-v1340 ::= SEQUENCE {
	p-b-r13								INTEGER (0..3)			OPTIONAL,	-- Need ON
	nonCriticalExtension				SEQUENCE {}				OPTIONAL
}


SCPTMConfiguration-BR-r14 ::=	SEQUENCE {
	sc-mtch-InfoList-r14			SC-MTCH-InfoList-BR-r14,
	scptm-NeighbourCellList-r14		SCPTM-NeighbourCellList-r13			OPTIONAL,	-- Need OP
	p-b-r14							INTEGER (0..3)						OPTIONAL,	-- Need OR
	lateNonCriticalExtension		OCTET STRING						OPTIONAL,
	nonCriticalExtension			SEQUENCE {}							OPTIONAL
}


SecurityModeCommand ::=				SEQUENCE {
	rrc-TransactionIdentifier			RRC-TransactionIdentifier,
	criticalExtensions					CHOICE {
		c1									CHOICE{
			securityModeCommand-r8				SecurityModeCommand-r8-IEs,
			spare3 NULL, spare2 NULL, spare1 NULL
		},
		criticalExtensionsFuture			SEQUENCE {}
	}
}

SecurityModeCommand-r8-IEs ::=		SEQUENCE {
	securityConfigSMC					SecurityConfigSMC,
	nonCriticalExtension				SecurityModeCommand-v8a0-IEs		OPTIONAL
}

SecurityModeCommand-v8a0-IEs ::= SEQUENCE {
	lateNonCriticalExtension			OCTET STRING						OPTIONAL,
	nonCriticalExtension				SEQUENCE {}							OPTIONAL
}

SecurityConfigSMC ::=					SEQUENCE {
	securityAlgorithmConfig					SecurityAlgorithmConfig,
	...
}


SecurityModeComplete ::=			SEQUENCE {
	rrc-TransactionIdentifier			RRC-TransactionIdentifier,
	criticalExtensions					CHOICE {
		securityModeComplete-r8				SecurityModeComplete-r8-IEs,
		criticalExtensionsFuture			SEQUENCE {}
	}
}

SecurityModeComplete-r8-IEs ::=		SEQUENCE {
	nonCriticalExtension				SecurityModeComplete-v8a0-IEs							OPTIONAL
}

SecurityModeComplete-v8a0-IEs ::= SEQUENCE {
	lateNonCriticalExtension			OCTET STRING						OPTIONAL,
	nonCriticalExtension				SEQUENCE {}							OPTIONAL
}


SecurityModeFailure ::=				SEQUENCE {
	rrc-TransactionIdentifier			RRC-TransactionIdentifier,
	criticalExtensions					CHOICE {
		securityModeFailure-r8				SecurityModeFailure-r8-IEs,
		criticalExtensionsFuture			SEQUENCE {}
	}
}

SecurityModeFailure-r8-IEs ::=		SEQUENCE {
	nonCriticalExtension				SecurityModeFailure-v8a0-IEs							OPTIONAL
}

SecurityModeFailure-v8a0-IEs ::= SEQUENCE {
	lateNonCriticalExtension			OCTET STRING						OPTIONAL,
	nonCriticalExtension				SEQUENCE {}							OPTIONAL
}


SidelinkUEInformation-r12 ::=		SEQUENCE {
	criticalExtensions				CHOICE {
		c1								CHOICE {
			sidelinkUEInformation-r12		SidelinkUEInformation-r12-IEs,
			spare3 NULL, spare2 NULL, spare1 NULL
		},
		criticalExtensionsFuture			SEQUENCE {}
	}
}

SidelinkUEInformation-r12-IEs ::=	SEQUENCE {
	commRxInterestedFreq-r12		ARFCN-ValueEUTRA-r9			OPTIONAL,
	commTxResourceReq-r12			SL-CommTxResourceReq-r12	OPTIONAL,
	discRxInterest-r12				ENUMERATED {true}			OPTIONAL,
	discTxResourceReq-r12			INTEGER (1..63)				OPTIONAL,
	lateNonCriticalExtension		OCTET STRING				OPTIONAL,
	nonCriticalExtension			SidelinkUEInformation-v1310-IEs	OPTIONAL
}

SidelinkUEInformation-v1310-IEs ::=	SEQUENCE {
	commTxResourceReqUC-r13		SL-CommTxResourceReq-r12	OPTIONAL,
	commTxResourceInfoReqRelay-r13		SEQUENCE {
		commTxResourceReqRelay-r13		SL-CommTxResourceReq-r12		OPTIONAL,
		commTxResourceReqRelayUC-r13	SL-CommTxResourceReq-r12		OPTIONAL,
		ue-Type-r13						ENUMERATED {relayUE, remoteUE}
	}															OPTIONAL,
	discTxResourceReq-v1310			SEQUENCE {
		carrierFreqDiscTx-r13			INTEGER (1..maxFreq)		OPTIONAL,
		discTxResourceReqAddFreq-r13	SL-DiscTxResourceReqPerFreqList-r13	OPTIONAL
	}															OPTIONAL,
	discTxResourceReqPS-r13			SL-DiscTxResourceReq-r13	OPTIONAL,
	discRxGapReq-r13					SL-GapRequest-r13			OPTIONAL,
	discTxGapReq-r13					SL-GapRequest-r13			OPTIONAL,
	discSysInfoReportFreqList-r13		SL-DiscSysInfoReportFreqList-r13	OPTIONAL,
	nonCriticalExtension			SidelinkUEInformation-v1430-IEs					OPTIONAL
}

SidelinkUEInformation-v1430-IEs ::=	SEQUENCE {
	v2x-CommRxInterestedFreqList-r14	SL-V2X-CommFreqList-r14				OPTIONAL,
	p2x-CommTxType-r14					ENUMERATED {true}					OPTIONAL,
	v2x-CommTxResourceReq-r14			SL-V2X-CommTxFreqList-r14			OPTIONAL,
	nonCriticalExtension				SEQUENCE {}							OPTIONAL
}

SL-CommTxResourceReq-r12 ::=		SEQUENCE {
	carrierFreq-r12					ARFCN-ValueEUTRA-r9			OPTIONAL,
	destinationInfoList-r12			SL-DestinationInfoList-r12
}

SL-DiscTxResourceReqPerFreqList-r13 ::=	SEQUENCE (SIZE (1..maxFreq)) OF SL-DiscTxResourceReq-r13

SL-DiscTxResourceReq-r13 ::=		SEQUENCE {
	carrierFreqDiscTx-r13			INTEGER (1..maxFreq)			OPTIONAL,
	discTxResourceReq-r13			INTEGER (1..63)
}

SL-DestinationInfoList-r12 ::=	SEQUENCE (SIZE (1..maxSL-Dest-r12)) OF SL-DestinationIdentity-r12

SL-DestinationIdentity-r12 ::=	BIT STRING (SIZE (24))

SL-DiscSysInfoReportFreqList-r13 ::=	SEQUENCE (SIZE (1.. maxSL-DiscSysInfoReportFreq-r13)) OF SL-DiscSysInfoReport-r13

SL-V2X-CommFreqList-r14 ::=	SEQUENCE (SIZE (1..maxFreqV2X-r14)) OF INTEGER (0..maxFreqV2X-1-r14)

SL-V2X-CommTxFreqList-r14 ::=	SEQUENCE (SIZE (1..maxFreqV2X-r14)) OF SL-V2X-CommTxResourceReq-r14

SL-V2X-CommTxResourceReq-r14 ::=		SEQUENCE {
	carrierFreqCommTx-r14			INTEGER (0.. maxFreqV2X-1-r14)			OPTIONAL,
	v2x-TypeTxSync-r14				SL-TypeTxSync-r14				OPTIONAL,
	v2x-DestinationInfoList-r14		SL-DestinationInfoList-r12		OPTIONAL
}


SystemInformation-BR-r13 ::=	SystemInformation

SystemInformation-MBMS-r14 ::=	SystemInformation

SystemInformation ::=				SEQUENCE {
	criticalExtensions					CHOICE {
		systemInformation-r8				SystemInformation-r8-IEs,
		criticalExtensionsFuture			SEQUENCE {}
	}
}
SystemInformation-r8-IEs ::=		SEQUENCE {
	sib-TypeAndInfo						SEQUENCE (SIZE (1..maxSIB)) OF CHOICE {
		sib2								SystemInformationBlockType2,
		sib3								SystemInformationBlockType3,
		sib4								SystemInformationBlockType4,
		sib5								SystemInformationBlockType5,
		sib6								SystemInformationBlockType6,
		sib7								SystemInformationBlockType7,
		sib8								SystemInformationBlockType8,
		sib9								SystemInformationBlockType9,
		sib10								SystemInformationBlockType10,
		sib11								SystemInformationBlockType11,
		...,
		sib12-v920							SystemInformationBlockType12-r9,
		sib13-v920							SystemInformationBlockType13-r9,
		sib14-v1130							SystemInformationBlockType14-r11,
		sib15-v1130							SystemInformationBlockType15-r11,
		sib16-v1130							SystemInformationBlockType16-r11,
		sib17-v1250							SystemInformationBlockType17-r12,
		sib18-v1250							SystemInformationBlockType18-r12,
		sib19-v1250							SystemInformationBlockType19-r12,
		sib20-v1310							SystemInformationBlockType20-r13,
		sib21-v1430							SystemInformationBlockType21-r14
	},
	nonCriticalExtension				SystemInformation-v8a0-IEs			OPTIONAL
}

SystemInformation-v8a0-IEs ::= SEQUENCE {
	lateNonCriticalExtension			OCTET STRING						OPTIONAL,
	nonCriticalExtension				SEQUENCE {}							OPTIONAL
}


SystemInformationBlockType1-BR-r13 ::=	SystemInformationBlockType1

SystemInformationBlockType1 ::=		SEQUENCE {
	cellAccessRelatedInfo				SEQUENCE {
		plmn-IdentityList					PLMN-IdentityList,
		trackingAreaCode					TrackingAreaCode,
		cellIdentity						CellIdentity,
		cellBarred							ENUMERATED {barred, notBarred},
		intraFreqReselection				ENUMERATED {allowed, notAllowed},
		csg-Indication						BOOLEAN,
		csg-Identity						CSG-Identity			OPTIONAL	-- Need OR
	},
	cellSelectionInfo					SEQUENCE {
		q-RxLevMin							Q-RxLevMin,
		q-RxLevMinOffset					INTEGER (1..8)			OPTIONAL	-- Need OP
	},
	p-Max								P-Max						OPTIONAL,			-- Need OP
	freqBandIndicator					FreqBandIndicator,
	schedulingInfoList					SchedulingInfoList,
	tdd-Config							TDD-Config					OPTIONAL,	-- Cond TDD
	si-WindowLength						ENUMERATED {
											ms1, ms2, ms5, ms10, ms15, ms20,
											ms40},
	systemInfoValueTag					INTEGER (0..31),
	nonCriticalExtension				SystemInformationBlockType1-v890-IEs	OPTIONAL
}

SystemInformationBlockType1-v890-IEs::=	SEQUENCE {
	lateNonCriticalExtension			OCTET STRING (CONTAINING SystemInformationBlockType1-v8h0-IEs)			OPTIONAL,
	nonCriticalExtension				SystemInformationBlockType1-v920-IEs	OPTIONAL
}

-- Late non critical extensions
SystemInformationBlockType1-v8h0-IEs ::=	SEQUENCE {
	multiBandInfoList					MultiBandInfoList		OPTIONAL,	-- Need OR
	nonCriticalExtension				SystemInformationBlockType1-v9e0-IEs	OPTIONAL
}

SystemInformationBlockType1-v9e0-IEs ::= SEQUENCE {
	freqBandIndicator-v9e0				FreqBandIndicator-v9e0		OPTIONAL,	-- Cond FBI-max
	multiBandInfoList-v9e0				MultiBandInfoList-v9e0		OPTIONAL,	-- Cond mFBI-max
	nonCriticalExtension				SystemInformationBlockType1-v10j0-IEs	OPTIONAL
}

SystemInformationBlockType1-v10j0-IEs ::= SEQUENCE {
	freqBandInfo-r10					NS-PmaxList-r10				OPTIONAL,	-- Need OR
	multiBandInfoList-v10j0				MultiBandInfoList-v10j0		OPTIONAL,	-- Need OR
	nonCriticalExtension				SystemInformationBlockType1-v10l0-IEs					OPTIONAL
}

SystemInformationBlockType1-v10l0-IEs ::= SEQUENCE {
	freqBandInfo-v10l0					NS-PmaxList-v10l0			OPTIONAL,	-- Need OR
	multiBandInfoList-v10l0				MultiBandInfoList-v10l0		OPTIONAL,	-- Need OR
	nonCriticalExtension				SEQUENCE {}					OPTIONAL
}

-- Regular non critical extensions
SystemInformationBlockType1-v920-IEs ::=	SEQUENCE {
	ims-EmergencySupport-r9				ENUMERATED {true}			OPTIONAL,	-- Need OR
	cellSelectionInfo-v920				CellSelectionInfo-v920		OPTIONAL,	-- Cond RSRQ
	nonCriticalExtension				SystemInformationBlockType1-v1130-IEs	OPTIONAL
}

SystemInformationBlockType1-v1130-IEs ::=	SEQUENCE {
	tdd-Config-v1130				TDD-Config-v1130			OPTIONAL,	-- Cond TDD-OR
	cellSelectionInfo-v1130			CellSelectionInfo-v1130		OPTIONAL,	-- Cond WB-RSRQ
	nonCriticalExtension			SystemInformationBlockType1-v1250-IEs	OPTIONAL
}

SystemInformationBlockType1-v1250-IEs ::=	SEQUENCE {
	cellAccessRelatedInfo-v1250					SEQUENCE {
		category0Allowed-r12						ENUMERATED {true}		OPTIONAL	-- Need OP
	},
	cellSelectionInfo-v1250					CellSelectionInfo-v1250		OPTIONAL,	-- Cond RSRQ2
	freqBandIndicatorPriority-r12			ENUMERATED {true}			OPTIONAL,	-- Cond mFBI
	nonCriticalExtension			SystemInformationBlockType1-v1310-IEs	OPTIONAL
}

SystemInformationBlockType1-v1310-IEs ::=	SEQUENCE {
	hyperSFN-r13								BIT STRING (SIZE (10))		OPTIONAL,	-- Need OR
	eDRX-Allowed-r13							ENUMERATED {true}			OPTIONAL,	-- Need OR
	cellSelectionInfoCE-r13					CellSelectionInfoCE-r13	OPTIONAL,	-- Need OP
	bandwidthReducedAccessRelatedInfo-r13	SEQUENCE {
		si-WindowLength-BR-r13					ENUMERATED {
													ms20, ms40, ms60, ms80, ms120,
													ms160, ms200, spare},
		si-RepetitionPattern-r13				ENUMERATED {everyRF, every2ndRF, every4thRF,
															every8thRF},
		schedulingInfoList-BR-r13				SchedulingInfoList-BR-r13	OPTIONAL,	-- Cond SI-BR
		fdd-DownlinkOrTddSubframeBitmapBR-r13	CHOICE {
			subframePattern10-r13					BIT STRING (SIZE (10)),
			subframePattern40-r13					BIT STRING (SIZE (40))
		}																	OPTIONAL,	-- Need OP
		fdd-UplinkSubframeBitmapBR-r13			BIT STRING (SIZE (10))		OPTIONAL,	-- Need OP
		startSymbolBR-r13						INTEGER (1..4),
		si-HoppingConfigCommon-r13				ENUMERATED {on,off},
		si-ValidityTime-r13						ENUMERATED {true}	OPTIONAL,			-- Need OP
		systemInfoValueTagList-r13				SystemInfoValueTagList-r13	OPTIONAL	-- Need OR
	}																OPTIONAL,	-- Cond BW-reduced
	nonCriticalExtension						SystemInformationBlockType1-v1320-IEs	OPTIONAL
}

SystemInformationBlockType1-v1320-IEs ::=	SEQUENCE {
	freqHoppingParametersDL-r13				SEQUENCE {
		mpdcch-pdsch-HoppingNB-r13				ENUMERATED {nb2, nb4}		OPTIONAL,	-- Need OR
		interval-DLHoppingConfigCommonModeA-r13	CHOICE {
			interval-FDD-r13					ENUMERATED {int1, int2, int4, int8},
			interval-TDD-r13					ENUMERATED {int1, int5, int10, int20}
		}																	OPTIONAL,	-- Need OR
		interval-DLHoppingConfigCommonModeB-r13	CHOICE {
			interval-FDD-r13					ENUMERATED {int2, int4, int8, int16},
			interval-TDD-r13					ENUMERATED { int5, int10, int20, int40}
		}																	OPTIONAL,	-- Need OR
		mpdcch-pdsch-HoppingOffset-r13			INTEGER (1..maxAvailNarrowBands-r13)	OPTIONAL	-- Need OR
	}																OPTIONAL,	-- Cond Hopping
	nonCriticalExtension						SystemInformationBlockType1-v1350-IEs					OPTIONAL
}

SystemInformationBlockType1-v1350-IEs ::=	SEQUENCE {
	cellSelectionInfoCE1-r13				CellSelectionInfoCE1-r13	OPTIONAL,	-- Need OP
	nonCriticalExtension					SystemInformationBlockType1-v1360-IEs				OPTIONAL
}

SystemInformationBlockType1-v1360-IEs ::=	SEQUENCE {
	cellSelectionInfoCE1-v1360				CellSelectionInfoCE1-v1360	OPTIONAL,	-- Cond QrxlevminCE1
	nonCriticalExtension						SystemInformationBlockType1-v1430-IEs		OPTIONAL
}

SystemInformationBlockType1-v1430-IEs ::=	SEQUENCE {
	eCallOverIMS-Support-r14				ENUMERATED {true}			OPTIONAL,	-- Need OR
	tdd-Config-v1430						TDD-Config-v1430			OPTIONAL,	-- Cond TDD-OR
	cellAccessRelatedInfoList-r14			SEQUENCE (SIZE (1..maxPLMN-1-r14)) OF
											CellAccessRelatedInfo-r14	OPTIONAL,	-- Need OR
	nonCriticalExtension					SystemInformationBlockType1-v1450-IEs				OPTIONAL
}

SystemInformationBlockType1-v1450-IEs ::=	SEQUENCE {
	tdd-Config-v1450						TDD-Config-v1450		OPTIONAL,	-- Cond TDD-OR
	nonCriticalExtension					SEQUENCE {}					OPTIONAL
}

PLMN-IdentityList ::=					SEQUENCE (SIZE (1..maxPLMN-r11)) OF PLMN-IdentityInfo

PLMN-IdentityInfo ::=					SEQUENCE {
	plmn-Identity							PLMN-Identity,
	cellReservedForOperatorUse				ENUMERATED {reserved, notReserved}
}

SchedulingInfoList ::= SEQUENCE (SIZE (1..maxSI-Message)) OF SchedulingInfo

SchedulingInfo ::=	SEQUENCE {
	si-Periodicity						ENUMERATED {
											rf8, rf16, rf32, rf64, rf128, rf256, rf512},
	sib-MappingInfo						SIB-MappingInfo
}

SchedulingInfoList-BR-r13 ::= SEQUENCE (SIZE (1..maxSI-Message)) OF SchedulingInfo-BR-r13

SchedulingInfo-BR-r13 ::=	SEQUENCE {
	si-Narrowband-r13				INTEGER (1..maxAvailNarrowBands-r13),
	si-TBS-r13						ENUMERATED {b152, b208, b256, b328, b408, b504, b600, b712,
												b808, b936}
}

SIB-MappingInfo ::= SEQUENCE (SIZE (0..maxSIB-1)) OF SIB-Type

SIB-Type ::=						ENUMERATED {
										sibType3, sibType4, sibType5, sibType6,
										sibType7, sibType8, sibType9, sibType10,
										sibType11, sibType12-v920, sibType13-v920,
										sibType14-v1130, sibType15-v1130,
										sibType16-v1130, sibType17-v1250, sibType18-v1250,
										..., sibType19-v1250, sibType20-v1310, sibType21-v1430}

SystemInfoValueTagList-r13 ::=		SEQUENCE (SIZE (1..maxSI-Message)) OF SystemInfoValueTagSI-r13

SystemInfoValueTagSI-r13 ::=		INTEGER (0..3)

CellSelectionInfo-v920 ::=			SEQUENCE {
	q-QualMin-r9						Q-QualMin-r9,
	q-QualMinOffset-r9					INTEGER (1..8)						OPTIONAL	-- Need OP
}

CellSelectionInfo-v1130 ::=			SEQUENCE {
	q-QualMinWB-r11						Q-QualMin-r9
}

CellSelectionInfo-v1250 ::=			SEQUENCE {
	q-QualMinRSRQ-OnAllSymbols-r12						Q-QualMin-r9
}

CellAccessRelatedInfo-r14 ::=	SEQUENCE {
	plmn-IdentityList-r14				PLMN-IdentityList,
	trackingAreaCode-r14				TrackingAreaCode,
	cellIdentity-r14					CellIdentity
}


SystemInformationBlockType1-MBMS-r14 ::=	SEQUENCE {
	cellAccessRelatedInfo-r14				SEQUENCE {
		plmn-IdentityList-r14					PLMN-IdentityList-MBMS-r14,
		trackingAreaCode-r14						TrackingAreaCode,
		cellIdentity-r14							CellIdentity
	},
	freqBandIndicator-r14					FreqBandIndicator-r11,
	multiBandInfoList-r14					MultiBandInfoList-r11				OPTIONAL, -- Need OR
	schedulingInfoList-MBMS-r14			SchedulingInfoList-MBMS-r14,
	si-WindowLength-r14						ENUMERATED {
												ms1, ms2, ms5, ms10, ms15, ms20,ms40, ms80},
	systemInfoValueTag-r14					INTEGER (0..31),
	nonMBSFN-SubframeConfig-r14				NonMBSFN-SubframeConfig-r14		OPTIONAL, --Need OR
	pdsch-ConfigCommon-r14					PDSCH-ConfigCommon,
	systemInformationBlockType13-r14		SystemInformationBlockType13-r9	OPTIONAL, --Need OR
	cellAccessRelatedInfoList-r14		SEQUENCE (SIZE (1..maxPLMN-1-r14)) OF
											CellAccessRelatedInfo-r14	OPTIONAL,	-- Need OR
	nonCriticalExtension					SEQUENCE {}							OPTIONAL
}

PLMN-IdentityList-MBMS-r14 ::=				SEQUENCE (SIZE (1..maxPLMN-r11)) OF PLMN-Identity

SchedulingInfoList-MBMS-r14 ::= SEQUENCE (SIZE (1..maxSI-Message)) OF SchedulingInfo-MBMS-r14

SchedulingInfo-MBMS-r14 ::=	SEQUENCE {
	si-Periodicity-r14						ENUMERATED {
												rf16, rf32, rf64, rf128, rf256, rf512},
	sib-MappingInfo-r14						SIB-MappingInfo-MBMS-r14
}

SIB-MappingInfo-MBMS-r14 ::= SEQUENCE (SIZE (0..maxSIB-1)) OF SIB-Type-MBMS-r14

SIB-Type-MBMS-r14 ::=					ENUMERATED {
											sibType10, sibType11, sibType12-v920, sibType13-v920,
											sibType15-v1130, sibType16-v1130, ...}


NonMBSFN-SubframeConfig-r14 ::=			SEQUENCE {
	radioFrameAllocationPeriod-r14		ENUMERATED {rf4, rf8, rf16, rf32, rf64, rf128, rf512},
	radioFrameAllocationOffset-r14		INTEGER (0..7),
	subframeAllocation-r14				BIT STRING (SIZE(9))
}


UEAssistanceInformation-r11 ::=				SEQUENCE {
	criticalExtensions					CHOICE {
		c1									CHOICE {
			ueAssistanceInformation-r11			UEAssistanceInformation-r11-IEs,
			spare3 NULL, spare2 NULL, spare1 NULL
		},
		criticalExtensionsFuture			SEQUENCE {}
	}
}

UEAssistanceInformation-r11-IEs ::=		SEQUENCE {
	powerPrefIndication-r11				ENUMERATED	{normal, lowPowerConsumption}	OPTIONAL,
	lateNonCriticalExtension			OCTET STRING									OPTIONAL,
	nonCriticalExtension				UEAssistanceInformation-v1430-IEs			OPTIONAL
}

UEAssistanceInformation-v1430-IEs ::=		SEQUENCE	{
	bw-Preference-r14					BW-Preference-r14									OPTIONAL,
	sps-AssistanceInformation-r14		SEQUENCE {
		trafficPatternInfoListSL-r14		TrafficPatternInfoList-r14		OPTIONAL,
		trafficPatternInfoListUL-r14		TrafficPatternInfoList-r14		OPTIONAL
	}			OPTIONAL,
	rlm-Report-r14						SEQUENCE {
		rlm-Event-r14						ENUMERATED {earlyOutOfSync, earlyInSync},
		excessRep-MPDCCH-r14				ENUMERATED {excessRep1, excessRep2}		OPTIONAL
	}																				OPTIONAL,	delayBudgetReport-r14				DelayBudgetReport-r14						OPTIONAL,
	nonCriticalExtension				UEAssistanceInformation-v1450-IEs			OPTIONAL
}

UEAssistanceInformation-v1450-IEs ::=		SEQUENCE {
	overheatingAssistance-r14				OverheatingAssistance-r14				OPTIONAL,
	nonCriticalExtension					SEQUENCE {}								OPTIONAL
}

BW-Preference-r14 ::= SEQUENCE {
	dl-Preference-r14		ENUMERATED	{mhz1dot4, mhz5, mhz20 }						OPTIONAL,
	ul-Preference-r14		ENUMERATED	{mhz1dot4, mhz5}						OPTIONAL
}

TrafficPatternInfoList-r14 ::= SEQUENCE (SIZE (1..maxTrafficPattern-r14)) OF TrafficPatternInfo-r14

TrafficPatternInfo-r14 ::=	SEQUENCE {
	trafficPeriodicity-r14			ENUMERATED {
											sf20, sf50, sf100, sf200, sf300, sf400, sf500,
											sf600, sf700, sf800, sf900, sf1000},
	timingOffset-r14					INTEGER (0..10239),
	priorityInfoSL-r14					SL-Priority-r13								OPTIONAL,
	logicalChannelIdentityUL-r14		INTEGER (3..10)								OPTIONAL,
	messageSize-r14					BIT STRING (SIZE (6))
}

DelayBudgetReport-r14::=	CHOICE {
	type1							ENUMERATED {
										msMinus1280, msMinus640, msMinus320, msMinus160,
										msMinus80, msMinus60, msMinus40, msMinus20, ms0, ms20,												ms40, ms60, ms80, ms160, ms320, ms640, ms1280},

	type2							ENUMERATED {
										msMinus192, msMinus168,msMinus144, msMinus120,
										msMinus96, msMinus72, msMinus48, msMinus24, ms0, ms24,												ms48, ms72, ms96, ms120, ms144, ms168, ms192}
}

OverheatingAssistance-r14 ::=	SEQUENCE {
		reducedUE-Category			SEQUENCE {
			reducedUE-CategoryDL				INTEGER (0..19),
			reducedUE-CategoryUL				INTEGER (0..21)
		}		OPTIONAL,
		reducedMaxCCs				SEQUENCE {
			reducedCCsDL						INTEGER (0..31),
			reducedCCsUL						INTEGER (0..31)
		}		OPTIONAL
}


UECapabilityEnquiry ::=				SEQUENCE {
	rrc-TransactionIdentifier			RRC-TransactionIdentifier,
	criticalExtensions					CHOICE {
		c1									CHOICE {
			ueCapabilityEnquiry-r8				UECapabilityEnquiry-r8-IEs,
			spare3 NULL, spare2 NULL, spare1 NULL
		},
		criticalExtensionsFuture			SEQUENCE {}
	}
}

UECapabilityEnquiry-r8-IEs ::=		SEQUENCE {
	ue-CapabilityRequest				UE-CapabilityRequest,
	nonCriticalExtension				UECapabilityEnquiry-v8a0-IEs		OPTIONAL
}

UECapabilityEnquiry-v8a0-IEs ::=	SEQUENCE {
	lateNonCriticalExtension			OCTET STRING						OPTIONAL,
	nonCriticalExtension				UECapabilityEnquiry-v1180-IEs							OPTIONAL
}

UECapabilityEnquiry-v1180-IEs ::=	SEQUENCE {
	requestedFrequencyBands-r11			SEQUENCE (SIZE (1..16)) OF FreqBandIndicator-r11							OPTIONAL,
	nonCriticalExtension				UECapabilityEnquiry-v1310-IEs							OPTIONAL
}

UECapabilityEnquiry-v1310-IEs ::=	SEQUENCE {
	requestReducedFormat-r13			ENUMERATED {true}					OPTIONAL,	-- Need ON
	requestSkipFallbackComb-r13		ENUMERATED {true}					OPTIONAL,	-- Need ON
	requestedMaxCCsDL-r13				INTEGER (2..32)					OPTIONAL,	-- Need ON
	requestedMaxCCsUL-r13				INTEGER (2..32)					OPTIONAL,	-- Need ON
	requestReducedIntNonContComb-r13	ENUMERATED {true}					OPTIONAL,	-- Need ON
	nonCriticalExtension				UECapabilityEnquiry-v1430-IEs		OPTIONAL
}

UECapabilityEnquiry-v1430-IEs ::=	SEQUENCE {
	requestDiffFallbackCombList-r14		BandCombinationList-r14			OPTIONAL,	-- Need ON
	nonCriticalExtension				SEQUENCE {}						OPTIONAL
}

UE-CapabilityRequest ::=			SEQUENCE (SIZE (1..maxRAT-Capabilities)) OF RAT-Type


UECapabilityInformation ::=			SEQUENCE {
	rrc-TransactionIdentifier			RRC-TransactionIdentifier,
	criticalExtensions					CHOICE {
		c1									CHOICE{
			ueCapabilityInformation-r8			UECapabilityInformation-r8-IEs,
			spare7 NULL,
			spare6 NULL, spare5 NULL, spare4 NULL,
			spare3 NULL, spare2 NULL, spare1 NULL
		},
		criticalExtensionsFuture			SEQUENCE {}
	}
}

UECapabilityInformation-r8-IEs ::=	SEQUENCE {
	ue-CapabilityRAT-ContainerList		UE-CapabilityRAT-ContainerList,
	nonCriticalExtension				UECapabilityInformation-v8a0-IEs	OPTIONAL
}

UECapabilityInformation-v8a0-IEs ::= SEQUENCE {
	lateNonCriticalExtension			OCTET STRING						OPTIONAL,
	nonCriticalExtension				UECapabilityInformation-v1250-IEs	OPTIONAL
}

UECapabilityInformation-v1250-IEs ::= SEQUENCE {
	ue-RadioPagingInfo-r12				UE-RadioPagingInfo-r12				OPTIONAL,
	nonCriticalExtension				SEQUENCE {}							OPTIONAL
}


UEInformationRequest-r9		::=				SEQUENCE {
	rrc-TransactionIdentifier		RRC-TransactionIdentifier,
	criticalExtensions				CHOICE {
		c1								CHOICE {
			ueInformationRequest-r9				UEInformationRequest-r9-IEs,
			spare3 NULL, spare2 NULL, spare1 NULL
		},
		criticalExtensionsFuture			SEQUENCE {}
	}
}

UEInformationRequest-r9-IEs ::=		SEQUENCE {
	rach-ReportReq-r9					BOOLEAN,
	rlf-ReportReq-r9					BOOLEAN,
	nonCriticalExtension				UEInformationRequest-v930-IEs		OPTIONAL
}

UEInformationRequest-v930-IEs ::= SEQUENCE {
	lateNonCriticalExtension			OCTET STRING						OPTIONAL,
	nonCriticalExtension				UEInformationRequest-v1020-IEs		OPTIONAL
}

UEInformationRequest-v1020-IEs ::=	SEQUENCE {
	logMeasReportReq-r10				ENUMERATED {true}					OPTIONAL,	-- Need ON
	nonCriticalExtension				UEInformationRequest-v1130-IEs		OPTIONAL
}

UEInformationRequest-v1130-IEs ::= SEQUENCE {
	connEstFailReportReq-r11			ENUMERATED {true}					OPTIONAL,	-- Need ON
	nonCriticalExtension				UEInformationRequest-v1250-IEs		OPTIONAL
}

UEInformationRequest-v1250-IEs ::= SEQUENCE {
	mobilityHistoryReportReq-r12		ENUMERATED {true}					OPTIONAL,	-- Need ON
	nonCriticalExtension				SEQUENCE {}							OPTIONAL
}


UEInformationResponse-r9	::=			SEQUENCE {
	rrc-TransactionIdentifier			RRC-TransactionIdentifier,
	criticalExtensions					CHOICE {
		c1								CHOICE {
			ueInformationResponse-r9				UEInformationResponse-r9-IEs,
			spare3 NULL, spare2 NULL, spare1 NULL
		},
		criticalExtensionsFuture				SEQUENCE {}
	}
}

UEInformationResponse-r9-IEs ::=		SEQUENCE {
	rach-Report-r9							SEQUENCE {
		numberOfPreamblesSent-r9				NumberOfPreamblesSent-r11,
		contentionDetected-r9					BOOLEAN
	}																OPTIONAL,
	rlf-Report-r9							RLF-Report-r9			OPTIONAL,
	nonCriticalExtension					UEInformationResponse-v930-IEs				OPTIONAL
}

-- Late non critical extensions
UEInformationResponse-v9e0-IEs ::= SEQUENCE {
	rlf-Report-v9e0						RLF-Report-v9e0					OPTIONAL,
	nonCriticalExtension				SEQUENCE {}						OPTIONAL
}

-- Regular non critical extensions
UEInformationResponse-v930-IEs ::=	SEQUENCE {
	lateNonCriticalExtension			OCTET STRING (CONTAINING UEInformationResponse-v9e0-IEs)	OPTIONAL,
	nonCriticalExtension				UEInformationResponse-v1020-IEs		OPTIONAL
}

UEInformationResponse-v1020-IEs ::= SEQUENCE {
	logMeasReport-r10					LogMeasReport-r10				OPTIONAL,
	nonCriticalExtension				UEInformationResponse-v1130-IEs		OPTIONAL
}

UEInformationResponse-v1130-IEs ::= SEQUENCE {
	connEstFailReport-r11				ConnEstFailReport-r11			OPTIONAL,
	nonCriticalExtension				UEInformationResponse-v1250-IEs	OPTIONAL
}

UEInformationResponse-v1250-IEs ::= SEQUENCE {
	mobilityHistoryReport-r12			MobilityHistoryReport-r12		OPTIONAL,
	nonCriticalExtension				SEQUENCE {}						OPTIONAL
}

RLF-Report-r9 ::=					SEQUENCE {
	measResultLastServCell-r9				SEQUENCE {
		rsrpResult-r9							RSRP-Range,
		rsrqResult-r9							RSRQ-Range			OPTIONAL
	},
	measResultNeighCells-r9				SEQUENCE {
		measResultListEUTRA-r9				MeasResultList2EUTRA-r9			OPTIONAL,
		measResultListUTRA-r9				MeasResultList2UTRA-r9			OPTIONAL,
		measResultListGERAN-r9				MeasResultListGERAN				OPTIONAL,
		measResultsCDMA2000-r9				MeasResultList2CDMA2000-r9		OPTIONAL
	}	OPTIONAL,
	...,
	[[	locationInfo-r10				LocationInfo-r10		OPTIONAL,
		failedPCellId-r10						CHOICE {
			cellGlobalId-r10						CellGlobalIdEUTRA,
			pci-arfcn-r10							SEQUENCE {
				physCellId-r10							PhysCellId,
				carrierFreq-r10							ARFCN-ValueEUTRA
			}
		}																OPTIONAL,
		reestablishmentCellId-r10		CellGlobalIdEUTRA				OPTIONAL,
		timeConnFailure-r10				INTEGER (0..1023)				OPTIONAL,
		connectionFailureType-r10		ENUMERATED {rlf, hof}			OPTIONAL,
		previousPCellId-r10				CellGlobalIdEUTRA				OPTIONAL
	]],
	[[	failedPCellId-v1090				SEQUENCE {
			carrierFreq-v1090				ARFCN-ValueEUTRA-v9e0
		}																OPTIONAL
	]],
	[[	basicFields-r11					SEQUENCE {
			c-RNTI-r11						C-RNTI,
			rlf-Cause-r11					ENUMERATED {
												t310-Expiry, randomAccessProblem,
												rlc-MaxNumRetx, t312-Expiry-r12},
			timeSinceFailure-r11			TimeSinceFailure-r11
		}																OPTIONAL,
		previousUTRA-CellId-r11			SEQUENCE {
			carrierFreq-r11					ARFCN-ValueUTRA,
			physCellId-r11					CHOICE {
				fdd-r11							PhysCellIdUTRA-FDD,
				tdd-r11							PhysCellIdUTRA-TDD
			},
			cellGlobalId-r11				CellGlobalIdUTRA			OPTIONAL
		}																OPTIONAL,
		selectedUTRA-CellId-r11			SEQUENCE {
			carrierFreq-r11					ARFCN-ValueUTRA,
			physCellId-r11					CHOICE {
				fdd-r11							PhysCellIdUTRA-FDD,
				tdd-r11							PhysCellIdUTRA-TDD
			}
		}																OPTIONAL
	]],
	[[	failedPCellId-v1250				SEQUENCE {
			tac-FailedPCell-r12			TrackingAreaCode
		}																OPTIONAL,
		measResultLastServCell-v1250	RSRQ-Range-v1250				OPTIONAL,
		lastServCellRSRQ-Type-r12		RSRQ-Type-r12					OPTIONAL,
		measResultListEUTRA-v1250		MeasResultList2EUTRA-v1250		OPTIONAL
	]],
	[[	drb-EstablishedWithQCI-1-r13			ENUMERATED {qci1}				OPTIONAL
	]],
	[[	measResultLastServCell-v1360			RSRP-Range-v1360				OPTIONAL
	]]
}

RLF-Report-v9e0 ::=				SEQUENCE {
	measResultListEUTRA-v9e0			MeasResultList2EUTRA-v9e0
}

MeasResultList2EUTRA-r9 ::=				SEQUENCE (SIZE (1..maxFreq)) OF MeasResult2EUTRA-r9

MeasResultList2EUTRA-v9e0 ::=			SEQUENCE (SIZE (1..maxFreq)) OF MeasResult2EUTRA-v9e0

MeasResultList2EUTRA-v1250 ::=			SEQUENCE (SIZE (1..maxFreq)) OF MeasResult2EUTRA-v1250

MeasResult2EUTRA-r9 ::=				SEQUENCE {
	carrierFreq-r9						ARFCN-ValueEUTRA,
	measResultList-r9					MeasResultListEUTRA
}

MeasResult2EUTRA-v9e0 ::=				SEQUENCE {
	carrierFreq-v9e0						ARFCN-ValueEUTRA-v9e0		OPTIONAL
}

MeasResult2EUTRA-v1250 ::=				SEQUENCE {
	rsrq-Type-r12							RSRQ-Type-r12		OPTIONAL
}

MeasResultList2UTRA-r9 ::=			SEQUENCE (SIZE (1..maxFreq)) OF MeasResult2UTRA-r9

MeasResult2UTRA-r9 ::=				SEQUENCE {
	carrierFreq-r9						ARFCN-ValueUTRA,
	measResultList-r9					MeasResultListUTRA
}

MeasResultList2CDMA2000-r9 ::=		SEQUENCE (SIZE (1..maxFreq)) OF MeasResult2CDMA2000-r9

MeasResult2CDMA2000-r9 ::=			SEQUENCE {
	carrierFreq-r9						CarrierFreqCDMA2000,
	measResultList-r9					MeasResultsCDMA2000
}

LogMeasReport-r10 ::=				SEQUENCE {
	absoluteTimeStamp-r10				AbsoluteTimeInfo-r10,
	traceReference-r10					TraceReference-r10,
	traceRecordingSessionRef-r10		OCTET STRING (SIZE (2)),
	tce-Id-r10							OCTET STRING (SIZE (1)),
	logMeasInfoList-r10					LogMeasInfoList-r10,
	logMeasAvailable-r10				ENUMERATED {true}				OPTIONAL,
	...
}

LogMeasInfoList-r10 ::=		SEQUENCE (SIZE (1..maxLogMeasReport-r10)) OF LogMeasInfo-r10

LogMeasInfo-r10 ::=		SEQUENCE {
	locationInfo-r10					LocationInfo-r10		OPTIONAL,
	relativeTimeStamp-r10				INTEGER (0..7200),
	servCellIdentity-r10				CellGlobalIdEUTRA,
	measResultServCell-r10				SEQUENCE {
		rsrpResult-r10						RSRP-Range,
		rsrqResult-r10						RSRQ-Range
	},
	measResultNeighCells-r10			SEQUENCE {
		measResultListEUTRA-r10				MeasResultList2EUTRA-r9		OPTIONAL,
		measResultListUTRA-r10				MeasResultList2UTRA-r9		OPTIONAL,
		measResultListGERAN-r10				MeasResultList2GERAN-r10	OPTIONAL,
		measResultListCDMA2000-r10			MeasResultList2CDMA2000-r9	OPTIONAL
	}	OPTIONAL,
	...,
	[[	measResultListEUTRA-v1090			MeasResultList2EUTRA-v9e0	OPTIONAL
	]],
	[[	measResultListMBSFN-r12				MeasResultListMBSFN-r12	OPTIONAL,
		measResultServCell-v1250			RSRQ-Range-v1250			OPTIONAL,
		servCellRSRQ-Type-r12				RSRQ-Type-r12				OPTIONAL,
		measResultListEUTRA-v1250			MeasResultList2EUTRA-v1250	OPTIONAL
	]],
	[[	inDeviceCoexDetected-r13			ENUMERATED {true}			OPTIONAL
	]],
	[[	measResultServCell-v1360			RSRP-Range-v1360			OPTIONAL
	]]
}

MeasResultListMBSFN-r12 ::=			SEQUENCE (SIZE (1..maxMBSFN-Area)) OF MeasResultMBSFN-r12

MeasResultMBSFN-r12 ::=			SEQUENCE {
	mbsfn-Area-r12							SEQUENCE {
		mbsfn-AreaId-r12						MBSFN-AreaId-r12,
		carrierFreq-r12							ARFCN-ValueEUTRA-r9
	},
	rsrpResultMBSFN-r12						RSRP-Range,
	rsrqResultMBSFN-r12						MBSFN-RSRQ-Range-r12,
	signallingBLER-Result-r12				BLER-Result-r12				OPTIONAL,
	dataBLER-MCH-ResultList-r12				DataBLER-MCH-ResultList-r12	OPTIONAL,
	...
}

DataBLER-MCH-ResultList-r12 ::=			SEQUENCE (SIZE (1.. maxPMCH-PerMBSFN)) OF DataBLER-MCH-Result-r12

DataBLER-MCH-Result-r12 ::=			SEQUENCE {
	mch-Index-r12							INTEGER (1..maxPMCH-PerMBSFN),
	dataBLER-Result-r12						BLER-Result-r12
}

BLER-Result-r12 ::=					SEQUENCE {
	bler-r12									BLER-Range-r12,
	blocksReceived-r12						SEQUENCE {
		n-r12									BIT STRING (SIZE (3)),
		m-r12									BIT STRING (SIZE (8))
	}
}

BLER-Range-r12 ::=						INTEGER(0..31)

MeasResultList2GERAN-r10 ::=			SEQUENCE (SIZE (1..maxCellListGERAN)) OF MeasResultListGERAN

ConnEstFailReport-r11 ::=				SEQUENCE {
	failedCellId-r11					CellGlobalIdEUTRA,
	locationInfo-r11					LocationInfo-r10				OPTIONAL,
	measResultFailedCell-r11				SEQUENCE {
		rsrpResult-r11							RSRP-Range,
		rsrqResult-r11							RSRQ-Range				OPTIONAL
	},
	measResultNeighCells-r11				SEQUENCE {
		measResultListEUTRA-r11				MeasResultList2EUTRA-r9			OPTIONAL,
		measResultListUTRA-r11				MeasResultList2UTRA-r9			OPTIONAL,
		measResultListGERAN-r11				MeasResultListGERAN				OPTIONAL,
		measResultsCDMA2000-r11				MeasResultList2CDMA2000-r9		OPTIONAL
	}	OPTIONAL,
	numberOfPreamblesSent-r11			NumberOfPreamblesSent-r11,
	contentionDetected-r11				BOOLEAN,
	maxTxPowerReached-r11				BOOLEAN,
	timeSinceFailure-r11				TimeSinceFailure-r11,
	measResultListEUTRA-v1130			MeasResultList2EUTRA-v9e0		OPTIONAL,
	...,
	[[	measResultFailedCell-v1250		RSRQ-Range-v1250				OPTIONAL,
		failedCellRSRQ-Type-r12			RSRQ-Type-r12					OPTIONAL,
		measResultListEUTRA-v1250		MeasResultList2EUTRA-v1250		OPTIONAL
	]],
	[[	measResultFailedCell-v1360		RSRP-Range-v1360			OPTIONAL
	]]
}

NumberOfPreamblesSent-r11::=			INTEGER (1..200)

TimeSinceFailure-r11 ::=				INTEGER (0..172800)

MobilityHistoryReport-r12 ::=	VisitedCellInfoList-r12


ULHandoverPreparationTransfer ::=	SEQUENCE {
	criticalExtensions					CHOICE {
		c1									CHOICE {
			ulHandoverPreparationTransfer-r8		ULHandoverPreparationTransfer-r8-IEs,
			spare3 NULL, spare2 NULL, spare1 NULL
		},
		criticalExtensionsFuture				SEQUENCE {}
	}
}

ULHandoverPreparationTransfer-r8-IEs ::= SEQUENCE {
	cdma2000-Type						CDMA2000-Type,
	meid								BIT STRING (SIZE (56))	OPTIONAL,
	dedicatedInfo						DedicatedInfoCDMA2000,
	nonCriticalExtension				ULHandoverPreparationTransfer-v8a0-IEs	OPTIONAL
}

ULHandoverPreparationTransfer-v8a0-IEs ::= SEQUENCE {
	lateNonCriticalExtension			OCTET STRING						OPTIONAL,
	nonCriticalExtension				SEQUENCE {}							OPTIONAL
}


ULInformationTransfer ::=			SEQUENCE {
	criticalExtensions					CHOICE {
		c1									CHOICE {
			ulInformationTransfer-r8			ULInformationTransfer-r8-IEs,
			spare3 NULL, spare2 NULL, spare1 NULL
		},
		criticalExtensionsFuture			SEQUENCE {}
	}
}

ULInformationTransfer-r8-IEs ::=	SEQUENCE {
	dedicatedInfoType			CHOICE {
		dedicatedInfoNAS					DedicatedInfoNAS,
		dedicatedInfoCDMA2000-1XRTT			DedicatedInfoCDMA2000,
		dedicatedInfoCDMA2000-HRPD			DedicatedInfoCDMA2000
	},
	nonCriticalExtension				ULInformationTransfer-v8a0-IEs							OPTIONAL
}

ULInformationTransfer-v8a0-IEs ::= SEQUENCE {
	lateNonCriticalExtension			OCTET STRING						OPTIONAL,
	nonCriticalExtension				SEQUENCE {}							OPTIONAL
}


WLANConnectionStatusReport-r13 ::=	SEQUENCE {
	criticalExtensions					CHOICE {
		c1									CHOICE {
			wlanConnectionStatusReport-r13	WLANConnectionStatusReport-r13-IEs,
			spare3 NULL, spare2 NULL, spare1 NULL
		},
		criticalExtensionsFuture			SEQUENCE {}
	}
}

WLANConnectionStatusReport-r13-IEs ::=	SEQUENCE {
	wlan-Status-r13					WLAN-Status-r13,
	lateNonCriticalExtension		OCTET STRING						OPTIONAL,
	nonCriticalExtension			WLANConnectionStatusReport-v1430-IEs	OPTIONAL
}

WLANConnectionStatusReport-v1430-IEs ::=	SEQUENCE {
	wlan-Status-v1430				WLAN-Status-v1430,
	nonCriticalExtension			SEQUENCE {}							OPTIONAL
}


SystemInformationBlockType2 ::=		SEQUENCE {
	ac-BarringInfo						SEQUENCE {
		ac-BarringForEmergency				BOOLEAN,
		ac-BarringForMO-Signalling			AC-BarringConfig				OPTIONAL,	-- Need OP
		ac-BarringForMO-Data				AC-BarringConfig				OPTIONAL	-- Need OP
	}																		OPTIONAL,	-- Need OP
	radioResourceConfigCommon			RadioResourceConfigCommonSIB,
	ue-TimersAndConstants				UE-TimersAndConstants,
	freqInfo							SEQUENCE {
		ul-CarrierFreq						ARFCN-ValueEUTRA				OPTIONAL,	-- Need OP
		ul-Bandwidth						ENUMERATED {n6, n15, n25, n50, n75, n100}
																			OPTIONAL,	-- Need OP
		additionalSpectrumEmission			AdditionalSpectrumEmission
	},
	mbsfn-SubframeConfigList			MBSFN-SubframeConfigList			OPTIONAL,	-- Need OR
	timeAlignmentTimerCommon			TimeAlignmentTimer,
	...,
	lateNonCriticalExtension		OCTET STRING (CONTAINING SystemInformationBlockType2-v8h0-IEs)						OPTIONAL,
	[[	ssac-BarringForMMTEL-Voice-r9		AC-BarringConfig				OPTIONAL,	-- Need OP
		ssac-BarringForMMTEL-Video-r9		AC-BarringConfig				OPTIONAL	-- Need OP
	]],
	[[	ac-BarringForCSFB-r10				AC-BarringConfig			OPTIONAL	-- Need OP
	]],
	[[	ac-BarringSkipForMMTELVoice-r12		ENUMERATED {true}			OPTIONAL,	-- Need OP
		ac-BarringSkipForMMTELVideo-r12		ENUMERATED {true}			OPTIONAL,	-- Need OP
		ac-BarringSkipForSMS-r12			ENUMERATED {true}			OPTIONAL,	-- Need OP
		ac-BarringPerPLMN-List-r12			AC-BarringPerPLMN-List-r12	OPTIONAL	-- Need OP
	]],
	[[	voiceServiceCauseIndication-r12		ENUMERATED {true}			OPTIONAL	-- Need OP
	]],
	[[	acdc-BarringForCommon-r13			ACDC-BarringForCommon-r13		OPTIONAL,	-- Need OP
		acdc-BarringPerPLMN-List-r13		ACDC-BarringPerPLMN-List-r13	OPTIONAL	-- Need OP
	]],
	[[
		udt-RestrictingForCommon-r13		UDT-Restricting-r13				OPTIONAL,	-- Need OR
		udt-RestrictingPerPLMN-List-r13		UDT-RestrictingPerPLMN-List-r13	OPTIONAL,	-- Need OR
		cIoT-EPS-OptimisationInfo-r13		CIOT-EPS-OptimisationInfo-r13	OPTIONAL,	-- Need OP
		useFullResumeID-r13					ENUMERATED {true}				OPTIONAL	-- Need OP
	]],
	[[	unicastFreqHoppingInd-r13			ENUMERATED {true}				OPTIONAL	-- Need OP
	]],
	[[	mbsfn-SubframeConfigList-v1430		MBSFN-SubframeConfigList-v1430	OPTIONAL,	-- Need OP
		videoServiceCauseIndication-r14		ENUMERATED {true}				OPTIONAL	-- Need OP
	]]

}

SystemInformationBlockType2-v8h0-IEs ::=	SEQUENCE {
	multiBandInfoList				SEQUENCE (SIZE (1..maxMultiBands)) OF AdditionalSpectrumEmission	OPTIONAL,	-- Need OR
	nonCriticalExtension			SystemInformationBlockType2-v9e0-IEs	OPTIONAL
}

SystemInformationBlockType2-v9e0-IEs ::= SEQUENCE {
	ul-CarrierFreq-v9e0					ARFCN-ValueEUTRA-v9e0		OPTIONAL,	-- Cond ul-FreqMax
	nonCriticalExtension				SystemInformationBlockType2-v9i0-IEs					OPTIONAL
}

SystemInformationBlockType2-v9i0-IEs ::= SEQUENCE {
-- Following field is for any non-critical extensions from REL-9
	nonCriticalExtension			OCTET STRING (CONTAINING SystemInformationBlockType2-v10m0-IEs)						OPTIONAL,
	dummy		SEQUENCE {}		OPTIONAL
}

SystemInformationBlockType2-v10m0-IEs ::= SEQUENCE {
	freqInfo-v10l0						SEQUENCE {
		additionalSpectrumEmission-v10l0			AdditionalSpectrumEmission-v10l0
		}														OPTIONAL,
		multiBandInfoList-v10l0				SEQUENCE (SIZE (1..maxMultiBands)) OF
				AdditionalSpectrumEmission-v10l0				OPTIONAL,
-- Following field is for non-critical extensions from REL-10
	nonCriticalExtension				SEQUENCE {}					OPTIONAL
}

AC-BarringConfig ::=				SEQUENCE {
	ac-BarringFactor					ENUMERATED {
											p00, p05, p10, p15, p20, p25, p30, p40,
											p50, p60, p70, p75, p80, p85, p90, p95},
	ac-BarringTime						ENUMERATED {s4, s8, s16, s32, s64, s128, s256, s512},
	ac-BarringForSpecialAC				BIT STRING (SIZE(5))
}

MBSFN-SubframeConfigList ::=		SEQUENCE (SIZE (1..maxMBSFN-Allocations)) OF MBSFN-SubframeConfig

MBSFN-SubframeConfigList-v1430 ::=		SEQUENCE (SIZE (1..maxMBSFN-Allocations)) OF MBSFN-SubframeConfig-v1430

AC-BarringPerPLMN-List-r12 ::=		SEQUENCE (SIZE (1.. maxPLMN-r11)) OF AC-BarringPerPLMN-r12

AC-BarringPerPLMN-r12 ::=			SEQUENCE {
	plmn-IdentityIndex-r12					INTEGER (1..maxPLMN-r11),
	ac-BarringInfo-r12						SEQUENCE {
		ac-BarringForEmergency-r12			BOOLEAN,
		ac-BarringForMO-Signalling-r12		AC-BarringConfig	OPTIONAL,	-- Need OP
		ac-BarringForMO-Data-r12			AC-BarringConfig	OPTIONAL	-- Need OP
	}															OPTIONAL,	-- Need OP
	ac-BarringSkipForMMTELVoice-r12		ENUMERATED {true}		OPTIONAL,	-- Need OP
	ac-BarringSkipForMMTELVideo-r12		ENUMERATED {true}		OPTIONAL,	-- Need OP
	ac-BarringSkipForSMS-r12			ENUMERATED {true}		OPTIONAL,	-- Need OP
	ac-BarringForCSFB-r12				AC-BarringConfig		OPTIONAL,	-- Need OP
	ssac-BarringForMMTEL-Voice-r12		AC-BarringConfig		OPTIONAL,	-- Need OP
	ssac-BarringForMMTEL-Video-r12		AC-BarringConfig		OPTIONAL	-- Need OP
}

ACDC-BarringForCommon-r13 ::=			SEQUENCE {
	acdc-HPLMNonly-r13					BOOLEAN,
	barringPerACDC-CategoryList-r13				BarringPerACDC-CategoryList-r13
}

ACDC-BarringPerPLMN-List-r13 ::=		SEQUENCE (SIZE (1.. maxPLMN-r11)) OF ACDC-BarringPerPLMN-r13

ACDC-BarringPerPLMN-r13 ::=			SEQUENCE {
	plmn-IdentityIndex-r13				INTEGER (1..maxPLMN-r11),
	acdc-OnlyForHPLMN-r13					BOOLEAN,
	barringPerACDC-CategoryList-r13				BarringPerACDC-CategoryList-r13
}

BarringPerACDC-CategoryList-r13 ::= SEQUENCE (SIZE (1..maxACDC-Cat-r13)) OF BarringPerACDC-Category-r13

BarringPerACDC-Category-r13 ::= SEQUENCE {
	acdc-Category-r13				INTEGER (1..maxACDC-Cat-r13),
	acdc-BarringConfig-r13			SEQUENCE {
		ac-BarringFactor-r13			ENUMERATED {
											p00, p05, p10, p15, p20, p25, p30, p40,
											p50, p60, p70, p75, p80, p85, p90, p95},
		ac-BarringTime-r13				ENUMERATED {s4, s8, s16, s32, s64, s128, s256, s512}
	}										OPTIONAL	-- Need OP
}

UDT-Restricting-r13	::= SEQUENCE {
	udt-Restricting-r13					ENUMERATED {true}			OPTIONAL, --Need OR
	udt-RestrictingTime-r13				ENUMERATED {s4, s8, s16, s32, s64, s128, s256, s512} OPTIONAL --Need OR
}

UDT-RestrictingPerPLMN-List-r13 ::=	SEQUENCE (SIZE (1..maxPLMN-r11)) OF UDT-RestrictingPerPLMN-r13

UDT-RestrictingPerPLMN-r13 ::= SEQUENCE {
	plmn-IdentityIndex-r13					INTEGER (1..maxPLMN-r11),
	udt-Restricting-r13						UDT-Restricting-r13		OPTIONAL	--Need OR
}

CIOT-EPS-OptimisationInfo-r13 ::=	SEQUENCE (SIZE (1.. maxPLMN-r11)) OF CIOT-OptimisationPLMN-r13

CIOT-OptimisationPLMN-r13::= SEQUENCE {
		up-CIoT-EPS-Optimisation-r13		ENUMERATED {true}			OPTIONAL,	-- Need OP
		cp-CIoT-EPS-Optimisation-r13		ENUMERATED {true}			OPTIONAL,	-- Need OP
		attachWithoutPDN-Connectivity-r13	ENUMERATED {true}			OPTIONAL	-- Need OP
}


SystemInformationBlockType3 ::=		SEQUENCE {
	cellReselectionInfoCommon			SEQUENCE {
		q-Hyst								ENUMERATED {
												dB0, dB1, dB2, dB3, dB4, dB5, dB6, dB8, dB10,
												dB12, dB14, dB16, dB18, dB20, dB22, dB24},
		speedStateReselectionPars			SEQUENCE {
			mobilityStateParameters				MobilityStateParameters,
			q-HystSF						SEQUENCE {
				sf-Medium						ENUMERATED {
														dB-6, dB-4, dB-2, dB0},
				sf-High							ENUMERATED {
														dB-6, dB-4, dB-2, dB0}
			}
		}																OPTIONAL		-- Need OP
	},
	cellReselectionServingFreqInfo		SEQUENCE {
		s-NonIntraSearch					ReselectionThreshold		OPTIONAL,		-- Need OP
		threshServingLow					ReselectionThreshold,
		cellReselectionPriority				CellReselectionPriority
	},
	intraFreqCellReselectionInfo		SEQUENCE {
		q-RxLevMin							Q-RxLevMin,
		p-Max								P-Max						OPTIONAL,		-- Need OP
		s-IntraSearch						ReselectionThreshold		OPTIONAL,		-- Need OP
		allowedMeasBandwidth				AllowedMeasBandwidth		OPTIONAL,		-- Need OP
		presenceAntennaPort1				PresenceAntennaPort1,
		neighCellConfig						NeighCellConfig,
		t-ReselectionEUTRA					T-Reselection,
		t-ReselectionEUTRA-SF				SpeedStateScaleFactors		OPTIONAL		-- Need OP
	},
	...,
	lateNonCriticalExtension				OCTET STRING (CONTAINING SystemInformationBlockType3-v10j0-IEs)	OPTIONAL,
	[[	s-IntraSearch-v920					SEQUENCE {
			s-IntraSearchP-r9					ReselectionThreshold,
			s-IntraSearchQ-r9					ReselectionThresholdQ-r9
		}																OPTIONAL,		-- Need OP
		s-NonIntraSearch-v920				SEQUENCE {
			s-NonIntraSearchP-r9				ReselectionThreshold,
			s-NonIntraSearchQ-r9				ReselectionThresholdQ-r9
		}																OPTIONAL,		-- Need OP
		q-QualMin-r9						Q-QualMin-r9				OPTIONAL,		-- Need OP
		threshServingLowQ-r9				ReselectionThresholdQ-r9	OPTIONAL		-- Need OP
	]],
	[[	q-QualMinWB-r11						Q-QualMin-r9				OPTIONAL	-- Cond WB-RSRQ
	]],
	[[	q-QualMinRSRQ-OnAllSymbols-r12			Q-QualMin-r9				OPTIONAL			-- Cond RSRQ
	]],
	[[	cellReselectionServingFreqInfo-v1310 CellReselectionServingFreqInfo-v1310	OPTIONAL,		-- Need OP
		redistributionServingInfo-r13			RedistributionServingInfo-r13 OPTIONAL,	--Need OR
		cellSelectionInfoCE-r13					CellSelectionInfoCE-r13		OPTIONAL,		-- Need OP
		t-ReselectionEUTRA-CE-r13				T-ReselectionEUTRA-CE-r13	OPTIONAL		-- Need OP
	]],
	[[	cellSelectionInfoCE1-r13				CellSelectionInfoCE1-r13	OPTIONAL	-- Need OP
	]],
	[[	cellSelectionInfoCE1-v1360			CellSelectionInfoCE1-v1360	OPTIONAL		-- Cond QrxlevminCE1
	]],
	[[	cellReselectionInfoCommon-v1460		CellReselectionInfoCommon-v1460	OPTIONAL	-- Need OR
	]]
}

RedistributionServingInfo-r13 ::=		SEQUENCE {
	redistributionFactorServing-r13		INTEGER(0..10),
	redistributionFactorCell-r13		ENUMERATED{true}				OPTIONAL,	--Need OP
	t360-r13							ENUMERATED {min4, min8, min16, min32,infinity,
											spare3,spare2,spare1},
	redistrOnPagingOnly-r13				ENUMERATED {true}		OPTIONAL	--Need OP
}

CellReselectionServingFreqInfo-v1310 ::=	SEQUENCE {
	cellReselectionSubPriority-r13				CellReselectionSubPriority-r13
}

-- Late non critical extensions
SystemInformationBlockType3-v10j0-IEs ::= SEQUENCE {
	freqBandInfo-r10					NS-PmaxList-r10				OPTIONAL,	-- Need OR
	multiBandInfoList-v10j0				MultiBandInfoList-v10j0		OPTIONAL,	-- Need OR
	nonCriticalExtension				SystemInformationBlockType3-v10l0-IEs					OPTIONAL
}

SystemInformationBlockType3-v10l0-IEs ::= SEQUENCE {
	freqBandInfo-v10l0					NS-PmaxList-v10l0			OPTIONAL,	-- Need OR
	multiBandInfoList-v10l0				MultiBandInfoList-v10l0		OPTIONAL,	-- Need OR
	nonCriticalExtension				SEQUENCE {}					OPTIONAL
}

CellReselectionInfoCommon-v1460 ::=	SEQUENCE {
	s-SearchDeltaP-r14					ENUMERATED {dB6, dB9, dB12, dB15}
}


SystemInformationBlockType4 ::=		SEQUENCE {
	intraFreqNeighCellList				IntraFreqNeighCellList		OPTIONAL,	-- Need OR
	intraFreqBlackCellList				IntraFreqBlackCellList				OPTIONAL,	-- Need OR
	csg-PhysCellIdRange					PhysCellIdRange				OPTIONAL,	-- Cond CSG
	...,
	lateNonCriticalExtension				OCTET STRING				OPTIONAL
}

IntraFreqNeighCellList ::=		SEQUENCE (SIZE (1..maxCellIntra)) OF IntraFreqNeighCellInfo

IntraFreqNeighCellInfo ::=		SEQUENCE {
	physCellId								PhysCellId,
	q-OffsetCell							Q-OffsetRange,
	...
}

IntraFreqBlackCellList ::=		SEQUENCE (SIZE (1..maxCellBlack)) OF PhysCellIdRange


SystemInformationBlockType5 ::=		SEQUENCE {
	interFreqCarrierFreqList			InterFreqCarrierFreqList,
	...,
	lateNonCriticalExtension				OCTET STRING	(CONTAINING SystemInformationBlockType5-v8h0-IEs)				OPTIONAL,
	[[	interFreqCarrierFreqList-v1250	InterFreqCarrierFreqList-v1250		OPTIONAL,	-- Need OR
		interFreqCarrierFreqListExt-r12	InterFreqCarrierFreqListExt-r12	OPTIONAL	-- Need OR
	]],
	[[	interFreqCarrierFreqListExt-v1280	InterFreqCarrierFreqListExt-v1280	OPTIONAL	-- Need OR
	]],
	[[	interFreqCarrierFreqList-v1310		InterFreqCarrierFreqList-v1310		OPTIONAL,	-- Need OR
		interFreqCarrierFreqListExt-v1310	InterFreqCarrierFreqListExt-v1310	OPTIONAL	-- Need OR
	]],
	[[	interFreqCarrierFreqList-v1350		InterFreqCarrierFreqList-v1350	OPTIONAL,	-- Need OR
	interFreqCarrierFreqListExt-v1350	InterFreqCarrierFreqListExt-v1350	OPTIONAL	-- Need OR
	]],
	[[	interFreqCarrierFreqListExt-v1360	InterFreqCarrierFreqListExt-v1360	OPTIONAL	-- Need OR
	]],
	[[	scptm-FreqOffset-r14				INTEGER (1..8)					OPTIONAL	-- Need OP
	]]
}

-- Late non critical extensions
SystemInformationBlockType5-v8h0-IEs ::=	SEQUENCE {
	interFreqCarrierFreqList-v8h0 SEQUENCE (SIZE (1..maxFreq)) OF InterFreqCarrierFreqInfo-v8h0				OPTIONAL,	-- Need OP
	nonCriticalExtension			SystemInformationBlockType5-v9e0-IEs							OPTIONAL
}

SystemInformationBlockType5-v9e0-IEs ::=	SEQUENCE {
	interFreqCarrierFreqList-v9e0	SEQUENCE (SIZE (1..maxFreq)) OF InterFreqCarrierFreqInfo-v9e0				OPTIONAL,	-- Need OR
	nonCriticalExtension			SystemInformationBlockType5-v10j0-IEs	OPTIONAL
}

SystemInformationBlockType5-v10j0-IEs ::=	SEQUENCE {
	interFreqCarrierFreqList-v10j0	SEQUENCE (SIZE (1..maxFreq)) OF InterFreqCarrierFreqInfo-v10j0				OPTIONAL,	-- Need OR
	nonCriticalExtension			SystemInformationBlockType5-v10l0-IEs						OPTIONAL
}

SystemInformationBlockType5-v10l0-IEs ::=	SEQUENCE {
	interFreqCarrierFreqList-v10l0	SEQUENCE (SIZE (1..maxFreq)) OF InterFreqCarrierFreqInfo-v10l0				OPTIONAL,	-- Need OR
	nonCriticalExtension			SystemInformationBlockType5-v13a0-IEs		OPTIONAL
}

SystemInformationBlockType5-v13a0-IEs ::=	SEQUENCE {
	-- Late non critical extensions from REL-10 upto REL-12
	lateNonCriticalExtension		OCTET STRING					OPTIONAL,	-- Need OR
	interFreqCarrierFreqList-v13a0	InterFreqCarrierFreqList-v13a0	OPTIONAL,	-- Need OR
	-- Late non critical extensions from REL-13
	nonCriticalExtension			SEQUENCE {}						OPTIONAL
}

InterFreqCarrierFreqList ::=		SEQUENCE (SIZE (1..maxFreq)) OF InterFreqCarrierFreqInfo

InterFreqCarrierFreqList-v1250 ::=	SEQUENCE (SIZE (1.. maxFreq)) OF InterFreqCarrierFreqInfo-v1250

InterFreqCarrierFreqList-v1310 ::=	SEQUENCE (SIZE (1.. maxFreq)) OF InterFreqCarrierFreqInfo-v1310

InterFreqCarrierFreqList-v1350 ::=	SEQUENCE (SIZE (1.. maxFreq)) OF InterFreqCarrierFreqInfo-v1350

InterFreqCarrierFreqList-v13a0 ::=	SEQUENCE (SIZE (1.. maxFreq)) OF InterFreqCarrierFreqInfo-v1360

InterFreqCarrierFreqListExt-r12 ::=	SEQUENCE (SIZE (1.. maxFreq)) OF InterFreqCarrierFreqInfo-r12

InterFreqCarrierFreqListExt-v1280 ::=	SEQUENCE (SIZE (1.. maxFreq)) OF InterFreqCarrierFreqInfo-v10j0

InterFreqCarrierFreqListExt-v1310 ::=	SEQUENCE (SIZE (1.. maxFreq)) OF InterFreqCarrierFreqInfo-v1310

InterFreqCarrierFreqListExt-v1350 ::=	SEQUENCE (SIZE (1.. maxFreq)) OF InterFreqCarrierFreqInfo-v1350

InterFreqCarrierFreqListExt-v1360 ::=	SEQUENCE (SIZE (1..maxFreq)) OF InterFreqCarrierFreqInfo-v1360

InterFreqCarrierFreqInfo ::=	SEQUENCE {
	dl-CarrierFreq						ARFCN-ValueEUTRA,
	q-RxLevMin							Q-RxLevMin,
	p-Max								P-Max							OPTIONAL,		-- Need OP
	t-ReselectionEUTRA					T-Reselection,
	t-ReselectionEUTRA-SF				SpeedStateScaleFactors			OPTIONAL,		-- Need OP
	threshX-High						ReselectionThreshold,
	threshX-Low							ReselectionThreshold,
	allowedMeasBandwidth				AllowedMeasBandwidth,
	presenceAntennaPort1				PresenceAntennaPort1,
	cellReselectionPriority				CellReselectionPriority			OPTIONAL,		-- Need OP
	neighCellConfig						NeighCellConfig,
	q-OffsetFreq						Q-OffsetRange					DEFAULT dB0,
	interFreqNeighCellList				InterFreqNeighCellList			OPTIONAL,		-- Need OR
	interFreqBlackCellList				InterFreqBlackCellList			OPTIONAL,		-- Need OR
	...,
	[[	q-QualMin-r9					Q-QualMin-r9					OPTIONAL,		-- Need OP
		threshX-Q-r9					SEQUENCE {
			threshX-HighQ-r9				ReselectionThresholdQ-r9,
			threshX-LowQ-r9					ReselectionThresholdQ-r9
		}																OPTIONAL		-- Cond RSRQ
	]],
	[[	q-QualMinWB-r11					Q-QualMin-r9					OPTIONAL	-- Cond WB-RSRQ
	]]
}

InterFreqCarrierFreqInfo-v8h0 ::=		SEQUENCE {
	multiBandInfoList					MultiBandInfoList				OPTIONAL	-- Need OR
}

InterFreqCarrierFreqInfo-v9e0 ::=	SEQUENCE {
	dl-CarrierFreq-v9e0					ARFCN-ValueEUTRA-v9e0	OPTIONAL,	-- Cond dl-FreqMax
	multiBandInfoList-v9e0				MultiBandInfoList-v9e0	OPTIONAL	-- Need OR
}

InterFreqCarrierFreqInfo-v10j0 ::=	SEQUENCE {
	freqBandInfo-r10					NS-PmaxList-r10				OPTIONAL,	-- Need OR
	multiBandInfoList-v10j0				MultiBandInfoList-v10j0		OPTIONAL	-- Need OR
}

InterFreqCarrierFreqInfo-v10l0 ::=	SEQUENCE {
	freqBandInfo-v10l0					NS-PmaxList-v10l0			OPTIONAL,	-- Need OR
	multiBandInfoList-v10l0				MultiBandInfoList-v10l0		OPTIONAL	-- Need OR
}

InterFreqCarrierFreqInfo-v1250 ::=		SEQUENCE {
	reducedMeasPerformance-r12		ENUMERATED {true}		OPTIONAL,		-- Need OP
	q-QualMinRSRQ-OnAllSymbols-r12	Q-QualMin-r9					OPTIONAL	-- Cond RSRQ2
}

InterFreqCarrierFreqInfo-r12 ::=		SEQUENCE {
	dl-CarrierFreq-r12					ARFCN-ValueEUTRA-r9,
	q-RxLevMin-r12						Q-RxLevMin,
	p-Max-r12							P-Max							OPTIONAL,		-- Need OP
	t-ReselectionEUTRA-r12				T-Reselection,
	t-ReselectionEUTRA-SF-r12			SpeedStateScaleFactors			OPTIONAL,		-- Need OP
	threshX-High-r12					ReselectionThreshold,
	threshX-Low-r12						ReselectionThreshold,
	allowedMeasBandwidth-r12			AllowedMeasBandwidth,
	presenceAntennaPort1-r12			PresenceAntennaPort1,
	cellReselectionPriority-r12			CellReselectionPriority			OPTIONAL,		-- Need OP
	neighCellConfig-r12					NeighCellConfig,
	q-OffsetFreq-r12					Q-OffsetRange					DEFAULT dB0,
	interFreqNeighCellList-r12			InterFreqNeighCellList			OPTIONAL,		-- Need OR
	interFreqBlackCellList-r12			InterFreqBlackCellList			OPTIONAL,		-- Need OR
	q-QualMin-r12						Q-QualMin-r9					OPTIONAL,		-- Need OP
	threshX-Q-r12						SEQUENCE {
		threshX-HighQ-r12					ReselectionThresholdQ-r9,
		threshX-LowQ-r12					ReselectionThresholdQ-r9
	}																	OPTIONAL,	-- Cond RSRQ
	q-QualMinWB-r12						Q-QualMin-r9					OPTIONAL,	-- Cond WB-RSRQ
	multiBandInfoList-r12				MultiBandInfoList-r11			OPTIONAL,	-- Need OR
	reducedMeasPerformance-r12			ENUMERATED {true}				OPTIONAL,	-- Need OP
	q-QualMinRSRQ-OnAllSymbols-r12		Q-QualMin-r9					OPTIONAL,	-- Cond RSRQ2
...
}

InterFreqCarrierFreqInfo-v1310	::=	SEQUENCE {
	cellReselectionSubPriority-r13		CellReselectionSubPriority-r13		OPTIONAL,		-- Need OP
	redistributionInterFreqInfo-r13		RedistributionInterFreqInfo-r13		OPTIONAL, --Need OP
	cellSelectionInfoCE-r13				CellSelectionInfoCE-r13			OPTIONAL,	-- Need OP
	t-ReselectionEUTRA-CE-r13			T-ReselectionEUTRA-CE-r13		OPTIONAL	-- Need OP
}

InterFreqCarrierFreqInfo-v1350	::= SEQUENCE {
	cellSelectionInfoCE1-r13			CellSelectionInfoCE1-r13			OPTIONAL	-- Need OP
}

InterFreqCarrierFreqInfo-v1360	::= SEQUENCE {
	cellSelectionInfoCE1-v1360		CellSelectionInfoCE1-v1360	OPTIONAL	-- Cond QrxlevminCE1
}

InterFreqNeighCellList ::=			SEQUENCE (SIZE (1..maxCellInter)) OF InterFreqNeighCellInfo

InterFreqNeighCellInfo ::=			SEQUENCE {
	physCellId							PhysCellId,
	q-OffsetCell						Q-OffsetRange
}

InterFreqBlackCellList ::=			SEQUENCE (SIZE (1..maxCellBlack)) OF PhysCellIdRange

RedistributionInterFreqInfo-r13 ::=		SEQUENCE {
	redistributionFactorFreq-r13			RedistributionFactor-r13	OPTIONAL,	--Need OP
	redistributionNeighCellList-r13			RedistributionNeighCellList-r13		OPTIONAL	--Need OP
}

RedistributionNeighCellList-r13 ::=		SEQUENCE (SIZE (1..maxCellInter)) OF RedistributionNeighCell-r13

RedistributionNeighCell-r13 ::=		SEQUENCE {
	physCellId-r13									PhysCellId,
	redistributionFactorCell-r13					RedistributionFactor-r13
}

RedistributionFactor-r13 ::=	INTEGER(1..10)


SystemInformationBlockType6 ::=		SEQUENCE {
	carrierFreqListUTRA-FDD				CarrierFreqListUTRA-FDD			OPTIONAL,		-- Need OR
	carrierFreqListUTRA-TDD				CarrierFreqListUTRA-TDD			OPTIONAL,		-- Need OR
	t-ReselectionUTRA					T-Reselection,
	t-ReselectionUTRA-SF				SpeedStateScaleFactors			OPTIONAL,		-- Need OP
	...,
	lateNonCriticalExtension			OCTET STRING	(CONTAINING SystemInformationBlockType6-v8h0-IEs)					OPTIONAL,
	[[	carrierFreqListUTRA-FDD-v1250 SEQUENCE (SIZE (1..maxUTRA-FDD-Carrier)) OF
										CarrierFreqInfoUTRA-v1250		OPTIONAL,	-- Cond UTRA-FDD
		carrierFreqListUTRA-TDD-v1250 SEQUENCE (SIZE (1..maxUTRA-TDD-Carrier)) OF
										CarrierFreqInfoUTRA-v1250		OPTIONAL,	-- Cond UTRA-TDD
		carrierFreqListUTRA-FDD-Ext-r12	CarrierFreqListUTRA-FDD-Ext-r12 OPTIONAL,	-- Cond UTRA-FDD
		carrierFreqListUTRA-TDD-Ext-r12	CarrierFreqListUTRA-TDD-Ext-r12 OPTIONAL		-- Cond UTRA-TDD
	]]
}

SystemInformationBlockType6-v8h0-IEs ::=	SEQUENCE {
	carrierFreqListUTRA-FDD-v8h0 SEQUENCE (SIZE (1..maxUTRA-FDD-Carrier)) OF CarrierFreqInfoUTRA-FDD-v8h0 OPTIONAL,	-- Cond UTRA-FDD
	nonCriticalExtension				SEQUENCE {}							OPTIONAL
}

CarrierFreqInfoUTRA-v1250 ::=		SEQUENCE {
	reducedMeasPerformance-r12		ENUMERATED {true}		OPTIONAL		-- Need OP
}

CarrierFreqListUTRA-FDD ::=		SEQUENCE (SIZE (1..maxUTRA-FDD-Carrier)) OF CarrierFreqUTRA-FDD

CarrierFreqUTRA-FDD ::=				SEQUENCE {
	carrierFreq							ARFCN-ValueUTRA,
	cellReselectionPriority				CellReselectionPriority			OPTIONAL,		-- Need OP
	threshX-High						ReselectionThreshold,
	threshX-Low							ReselectionThreshold,
	q-RxLevMin							INTEGER (-60..-13),
	p-MaxUTRA							INTEGER (-50..33),
	q-QualMin							INTEGER (-24..0),
	...,
	[[	threshX-Q-r9					SEQUENCE {
			threshX-HighQ-r9				ReselectionThresholdQ-r9,
			threshX-LowQ-r9					ReselectionThresholdQ-r9
		}																OPTIONAL		-- Cond RSRQ
	]]
}

CarrierFreqInfoUTRA-FDD-v8h0 ::=			SEQUENCE {
	multiBandInfoList					SEQUENCE (SIZE (1..maxMultiBands)) OF FreqBandIndicator-UTRA-FDD				OPTIONAL	-- Need OR
}

CarrierFreqListUTRA-FDD-Ext-r12 ::=	SEQUENCE (SIZE (1..maxUTRA-FDD-Carrier)) OF
									CarrierFreqUTRA-FDD-Ext-r12

CarrierFreqUTRA-FDD-Ext-r12 ::=				SEQUENCE {
	carrierFreq-r12						ARFCN-ValueUTRA,
	cellReselectionPriority-r12			CellReselectionPriority			OPTIONAL,	-- Need OP
	threshX-High-r12					ReselectionThreshold,
	threshX-Low-r12						ReselectionThreshold,
	q-RxLevMin-r12						INTEGER (-60..-13),
	p-MaxUTRA-r12						INTEGER (-50..33),
	q-QualMin-r12						INTEGER (-24..0),
	threshX-Q-r12						SEQUENCE {
			threshX-HighQ-r12				ReselectionThresholdQ-r9,
			threshX-LowQ-r12				ReselectionThresholdQ-r9
	}																OPTIONAL,		-- Cond RSRQ
	multiBandInfoList-r12				SEQUENCE (SIZE (1..maxMultiBands)) OF FreqBandIndicator-UTRA-FDD				OPTIONAL,	-- Need OR
	reducedMeasPerformance-r12			ENUMERATED {true}				OPTIONAL,	-- Need OP
	...
}

CarrierFreqListUTRA-TDD ::=		SEQUENCE (SIZE (1..maxUTRA-TDD-Carrier)) OF CarrierFreqUTRA-TDD

CarrierFreqUTRA-TDD ::=				SEQUENCE {
	carrierFreq							ARFCN-ValueUTRA,
	cellReselectionPriority				CellReselectionPriority			OPTIONAL,		-- Need OP
	threshX-High						ReselectionThreshold,
	threshX-Low							ReselectionThreshold,
	q-RxLevMin							INTEGER (-60..-13),
	p-MaxUTRA							INTEGER (-50..33),
	...
}

CarrierFreqListUTRA-TDD-Ext-r12 ::=	SEQUENCE (SIZE (1..maxUTRA-TDD-Carrier)) OF
									CarrierFreqUTRA-TDD-r12

CarrierFreqUTRA-TDD-r12 ::=	SEQUENCE {
	carrierFreq-r12						ARFCN-ValueUTRA,
	cellReselectionPriority-r12			CellReselectionPriority			OPTIONAL,		-- Need OP
	threshX-High-r12					ReselectionThreshold,
	threshX-Low-r12						ReselectionThreshold,
	q-RxLevMin-r12						INTEGER (-60..-13),
	p-MaxUTRA-r12						INTEGER (-50..33),
	reducedMeasPerformance-r12			ENUMERATED {true}				OPTIONAL,	-- Need OP
	...
}

FreqBandIndicator-UTRA-FDD ::=				INTEGER (1..86)


SystemInformationBlockType7 ::=		SEQUENCE {
	t-ReselectionGERAN					T-Reselection,
	t-ReselectionGERAN-SF				SpeedStateScaleFactors				OPTIONAL,	-- Need OR
	carrierFreqsInfoList				CarrierFreqsInfoListGERAN			OPTIONAL,	-- Need OR
	...,
	lateNonCriticalExtension				OCTET STRING				OPTIONAL
}

CarrierFreqsInfoListGERAN ::=			SEQUENCE (SIZE (1..maxGNFG)) OF CarrierFreqsInfoGERAN

CarrierFreqsInfoGERAN ::=			SEQUENCE {
	carrierFreqs						CarrierFreqsGERAN,
	commonInfo							SEQUENCE {
		cellReselectionPriority				CellReselectionPriority			OPTIONAL,	-- Need OP
		ncc-Permitted						BIT STRING (SIZE (8)),
		q-RxLevMin							INTEGER (0..45),
		p-MaxGERAN							INTEGER (0..39)					OPTIONAL,	-- Need OP
		threshX-High						ReselectionThreshold,
		threshX-Low							ReselectionThreshold
	},
	...
}


SystemInformationBlockType8 ::=		SEQUENCE {
	systemTimeInfo						SystemTimeInfoCDMA2000				OPTIONAL,	-- Need OR
	searchWindowSize					INTEGER (0..15)						OPTIONAL,	-- Need OR
	parametersHRPD						SEQUENCE {
		preRegistrationInfoHRPD				PreRegistrationInfoHRPD,
		cellReselectionParametersHRPD		CellReselectionParametersCDMA2000	OPTIONAL -- Need OR
	}																		OPTIONAL,	-- Need OR
	parameters1XRTT						SEQUENCE {
		csfb-RegistrationParam1XRTT			CSFB-RegistrationParam1XRTT		OPTIONAL,	-- Need OP
		longCodeState1XRTT					BIT STRING (SIZE (42))			OPTIONAL,	-- Need OR
		cellReselectionParameters1XRTT		CellReselectionParametersCDMA2000	OPTIONAL -- Need OR
	}																		OPTIONAL,	-- Need OR
	...,
	lateNonCriticalExtension			OCTET STRING						OPTIONAL,
	[[	csfb-SupportForDualRxUEs-r9			BOOLEAN							OPTIONAL,	-- Need OR
		cellReselectionParametersHRPD-v920	CellReselectionParametersCDMA2000-v920	OPTIONAL,	-- Cond NCL-HRPD
		cellReselectionParameters1XRTT-v920	CellReselectionParametersCDMA2000-v920	OPTIONAL,	-- Cond NCL-1XRTT
		csfb-RegistrationParam1XRTT-v920	CSFB-RegistrationParam1XRTT-v920		OPTIONAL,	-- Cond REG-1XRTT
		ac-BarringConfig1XRTT-r9			AC-BarringConfig1XRTT-r9	OPTIONAL	-- Cond REG-1XRTT
	]],
	[[	csfb-DualRxTxSupport-r10			ENUMERATED {true}			OPTIONAL	-- Cond REG-1XRTT
	]],
	[[	sib8-PerPLMN-List-r11				SIB8-PerPLMN-List-r11		OPTIONAL	-- Need OR
	]]
}

CellReselectionParametersCDMA2000 ::= SEQUENCE {
	bandClassList						BandClassListCDMA2000,
	neighCellList						NeighCellListCDMA2000,
	t-ReselectionCDMA2000			T-Reselection,
	t-ReselectionCDMA2000-SF			SpeedStateScaleFactors				OPTIONAL	-- Need OP
}

CellReselectionParametersCDMA2000-r11 ::= SEQUENCE {
	bandClassList						BandClassListCDMA2000,
	neighCellList-r11					SEQUENCE (SIZE (1..16)) OF NeighCellCDMA2000-r11,
	t-ReselectionCDMA2000				T-Reselection,
	t-ReselectionCDMA2000-SF			SpeedStateScaleFactors				OPTIONAL	-- Need OP
}

CellReselectionParametersCDMA2000-v920 ::= SEQUENCE {
	neighCellList-v920						NeighCellListCDMA2000-v920
}

NeighCellListCDMA2000 ::=			SEQUENCE (SIZE (1..16)) OF NeighCellCDMA2000

NeighCellCDMA2000 ::=	SEQUENCE {
	bandClass							BandclassCDMA2000,
	neighCellsPerFreqList				NeighCellsPerBandclassListCDMA2000
}

NeighCellCDMA2000-r11 ::=	SEQUENCE {
	bandClass							BandclassCDMA2000,
	neighFreqInfoList-r11				SEQUENCE (SIZE (1..16)) OF NeighCellsPerBandclassCDMA2000-r11
}

NeighCellsPerBandclassListCDMA2000 ::= SEQUENCE (SIZE (1..16)) OF NeighCellsPerBandclassCDMA2000

NeighCellsPerBandclassCDMA2000 ::=	SEQUENCE {
	arfcn								ARFCN-ValueCDMA2000,
	physCellIdList						PhysCellIdListCDMA2000
}

NeighCellsPerBandclassCDMA2000-r11 ::=	SEQUENCE {
	arfcn								ARFCN-ValueCDMA2000,
	physCellIdList-r11					SEQUENCE (SIZE (1..40)) OF PhysCellIdCDMA2000
}

NeighCellListCDMA2000-v920 ::=		SEQUENCE (SIZE (1..16)) OF NeighCellCDMA2000-v920

NeighCellCDMA2000-v920 ::=			SEQUENCE {
	neighCellsPerFreqList-v920			NeighCellsPerBandclassListCDMA2000-v920
}

NeighCellsPerBandclassListCDMA2000-v920 ::= SEQUENCE (SIZE (1..16)) OF NeighCellsPerBandclassCDMA2000-v920

NeighCellsPerBandclassCDMA2000-v920 ::=	SEQUENCE {
	physCellIdList-v920					PhysCellIdListCDMA2000-v920
}

PhysCellIdListCDMA2000 ::=			SEQUENCE (SIZE (1..16)) OF PhysCellIdCDMA2000

PhysCellIdListCDMA2000-v920 ::=		SEQUENCE (SIZE (0..24)) OF PhysCellIdCDMA2000

BandClassListCDMA2000 ::=			SEQUENCE (SIZE (1..maxCDMA-BandClass)) OF BandClassInfoCDMA2000

BandClassInfoCDMA2000 ::=	SEQUENCE {
	bandClass							BandclassCDMA2000,
	cellReselectionPriority				CellReselectionPriority				OPTIONAL,	-- Need OP
	threshX-High						INTEGER (0..63),
	threshX-Low							INTEGER (0..63),
	...
}

AC-BarringConfig1XRTT-r9 ::=		SEQUENCE {
	ac-Barring0to9-r9					INTEGER (0..63),
	ac-Barring10-r9						INTEGER (0..7),
	ac-Barring11-r9						INTEGER (0..7),
	ac-Barring12-r9						INTEGER (0..7),
	ac-Barring13-r9						INTEGER (0..7),
	ac-Barring14-r9						INTEGER (0..7),
	ac-Barring15-r9						INTEGER (0..7),
	ac-BarringMsg-r9					INTEGER (0..7),
	ac-BarringReg-r9					INTEGER (0..7),
	ac-BarringEmg-r9					INTEGER (0..7)
}

SIB8-PerPLMN-List-r11 ::=			SEQUENCE (SIZE (1..maxPLMN-r11)) OF SIB8-PerPLMN-r11

SIB8-PerPLMN-r11 ::=				SEQUENCE {
	plmn-Identity-r11					INTEGER (1..maxPLMN-r11),
	parametersCDMA2000-r11				CHOICE {
		explicitValue						ParametersCDMA2000-r11,
		defaultValue						NULL
	}
}

ParametersCDMA2000-r11 ::=			SEQUENCE {
	systemTimeInfo-r11					CHOICE	{
		explicitValue						SystemTimeInfoCDMA2000,
		defaultValue						NULL
	}																OPTIONAL,	-- Need OR
	searchWindowSize-r11				INTEGER (0..15),
	parametersHRPD-r11					SEQUENCE {
		preRegistrationInfoHRPD-r11			PreRegistrationInfoHRPD,
		cellReselectionParametersHRPD-r11	CellReselectionParametersCDMA2000-r11	OPTIONAL -- Need OR
	}		OPTIONAL,	-- Need OR
	parameters1XRTT-r11					SEQUENCE {
		csfb-RegistrationParam1XRTT-r11		CSFB-RegistrationParam1XRTT			OPTIONAL, -- Need OP
		csfb-RegistrationParam1XRTT-Ext-r11	CSFB-RegistrationParam1XRTT-v920	OPTIONAL, -- Cond REG-1XRTT-PerPLMN
		longCodeState1XRTT-r11				BIT STRING (SIZE (42))	OPTIONAL, -- Cond PerPLMN-LC
		cellReselectionParameters1XRTT-r11	CellReselectionParametersCDMA2000-r11	OPTIONAL, -- Need OR
		ac-BarringConfig1XRTT-r11			AC-BarringConfig1XRTT-r9			OPTIONAL, -- Cond REG-1XRTT-PerPLMN
		csfb-SupportForDualRxUEs-r11		BOOLEAN								OPTIONAL, -- Need OR
		csfb-DualRxTxSupport-r11			ENUMERATED {true}			OPTIONAL -- Cond REG-1XRTT-PerPLMN
	}		OPTIONAL,	-- Need OR
	...
}


SystemInformationBlockType9 ::=		SEQUENCE {
	hnb-Name							OCTET STRING (SIZE(1..48))		OPTIONAL,	-- Need OR
	...,
	lateNonCriticalExtension				OCTET STRING				OPTIONAL
}


SystemInformationBlockType10 ::=	SEQUENCE {
	messageIdentifier					BIT STRING (SIZE (16)),
	serialNumber						BIT STRING (SIZE (16)),
	warningType							OCTET STRING (SIZE (2)),
	dummy								OCTET STRING (SIZE (50))	OPTIONAL,		-- Need OP
	...,
	lateNonCriticalExtension			OCTET STRING				OPTIONAL
}


SystemInformationBlockType11 ::=	SEQUENCE {
	messageIdentifier					BIT STRING (SIZE (16)),
	serialNumber						BIT STRING (SIZE (16)),
	warningMessageSegmentType			ENUMERATED {notLastSegment, lastSegment},
	warningMessageSegmentNumber			INTEGER (0..63),
	warningMessageSegment				OCTET STRING,
	dataCodingScheme					OCTET STRING (SIZE (1))		OPTIONAL,	-- Cond Segment1
	...,
	lateNonCriticalExtension				OCTET STRING				OPTIONAL
}


SystemInformationBlockType12-r9 ::=	SEQUENCE {
	messageIdentifier-r9				BIT STRING (SIZE (16)),
	serialNumber-r9						BIT STRING (SIZE (16)),
	warningMessageSegmentType-r9		ENUMERATED {notLastSegment, lastSegment},
	warningMessageSegmentNumber-r9		INTEGER (0..63),
	warningMessageSegment-r9			OCTET STRING,
	dataCodingScheme-r9					OCTET STRING (SIZE (1))		OPTIONAL,	-- Cond Segment1
	lateNonCriticalExtension			OCTET STRING					OPTIONAL,
	...
}


SystemInformationBlockType13-r9 ::=	SEQUENCE {
	mbsfn-AreaInfoList-r9				MBSFN-AreaInfoList-r9,
	notificationConfig-r9				MBMS-NotificationConfig-r9,
	lateNonCriticalExtension			OCTET STRING					OPTIONAL,
	...,
	[[
	notificationConfig-v1430			MBMS-NotificationConfig-v1430		OPTIONAL
	]]
}


SystemInformationBlockType14-r11 ::=	SEQUENCE {
	eab-Param-r11							CHOICE {
		eab-Common-r11							EAB-Config-r11,
		eab-PerPLMN-List-r11					SEQUENCE (SIZE (1..maxPLMN-r11)) OF EAB-ConfigPLMN-r11
	}														OPTIONAL, -- Need OR
	lateNonCriticalExtension				OCTET STRING			OPTIONAL,
	...
}

EAB-ConfigPLMN-r11 ::=				SEQUENCE {
	eab-Config-r11						EAB-Config-r11				OPTIONAL -- Need OR
}

EAB-Config-r11 ::=					SEQUENCE {
	eab-Category-r11					ENUMERATED {a, b, c},
	eab-BarringBitmap-r11				BIT STRING (SIZE (10))
}


SystemInformationBlockType15-r11 ::=	SEQUENCE {
	mbms-SAI-IntraFreq-r11					MBMS-SAI-List-r11				OPTIONAL,	-- Need OR
	mbms-SAI-InterFreqList-r11				MBMS-SAI-InterFreqList-r11		OPTIONAL,	-- Need OR
	lateNonCriticalExtension				OCTET STRING					OPTIONAL,
	...,
	[[	mbms-SAI-InterFreqList-v1140		MBMS-SAI-InterFreqList-v1140	OPTIONAL	-- Cond InterFreq
	]],
	[[	mbms-IntraFreqCarrierType-r14		MBMS-CarrierType-r14			OPTIONAL,	-- Need OR
		mbms-InterFreqCarrierTypeList-r14
											MBMS-InterFreqCarrierTypeList-r14	OPTIONAL	-- Need OR
	]]
}

MBMS-SAI-List-r11 ::=					SEQUENCE (SIZE (1..maxSAI-MBMS-r11)) OF MBMS-SAI-r11

MBMS-SAI-r11 ::=						INTEGER (0..65535)

MBMS-SAI-InterFreqList-r11 ::=			SEQUENCE (SIZE (1..maxFreq)) OF MBMS-SAI-InterFreq-r11

MBMS-SAI-InterFreqList-v1140 ::=		SEQUENCE (SIZE (1..maxFreq)) OF MBMS-SAI-InterFreq-v1140

MBMS-SAI-InterFreq-r11 ::=				SEQUENCE {
	dl-CarrierFreq-r11						ARFCN-ValueEUTRA-r9,
	mbms-SAI-List-r11						MBMS-SAI-List-r11
}

MBMS-SAI-InterFreq-v1140 ::=			SEQUENCE {
		multiBandInfoList-r11				MultiBandInfoList-r11			OPTIONAL	-- Need OR
}

MBMS-InterFreqCarrierTypeList-r14 ::=	SEQUENCE (SIZE (1..maxFreq)) OF MBMS-CarrierType-r14

MBMS-CarrierType-r14 ::=				SEQUENCE {
	carrierType-r14							ENUMERATED {mbms, fembmsMixed, fembmsDedicated},
	frameOffset-r14							INTEGER (0..3)					OPTIONAL	-- Need OR
}


SystemInformationBlockType16-r11 ::=		SEQUENCE {
	timeInfo-r11							SEQUENCE {
		timeInfoUTC-r11						INTEGER (0..549755813887),
		dayLightSavingTime-r11				BIT STRING (SIZE (2))		OPTIONAL,	-- Need OR
		leapSeconds-r11						INTEGER (-127..128)			OPTIONAL,	-- Need OR
		localTimeOffset-r11					INTEGER (-63..64)			OPTIONAL	-- Need OR
	}																	OPTIONAL,	-- Need OR
	lateNonCriticalExtension			OCTET STRING				OPTIONAL,
	...
}


SystemInformationBlockType17-r12 ::=	SEQUENCE {
	wlan-OffloadInfoPerPLMN-List-r12		SEQUENCE (SIZE (1..maxPLMN-r11)) OF
										WLAN-OffloadInfoPerPLMN-r12			OPTIONAL, -- Need OR
	lateNonCriticalExtension				OCTET STRING				OPTIONAL,
	...
}

WLAN-OffloadInfoPerPLMN-r12 ::=			SEQUENCE {
		wlan-OffloadConfigCommon-r12		WLAN-OffloadConfig-r12		OPTIONAL,	-- Need OR
		wlan-Id-List-r12					WLAN-Id-List-r12			OPTIONAL,	-- Need OR
		...
}

WLAN-Id-List-r12 ::=				SEQUENCE (SIZE (1..maxWLAN-Id-r12)) OF WLAN-Identifiers-r12

WLAN-Identifiers-r12 ::=			SEQUENCE {
	ssid-r12						OCTET STRING (SIZE (1..32))		OPTIONAL,	-- Need OR
	bssid-r12						OCTET STRING (SIZE (6))			OPTIONAL,	-- Need OR
	hessid-r12						OCTET STRING (SIZE (6))			OPTIONAL,	-- Need OR
	...
}


SystemInformationBlockType18-r12 ::= SEQUENCE {
	commConfig-r12						SEQUENCE {
		commRxPool-r12						SL-CommRxPoolList-r12,
		commTxPoolNormalCommon-r12			SL-CommTxPoolList-r12			OPTIONAL,	-- Need OR
		commTxPoolExceptional-r12			SL-CommTxPoolList-r12			OPTIONAL,	-- Need OR
		commSyncConfig-r12					SL-SyncConfigList-r12		OPTIONAL	-- Need OR
	}																		OPTIONAL,	-- Need OR
	lateNonCriticalExtension			OCTET STRING						OPTIONAL,
	...,
	[[	commTxPoolNormalCommonExt-r13			SL-CommTxPoolListExt-r13	OPTIONAL,	-- Need OR
		commTxResourceUC-ReqAllowed-r13			ENUMERATED {true}		OPTIONAL,	-- Need OR
		commTxAllowRelayCommon-r13				ENUMERATED {true}			OPTIONAL	-- Need OR
	]]
}


SystemInformationBlockType19-r12 ::= SEQUENCE {
	discConfig-r12						SEQUENCE {
		discRxPool-r12						SL-DiscRxPoolList-r12,
		discTxPoolCommon-r12				SL-DiscTxPoolList-r12			OPTIONAL,	-- Need OR
		discTxPowerInfo-r12				SL-DiscTxPowerInfoList-r12	OPTIONAL,	-- Cond Tx
		discSyncConfig-r12					SL-SyncConfigList-r12		OPTIONAL	-- Need OR
	}																		OPTIONAL,	-- Need OR
	discInterFreqList-r12				SL-CarrierFreqInfoList-r12		OPTIONAL,	-- Need OR
	lateNonCriticalExtension			OCTET STRING						OPTIONAL,
	...,
	[[	discConfig-v1310				SEQUENCE {
			discInterFreqList-v1310			SL-CarrierFreqInfoList-v1310	OPTIONAL,	-- Need OR
			gapRequestsAllowedCommon		ENUMERATED {true}			OPTIONAL	-- Need OR
		}																OPTIONAL,	-- Need OR
		discConfigRelay-r13				SEQUENCE {
			relayUE-Config-r13				SL-DiscConfigRelayUE-r13,
			remoteUE-Config-r13				SL-DiscConfigRemoteUE-r13
		}																OPTIONAL,	-- Need OR
		discConfigPS-13					SEQUENCE {
			discRxPoolPS-r13				SL-DiscRxPoolList-r12,
			discTxPoolPS-Common-r13			SL-DiscTxPoolList-r12		OPTIONAL	-- Need OR
		}																OPTIONAL	-- Need OR
	]]
}

SL-CarrierFreqInfoList-r12 ::=	SEQUENCE (SIZE (1..maxFreq)) OF SL-CarrierFreqInfo-r12

SL-CarrierFreqInfoList-v1310 ::=	SEQUENCE (SIZE (1..maxFreq)) OF SL-CarrierFreqInfo-v1310

SL-CarrierFreqInfo-r12::=		SEQUENCE {
	carrierFreq-r12					ARFCN-ValueEUTRA-r9,
	plmn-IdentityList-r12			PLMN-IdentityList4-r12			OPTIONAL	-- Need OP
}

SL-DiscConfigRelayUE-r13	::= SEQUENCE {
	threshHigh-r13			RSRP-RangeSL4-r13						OPTIONAL,	-- Need OR
	threshLow-r13			RSRP-RangeSL4-r13						OPTIONAL,	-- Need OR
	hystMax-r13				ENUMERATED {dB0, dB3, dB6, dB9, dB12, dBinf}	OPTIONAL,	-- Cond ThreshHigh
	hystMin-r13				ENUMERATED {dB0, dB3, dB6, dB9, dB12}	OPTIONAL	-- Cond ThreshLow
}

SL-DiscConfigRemoteUE-r13	::= SEQUENCE {
	threshHigh-r13			RSRP-RangeSL4-r13						OPTIONAL,	-- Need OR
	hystMax-r13				ENUMERATED {dB0, dB3, dB6, dB9, dB12}	OPTIONAL,	-- Cond ThreshHigh
	reselectionInfoIC-r13	ReselectionInfoRelay-r13
}

ReselectionInfoRelay-r13 ::=	SEQUENCE {
	q-RxLevMin-r13					Q-RxLevMin,
	-- Note that the mapping of invidual values may be different for PC5, but the granularity/
	-- number of values is same as for Uu
	filterCoefficient-r13			FilterCoefficient,
	minHyst-r13					ENUMERATED {dB0, dB3,
										dB6, dB9, dB12, dBinf}	OPTIONAL	-- Need OR
}

SL-CarrierFreqInfo-v1310::=	SEQUENCE {
	discResourcesNonPS-r13			SL-ResourcesInterFreq-r13		OPTIONAL,	-- Need OR
	discResourcesPS-r13				SL-ResourcesInterFreq-r13		OPTIONAL,	-- Need OR
	discConfigOther-r13			SL-DiscConfigOtherInterFreq-r13		OPTIONAL,	-- Need OR
	...
}

PLMN-IdentityList4-r12 ::=	SEQUENCE (SIZE (1..maxPLMN-r11)) OF	PLMN-IdentityInfo2-r12

PLMN-IdentityInfo2-r12 ::=		CHOICE	{
	plmn-Index-r12					INTEGER (1..maxPLMN-r11),
	plmnIdentity-r12				PLMN-Identity
}

SL-DiscTxResourcesInterFreq-r13 ::=	CHOICE {
	acquireSI-FromCarrier-r13		NULL,
	discTxPoolCommon-r13			SL-DiscTxPoolList-r12,
	requestDedicated-r13			NULL,
	noTxOnCarrier-r13				NULL
}

SL-DiscConfigOtherInterFreq-r13::=	SEQUENCE {
	txPowerInfo-r13					SL-DiscTxPowerInfoList-r12			OPTIONAL,	-- Cond Tx
	refCarrierCommon-r13			ENUMERATED {pCell}					OPTIONAL,	-- Need OR
	discSyncConfig-r13				SL-SyncConfigListNFreq-r13			OPTIONAL,	-- Need OR
	discCellSelectionInfo-r13		CellSelectionInfoNFreq-r13			OPTIONAL	-- Need OR
}

SL-ResourcesInterFreq-r13 ::= SEQUENCE {
	discRxResourcesInterFreq-r13	SL-DiscRxPoolList-r12				OPTIONAL,	-- Need OR
	discTxResourcesInterFreq-r13	SL-DiscTxResourcesInterFreq-r13		OPTIONAL	-- Need OR
}


SystemInformationBlockType20-r13 ::=	SEQUENCE {
	sc-mcch-RepetitionPeriod-r13		ENUMERATED {rf2, rf4, rf8, rf16, rf32, rf64, rf128, rf256},
	sc-mcch-Offset-r13				INTEGER (0..10),
	sc-mcch-FirstSubframe-r13		INTEGER (0..9),
	sc-mcch-duration-r13			INTEGER (2..9)	OPTIONAL,
	sc-mcch-ModificationPeriod-r13	ENUMERATED {rf2, rf4, rf8, rf16, rf32, rf64, rf128, rf256,
										rf512, rf1024, r2048, rf4096, rf8192, rf16384, rf32768,												rf65536},
	lateNonCriticalExtension			OCTET STRING						OPTIONAL,
	...,
	[[	br-BCCH-Config-r14					SEQUENCE {
			dummy		ENUMERATED {rf1},
			dummy2	ENUMERATED {rf1},
			mpdcch-Narrowband-SC-MCCH-r14		INTEGER (1..maxAvailNarrowBands-r13),
			mpdcch-NumRepetition-SC-MCCH-r14	ENUMERATED {r1, r2, r4, r8, r16,
															r32, r64, r128, r256},
			mpdcch-StartSF-SC-MCCH-r14			CHOICE {
				fdd-r14								ENUMERATED {v1, v1dot5, v2, v2dot5, v4,
																v5, v8, v10},
				tdd-r14								ENUMERATED {v1, v2, v4, v5, v8, v10, v20}
			},
			mpdcch-PDSCH-HoppingConfig-SC-MCCH-r14	ENUMERATED {off, ce-ModeA, ce-ModeB},
			sc-mcch-CarrierFreq-r14				ARFCN-ValueEUTRA-r9,
			sc-mcch-Offset-BR-r14				INTEGER (0..10),
			sc-mcch-RepetitionPeriod-BR-r14		ENUMERATED {rf32, rf128, rf512, rf1024,
													rf2048, rf4096, rf8192, rf16384},
			sc-mcch-ModificationPeriod-BR-r14	ENUMERATED { rf32, rf128, rf256, rf512, rf1024,
													rf2048, rf4096, rf8192, rf16384, rf32768,
													rf65536, rf131072, rf262144, rf524288,
													rf1048576}
		}																	OPTIONAL,	-- Need OR
		sc-mcch-SchedulingInfo-r14			SC-MCCH-SchedulingInfo-r14		OPTIONAL,	-- Need OP
		pdsch-maxNumRepetitionCEmodeA-SC-MTCH-r14
											ENUMERATED { r16, r32 }		OPTIONAL,	-- Need OR
		pdsch-maxNumRepetitionCEmodeB-SC-MTCH-r14
											ENUMERATED {
												r192, r256, r384, r512, r768, r1024,
												r1536, r2048}				OPTIONAL	-- Need OR
	]],
	 [[	sc-mcch-RepetitionPeriod-v1470		ENUMERATED {rf1} 				OPTIONAL,	-- Need OR
		sc-mcch-ModificationPeriod-v1470	ENUMERATED {rf1} 				OPTIONAL	-- Need OR
	]]
}

SC-MCCH-SchedulingInfo-r14::=	SEQUENCE	{
	onDurationTimerSCPTM-r14			ENUMERATED {psf10, psf20, psf100, psf300,
												psf500, psf1000, psf1200, psf1600},
	drx-InactivityTimerSCPTM-r14		ENUMERATED {psf0, psf1, psf2, psf4, psf8, psf16,
												psf32, psf64, psf128, psf256, ps512,
												psf1024, psf2048, psf4096, psf8192, psf16384},
	schedulingPeriodStartOffsetSCPTM-r14	CHOICE {
		sf10									INTEGER(0..9),
		sf20									INTEGER(0..19),
		sf32									INTEGER(0..31),
		sf40									INTEGER(0..39),
		sf64									INTEGER(0..63),
		sf80									INTEGER(0..79),
		sf128									INTEGER(0..127),
		sf160									INTEGER(0..159),
		sf256									INTEGER(0..255),
		sf320									INTEGER(0..319),
		sf512									INTEGER(0..511),
		sf640									INTEGER(0..639),
		sf1024									INTEGER(0..1023),
		sf2048									INTEGER(0..2047),
		sf4096									INTEGER(0..4095),
		sf8192									INTEGER(0..8191)
	},
	...
}


SystemInformationBlockType21-r14 ::= SEQUENCE {
	sl-V2X-ConfigCommon-r14				SL-V2X-ConfigCommon-r14				OPTIONAL,	-- Need OR
	lateNonCriticalExtension			OCTET STRING						OPTIONAL,
	...
}

SL-V2X-ConfigCommon-r14 ::=		SEQUENCE {
	v2x-CommRxPool-r14					SL-CommRxPoolListV2X-r14			OPTIONAL,	-- Need OR
	v2x-CommTxPoolNormalCommon-r14		SL-CommTxPoolListV2X-r14			OPTIONAL,	-- Need OR
	p2x-CommTxPoolNormalCommon-r14		SL-CommTxPoolListV2X-r14			OPTIONAL,	-- Need OR
	v2x-CommTxPoolExceptional-r14		SL-CommResourcePoolV2X-r14			OPTIONAL,	-- Need OR
	v2x-SyncConfig-r14					SL-SyncConfigListV2X-r14			OPTIONAL,	-- Need OR
	v2x-InterFreqInfoList-r14			SL-InterFreqInfoListV2X-r14			OPTIONAL,	-- Need OR
	v2x-ResourceSelectionConfig-r14		SL-CommTxPoolSensingConfig-r14		OPTIONAL,	-- Need OR
	zoneConfig-r14						SL-ZoneConfig-r14					OPTIONAL,	-- Need OR
	typeTxSync-r14						SL-TypeTxSync-r14					OPTIONAL,	-- Need OR
	thresSL-TxPrioritization-r14		SL-Priority-r13						OPTIONAL,	-- Need OR
	anchorCarrierFreqList-r14			SL-AnchorCarrierFreqList-V2X-r14	OPTIONAL,	-- Need OR
	offsetDFN-r14						INTEGER (0..1000)					OPTIONAL,	-- Need OR
	cbr-CommonTxConfigList-r14			SL-CBR-CommonTxConfigList-r14		OPTIONAL	-- Need OR
}



AntennaInfoCommon ::=				SEQUENCE {
	antennaPortsCount					ENUMERATED {an1, an2, an4, spare1}
}

AntennaInfoDedicated ::=			SEQUENCE {
	transmissionMode					ENUMERATED {
											tm1, tm2, tm3, tm4, tm5, tm6,
											tm7, tm8-v920},
	codebookSubsetRestriction			CHOICE {
		n2TxAntenna-tm3						BIT STRING (SIZE (2)),
		n4TxAntenna-tm3						BIT STRING (SIZE (4)),
		n2TxAntenna-tm4						BIT STRING (SIZE (6)),
		n4TxAntenna-tm4						BIT STRING (SIZE (64)),
		n2TxAntenna-tm5						BIT STRING (SIZE (4)),
		n4TxAntenna-tm5						BIT STRING (SIZE (16)),
		n2TxAntenna-tm6						BIT STRING (SIZE (4)),
		n4TxAntenna-tm6						BIT STRING (SIZE (16))
	}		OPTIONAL,															-- Cond TM
	ue-TransmitAntennaSelection			CHOICE{
		release							NULL,
		setup							ENUMERATED {closedLoop, openLoop}
	}
}

AntennaInfoDedicated-v920 ::=		SEQUENCE {
	codebookSubsetRestriction-v920		CHOICE {
		n2TxAntenna-tm8-r9					BIT STRING (SIZE (6)),
		n4TxAntenna-tm8-r9					BIT STRING (SIZE (32))
	}		OPTIONAL															-- Cond TM8
}

AntennaInfoDedicated-r10 ::=		SEQUENCE {
	transmissionMode-r10				ENUMERATED {
											tm1, tm2, tm3, tm4, tm5, tm6, tm7, tm8-v920,
											tm9-v1020, tm10-v1130, spare6, spare5, spare4,
											spare3, spare2, spare1},
	codebookSubsetRestriction-r10		BIT STRING			OPTIONAL,			-- Cond TMX
	ue-TransmitAntennaSelection		CHOICE{
		release							NULL,
		setup							ENUMERATED {closedLoop, openLoop}
	}
}

AntennaInfoDedicated-v10i0::=	SEQUENCE {
	maxLayersMIMO-r10			ENUMERATED {twoLayers, fourLayers, eightLayers}		OPTIONAL	-- Need OR
}

AntennaInfoDedicated-v1250 ::=		SEQUENCE {
	alternativeCodebookEnabledFor4TX-r12	BOOLEAN
}

AntennaInfoDedicated-v1430 ::=		SEQUENCE {
	ce-UE-TxAntennaSelection-config-r14			ENUMERATED {on}		OPTIONAL	-- Need OR
}


AntennaInfoUL-r10 ::=		SEQUENCE {
	transmissionModeUL-r10				ENUMERATED {tm1, tm2, spare6, spare5,
													spare4, spare3, spare2, spare1}	OPTIONAL,	-- Need OR
	fourAntennaPortActivated-r10			ENUMERATED {setup}			OPTIONAL		-- Need OR
}


CQI-ReportAperiodic-r10	::=		CHOICE {
	release								NULL,
	setup								SEQUENCE {
		cqi-ReportModeAperiodic-r10			CQI-ReportModeAperiodic,
		aperiodicCSI-Trigger-r10			SEQUENCE {
			trigger1-r10					BIT STRING (SIZE (8)),
			trigger2-r10					BIT STRING (SIZE (8))
		}																	OPTIONAL	-- Need OR
	}
}

CQI-ReportAperiodic-v1250	::=		CHOICE {
	release								NULL,
	setup								SEQUENCE {
		aperiodicCSI-Trigger-v1250			SEQUENCE {
			trigger-SubframeSetIndicator-r12	ENUMERATED {s1, s2},
			trigger1-SubframeSetIndicator-r12	BIT STRING (SIZE (8)),
			trigger2-SubframeSetIndicator-r12	BIT STRING (SIZE (8))
		}
	}
}

CQI-ReportAperiodic-v1310	::=		CHOICE {
	release								NULL,
	setup								SEQUENCE {
		aperiodicCSI-Trigger-v1310			SEQUENCE {
			trigger1-r13					BIT STRING (SIZE (32)),
			trigger2-r13					BIT STRING (SIZE (32)),
			trigger3-r13					BIT STRING (SIZE (32)),
			trigger4-r13					BIT STRING (SIZE (32)),
			trigger5-r13					BIT STRING (SIZE (32)),
			trigger6-r13					BIT STRING (SIZE (32))
		}																	OPTIONAL,	-- Need ON
		aperiodicCSI-Trigger2-r13		CHOICE {
			release							NULL,
			setup						SEQUENCE {
				trigger1-SubframeSetIndicator-r13	BIT STRING (SIZE (32)),
				trigger2-SubframeSetIndicator-r13	BIT STRING (SIZE (32)),
				trigger3-SubframeSetIndicator-r13	BIT STRING (SIZE (32)),
				trigger4-SubframeSetIndicator-r13	BIT STRING (SIZE (32)),
				trigger5-SubframeSetIndicator-r13	BIT STRING (SIZE (32)),
				trigger6-SubframeSetIndicator-r13	BIT STRING (SIZE (32))
			}
		}																	OPTIONAL	-- Need ON
	}
}

CQI-ReportAperiodicProc-r11	::=		SEQUENCE {
	cqi-ReportModeAperiodic-r11			CQI-ReportModeAperiodic,
	trigger01-r11						BOOLEAN,
	trigger10-r11						BOOLEAN,
	trigger11-r11						BOOLEAN
}

CQI-ReportAperiodicProc-v1310	::=		SEQUENCE {
	trigger001-r13						BOOLEAN,
	trigger010-r13						BOOLEAN,
	trigger011-r13						BOOLEAN,
	trigger100-r13						BOOLEAN,
	trigger101-r13						BOOLEAN,
	trigger110-r13						BOOLEAN,
	trigger111-r13						BOOLEAN
}

CQI-ReportAperiodicHybrid-r14	::=		SEQUENCE {
	triggers-r14						CHOICE {
		oneBit-r14							SEQUENCE {
			trigger1-Indicator-r14				BIT STRING (SIZE (8))
		},
		twoBit-r14							SEQUENCE {
			trigger01-Indicator-r14				BIT STRING (SIZE (8)),
			trigger10-Indicator-r14				BIT STRING (SIZE (8)),
			trigger11-Indicator-r14				BIT STRING (SIZE (8))
		},
		threeBit-r14						SEQUENCE {
			trigger001-Indicator-r14			BIT STRING (SIZE (32)),
			trigger010-Indicator-r14			BIT STRING (SIZE (32)),
			trigger011-Indicator-r14			BIT STRING (SIZE (32)),
			trigger100-Indicator-r14			BIT STRING (SIZE (32)) ,
			trigger101-Indicator-r14			BIT STRING (SIZE (32)),
			trigger110-Indicator-r14			BIT STRING (SIZE (32)),
			trigger111-Indicator-r14			BIT STRING (SIZE (32))
		}
	}																OPTIONAL	-- Need OR
}

CQI-ReportModeAperiodic ::=				ENUMERATED {
											rm12, rm20, rm22, rm30, rm31,
											rm32-v1250, rm10-v1310, rm11-v1310
}


CQI-ReportBoth-r11 ::=			SEQUENCE {
	csi-IM-ConfigToReleaseList-r11		CSI-IM-ConfigToReleaseList-r11	OPTIONAL,	-- Need ON
	csi-IM-ConfigToAddModList-r11		CSI-IM-ConfigToAddModList-r11	OPTIONAL,	-- Need ON
	csi-ProcessToReleaseList-r11		CSI-ProcessToReleaseList-r11	OPTIONAL,	-- Need ON
	csi-ProcessToAddModList-r11			CSI-ProcessToAddModList-r11		OPTIONAL	-- Need ON
}

CQI-ReportBoth-v1250 ::=			SEQUENCE {
	csi-IM-ConfigToReleaseListExt-r12		CSI-IM-ConfigId-v1250	OPTIONAL,	-- Need ON
	csi-IM-ConfigToAddModListExt-r12		CSI-IM-ConfigExt-r12	OPTIONAL	-- Need ON
}

CQI-ReportBoth-v1310 ::=			SEQUENCE {
	csi-IM-ConfigToReleaseListExt-r13	CSI-IM-ConfigToReleaseListExt-r13	OPTIONAL,	-- Need ON
	csi-IM-ConfigToAddModListExt-r13	CSI-IM-ConfigToAddModListExt-r13	OPTIONAL	-- Need ON
}

CSI-IM-ConfigToAddModList-r11 ::=		SEQUENCE (SIZE (1..maxCSI-IM-r11)) OF CSI-IM-Config-r11

CSI-IM-ConfigToAddModListExt-r13 ::=	SEQUENCE (SIZE (1..maxCSI-IM-v1310)) OF CSI-IM-ConfigExt-r12

CSI-IM-ConfigToReleaseList-r11 ::=		SEQUENCE (SIZE (1..maxCSI-IM-r11)) OF CSI-IM-ConfigId-r11

CSI-IM-ConfigToReleaseListExt-r13 ::=	SEQUENCE (SIZE (1..maxCSI-IM-v1310)) OF CSI-IM-ConfigId-v1310

CSI-ProcessToAddModList-r11 ::=		SEQUENCE (SIZE (1..maxCSI-Proc-r11)) OF CSI-Process-r11

CSI-ProcessToReleaseList-r11 ::=	SEQUENCE (SIZE (1..maxCSI-Proc-r11)) OF CSI-ProcessId-r11

CQI-ReportBothProc-r11 ::=			SEQUENCE {
	ri-Ref-CSI-ProcessId-r11			CSI-ProcessId-r11				OPTIONAL,		-- Need OR
	pmi-RI-Report-r11					ENUMERATED {setup}				OPTIONAL		-- Need OR
}


CQI-ReportConfig ::=				SEQUENCE {
	cqi-ReportModeAperiodic			CQI-ReportModeAperiodic	OPTIONAL,			-- Need OR
	nomPDSCH-RS-EPRE-Offset				INTEGER (-1..6),
	cqi-ReportPeriodic				CQI-ReportPeriodic	OPTIONAL				-- Need ON
}

CQI-ReportConfig-v920 ::=		SEQUENCE {
	cqi-Mask-r9						ENUMERATED {setup}		OPTIONAL,		-- Cond cqi-Setup
	pmi-RI-Report-r9				ENUMERATED {setup}		OPTIONAL		-- Cond PMIRI
}

CQI-ReportConfig-r10 ::=	SEQUENCE {
	cqi-ReportAperiodic-r10				CQI-ReportAperiodic-r10			OPTIONAL,	-- Need ON
	nomPDSCH-RS-EPRE-Offset			INTEGER (-1..6),
	cqi-ReportPeriodic-r10				CQI-ReportPeriodic-r10			OPTIONAL,	-- Need ON
	pmi-RI-Report-r9					ENUMERATED {setup}				OPTIONAL,	-- Cond PMIRIPCell
	csi-SubframePatternConfig-r10		CHOICE {
		release							NULL,
		setup							SEQUENCE {
			csi-MeasSubframeSet1-r10			MeasSubframePattern-r10,
			csi-MeasSubframeSet2-r10			MeasSubframePattern-r10
		}
	}																	OPTIONAL	-- Need ON
}

CQI-ReportConfig-v1130 ::=	SEQUENCE {
	cqi-ReportPeriodic-v1130			CQI-ReportPeriodic-v1130,
	cqi-ReportBoth-r11					CQI-ReportBoth-r11
}

CQI-ReportConfig-v1250 ::=		SEQUENCE {
	csi-SubframePatternConfig-r12		CHOICE {
		release							NULL,
		setup							SEQUENCE {
			csi-MeasSubframeSets-r12			BIT STRING (SIZE (10))
		}
	}																OPTIONAL,	-- Need ON
	cqi-ReportBoth-v1250					CQI-ReportBoth-v1250		OPTIONAL,	-- Need ON
	cqi-ReportAperiodic-v1250	CQI-ReportAperiodic-v1250		OPTIONAL,	-- Need ON
	altCQI-Table-r12			ENUMERATED {
									allSubframes, csi-SubframeSet1,
									csi-SubframeSet2, spare1}		OPTIONAL		-- Need OP
}

CQI-ReportConfig-v1310 ::=			SEQUENCE {
		cqi-ReportBoth-v1310				CQI-ReportBoth-v1310		OPTIONAL,	-- Need ON
		cqi-ReportAperiodic-v1310			CQI-ReportAperiodic-v1310	OPTIONAL,		-- Need ON
		cqi-ReportPeriodic-v1310			CQI-ReportPeriodic-v1310	OPTIONAL		-- Need ON
}

CQI-ReportConfig-v1320 ::=			SEQUENCE {
		cqi-ReportPeriodic-v1320			CQI-ReportPeriodic-v1320	OPTIONAL	-- Need ON
}

CQI-ReportConfig-v1430 ::=			SEQUENCE {
		cqi-ReportAperiodicHybrid-r14		CQI-ReportAperiodicHybrid-r14	OPTIONAL	-- Need ON
}

CQI-ReportConfigSCell-r10 ::=				SEQUENCE {
	cqi-ReportModeAperiodic-r10			CQI-ReportModeAperiodic OPTIONAL,			-- Need OR
	nomPDSCH-RS-EPRE-Offset-r10				INTEGER (-1..6),
	cqi-ReportPeriodicSCell-r10			CQI-ReportPeriodic-r10			OPTIONAL,	-- Need ON
	pmi-RI-Report-r10					ENUMERATED {setup}				OPTIONAL	-- Cond PMIRISCell
}



CQI-ReportPeriodic ::=		CHOICE {
	release							NULL,
	setup							SEQUENCE {
		cqi-PUCCH-ResourceIndex				INTEGER (0..1185),
		cqi-pmi-ConfigIndex					INTEGER (0..1023),
		cqi-FormatIndicatorPeriodic			CHOICE {
			widebandCQI							NULL,
			subbandCQI							SEQUENCE {
				k									INTEGER (1..4)
			}
		},
		ri-ConfigIndex						INTEGER (0..1023)	OPTIONAL,				-- Need OR
		simultaneousAckNackAndCQI			BOOLEAN
	}
}

CQI-ReportPeriodic-r10 ::=		CHOICE {
	release								NULL,
	setup								SEQUENCE {
		cqi-PUCCH-ResourceIndex-r10			INTEGER (0..1184),
		cqi-PUCCH-ResourceIndexP1-r10		INTEGER (0..1184)				OPTIONAL,	-- Need OR
		cqi-pmi-ConfigIndex				INTEGER (0..1023),
		cqi-FormatIndicatorPeriodic-r10		CHOICE {
			widebandCQI-r10						SEQUENCE {
				csi-ReportMode-r10		ENUMERATED {submode1, submode2}		OPTIONAL	-- Need OR
			},
			subbandCQI-r10						SEQUENCE {
				k								INTEGER (1..4),
				periodicityFactor-r10				ENUMERATED {n2, n4}
			}
		},
		ri-ConfigIndex					INTEGER (0..1023)		OPTIONAL,				-- Need OR
		simultaneousAckNackAndCQI		BOOLEAN,
		cqi-Mask-r9						ENUMERATED {setup}		OPTIONAL,				-- Need OR
		csi-ConfigIndex-r10				CHOICE {
			release							NULL,
			setup							SEQUENCE {
				cqi-pmi-ConfigIndex2-r10		INTEGER (0..1023),
				ri-ConfigIndex2-r10				INTEGER (0..1023)		OPTIONAL		-- Need OR
			}
		}		OPTIONAL																-- Need ON
	}
}


CQI-ReportPeriodic-v1130 ::=	SEQUENCE {
	simultaneousAckNackAndCQI-Format3-r11		ENUMERATED {setup}		OPTIONAL,	-- Need OR
	cqi-ReportPeriodicProcExtToReleaseList-r11	CQI-ReportPeriodicProcExtToReleaseList-r11	OPTIONAL,	-- Need ON
	cqi-ReportPeriodicProcExtToAddModList-r11	CQI-ReportPeriodicProcExtToAddModList-r11	OPTIONAL	-- Need ON
}

CQI-ReportPeriodic-v1310 ::=	SEQUENCE {
	cri-ReportConfig-r13			CRI-ReportConfig-r13				OPTIONAL,	-- Need OR
	simultaneousAckNackAndCQI-Format4-Format5-r13		ENUMERATED {setup}		OPTIONAL-- Need OR
}

CQI-ReportPeriodic-v1320 ::=	SEQUENCE {
	periodicityFactorWB-r13			ENUMERATED {n2, n4}			OPTIONAL		-- Need OR
}

CQI-ReportPeriodicProcExtToAddModList-r11 ::=		SEQUENCE (SIZE (1..maxCQI-ProcExt-r11)) OF CQI-ReportPeriodicProcExt-r11

CQI-ReportPeriodicProcExtToReleaseList-r11 ::=	SEQUENCE (SIZE (1..maxCQI-ProcExt-r11)) OF CQI-ReportPeriodicProcExtId-r11

CQI-ReportPeriodicProcExt-r11 ::=		SEQUENCE {
	cqi-ReportPeriodicProcExtId-r11	CQI-ReportPeriodicProcExtId-r11,
	cqi-pmi-ConfigIndex-r11			INTEGER (0..1023),
	cqi-FormatIndicatorPeriodic-r11	CHOICE {
		widebandCQI-r11				SEQUENCE {
			csi-ReportMode-r11			ENUMERATED {submode1, submode2}	OPTIONAL	-- Need OR
		},
		subbandCQI-r11				SEQUENCE {
			k							INTEGER (1..4),
			periodicityFactor-r11		ENUMERATED {n2, n4}
		}
	},
	ri-ConfigIndex-r11				INTEGER (0..1023)					OPTIONAL,	-- Need OR
	csi-ConfigIndex-r11				CHOICE {
		release							NULL,
		setup							SEQUENCE {
			cqi-pmi-ConfigIndex2-r11		INTEGER (0..1023),
			ri-ConfigIndex2-r11				INTEGER (0..1023)		OPTIONAL		-- Need OR
		}
	}																OPTIONAL,		-- Need ON
	...,
	[[	cri-ReportConfig-r13			CRI-ReportConfig-r13				OPTIONAL	-- Need ON
	]],
	[[	periodicityFactorWB-r13			ENUMERATED {n2, n4}			OPTIONAL		-- Need ON
	]]
}

CRI-ReportConfig-r13 ::=			CHOICE {
	release								NULL,
	setup								SEQUENCE {
		cri-ConfigIndex-r13					CRI-ConfigIndex-r13,
		cri-ConfigIndex2-r13				CRI-ConfigIndex-r13	OPTIONAL	-- Need OR
	}
}

CRI-ConfigIndex-r13 ::=				INTEGER (0..1023)


CQI-ReportPeriodicProcExtId-r11 ::=					INTEGER (1..maxCQI-ProcExt-r11)


CrossCarrierSchedulingConfig-r10 ::=		SEQUENCE {
	schedulingCellInfo-r10				CHOICE {
		own-r10								SEQUENCE {					-- No cross carrier scheduling
			cif-Presence-r10						BOOLEAN
		},
		other-r10								SEQUENCE {					-- Cross carrier scheduling
			schedulingCellId-r10				ServCellIndex-r10,
			pdsch-Start-r10						INTEGER (1..4)
		}
	}
}

CrossCarrierSchedulingConfig-r13 ::=		SEQUENCE {
	schedulingCellInfo-r13				CHOICE {
		own-r13								SEQUENCE {					-- No cross carrier scheduling
			cif-Presence-r13						BOOLEAN
		},
		other-r13							SEQUENCE {					-- Cross carrier scheduling
			schedulingCellId-r13				ServCellIndex-r13,
			pdsch-Start-r13						INTEGER (1..4),
			cif-InSchedulingCell-r13				INTEGER (1..7)
		}
	}
}

CrossCarrierSchedulingConfigLAA-UL-r14 ::=		SEQUENCE {
	schedulingCellId-r14							ServCellIndex-r13,
	cif-InSchedulingCell-r14						INTEGER (1..7)
}

CSI-IM-Config-r11 ::=		SEQUENCE {
	csi-IM-ConfigId-r11			CSI-IM-ConfigId-r11,
	resourceConfig-r11			INTEGER (0..31),
	subframeConfig-r11			INTEGER (0..154),
	...,
	[[	interferenceMeasRestriction-r13		BOOLEAN		OPTIONAL	-- Need ON
	]]
}

CSI-IM-ConfigExt-r12 ::=		SEQUENCE {
	csi-IM-ConfigId-v1250			CSI-IM-ConfigId-v1250,
	resourceConfig-r12			INTEGER (0..31),
	subframeConfig-r12			INTEGER (0..154),
	...,
	[[	interferenceMeasRestriction-r13	BOOLEAN				OPTIONAL,	-- Need ON
		csi-IM-ConfigId-v1310		CSI-IM-ConfigId-v1310	OPTIONAL	-- Need ON
	]]
}


CSI-IM-ConfigId-r11 ::=					INTEGER (1..maxCSI-IM-r11)
CSI-IM-ConfigId-r12 ::=					INTEGER (1..maxCSI-IM-r12)
CSI-IM-ConfigId-v1250 ::=				INTEGER (maxCSI-IM-r12)
CSI-IM-ConfigId-v1310 ::=				INTEGER (minCSI-IM-r13..maxCSI-IM-r13)
CSI-IM-ConfigId-r13 ::=					INTEGER (1..maxCSI-IM-r13)


CSI-Process-r11 ::=		SEQUENCE {
	csi-ProcessId-r11			CSI-ProcessId-r11,
	csi-RS-ConfigNZPId-r11		CSI-RS-ConfigNZPId-r11,
	csi-IM-ConfigId-r11			CSI-IM-ConfigId-r11,
	p-C-AndCBSRList-r11			P-C-AndCBSR-Pair-r13a,
	cqi-ReportBothProc-r11		CQI-ReportBothProc-r11					OPTIONAL,		-- Need OR
	cqi-ReportPeriodicProcId-r11	INTEGER (0..maxCQI-ProcExt-r11)		OPTIONAL,		-- Need OR
	cqi-ReportAperiodicProc-r11	CQI-ReportAperiodicProc-r11				OPTIONAL,		-- Need OR
	...,
	[[	alternativeCodebookEnabledFor4TXProc-r12	ENUMERATED {true}	OPTIONAL,	-- Need ON
		csi-IM-ConfigIdList-r12		CHOICE {
			release						NULL,
			setup						SEQUENCE (SIZE (1..2)) OF CSI-IM-ConfigId-r12
		}																OPTIONAL,	-- Need ON
		cqi-ReportAperiodicProc2-r12	CHOICE {
			release						NULL,
			setup						CQI-ReportAperiodicProc-r11
		}																OPTIONAL	-- Need ON
	]],
	[[	cqi-ReportAperiodicProc-v1310	CHOICE {
			release							NULL,
			setup							CQI-ReportAperiodicProc-v1310
		}																OPTIONAL,		-- Need ON
		cqi-ReportAperiodicProc2-v1310	CHOICE {
			release							NULL,
			setup							CQI-ReportAperiodicProc-v1310
		}																OPTIONAL,		-- Need ON
		eMIMO-Type-r13					CSI-RS-ConfigEMIMO-r13			OPTIONAL		-- Need ON
	]],
	[[	eMIMO-Type-v1430				CSI-RS-ConfigEMIMO-v1430		OPTIONAL,		-- Need ON
		eMIMO-Hybrid-r14				CSI-RS-ConfigEMIMO-Hybrid-r14		OPTIONAL,	-- Need ON
		advancedCodebookEnabled-r14		BOOLEAN							OPTIONAL		-- Need ON
	]]
}

CSI-ProcessId-r11 ::=		INTEGER (1..maxCSI-Proc-r11)


CSI-RS-Config-r10 ::=		SEQUENCE {
	csi-RS-r10					CHOICE {
		release						NULL,
		setup						SEQUENCE {
			antennaPortsCount-r10			ENUMERATED {an1, an2, an4, an8},
			resourceConfig-r10				INTEGER (0..31),
			subframeConfig-r10				INTEGER (0..154),
			p-C-r10							INTEGER (-8..15)
		}
	}																OPTIONAL,			-- Need ON
	zeroTxPowerCSI-RS-r10		ZeroTxPowerCSI-RS-Conf-r12			OPTIONAL			-- Need ON
}

CSI-RS-Config-v1250 ::=		SEQUENCE {
	zeroTxPowerCSI-RS2-r12		ZeroTxPowerCSI-RS-Conf-r12			OPTIONAL,			-- Need ON
	ds-ZeroTxPowerCSI-RS-r12		CHOICE {
		release							NULL,
		setup							SEQUENCE {
			zeroTxPowerCSI-RS-List-r12		SEQUENCE (SIZE (1..maxDS-ZTP-CSI-RS-r12)) OF ZeroTxPowerCSI-RS-r12
		}
	}																OPTIONAL				-- Need ON
}

CSI-RS-Config-v1310 ::=		SEQUENCE {
	eMIMO-Type-r13				CSI-RS-ConfigEMIMO-r13			OPTIONAL	-- Need ON
}

CSI-RS-Config-v1430 ::=		SEQUENCE {
	eMIMO-Type-v1430				CSI-RS-ConfigEMIMO-v1430			OPTIONAL,	-- Need ON
	eMIMO-Hybrid-r14				CSI-RS-ConfigEMIMO-Hybrid-r14		OPTIONAL,	-- Need ON
	advancedCodebookEnabled-r14		BOOLEAN								OPTIONAL	-- Need ON
}

ZeroTxPowerCSI-RS-Conf-r12 ::=	CHOICE {
		release							NULL,
		setup							ZeroTxPowerCSI-RS-r12
}

ZeroTxPowerCSI-RS-r12 ::=	SEQUENCE {
	zeroTxPowerResourceConfigList-r12		BIT STRING (SIZE (16)),
	zeroTxPowerSubframeConfig-r12			INTEGER (0..154)
}


CSI-RS-ConfigBeamformed-r13 ::=			SEQUENCE	{
	csi-RS-ConfigNZPIdListExt-r13			SEQUENCE (SIZE (1..7)) OF CSI-RS-ConfigNZPId-r13	OPTIONAL,	-- Need OR
	csi-IM-ConfigIdList-r13					SEQUENCE (SIZE (1..8)) OF CSI-IM-ConfigId-r13	OPTIONAL,	-- Need OR
	p-C-AndCBSR-PerResourceConfigList-r13	SEQUENCE (SIZE (1..8)) OF P-C-AndCBSR-Pair-r13	OPTIONAL,	-- Need OR
	ace-For4Tx-PerResourceConfigList-r13	SEQUENCE (SIZE (1..7)) OF BOOLEAN	OPTIONAL,	-- Need OR
	alternativeCodebookEnabledBeamformed-r13	ENUMERATED {true}	OPTIONAL,	-- Need OR
	channelMeasRestriction-r13				ENUMERATED {on}			OPTIONAL	-- Need OR
}

CSI-RS-ConfigBeamformed-r14 ::=			SEQUENCE	{
	csi-RS-ConfigNZPIdListExt-r14			SEQUENCE (SIZE (1..7)) OF CSI-RS-ConfigNZPId-r13	OPTIONAL,	-- Need OR
	csi-IM-ConfigIdList-r14					SEQUENCE (SIZE (1..8)) OF CSI-IM-ConfigId-r13	OPTIONAL,	-- Need OR
	p-C-AndCBSR-PerResourceConfigList-r14	SEQUENCE (SIZE (1..8)) OF P-C-AndCBSR-Pair-r13	OPTIONAL,	-- Need OR
	ace-For4Tx-PerResourceConfigList-r14	SEQUENCE (SIZE (1..7)) OF BOOLEAN	OPTIONAL,	-- Need OR
	alternativeCodebookEnabledBeamformed-r14	ENUMERATED {true}	OPTIONAL,	-- Need OR
	channelMeasRestriction-r14				ENUMERATED {on}			OPTIONAL,	-- Need OR
	csi-RS-ConfigNZP-ApList-r14				SEQUENCE (SIZE (1..8)) OF CSI-RS-ConfigNZP-r11
																			OPTIONAL,	-- Need OR
	nzp-ResourceConfigOriginal-v1430	CSI-RS-Config-NZP-v1430		OPTIONAL,	-- Need OR
	csi-RS-NZP-Activation-r14				CSI-RS-ConfigNZP-Activation-r14	OPTIONAL		-- Need OR
}

CSI-RS-ConfigBeamformed-v1430::=		SEQUENCE {
	csi-RS-ConfigNZP-ApList-r14				SEQUENCE (SIZE (1..8)) OF CSI-RS-ConfigNZP-r11
																			OPTIONAL,	-- Need OR
	nzp-ResourceConfigOriginal-v1430	CSI-RS-Config-NZP-v1430		OPTIONAL,	-- Need OR
	csi-RS-NZP-Activation-r14				CSI-RS-ConfigNZP-Activation-r14	OPTIONAL		-- Need OR
}

CSI-RS-Config-NZP-v1430::=		SEQUENCE {
	transmissionComb-r14					NZP-TransmissionComb-r14	OPTIONAL,	-- Need OR
	frequencyDensity-r14					NZP-FrequencyDensity-r14	OPTIONAL	-- Need OR
}

CSI-RS-ConfigNZP-Activation-r14::=		SEQUENCE {
	csi-RS-NZP-mode-r14						ENUMERATED {semiPersistent, aperiodic},
	activatedResources-r14					INTEGER (0..4)
}


CSI-RS-ConfigEMIMO-r13 ::=	CHOICE {
	release						NULL,
	setup						CHOICE {
		nonPrecoded-r13				CSI-RS-ConfigNonPrecoded-r13,
		beamformed-r13				CSI-RS-ConfigBeamformed-r13
	}
}

CSI-RS-ConfigEMIMO-v1430 ::=	CHOICE {
	release						NULL,
	setup						CHOICE {
		nonPrecoded-v1430				CSI-RS-ConfigNonPrecoded-v1430,
		beamformed-v1430				CSI-RS-ConfigBeamformed-v1430
	}
}

CSI-RS-ConfigEMIMO2-r14 ::=	CHOICE {
	release						NULL,
	setup						CSI-RS-ConfigBeamformed-r14
}

CSI-RS-ConfigEMIMO-Hybrid-r14 ::=	CHOICE {
	release						NULL,
	setup						SEQUENCE {
		periodicityOffsetIndex-r14			INTEGER (0..1023)				OPTIONAL,	-- Need OR
		eMIMO-Type2-r14						CSI-RS-ConfigEMIMO2-r14		OPTIONAL	-- Need ON
	}
}



CSI-RS-ConfigNonPrecoded-r13 ::=		SEQUENCE {
	p-C-AndCBSRList-r13						P-C-AndCBSR-Pair-r13			OPTIONAL,	-- Need OR
	codebookConfigN1-r13					ENUMERATED {n1, n2, n3, n4, n8},
	codebookConfigN2-r13					ENUMERATED {n1, n2, n3, n4, n8},
	codebookOverSamplingRateConfig-O1-r13	ENUMERATED {n4, n8}				OPTIONAL,	-- Need OR
	codebookOverSamplingRateConfig-O2-r13	ENUMERATED {n4, n8}				OPTIONAL,	-- Need OR
	codebookConfig-r13						INTEGER (1..4),
	csi-IM-ConfigIdList-r13					SEQUENCE (SIZE (1..2)) OF CSI-IM-ConfigId-r13	OPTIONAL,	-- Need OR
	csi-RS-ConfigNZP-EMIMO-r13				CSI-RS-ConfigNZP-EMIMO-r13		OPTIONAL	-- Need ON
}

CSI-RS-ConfigNonPrecoded-v1430::=		SEQUENCE {
	csi-RS-ConfigNZP-EMIMO-v1430			CSI-RS-ConfigNZP-EMIMO-v1430	OPTIONAL,	-- Need ON
	codebookConfigN1-v1430					ENUMERATED {n5, n6, n7, n10, n12, n14, n16},
	codebookConfigN2-r1430					ENUMERATED {n5, n6, n7 },
	nzp-ResourceConfigTM9-Original-v1430	CSI-RS-Config-NZP-v1430
}


CSI-RS-ConfigNZP-r11 ::=		SEQUENCE {
	csi-RS-ConfigNZPId-r11			CSI-RS-ConfigNZPId-r11,
	antennaPortsCount-r11			ENUMERATED {an1, an2, an4, an8},
	resourceConfig-r11				INTEGER (0..31),
	subframeConfig-r11				INTEGER (0..154),
	scramblingIdentity-r11			INTEGER (0..503),
	qcl-CRS-Info-r11				SEQUENCE {
		qcl-ScramblingIdentity-r11		INTEGER (0..503),
		crs-PortsCount-r11				ENUMERATED {n1, n2, n4, spare1},
		mbsfn-SubframeConfigList-r11	CHOICE {
				release						NULL,
				setup						SEQUENCE {
					subframeConfigList			MBSFN-SubframeConfigList
				}
		}																OPTIONAL	-- Need ON
	}																	OPTIONAL,	-- Need OR
	...,
	[[	csi-RS-ConfigNZPId-v1310		CSI-RS-ConfigNZPId-v1310		OPTIONAL	-- Need ON
	]],
	[[	transmissionComb-r14			NZP-TransmissionComb-r14		OPTIONAL,	-- Need OR
		frequencyDensity-r14			NZP-FrequencyDensity-r14		OPTIONAL	-- Need OR
	]],
	[[	mbsfn-SubframeConfigList-v1430	CHOICE {
				release						NULL,
				setup						SEQUENCE {
					subframeConfigList-v1430	MBSFN-SubframeConfigList-v1430
				}
		}																OPTIONAL	-- Need OP
	]]
}

CSI-RS-ConfigNZP-EMIMO-r13 ::=	CHOICE {
	release						NULL,
	setup						SEQUENCE {
		nzp-resourceConfigList-r13		SEQUENCE (SIZE (1..2)) OF NZP-ResourceConfig-r13,
		cdmType-r13						ENUMERATED {cdm2, cdm4}	OPTIONAL	-- Need OR
		}
}

CSI-RS-ConfigNZP-EMIMO-v1430 ::=	SEQUENCE {
	-- All extensions are for Non-Precoded so could be grouped by setup/ release choice
	nzp-resourceConfigListExt-r14	SEQUENCE (SIZE (0..4)) OF NZP-ResourceConfig-r13,
	cdmType-v1430					ENUMERATED {cdm8 }			OPTIONAL	-- Need OR
}

NZP-ResourceConfig-r13 ::=	SEQUENCE {
	resourceConfig-r13				ResourceConfig-r13,
	...,
	[[	transmissionComb-r14		NZP-TransmissionComb-r14		OPTIONAL,	-- Need OR
		frequencyDensity-r14		NZP-FrequencyDensity-r14		OPTIONAL	-- Need OR
	]]
}

ResourceConfig-r13 ::=				INTEGER (0..31)

NZP-TransmissionComb-r14 ::=			INTEGER (0..2)
NZP-FrequencyDensity-r14 ::=			ENUMERATED {d1, d2, d3}


CSI-RS-ConfigNZPId-r11 ::=					INTEGER (1..maxCSI-RS-NZP-r11)
CSI-RS-ConfigNZPId-v1310 ::=				INTEGER (minCSI-RS-NZP-r13..maxCSI-RS-NZP-r13)
CSI-RS-ConfigNZPId-r13 ::=					INTEGER (1..maxCSI-RS-NZP-r13)


CSI-RS-ConfigZP-r11 ::=		SEQUENCE {
	csi-RS-ConfigZPId-r11		CSI-RS-ConfigZPId-r11,
	resourceConfigList-r11		BIT STRING (SIZE (16)),
	subframeConfig-r11			INTEGER (0..154),
	...
}

CSI-RS-ConfigZP-ApList-r14 ::=	CHOICE {
	release							NULL,
	setup							SEQUENCE (SIZE (1.. maxCSI-RS-ZP-r11)) OF CSI-RS-ConfigZP-r11
}


CSI-RS-ConfigZPId-r11 ::=					INTEGER (1..maxCSI-RS-ZP-r11)


DataInactivityTimer-r14 ::=					ENUMERATED {
												s1, s2, s3, s5, s7, s10, s15, s20, s40, s50, s60,
												s80, s100, s120, s150, s180}


DMRS-Config-r11 ::=		CHOICE {
	release						NULL,
	setup						SEQUENCE {
		scramblingIdentity-r11		INTEGER (0..503),
		scramblingIdentity2-r11		INTEGER (0..503)
	}
}
DMRS-Config-v1310 ::=			SEQUENCE {
		dmrs-tableAlt-r13				ENUMERATED {true}			OPTIONAL	-- Need OR
}


DRB-Identity ::=					INTEGER (1..32)


EPDCCH-Config-r11 ::=		SEQUENCE{
	config-r11		CHOICE {
		release						NULL,
			setup						SEQUENCE {
			subframePatternConfig-r11	CHOICE {
				release						NULL,
				setup						SEQUENCE {
					subframePattern-r11			MeasSubframePattern-r10
				}
			}																	OPTIONAL, -- Need ON
			startSymbol-r11				INTEGER (1..4)							OPTIONAL, -- Need OP
			setConfigToReleaseList-r11	EPDCCH-SetConfigToReleaseList-r11		OPTIONAL, -- Need ON
			setConfigToAddModList-r11	EPDCCH-SetConfigToAddModList-r11		OPTIONAL -- Need ON
		}
	}
}

EPDCCH-SetConfigToAddModList-r11 ::=	SEQUENCE (SIZE(1..maxEPDCCH-Set-r11)) OF EPDCCH-SetConfig-r11

EPDCCH-SetConfigToReleaseList-r11 ::=	SEQUENCE (SIZE(1..maxEPDCCH-Set-r11)) OF EPDCCH-SetConfigId-r11

EPDCCH-SetConfig-r11 ::=		SEQUENCE {
	setConfigId-r11					EPDCCH-SetConfigId-r11,
	transmissionType-r11			ENUMERATED {localised, distributed},
	resourceBlockAssignment-r11		SEQUENCE{
		numberPRB-Pairs-r11				ENUMERATED {n2, n4, n8},
		resourceBlockAssignment-r11		BIT STRING (SIZE(4..38))
	},
	dmrs-ScramblingSequenceInt-r11	INTEGER (0..503),
	pucch-ResourceStartOffset-r11	INTEGER (0..2047),
	re-MappingQCL-ConfigId-r11		PDSCH-RE-MappingQCL-ConfigId-r11	OPTIONAL, -- Need OR
	...,
	[[	csi-RS-ConfigZPId2-r12				CHOICE {
			release						NULL,
			setup						CSI-RS-ConfigZPId-r11
		}															OPTIONAL	-- Need ON
	]],
	[[	numberPRB-Pairs-v1310			CHOICE {
			release							NULL,
			setup							ENUMERATED {n6}
		}															OPTIONAL,	-- Need ON
		mpdcch-config-r13				CHOICE {
			release							NULL,
			setup							SEQUENCE {
				csi-NumRepetitionCE-r13			ENUMERATED {sf1, sf2, sf4, sf8, sf16, sf32},
				mpdcch-pdsch-HoppingConfig-r13	ENUMERATED {on,off},
				mpdcch-StartSF-UESS-r13			CHOICE {
					fdd-r13							ENUMERATED {v1, v1dot5, v2, v2dot5, v4,
																v5, v8, v10},										tdd-r13							ENUMERATED {v1, v2, v4, v5, v8, v10,
																v20, spare1}
				},
				mpdcch-NumRepetition-r13		ENUMERATED {r1, r2, r4, r8, r16,
															r32, r64, r128, r256},
				mpdcch-Narrowband-r13			INTEGER (1.. maxAvailNarrowBands-r13)
			}
		}															OPTIONAL	-- Need ON
	]]
}

EPDCCH-SetConfigId-r11 ::=	INTEGER (0..1)


EIMTA-MainConfig-r12 ::=	CHOICE {
	release							NULL,
	setup							SEQUENCE {
		eimta-RNTI-r12				C-RNTI,
		eimta-CommandPeriodicity-r12	ENUMERATED {sf10, sf20, sf40, sf80},
		eimta-CommandSubframeSet-r12	BIT STRING (SIZE(10))
	}
}

EIMTA-MainConfigServCell-r12 ::=	CHOICE {
	release								NULL,
	setup								SEQUENCE {
		eimta-UL-DL-ConfigIndex-r12				INTEGER (1..5),
		eimta-HARQ-ReferenceConfig-r12		ENUMERATED {sa2, sa4, sa5},
		mbsfn-SubframeConfigList-v1250		CHOICE {
				release								NULL,
				setup								SEQUENCE {
				subframeConfigList-r12				MBSFN-SubframeConfigList
				}
		}
	}
}


LogicalChannelConfig ::=			SEQUENCE {
	ul-SpecificParameters				SEQUENCE {
		priority							INTEGER (1..16),
		prioritisedBitRate					ENUMERATED {
												kBps0, kBps8, kBps16, kBps32, kBps64, kBps128,
												kBps256, infinity, kBps512-v1020, kBps1024-v1020,
												kBps2048-v1020, spare5, spare4, spare3, spare2,
												spare1},
		bucketSizeDuration					ENUMERATED {
												ms50, ms100, ms150, ms300, ms500, ms1000, spare2,
												spare1},
		logicalChannelGroup					INTEGER (0..3)			OPTIONAL			-- Need OR
	}		OPTIONAL,																	-- Cond UL
	...,
	[[	logicalChannelSR-Mask-r9			ENUMERATED {setup}		OPTIONAL		-- Cond SRmask
	]],
	[[	logicalChannelSR-Prohibit-r12		BOOLEAN					OPTIONAL		-- Need ON
	]],
	[[	laa-UL-Allowed-r14					BOOLEAN					OPTIONAL,		-- Need ON
		bitRateQueryProhibitTimer-r14	ENUMERATED {
											s0, s0dot4, s0dot8, s1dot6, s3, s6, s12,
											s30}				OPTIONAL		--Need OR
	]]
}


LWA-Configuration-r13 ::=			CHOICE {
	release								NULL,
	setup								SEQUENCE {
		lwa-Config-r13					LWA-Config-r13
	}
}

LWA-Config-r13 ::=	SEQUENCE {
	lwa-MobilityConfig-r13			WLAN-MobilityConfig-r13		OPTIONAL,	-- Need ON
	lwa-WT-Counter-r13				INTEGER (0..65535)			OPTIONAL,	-- Need ON
	...,
	[[	wt-MAC-Address-r14		OCTET STRING (SIZE (6))	OPTIONAL	-- Need ON
	]]
}


LWIP-Configuration-r13 ::=			CHOICE {
	release								NULL,
	setup								SEQUENCE {
		lwip-Config-r13					LWIP-Config-r13
	}
}

LWIP-Config-r13 ::=	SEQUENCE {
	lwip-MobilityConfig-r13			WLAN-MobilityConfig-r13		OPTIONAL,	-- Need ON
	tunnelConfigLWIP-r13			TunnelConfigLWIP-r13		OPTIONAL,	-- Need ON
	...
}


MAC-MainConfig ::=					SEQUENCE {
	ul-SCH-Config						SEQUENCE {
		maxHARQ-Tx							ENUMERATED {
												n1, n2, n3, n4, n5, n6, n7, n8,
												n10, n12, n16, n20, n24, n28,
												spare2, spare1}		OPTIONAL,	-- Need ON
		periodicBSR-Timer					PeriodicBSR-Timer-r12	OPTIONAL,	-- Need ON
		retxBSR-Timer						RetxBSR-Timer-r12,
		ttiBundling							BOOLEAN
	}																OPTIONAL,	-- Need ON
	drx-Config							DRX-Config					OPTIONAL,	-- Need ON
	timeAlignmentTimerDedicated			TimeAlignmentTimer,
	phr-Config							CHOICE {
		release								NULL,
		setup								SEQUENCE {
			periodicPHR-Timer					ENUMERATED {sf10, sf20, sf50, sf100, sf200,
															sf500, sf1000, infinity},
			prohibitPHR-Timer					ENUMERATED {sf0, sf10, sf20, sf50, sf100,
																sf200, sf500, sf1000},
			dl-PathlossChange					ENUMERATED {dB1, dB3, dB6, infinity}
		}
	}																OPTIONAL,	-- Need ON
	...,
	[[	sr-ProhibitTimer-r9					INTEGER (0..7)			OPTIONAL	-- Need ON
	]],
	[[	mac-MainConfig-v1020				SEQUENCE {
			sCellDeactivationTimer-r10			ENUMERATED {
													rf2, rf4, rf8, rf16, rf32, rf64, rf128,
													spare}			OPTIONAL,	-- Need OP
			extendedBSR-Sizes-r10				ENUMERATED {setup}		OPTIONAL,	-- Need OR
			extendedPHR-r10						ENUMERATED {setup}		OPTIONAL	-- Need OR
		}															OPTIONAL	-- Need ON
	]],
	[[	stag-ToReleaseList-r11				STAG-ToReleaseList-r11	OPTIONAL,	-- Need ON
		stag-ToAddModList-r11				STAG-ToAddModList-r11	OPTIONAL,	-- Need ON
		drx-Config-v1130					DRX-Config-v1130		OPTIONAL	-- Need ON
	]],
	[[	e-HARQ-Pattern-r12					BOOLEAN					OPTIONAL,	-- Need ON
		dualConnectivityPHR					CHOICE {
			release								NULL,
			setup								SEQUENCE {
				phr-ModeOtherCG-r12					ENUMERATED {real, virtual}
			}
		}														OPTIONAL,	-- Need ON
		logicalChannelSR-Config-r12		CHOICE {
			release								NULL,
			setup								SEQUENCE {
				logicalChannelSR-ProhibitTimer-r12		ENUMERATED {sf20, sf40, sf64, sf128, sf512, sf1024, sf2560, spare1}
			}
		}															OPTIONAL		-- Need ON
	]],
	[[	drx-Config-v1310					DRX-Config-v1310		OPTIONAL,		-- Need ON
		extendedPHR2-r13					BOOLEAN		OPTIONAL,		-- Need ON
		eDRX-Config-CycleStartOffset-r13	CHOICE {
			release							NULL,
			setup
											CHOICE {
			sf5120									INTEGER(0..1),
			sf10240									INTEGER(0..3)
			}
		}										OPTIONAL	-- Need ON
	]],
	[[	drx-Config-r13						CHOICE {
			release								NULL,
			setup								DRX-Config-r13
		}															OPTIONAL	-- Need ON
	]],
	[[	skipUplinkTx-r14					CHOICE {
			release								NULL,
			setup								SEQUENCE {
				skipUplinkTxSPS-r14					ENUMERATED {true}		OPTIONAL,	-- Need OR
				skipUplinkTxDynamic-r14				ENUMERATED {true}		OPTIONAL	-- Need OR
			}
		}															OPTIONAL,	-- Need ON
		dataInactivityTimerConfig-r14		CHOICE {
			release								NULL,
			setup								SEQUENCE {
				dataInactivityTimer-r14				DataInactivityTimer-r14
			}
		}												OPTIONAL	-- Need ON
	]],
	[[	rai-Activation-r14					ENUMERATED {true}			OPTIONAL	-- Need OR
	]]
}

MAC-MainConfigSCell-r11 ::=			SEQUENCE {
	stag-Id-r11							STAG-Id-r11		OPTIONAL,	-- Need OP
	...
}

DRX-Config ::=						CHOICE {
	release								NULL,
	setup								SEQUENCE {
		onDurationTimer						ENUMERATED {
												psf1, psf2, psf3, psf4, psf5, psf6,
												psf8, psf10, psf20, psf30, psf40,
												psf50, psf60, psf80, psf100,
												psf200},
		drx-InactivityTimer					ENUMERATED {
												psf1, psf2, psf3, psf4, psf5, psf6,
												psf8, psf10, psf20, psf30, psf40,
												psf50, psf60, psf80, psf100,
												psf200, psf300, psf500, psf750,
												psf1280, psf1920, psf2560, psf0-v1020,
												spare9, spare8, spare7, spare6,
												spare5, spare4, spare3, spare2,
												spare1},
		drx-RetransmissionTimer				ENUMERATED {
												psf1, psf2, psf4, psf6, psf8, psf16,
												psf24, psf33},
		longDRX-CycleStartOffset		CHOICE {
			sf10							INTEGER(0..9),
			sf20							INTEGER(0..19),
			sf32							INTEGER(0..31),
			sf40							INTEGER(0..39),
			sf64							INTEGER(0..63),
			sf80							INTEGER(0..79),
			sf128							INTEGER(0..127),
			sf160							INTEGER(0..159),
			sf256							INTEGER(0..255),
			sf320							INTEGER(0..319),
			sf512							INTEGER(0..511),
			sf640							INTEGER(0..639),
			sf1024							INTEGER(0..1023),
			sf1280							INTEGER(0..1279),
			sf2048							INTEGER(0..2047),
			sf2560							INTEGER(0..2559)
		},
		shortDRX							SEQUENCE {
			shortDRX-Cycle						ENUMERATED	{
													sf2, sf5, sf8, sf10, sf16, sf20,
													sf32, sf40, sf64, sf80, sf128, sf160,
													sf256, sf320, sf512, sf640},
			drxShortCycleTimer					INTEGER (1..16)
		}		OPTIONAL													-- Need OR
	}
}

DRX-Config-v1130 ::=					SEQUENCE {
	drx-RetransmissionTimer-v1130			ENUMERATED {psf0-v1130}	OPTIONAL,	--Need OR
	longDRX-CycleStartOffset-v1130			CHOICE {
		sf60-v1130								INTEGER(0..59),
		sf70-v1130								INTEGER(0..69)
	}																OPTIONAL,	--Need OR
	shortDRX-Cycle-v1130					ENUMERATED	{sf4-v1130}	OPTIONAL	--Need OR
}
DRX-Config-v1310 ::=					SEQUENCE {
	longDRX-CycleStartOffset-v1310		SEQUENCE {
		sf60-v1310								INTEGER(0..59)
	}																OPTIONAL	--Need OR
}

DRX-Config-r13 ::=					SEQUENCE {
	onDurationTimer-v1310					ENUMERATED {psf300, psf400, psf500, psf600,
													psf800, psf1000, psf1200, psf1600}																		OPTIONAL,	--Need OR
	drx-RetransmissionTimer-v1310			ENUMERATED {psf40, psf64, psf80, psf96, psf112,
													psf128, psf160, psf320}
														OPTIONAL,	--Need OR
	drx-ULRetransmissionTimer-r13			ENUMERATED {psf0, psf1, psf2, psf4, psf6, psf8, psf16,
														psf24, psf33, psf40, psf64, psf80, psf96,
														psf112, psf128, psf160, psf320}
														OPTIONAL	--Need OR
}

PeriodicBSR-Timer-r12 ::=					ENUMERATED {
												sf5, sf10, sf16, sf20, sf32, sf40, sf64, sf80,
												sf128, sf160, sf320, sf640, sf1280, sf2560,
												infinity, spare1}

RetxBSR-Timer-r12 ::=							ENUMERATED {
												sf320, sf640, sf1280, sf2560, sf5120,
												sf10240, spare2, spare1}

STAG-ToReleaseList-r11 ::=	SEQUENCE (SIZE (1..maxSTAG-r11)) OF STAG-Id-r11

STAG-ToAddModList-r11 ::=	SEQUENCE (SIZE (1..maxSTAG-r11)) OF STAG-ToAddMod-r11

STAG-ToAddMod-r11 ::=		SEQUENCE {
	stag-Id-r11					STAG-Id-r11,
	timeAlignmentTimerSTAG-r11	TimeAlignmentTimer,
	...
}

STAG-Id-r11::=				INTEGER (1..maxSTAG-r11)


P-C-AndCBSR-r11 ::=	SEQUENCE {
	p-C-r11						INTEGER (-8..15),
	codebookSubsetRestriction-r11	BIT STRING
}

P-C-AndCBSR-r13 ::=	SEQUENCE {
	p-C-r13						INTEGER (-8..15),
	cbsr-Selection-r13			CHOICE{
		nonPrecoded-r13				SEQUENCE {
			codebookSubsetRestriction1-r13				BIT STRING,
			codebookSubsetRestriction2-r13				BIT STRING
		},
		beamformedK1a-r13			SEQUENCE {
			codebookSubsetRestriction3-r13				BIT STRING
		},
		beamformedKN-r13			SEQUENCE {
			codebookSubsetRestriction-r13				BIT STRING
		}
	},
	...
}

P-C-AndCBSR-Pair-r13a ::=	SEQUENCE (SIZE (1..2)) OF P-C-AndCBSR-r11

P-C-AndCBSR-Pair-r13 ::=	SEQUENCE (SIZE (1..2)) OF P-C-AndCBSR-r13


PDCCH-ConfigSCell-r13 ::=		SEQUENCE {
	skipMonitoringDCI-format0-1A-r13	ENUMERATED {true}				OPTIONAL	-- Need OR
}

PDCCH-ConfigLAA-r14 ::=		SEQUENCE {
	maxNumberOfSchedSubframes-Format0B-r14	ENUMERATED {sf2, sf3, sf4}	OPTIONAL,		-- Need OR
	maxNumberOfSchedSubframes-Format4B-r14	ENUMERATED {sf2, sf3, sf4}	OPTIONAL,		-- Need OR
	skipMonitoringDCI-Format0A-r14				ENUMERATED {true}		OPTIONAL,		-- Need OR
	skipMonitoringDCI-Format4A-r14				ENUMERATED {true}		OPTIONAL,		-- Need OR
	pdcch-CandidateReductions-Format0A-r14
								PDCCH-CandidateReductions-r13			OPTIONAL,		-- Need ON
	pdcch-CandidateReductions-Format4A-r14
								PDCCH-CandidateReductionsLAA-UL-r14		OPTIONAL,	-- Need ON
	pdcch-CandidateReductions-Format0B-r14
								PDCCH-CandidateReductionsLAA-UL-r14		OPTIONAL,	-- Need ON
	pdcch-CandidateReductions-Format4B-r14
								PDCCH-CandidateReductionsLAA-UL-r14	OPTIONAL		-- Need ON
}

PDCCH-CandidateReductionValue-r13 ::= ENUMERATED {n0, n33, n66, n100}

PDCCH-CandidateReductionValue-r14 ::= ENUMERATED {n0, n50, n100, n150}

PDCCH-CandidateReductions-r13 ::= CHOICE {
	release							NULL,
	setup							SEQUENCE {
		pdcch-candidateReductionAL1-r13		PDCCH-CandidateReductionValue-r13,
		pdcch-candidateReductionAL2-r13		PDCCH-CandidateReductionValue-r13,
		pdcch-candidateReductionAL3-r13		PDCCH-CandidateReductionValue-r13,
		pdcch-candidateReductionAL4-r13		PDCCH-CandidateReductionValue-r13,
		pdcch-candidateReductionAL5-r13		PDCCH-CandidateReductionValue-r13
	}
}

PDCCH-CandidateReductionsLAA-UL-r14 ::= CHOICE {
	release							NULL,
	setup							SEQUENCE {
		pdcch-candidateReductionAL1-r14		PDCCH-CandidateReductionValue-r13,
		pdcch-candidateReductionAL2-r14		PDCCH-CandidateReductionValue-r13,
		pdcch-candidateReductionAL3-r14		PDCCH-CandidateReductionValue-r14,
		pdcch-candidateReductionAL4-r14		PDCCH-CandidateReductionValue-r14,
		pdcch-candidateReductionAL5-r14		PDCCH-CandidateReductionValue-r14
	}
}


PDCP-Config ::=						SEQUENCE {
	discardTimer						ENUMERATED {
											ms50, ms100, ms150, ms300, ms500,
											ms750, ms1500, infinity
	}															OPTIONAL,			-- Cond Setup
	rlc-AM								SEQUENCE {
		statusReportRequired				BOOLEAN
	}															OPTIONAL,			-- Cond Rlc-AM
	rlc-UM								SEQUENCE {
		pdcp-SN-Size						ENUMERATED {len7bits, len12bits}
	}															OPTIONAL,			-- Cond Rlc-UM
	headerCompression					CHOICE {
		notUsed								NULL,
		rohc								SEQUENCE {
			maxCID								INTEGER (1..16383)				DEFAULT 15,
			profiles							SEQUENCE {
				profile0x0001						BOOLEAN,
				profile0x0002						BOOLEAN,
				profile0x0003						BOOLEAN,
				profile0x0004						BOOLEAN,
				profile0x0006						BOOLEAN,
				profile0x0101						BOOLEAN,
				profile0x0102						BOOLEAN,
				profile0x0103						BOOLEAN,
				profile0x0104						BOOLEAN
			},
			...
		}
	},
	...,
	[[	rn-IntegrityProtection-r10		ENUMERATED {enabled}	OPTIONAL	-- Cond RN
	]],
	[[	pdcp-SN-Size-v1130				ENUMERATED {len15bits}	OPTIONAL	-- Cond Rlc-AM2
	]],
	[[	ul-DataSplitDRB-ViaSCG-r12		BOOLEAN		OPTIONAL,	-- Need ON
		t-Reordering-r12				ENUMERATED {
										ms0, ms20, ms40, ms60, ms80, ms100, ms120, ms140,
										ms160, ms180, ms200, ms220, ms240, ms260, ms280, ms300,
										ms500, ms750, spare14, spare13, spare12, spare11, spare10,
										spare9, spare8, spare7, spare6, spare5, spare4, spare3,
										spare2, spare1}					OPTIONAL	-- Cond SetupS
	]],
	[[	ul-DataSplitThreshold-r13		CHOICE {
			release						NULL,
			setup						ENUMERATED {
										b0, b100, b200, b400, b800, b1600, b3200, b6400, b12800,
										b25600, b51200, b102400, b204800, b409600, b819200,
										spare1}
		}																OPTIONAL,	-- Need ON
		pdcp-SN-Size-v1310				ENUMERATED {len18bits}	OPTIONAL,	-- Cond Rlc-AM3
		statusFeedback-r13				CHOICE {
			release						NULL,
			setup						SEQUENCE {
				statusPDU-TypeForPolling-r13		ENUMERATED {type1, type2}		OPTIONAL,	-- Need ON
				statusPDU-Periodicity-Type1-r13		ENUMERATED {
										ms5, ms10, ms20, ms30, ms40, ms50, ms60, ms70, ms80, ms90,
										ms100, ms150, ms200, ms300, ms500, ms1000, ms2000, ms5000,
										ms10000, ms20000, ms50000}		OPTIONAL,	-- Need ON
				statusPDU-Periodicity-Type2-r13		ENUMERATED {
										ms5, ms10, ms20, ms30, ms40, ms50, ms60, ms70, ms80, ms90,
										ms100, ms150, ms200, ms300, ms500, ms1000, ms2000, ms5000,
										ms10000, ms20000, ms50000}		OPTIONAL,	-- Need ON
				statusPDU-Periodicity-Offset-r13	ENUMERATED {
										ms1, ms2, ms5, ms10, ms25, ms50, ms100, ms250, ms500,
										ms2500, ms5000, ms25000}	OPTIONAL	-- Need ON
			}
		}																OPTIONAL	-- Need ON
	]],
	[[	ul-LWA-Config-r14			CHOICE {
			release						NULL,
			setup						SEQUENCE {
				ul-LWA-DRB-ViaWLAN-r14		BOOLEAN,
				ul-LWA-DataSplitThreshold-r14	ENUMERATED {
										b0, b100, b200, b400, b800, b1600, b3200, b6400,
										b12800, b25600, b51200, b102400, b204800, b409600,
										b819200 }			OPTIONAL	-- Need OR
			}
		}														OPTIONAL,		-- Need ON
		uplinkOnlyHeaderCompression-r14		CHOICE {
			notUsed-r14							NULL,
			rohc-r14								SEQUENCE {
				maxCID-r14								INTEGER (1..16383)		DEFAULT 15,
				profiles-r14							SEQUENCE {
					profile0x0006-r14						BOOLEAN
				},
				...
			}
		}													OPTIONAL -- Need ON
	]]
}


PDSCH-ConfigCommon ::=		SEQUENCE {
	referenceSignalPower				INTEGER (-60..50),
	p-b									INTEGER (0..3)
}

PDSCH-ConfigCommon-v1310 ::=	SEQUENCE {
	pdsch-maxNumRepetitionCEmodeA-r13	ENUMERATED {
											r16, r32 }					OPTIONAL,	-- Need OR
	pdsch-maxNumRepetitionCEmodeB-r13	ENUMERATED {
											r192, r256, r384, r512, r768, r1024,
											r1536, r2048}					OPTIONAL	-- Need OR
}

PDSCH-ConfigDedicated::=		SEQUENCE {
	p-a									ENUMERATED {
											dB-6, dB-4dot77, dB-3, dB-1dot77,
											dB0, dB1, dB2, dB3}
}

PDSCH-ConfigDedicated-v1130 ::=		SEQUENCE {
	dmrs-ConfigPDSCH-r11				DMRS-Config-r11					OPTIONAL,	-- Need ON
	qcl-Operation						ENUMERATED {typeA, typeB}			OPTIONAL,	-- Need OR
	re-MappingQCLConfigToReleaseList-r11	RE-MappingQCLConfigToReleaseList-r11	OPTIONAL,	-- Need ON
	re-MappingQCLConfigToAddModList-r11		RE-MappingQCLConfigToAddModList-r11		OPTIONAL	-- Need ON
}

PDSCH-ConfigDedicated-v1280 ::=		SEQUENCE {
	tbsIndexAlt-r12						ENUMERATED {a26, a33}				OPTIONAL	-- Need OR
}

PDSCH-ConfigDedicated-v1310 ::=		SEQUENCE {
	dmrs-ConfigPDSCH-v1310				DMRS-Config-v1310					OPTIONAL	-- Need ON
}

PDSCH-ConfigDedicated-v1430 ::=		SEQUENCE {
	ce-PDSCH-MaxBandwidth-r14			ENUMERATED {bw5, bw20}				OPTIONAL,	-- Need OP
	ce-PDSCH-TenProcesses-r14			ENUMERATED {on}						OPTIONAL,	-- Need OR
	ce-HARQ-AckBundling-r14				ENUMERATED {on}						OPTIONAL,	-- Need OR
	ce-SchedulingEnhancement-r14		ENUMERATED {range1, range2}			OPTIONAL,	-- Need OR
	tbsIndexAlt2-r14						ENUMERATED {b33}				OPTIONAL	-- Need OR
}

PDSCH-ConfigDedicatedSCell-v1430 ::=		SEQUENCE {
	tbsIndexAlt2-r14						ENUMERATED {b33}				OPTIONAL	-- Need OR
}

RE-MappingQCLConfigToAddModList-r11 ::=		SEQUENCE (SIZE (1..maxRE-MapQCL-r11)) OF PDSCH-RE-MappingQCL-Config-r11

RE-MappingQCLConfigToReleaseList-r11 ::=	SEQUENCE (SIZE (1..maxRE-MapQCL-r11)) OF PDSCH-RE-MappingQCL-ConfigId-r11

PDSCH-RE-MappingQCL-Config-r11 ::=		SEQUENCE {
	pdsch-RE-MappingQCL-ConfigId-r11	PDSCH-RE-MappingQCL-ConfigId-r11,
	optionalSetOfFields-r11				SEQUENCE {
		crs-PortsCount-r11					ENUMERATED {n1, n2, n4, spare1},
		crs-FreqShift-r11					INTEGER (0..5),
		mbsfn-SubframeConfigList-r11		CHOICE {
			release								NULL,
			setup								SEQUENCE {
				subframeConfigList					MBSFN-SubframeConfigList
			}
		}																	OPTIONAL,	-- Need ON
		pdsch-Start-r11						ENUMERATED {reserved, n1, n2, n3, n4, assigned}
	}																		OPTIONAL,	-- Need OP
	csi-RS-ConfigZPId-r11				CSI-RS-ConfigZPId-r11,
	qcl-CSI-RS-ConfigNZPId-r11			CSI-RS-ConfigNZPId-r11				OPTIONAL,	-- Need OR
	...,
	[[	mbsfn-SubframeConfigList-v1430	CHOICE {
			release						NULL,
			setup						SEQUENCE {
				subframeConfigList-v1430	MBSFN-SubframeConfigList-v1430
			}
		}																	OPTIONAL	-- Need OP
	]]
}


PDSCH-RE-MappingQCL-ConfigId-r11 ::=		INTEGER (1..maxRE-MapQCL-r11)

PerCC-GapIndicationList-r14 ::=	SEQUENCE (SIZE (1..maxServCell-r13)) OF PerCC-GapIndication-r14

PerCC-GapIndication-r14 ::=			SEQUENCE {
	servCellId-r14								ServCellIndex-r13,
	gapIndication-r14							ENUMERATED {gap, ncsg, nogap-noNcsg}
}


PHICH-Config ::=					SEQUENCE {
	phich-Duration						ENUMERATED {normal, extended},
	phich-Resource						ENUMERATED {oneSixth, half, one, two}
}


PhysicalConfigDedicated ::=		SEQUENCE {
	pdsch-ConfigDedicated				PDSCH-ConfigDedicated			OPTIONAL,		-- Need ON
	pucch-ConfigDedicated				PUCCH-ConfigDedicated			OPTIONAL,		-- Need ON
	pusch-ConfigDedicated				PUSCH-ConfigDedicated			OPTIONAL,		-- Need ON
	uplinkPowerControlDedicated			UplinkPowerControlDedicated		OPTIONAL,		-- Need ON
	tpc-PDCCH-ConfigPUCCH				TPC-PDCCH-Config				OPTIONAL,		-- Need ON
	tpc-PDCCH-ConfigPUSCH				TPC-PDCCH-Config				OPTIONAL,		-- Need ON
	cqi-ReportConfig					CQI-ReportConfig				OPTIONAL,		-- Cond CQI-r8
	soundingRS-UL-ConfigDedicated		SoundingRS-UL-ConfigDedicated	OPTIONAL,		-- Need ON
	antennaInfo							CHOICE {
		explicitValue						AntennaInfoDedicated,
		defaultValue						NULL
	}																	OPTIONAL,	-- Cond AI-r8
	schedulingRequestConfig				SchedulingRequestConfig			OPTIONAL,		-- Need ON
	...,
	[[	cqi-ReportConfig-v920				CQI-ReportConfig-v920		OPTIONAL,		-- Cond CQI-r8
		antennaInfo-v920					AntennaInfoDedicated-v920	OPTIONAL		-- Cond AI-r8
	]],
	[[	antennaInfo-r10					CHOICE {
			explicitValue-r10				AntennaInfoDedicated-r10,
			defaultValue					NULL
		}																OPTIONAL,	-- Cond AI-r10
		antennaInfoUL-r10				AntennaInfoUL-r10				OPTIONAL,		-- Need ON
		cif-Presence-r10				BOOLEAN							OPTIONAL,		-- Need ON
		cqi-ReportConfig-r10			CQI-ReportConfig-r10			OPTIONAL,	-- Cond CQI-r10
		csi-RS-Config-r10				CSI-RS-Config-r10				OPTIONAL,		-- Need ON
		pucch-ConfigDedicated-v1020		PUCCH-ConfigDedicated-v1020		OPTIONAL,		-- Need ON
		pusch-ConfigDedicated-v1020		PUSCH-ConfigDedicated-v1020		OPTIONAL,		-- Need ON
		schedulingRequestConfig-v1020	SchedulingRequestConfig-v1020	OPTIONAL,		-- Need ON
		soundingRS-UL-ConfigDedicated-v1020
								SoundingRS-UL-ConfigDedicated-v1020		OPTIONAL,		-- Need ON
		soundingRS-UL-ConfigDedicatedAperiodic-r10
							SoundingRS-UL-ConfigDedicatedAperiodic-r10	OPTIONAL,		-- Need ON
		uplinkPowerControlDedicated-v1020
									UplinkPowerControlDedicated-v1020	OPTIONAL		-- Need ON
	]],
	[[	additionalSpectrumEmissionCA-r10			CHOICE {
			release									NULL,
			setup									SEQUENCE {
				additionalSpectrumEmissionPCell-r10		AdditionalSpectrumEmission
			}
		}			OPTIONAL	-- Need ON
	]],
	[[	-- DL configuration as well as configuration applicable for DL and UL
		csi-RS-ConfigNZPToReleaseList-r11
									CSI-RS-ConfigNZPToReleaseList-r11	OPTIONAL,		-- Need ON
		csi-RS-ConfigNZPToAddModList-r11
									CSI-RS-ConfigNZPToAddModList-r11	OPTIONAL,		-- Need ON
		csi-RS-ConfigZPToReleaseList-r11
									CSI-RS-ConfigZPToReleaseList-r11	OPTIONAL,		-- Need ON
		csi-RS-ConfigZPToAddModList-r11	CSI-RS-ConfigZPToAddModList-r11	OPTIONAL,		-- Need ON
		epdcch-Config-r11				EPDCCH-Config-r11				OPTIONAL,		-- Need ON
		pdsch-ConfigDedicated-v1130		PDSCH-ConfigDedicated-v1130		OPTIONAL,		-- Need ON
	-- UL configuration
		cqi-ReportConfig-v1130			CQI-ReportConfig-v1130			OPTIONAL,		-- Need ON
		pucch-ConfigDedicated-v1130		PUCCH-ConfigDedicated-v1130		OPTIONAL,		-- Need ON
		pusch-ConfigDedicated-v1130		PUSCH-ConfigDedicated-v1130		OPTIONAL,		-- Need ON
		uplinkPowerControlDedicated-v1130
									UplinkPowerControlDedicated-v1130	OPTIONAL		-- Need ON
	]],
	[[	antennaInfo-v1250				AntennaInfoDedicated-v1250		OPTIONAL,	-- Cond AI-r10
		eimta-MainConfig-r12			EIMTA-MainConfig-r12			OPTIONAL,		-- Need ON
		eimta-MainConfigPCell-r12		EIMTA-MainConfigServCell-r12	OPTIONAL,		-- Need ON
		pucch-ConfigDedicated-v1250		PUCCH-ConfigDedicated-v1250		OPTIONAL,		-- Need ON
		cqi-ReportConfigPCell-v1250		CQI-ReportConfig-v1250			OPTIONAL,		-- Need ON
		uplinkPowerControlDedicated-v1250
									UplinkPowerControlDedicated-v1250	OPTIONAL,		-- Need ON
		pusch-ConfigDedicated-v1250		PUSCH-ConfigDedicated-v1250		OPTIONAL,		-- Need ON
		csi-RS-Config-v1250					CSI-RS-Config-v1250			OPTIONAL		-- Need ON
	]],
	[[	pdsch-ConfigDedicated-v1280			PDSCH-ConfigDedicated-v1280	OPTIONAL		-- Need ON
	]],
	[[	pdsch-ConfigDedicated-v1310			PDSCH-ConfigDedicated-v1310	OPTIONAL,		-- Need ON
		pucch-ConfigDedicated-r13			PUCCH-ConfigDedicated-r13	OPTIONAL,		-- Need ON
		pusch-ConfigDedicated-r13			PUSCH-ConfigDedicated-r13	OPTIONAL,		-- Need ON
		pdcch-CandidateReductions-r13
										PDCCH-CandidateReductions-r13	OPTIONAL,		-- Need ON
		cqi-ReportConfig-v1310					CQI-ReportConfig-v1310	OPTIONAL,		-- Need ON
		soundingRS-UL-ConfigDedicated-v1310
								SoundingRS-UL-ConfigDedicated-v1310		OPTIONAL,		-- Need ON
		soundingRS-UL-ConfigDedicatedUpPTsExt-r13
						SoundingRS-UL-ConfigDedicatedUpPTsExt-r13		OPTIONAL,		-- Need ON
		soundingRS-UL-ConfigDedicatedAperiodic-v1310
						SoundingRS-UL-ConfigDedicatedAperiodic-v1310	OPTIONAL,		-- Need ON
		soundingRS-UL-ConfigDedicatedAperiodicUpPTsExt-r13
				SoundingRS-UL-ConfigDedicatedAperiodicUpPTsExt-r13		OPTIONAL,		-- Need ON
		csi-RS-Config-v1310				CSI-RS-Config-v1310				OPTIONAL,		-- Need ON
		ce-Mode-r13					CHOICE {
			release						NULL,
			setup						ENUMERATED {ce-ModeA,ce-ModeB}
		}																OPTIONAL,		-- Need ON
		csi-RS-ConfigNZPToAddModListExt-r13	CSI-RS-ConfigNZPToAddModListExt-r13	OPTIONAL,	-- Need ON
		csi-RS-ConfigNZPToReleaseListExt-r13	CSI-RS-ConfigNZPToReleaseListExt-r13	OPTIONAL	-- Need ON
	]],
	[[	cqi-ReportConfig-v1320					CQI-ReportConfig-v1320	OPTIONAL		-- Need ON
	]],
	[[	typeA-SRS-TPC-PDCCH-Group-r14	CHOICE {
			release							NULL,
			setup							SEQUENCE (SIZE (1..32)) OF SRS-TPC-PDCCH-Config-r14
		}																OPTIONAL,		-- Need ON
		must-Config-r14						CHOICE{
			release								NULL,
			setup								SEQUENCE {
				k-max-r14						ENUMERATED {l1, l3},
				p-a-must-r14					ENUMERATED {
													dB-6, dB-4dot77, dB-3, dB-1dot77,
													dB0, dB1, dB2, dB3}	OPTIONAL		-- Need ON
			}
		}															OPTIONAL,		-- Need ON
		pusch-EnhancementsConfig-r14		PUSCH-EnhancementsConfig-r14		OPTIONAL,	-- Need ON
		ce-pdsch-pusch-EnhancementConfig-r14		ENUMERATED {on}	OPTIONAL,	-- Need OR
		antennaInfo-v1430				AntennaInfoDedicated-v1430		OPTIONAL,	-- Need ON
		pucch-ConfigDedicated-v1430		PUCCH-ConfigDedicated-v1430		OPTIONAL,	-- Need ON
		pdsch-ConfigDedicated-v1430		PDSCH-ConfigDedicated-v1430		OPTIONAL,		-- Need ON
		pusch-ConfigDedicated-v1430		PUSCH-ConfigDedicated-v1430	OPTIONAL,		-- Need ON
		soundingRS-UL-PeriodicConfigDedicatedList-r14			SEQUENCE (SIZE (1..2)) OF SoundingRS-UL-ConfigDedicated	OPTIONAL,		-- Cond PeriodicSRSPCell
		soundingRS-UL-PeriodicConfigDedicatedUpPTsExtList-r14	SEQUENCE (SIZE (1..4)) OF SoundingRS-UL-ConfigDedicatedUpPTsExt-r13	OPTIONAL,		-- Cond PeriodicSRSExt
		soundingRS-UL-AperiodicConfigDedicatedList-r14			SEQUENCE (SIZE (1..2)) OF SoundingRS-UL-ConfigDedicatedAperiodic-r10	OPTIONAL,		-- Cond AperiodicSRS
		soundingRS-UL-ConfigDedicatedApUpPTsExtList-r14	SEQUENCE (SIZE (1..4)) OF SoundingRS-UL-ConfigDedicatedAperiodicUpPTsExt-r13	OPTIONAL,		-- Cond AperiodicSRSExt
		csi-RS-Config-v1430				CSI-RS-Config-v1430				OPTIONAL,		-- Need ON
		csi-RS-ConfigZP-ApList-r14				CSI-RS-ConfigZP-ApList-r14	OPTIONAL,	-- Need ON
		cqi-ReportConfig-v1430					CQI-ReportConfig-v1430	OPTIONAL,	-- Need ON
		semiOpenLoop-r14						BOOLEAN					OPTIONAL	-- Need ON
	]]
}

PhysicalConfigDedicated-v1370 ::=	SEQUENCE {
	pucch-ConfigDedicated-v1370			PUCCH-ConfigDedicated-v1370		OPTIONAL		-- Cond PUCCH-Format4or5
}

PhysicalConfigDedicatedSCell-r10 ::=		SEQUENCE {
	-- DL configuration as well as configuration applicable for DL and UL
	nonUL-Configuration-r10					SEQUENCE {
		antennaInfo-r10
											AntennaInfoDedicated-r10	OPTIONAL,		-- Need ON
		crossCarrierSchedulingConfig-r10
									CrossCarrierSchedulingConfig-r10	OPTIONAL,		-- Need ON
		csi-RS-Config-r10						CSI-RS-Config-r10		OPTIONAL,		-- Need ON
		pdsch-ConfigDedicated-r10				PDSCH-ConfigDedicated	OPTIONAL		-- Need ON
	}																	OPTIONAL,	-- Cond SCellAdd
	-- UL configuration
	ul-Configuration-r10					SEQUENCE {
		antennaInfoUL-r10						AntennaInfoUL-r10		OPTIONAL,		-- Need ON
		pusch-ConfigDedicatedSCell-r10
								PUSCH-ConfigDedicatedSCell-r10		OPTIONAL,	-- Cond PUSCH-SCell1
		uplinkPowerControlDedicatedSCell-r10
								UplinkPowerControlDedicatedSCell-r10	OPTIONAL,		-- Need ON
		cqi-ReportConfigSCell-r10			CQI-ReportConfigSCell-r10	OPTIONAL,		-- Need ON
		soundingRS-UL-ConfigDedicated-r10
										SoundingRS-UL-ConfigDedicated	OPTIONAL,		-- Need ON
		soundingRS-UL-ConfigDedicated-v1020
									SoundingRS-UL-ConfigDedicated-v1020	OPTIONAL,		-- Need ON
		soundingRS-UL-ConfigDedicatedAperiodic-r10
							SoundingRS-UL-ConfigDedicatedAperiodic-r10	OPTIONAL	-- Need ON
	}																	OPTIONAL,	-- Cond CommonUL
	...,
	[[	-- DL configuration as well as configuration applicable for DL and UL
		csi-RS-ConfigNZPToReleaseList-r11
									CSI-RS-ConfigNZPToReleaseList-r11	OPTIONAL,		-- Need ON
		csi-RS-ConfigNZPToAddModList-r11
									CSI-RS-ConfigNZPToAddModList-r11	OPTIONAL,		-- Need ON
		csi-RS-ConfigZPToReleaseList-r11
									CSI-RS-ConfigZPToReleaseList-r11	OPTIONAL,		-- Need ON
		csi-RS-ConfigZPToAddModList-r11
										CSI-RS-ConfigZPToAddModList-r11	OPTIONAL,		-- Need ON
		epdcch-Config-r11					EPDCCH-Config-r11			OPTIONAL,		-- Need ON
		pdsch-ConfigDedicated-v1130			PDSCH-ConfigDedicated-v1130	OPTIONAL,		-- Need ON
	-- UL configuration
		cqi-ReportConfig-v1130				CQI-ReportConfig-v1130		OPTIONAL,		-- Need ON
		pusch-ConfigDedicated-v1130
									PUSCH-ConfigDedicated-v1130		OPTIONAL,	-- Cond PUSCH-SCell1
		uplinkPowerControlDedicatedSCell-v1130
									UplinkPowerControlDedicated-v1130	OPTIONAL		-- Need ON
	]],
	[[	antennaInfo-v1250					AntennaInfoDedicated-v1250	OPTIONAL,		-- Need ON
		eimta-MainConfigSCell-r12
										EIMTA-MainConfigServCell-r12	OPTIONAL,		-- Need ON
		cqi-ReportConfigSCell-v1250			CQI-ReportConfig-v1250		OPTIONAL,		-- Need ON
		uplinkPowerControlDedicatedSCell-v1250
									UplinkPowerControlDedicated-v1250	OPTIONAL,		-- Need ON
		csi-RS-Config-v1250					CSI-RS-Config-v1250			OPTIONAL		-- Need ON
	]],
	[[	pdsch-ConfigDedicated-v1280			PDSCH-ConfigDedicated-v1280	OPTIONAL		-- Need ON
	]],
	[[	pucch-Cell-r13						ENUMERATED {true}		OPTIONAL,	-- Cond PUCCH-SCell1
		pucch-SCell							CHOICE{
			release								NULL,
			setup								SEQUENCE {
				pucch-ConfigDedicated-r13
											PUCCH-ConfigDedicated-r13	OPTIONAL,		-- Need ON
				schedulingRequestConfig-r13
									SchedulingRequestConfigSCell-r13	OPTIONAL,		-- Need ON
				tpc-PDCCH-ConfigPUCCH-SCell-r13
											TPC-PDCCH-ConfigSCell-r13	OPTIONAL,		-- Need ON
				pusch-ConfigDedicated-r13
										PUSCH-ConfigDedicated-r13	OPTIONAL,	-- Cond PUSCH-SCell
				uplinkPowerControlDedicated-r13
								UplinkPowerControlDedicatedSCell-v1310	OPTIONAL	-- Need ON
			}
		}																OPTIONAL,	-- Need ON
		crossCarrierSchedulingConfig-r13
						CrossCarrierSchedulingConfig-r13	OPTIONAL,	-- Cond Cross-Carrier-Config
		pdcch-ConfigSCell-r13				PDCCH-ConfigSCell-r13		OPTIONAL,		-- Need ON
		cqi-ReportConfig-v1310				CQI-ReportConfig-v1310		OPTIONAL,		-- Need ON
		pdsch-ConfigDedicated-v1310			PDSCH-ConfigDedicated-v1310	OPTIONAL,		-- Need ON
		soundingRS-UL-ConfigDedicated-v1310
								SoundingRS-UL-ConfigDedicated-v1310		OPTIONAL,		-- Need ON
		soundingRS-UL-ConfigDedicatedUpPTsExt-r13
							SoundingRS-UL-ConfigDedicatedUpPTsExt-r13	OPTIONAL,		-- Need ON
		soundingRS-UL-ConfigDedicatedAperiodic-v1310
						SoundingRS-UL-ConfigDedicatedAperiodic-v1310	OPTIONAL,		-- Need ON
		soundingRS-UL-ConfigDedicatedAperiodicUpPTsExt-r13
					SoundingRS-UL-ConfigDedicatedAperiodicUpPTsExt-r13	OPTIONAL,		-- Need ON
		csi-RS-Config-v1310					CSI-RS-Config-v1310			OPTIONAL,		-- Need ON
		laa-SCellConfiguration-r13			LAA-SCellConfiguration-r13	OPTIONAL,		-- Need ON
		csi-RS-ConfigNZPToAddModListExt-r13	CSI-RS-ConfigNZPToAddModListExt-r13	OPTIONAL,	-- Need ON
		csi-RS-ConfigNZPToReleaseListExt-r13	CSI-RS-ConfigNZPToReleaseListExt-r13	OPTIONAL	-- Need ON
	]],
	[[	cqi-ReportConfig-v1320				CQI-ReportConfig-v1320	OPTIONAL		-- Need ON
	]],
	[[	laa-SCellConfiguration-v1430		LAA-SCellConfiguration-v1430
																		OPTIONAL,	-- Need ON
		typeB-SRS-TPC-PDCCH-Config-r14		SRS-TPC-PDCCH-Config-r14	OPTIONAL,	-- Need ON

		uplinkPUSCH-LessPowerControlDedicated-v1430		UplinkPUSCH-LessPowerControlDedicated-v1430 OPTIONAL,		-- Need ON
		soundingRS-UL-PeriodicConfigDedicatedList-r14					SEQUENCE (SIZE (1..2)) OF SoundingRS-UL-ConfigDedicated						OPTIONAL,		-- Cond PeriodicSRS
		soundingRS-UL-PeriodicConfigDedicatedUpPTsExtList-r14					SEQUENCE (SIZE (1..4)) OF SoundingRS-UL-ConfigDedicatedUpPTsExt-r13						OPTIONAL,		-- Cond PeriodicSRSExt
		soundingRS-UL-AperiodicConfigDedicatedList-r14					SEQUENCE (SIZE (1..2)) OF SoundingRS-AperiodicSet-r14						OPTIONAL,		-- Cond AperiodicSRS
		soundingRS-UL-ConfigDedicatedApUpPTsExtList-r14					SEQUENCE (SIZE (1..4)) OF SoundingRS-AperiodicSetUpPTsExt-r14  			OPTIONAL,		-- Cond AperiodicSRSExt
		must-Config-r14						CHOICE{
			release								NULL,
			setup								SEQUENCE {
				k-max-r14						ENUMERATED {l1, l3},
				p-a-must-r14					ENUMERATED {
													dB-6, dB-4dot77, dB-3, dB-1dot77,
													dB0, dB1, dB2, dB3}	OPTIONAL		-- Need ON
			}
		}															OPTIONAL,		-- Need ON
		pusch-ConfigDedicated-v1430			PUSCH-ConfigDedicatedSCell-v1430	OPTIONAL,	-- Need ON
		csi-RS-Config-v1430						CSI-RS-Config-v1430			OPTIONAL,	-- Need ON
		csi-RS-ConfigZP-ApList-r14				CSI-RS-ConfigZP-ApList-r14		OPTIONAL,	-- Need ON
		cqi-ReportConfig-v1430					CQI-ReportConfig-v1430	OPTIONAL,	-- Need ON
		semiOpenLoop-r14						BOOLEAN						OPTIONAL,	-- Need ON
		pdsch-ConfigDedicatedSCell-v1430		PDSCH-ConfigDedicatedSCell-v1430		OPTIONAL		-- Need ON
	]]
}

PhysicalConfigDedicatedSCell-v1370 ::=	SEQUENCE {
	pucch-SCell-v1370				CHOICE{
		release							NULL,
		setup							SEQUENCE {
			pucch-ConfigDedicated-v1370		PUCCH-ConfigDedicated-v1370		OPTIONAL	-- Cond PUCCH-Format4or5
		}
	}
}

LAA-SCellConfiguration-r13 ::=			SEQUENCE {
	subframeStartPosition-r13				ENUMERATED {s0, s07},
	laa-SCellSubframeConfig-r13				BIT STRING (SIZE(8))
}

LAA-SCellConfiguration-v1430 ::=		SEQUENCE {
	crossCarrierSchedulingConfig-UL-r14	CHOICE {
		release									NULL,
		setup									SEQUENCE {
			crossCarrierSchedulingConfigLAA-UL-r14		CrossCarrierSchedulingConfigLAA-UL-r14
		}
	}													OPTIONAL,	-- Cond Cross-Carrier-ConfigUL
	lbt-Config-r14								LBT-Config-r14			OPTIONAL,		-- Need ON
	pdcch-ConfigLAA-r14							PDCCH-ConfigLAA-r14	OPTIONAL,		-- Need ON
	absenceOfAnyOtherTechnology-r14			ENUMERATED {true}		OPTIONAL,		-- Need OR
	soundingRS-UL-ConfigDedicatedAperiodic-v1430
						SoundingRS-UL-ConfigDedicatedAperiodic-v1430	OPTIONAL		-- Need ON
}

LBT-Config-r14 ::=		CHOICE{
	maxEnergyDetectionThreshold-r14				INTEGER(-85..-52),
	energyDetectionThresholdOffset-r14			INTEGER(-13..20)
}

CSI-RS-ConfigNZPToAddModList-r11 ::=	SEQUENCE (SIZE (1..maxCSI-RS-NZP-r11)) OF CSI-RS-ConfigNZP-r11

CSI-RS-ConfigNZPToAddModListExt-r13 ::=	SEQUENCE (SIZE (1..maxCSI-RS-NZP-v1310)) OF CSI-RS-ConfigNZP-r11

CSI-RS-ConfigNZPToReleaseList-r11 ::=	SEQUENCE (SIZE (1..maxCSI-RS-NZP-r11)) OF CSI-RS-ConfigNZPId-r11

CSI-RS-ConfigNZPToReleaseListExt-r13 ::=	SEQUENCE (SIZE (1..maxCSI-RS-NZP-v1310)) OF CSI-RS-ConfigNZPId-v1310

CSI-RS-ConfigZPToAddModList-r11 ::=	SEQUENCE (SIZE (1..maxCSI-RS-ZP-r11)) OF CSI-RS-ConfigZP-r11

CSI-RS-ConfigZPToReleaseList-r11 ::=	SEQUENCE (SIZE (1..maxCSI-RS-ZP-r11)) OF CSI-RS-ConfigZPId-r11

SoundingRS-AperiodicSet-r14 ::= SEQUENCE{
	srs-CC-SetIndexList-r14
								SEQUENCE (SIZE (1..4)) OF SRS-CC-SetIndex-r14
															OPTIONAL,	-- Cond SRS-Trigger-TypeA
	soundingRS-UL-ConfigDedicatedAperiodic-r14
												SoundingRS-UL-ConfigDedicatedAperiodic-r10
}

SoundingRS-AperiodicSetUpPTsExt-r14 ::= SEQUENCE{
	srs-CC-SetIndexList-r14
								SEQUENCE (SIZE (1..4)) OF SRS-CC-SetIndex-r14
															OPTIONAL,	-- Cond SRS-Trigger-TypeA
	soundingRS-UL-ConfigDedicatedAperiodicUpPTsExt-r14
											SoundingRS-UL-ConfigDedicatedAperiodicUpPTsExt-r13
}


P-Max ::=				INTEGER (-30..33)


PRACH-ConfigSIB ::=				SEQUENCE {
	rootSequenceIndex					INTEGER (0..837),
	prach-ConfigInfo					PRACH-ConfigInfo
}

PRACH-ConfigSIB-v1310 ::=			SEQUENCE {
	rsrp-ThresholdsPrachInfoList-r13		RSRP-ThresholdsPrachInfoList-r13,
	mpdcch-startSF-CSS-RA-r13			CHOICE {
		fdd-r13								ENUMERATED {v1, v1dot5, v2, v2dot5, v4, v5, v8,
												v10},
		tdd-r13								ENUMERATED {v1, v2, v4, v5, v8, v10, v20, spare}
	}																		OPTIONAL,	-- Cond MP
	prach-HoppingOffset-r13				INTEGER (0..94)						OPTIONAL,	-- Need OR
	prach-ParametersListCE-r13			PRACH-ParametersListCE-r13
}

PRACH-Config ::=					SEQUENCE {
	rootSequenceIndex					INTEGER (0..837),
	prach-ConfigInfo					PRACH-ConfigInfo					OPTIONAL	-- Need ON
}

PRACH-Config-v1310 ::=				SEQUENCE {
	rsrp-ThresholdsPrachInfoList-r13		RSRP-ThresholdsPrachInfoList-r13		OPTIONAL,	-- Cond MP
	mpdcch-startSF-CSS-RA-r13			CHOICE {
		fdd-r13								ENUMERATED {v1, v1dot5, v2, v2dot5, v4, v5, v8,
												v10},
		tdd-r13								ENUMERATED {v1, v2, v4, v5, v8, v10, v20, spare}
	}																		OPTIONAL,	-- Cond MP
	prach-HoppingOffset-r13				INTEGER (0..94)						OPTIONAL,	-- Need OR
	prach-ParametersListCE-r13			PRACH-ParametersListCE-r13			OPTIONAL,	-- Cond MP
	initial-CE-level-r13					INTEGER (0..3)		OPTIONAL	-- Need OR
}

PRACH-Config-v1430 ::=				SEQUENCE {
	rootSequenceIndexHighSpeed-r14				INTEGER (0..837),
	zeroCorrelationZoneConfigHighSpeed-r14		INTEGER (0..12),
	prach-ConfigIndexHighSpeed-r14				INTEGER (0..63),
	prach-FreqOffsetHighSpeed-r14				INTEGER (0..94)
}

PRACH-ConfigSCell-r10 ::=				SEQUENCE {
	prach-ConfigIndex-r10					INTEGER (0..63)
}

PRACH-ConfigInfo ::=				SEQUENCE {
	prach-ConfigIndex					INTEGER (0..63),
	highSpeedFlag						BOOLEAN,
	zeroCorrelationZoneConfig			INTEGER (0..15),
	prach-FreqOffset					INTEGER (0..94)
}

PRACH-ParametersListCE-r13 ::=	SEQUENCE (SIZE(1..maxCE-Level-r13)) OF PRACH-ParametersCE-r13

PRACH-ParametersCE-r13 ::=			SEQUENCE {
	prach-ConfigIndex-r13					INTEGER (0..63),
	prach-FreqOffset-r13						INTEGER (0..94),
	prach-StartingSubframe-r13				ENUMERATED {sf2, sf4, sf8, sf16, sf32, sf64, sf128,
														sf256}				OPTIONAL,	-- Need OP
	maxNumPreambleAttemptCE-r13
								ENUMERATED {n3, n4, n5, n6, n7, n8, n10}	OPTIONAL,	-- Need OP
	numRepetitionPerPreambleAttempt-r13		ENUMERATED {n1,n2,n4,n8,n16,n32,n64,n128},
	mpdcch-NarrowbandsToMonitor-r13			SEQUENCE (SIZE(1..2)) OF
													INTEGER (1..maxAvailNarrowBands-r13),
	mpdcch-NumRepetition-RA-r13				ENUMERATED {r1, r2, r4, r8, r16,
														r32, r64, r128, r256},
	prach-HoppingConfig-r13					ENUMERATED {on,off}
}

RSRP-ThresholdsPrachInfoList-r13 ::= SEQUENCE (SIZE(1..3)) OF RSRP-Range


PresenceAntennaPort1 ::=				BOOLEAN


PUCCH-ConfigCommon ::=				SEQUENCE {
	deltaPUCCH-Shift					ENUMERATED {ds1, ds2, ds3},
	nRB-CQI								INTEGER (0..98),
	nCS-AN								INTEGER (0..7),
	n1PUCCH-AN							INTEGER (0..2047)
}

PUCCH-ConfigCommon-v1310 ::=		SEQUENCE {
	n1PUCCH-AN-InfoList-r13					N1PUCCH-AN-InfoList-r13		OPTIONAL,	-- Need OR
	pucch-NumRepetitionCE-Msg4-Level0-r13	ENUMERATED {n1, n2, n4, n8}		OPTIONAL,	-- Need OR
	pucch-NumRepetitionCE-Msg4-Level1-r13	ENUMERATED {n1, n2, n4, n8}		OPTIONAL,	-- Need OR
	pucch-NumRepetitionCE-Msg4-Level2-r13	ENUMERATED {n4, n8, n16, n32}	OPTIONAL,	-- Need OR
	pucch-NumRepetitionCE-Msg4-Level3-r13	ENUMERATED {n4, n8, n16, n32}	OPTIONAL	-- Need OR
}

PUCCH-ConfigCommon-v1430 ::=		SEQUENCE {
	pucch-NumRepetitionCE-Msg4-Level3-r14	ENUMERATED {n64, n128}	OPTIONAL	-- Need OR
}

PUCCH-ConfigDedicated ::=			SEQUENCE {
	ackNackRepetition					CHOICE{
		release								NULL,
		setup								SEQUENCE {
			repetitionFactor					ENUMERATED {n2, n4, n6, spare1},
			n1PUCCH-AN-Rep						INTEGER (0..2047)
		}
	},
	tdd-AckNackFeedbackMode				ENUMERATED {bundling, multiplexing}	OPTIONAL	-- Cond TDD
}

PUCCH-ConfigDedicated-v1020 ::=		SEQUENCE {
	pucch-Format-r10					CHOICE {
		format3-r10						PUCCH-Format3-Conf-r13,
		channelSelection-r10				SEQUENCE {
			n1PUCCH-AN-CS-r10					CHOICE {
				release								NULL,
				setup								SEQUENCE {
					n1PUCCH-AN-CS-List-r10				SEQUENCE (SIZE (1..2)) OF N1PUCCH-AN-CS-r10
				}
			}																OPTIONAL	-- Need ON
		}
	}																		OPTIONAL,	-- Need OR
	twoAntennaPortActivatedPUCCH-Format1a1b-r10		ENUMERATED {true}		OPTIONAL,	-- Need OR
	simultaneousPUCCH-PUSCH-r10						ENUMERATED {true}		OPTIONAL,	-- Need OR
	n1PUCCH-AN-RepP1-r10							INTEGER (0..2047)		OPTIONAL	-- Need OR
}

PUCCH-ConfigDedicated-v1130 ::=		SEQUENCE {
	n1PUCCH-AN-CS-v1130					CHOICE {
		release								NULL,
		setup								SEQUENCE {
			n1PUCCH-AN-CS-ListP1-r11			SEQUENCE (SIZE (2..4)) OF INTEGER (0..2047)
		}
	}																		OPTIONAL,	-- Need ON
	nPUCCH-Param-r11					CHOICE {
		release								NULL,
		setup								SEQUENCE {
			nPUCCH-Identity-r11					INTEGER (0..503),
			n1PUCCH-AN-r11						INTEGER (0..2047)
		}
	}																		OPTIONAL	-- Need ON
}

PUCCH-ConfigDedicated-v1250 ::=		SEQUENCE {
	nkaPUCCH-Param-r12					CHOICE {
		release								NULL,
		setup								SEQUENCE {
			nkaPUCCH-AN-r12						INTEGER (0..2047)
		}
	}
}

PUCCH-ConfigDedicated-r13 ::=		SEQUENCE {
--Release 8
	ackNackRepetition-r13				CHOICE{
		release								NULL,
		setup								SEQUENCE {
			repetitionFactor-r13				ENUMERATED {n2, n4, n6, spare1},
			n1PUCCH-AN-Rep-r13				INTEGER (0..2047)
		}
	},
	tdd-AckNackFeedbackMode-r13			ENUMERATED {bundling, multiplexing}	OPTIONAL,	-- Cond TDD
--Release 10
	pucch-Format-r13					CHOICE {
		format3-r13								SEQUENCE {
			n3PUCCH-AN-List-r13	SEQUENCE (SIZE (1..4)) OF INTEGER (0..549)	OPTIONAL,	-- Need ON
			twoAntennaPortActivatedPUCCH-Format3-r13		CHOICE {
				release											NULL,
				setup											SEQUENCE {
					n3PUCCH-AN-ListP1-r13	SEQUENCE (SIZE (1..4)) OF INTEGER (0..549)
				}
			}																OPTIONAL	-- Need ON
		},
		channelSelection-r13				SEQUENCE {
			n1PUCCH-AN-CS-r13					CHOICE {
				release								NULL,
				setup								SEQUENCE {
					n1PUCCH-AN-CS-List-r13				SEQUENCE (SIZE (1..2)) OF N1PUCCH-AN-CS-r10,
					n1PUCCH-AN-CS-ListP1-r13			SEQUENCE (SIZE (2..4)) OF INTEGER (0..2047)
				}
			}																OPTIONAL	-- Need ON
		},
		format4-r13							SEQUENCE {
			format4-resourceConfiguration-r13			SEQUENCE (SIZE (4)) OF Format4-resource-r13,
			format4-MultiCSI-resourceConfiguration-r13	SEQUENCE (SIZE (1..2)) OF Format4-resource-r13 OPTIONAL	-- Need OR
		},
		format5-r13				SEQUENCE {
			format5-resourceConfiguration-r13			SEQUENCE (SIZE (4)) OF Format5-resource-r13,
			format5-MultiCSI-resourceConfiguration-r13	Format5-resource-r13 OPTIONAL	-- Need OR
		}
	}																		OPTIONAL,	-- Need OR
	twoAntennaPortActivatedPUCCH-Format1a1b-r13		ENUMERATED {true}		OPTIONAL,	-- Need OR
	simultaneousPUCCH-PUSCH-r13						ENUMERATED {true}		OPTIONAL,	-- Need OR
	n1PUCCH-AN-RepP1-r13							INTEGER (0..2047)		OPTIONAL,	-- Need OR
--Release 11
	nPUCCH-Param-r13					CHOICE {
		release								NULL,
		setup								SEQUENCE {
			nPUCCH-Identity-r13					INTEGER (0..503),
			n1PUCCH-AN-r13						INTEGER (0..2047)
		}
	}																		OPTIONAL,	-- Need ON
--Release 12
	nkaPUCCH-Param-r13					CHOICE {
		release								NULL,
		setup								SEQUENCE {
			nkaPUCCH-AN-r13						INTEGER (0..2047)
		}
	}																		OPTIONAL,	-- Need ON
--Release 13
	spatialBundlingPUCCH-r13			BOOLEAN,
	spatialBundlingPUSCH-r13			BOOLEAN,
	harq-TimingTDD-r13					BOOLEAN,
	codebooksizeDetermination-r13		ENUMERATED {dai,cc}					OPTIONAL,	-- Need OR
	maximumPayloadCoderate-r13			INTEGER (0..7)						OPTIONAL,	-- Need OR
	pucch-NumRepetitionCE-r13			CHOICE {
		release						NULL,
		setup						CHOICE {
			modeA						SEQUENCE {
				pucch-NumRepetitionCE-format1-r13					ENUMERATED {r1, r2, r4, r8},
				pucch-NumRepetitionCE-format2-r13					ENUMERATED {r1, r2, r4, r8}
			},
			modeB						SEQUENCE {
				pucch-NumRepetitionCE-format1-r13					ENUMERATED {r4, r8, r16, r32},
				pucch-NumRepetitionCE-format2-r13					ENUMERATED {r4, r8, r16, r32}
			}
		}
	}																		OPTIONAL	--Need ON
}

PUCCH-ConfigDedicated-v1370 ::=		SEQUENCE {
	pucch-Format-v1370					CHOICE {
		release	NULL,
		setup	PUCCH-Format3-Conf-r13
	}
}

PUCCH-Format3-Conf-r13 ::=	SEQUENCE {
	n3PUCCH-AN-List-r13	SEQUENCE (SIZE (1..4)) OF INTEGER (0..549)	OPTIONAL,	-- Need ON
	twoAntennaPortActivatedPUCCH-Format3-r13		CHOICE {
		release											NULL,
		setup											SEQUENCE {
			n3PUCCH-AN-ListP1-r13	SEQUENCE (SIZE (1..4)) OF INTEGER (0..549)
		}
	}																OPTIONAL	-- Need ON
}

PUCCH-ConfigDedicated-v1430 ::=		SEQUENCE {
	pucch-NumRepetitionCE-format1-r14		ENUMERATED {r64,r128}		OPTIONAL	-- Need OR
}

Format4-resource-r13	::=				SEQUENCE {
	startingPRB-format4-r13						INTEGER (0..109),
	numberOfPRB-format4-r13					INTEGER (0..7)
}

Format5-resource-r13	::=				SEQUENCE {
	startingPRB-format5-r13						INTEGER (0..109),
	cdm-index-format5-r13						INTEGER (0..1)
}



N1PUCCH-AN-CS-r10	::= SEQUENCE (SIZE (1..4)) OF INTEGER (0..2047)

N1PUCCH-AN-InfoList-r13 ::= SEQUENCE (SIZE(1..maxCE-Level-r13)) OF INTEGER (0..2047)


PUSCH-ConfigCommon ::=				SEQUENCE {
	pusch-ConfigBasic					SEQUENCE {
		n-SB								INTEGER (1..4),
		hoppingMode							ENUMERATED {interSubFrame, intraAndInterSubFrame},
		pusch-HoppingOffset					INTEGER (0..98),
		enable64QAM							BOOLEAN
	},
	ul-ReferenceSignalsPUSCH			UL-ReferenceSignalsPUSCH
}

PUSCH-ConfigCommon-v1270 ::=		SEQUENCE {
	enable64QAM-v1270						ENUMERATED {true}
}

PUSCH-ConfigCommon-v1310 ::=	SEQUENCE {
	pusch-maxNumRepetitionCEmodeA-r13	ENUMERATED {
											r8, r16, r32 }					OPTIONAL,	-- Need OR
	pusch-maxNumRepetitionCEmodeB-r13	ENUMERATED {
											r192, r256, r384, r512, r768, r1024,
											r1536, r2048}					OPTIONAL,	-- Need OR
	pusch-HoppingOffset-v1310
									INTEGER (1..maxAvailNarrowBands-r13)	OPTIONAL	-- Need OR
}

PUSCH-ConfigDedicated ::=			SEQUENCE {
	betaOffset-ACK-Index				INTEGER (0..15),
	betaOffset-RI-Index					INTEGER (0..15),
	betaOffset-CQI-Index				INTEGER (0..15)
}

PUSCH-ConfigDedicated-v1020 ::=		SEQUENCE {
	betaOffsetMC-r10					SEQUENCE {
		betaOffset-ACK-Index-MC-r10			INTEGER (0..15),
		betaOffset-RI-Index-MC-r10			INTEGER (0..15),
		betaOffset-CQI-Index-MC-r10			INTEGER (0..15)
	}																		OPTIONAL,	-- Need OR
	groupHoppingDisabled-r10			ENUMERATED {true}					OPTIONAL,	-- Need OR
	dmrs-WithOCC-Activated-r10			ENUMERATED {true}					OPTIONAL	-- Need OR
}

PUSCH-ConfigDedicated-v1130 ::=		SEQUENCE {
	pusch-DMRS-r11						CHOICE {
		release								NULL,
		setup								SEQUENCE {
			nPUSCH-Identity-r11					INTEGER (0..509),
			nDMRS-CSH-Identity-r11				INTEGER (0..509)
		}
	}
}

PUSCH-ConfigDedicated-v1250::=		SEQUENCE {
	uciOnPUSCH							CHOICE {
		release								NULL,
		setup									SEQUENCE {
			betaOffset-ACK-Index-SubframeSet2-r12			INTEGER (0..15),
			betaOffset-RI-Index-SubframeSet2-r12			INTEGER (0..15),
			betaOffset-CQI-Index-SubframeSet2-r12			INTEGER (0..15),
			betaOffsetMC-r12						SEQUENCE {
				betaOffset-ACK-Index-MC-SubframeSet2-r12	INTEGER (0..15),
				betaOffset-RI-Index-MC-SubframeSet2-r12		INTEGER (0..15),
				betaOffset-CQI-Index-MC-SubframeSet2-r12	INTEGER (0..15)
			}																OPTIONAL	-- Need OR
		}
	}
}
PUSCH-ConfigDedicated-r13 ::=			SEQUENCE {
	betaOffset-ACK-Index-r13				INTEGER (0..15),
	betaOffset2-ACK-Index-r13				INTEGER (0..15)					OPTIONAL,	-- Need OR
	betaOffset-RI-Index-r13					INTEGER (0..15),
	betaOffset-CQI-Index-r13				INTEGER (0..15),
	betaOffsetMC-r13						SEQUENCE {
		betaOffset-ACK-Index-MC-r13				INTEGER (0..15),
		betaOffset2-ACK-Index-MC-r13			INTEGER (0..15)				OPTIONAL,	-- Need OR
		betaOffset-RI-Index-MC-r13				INTEGER (0..15),
		betaOffset-CQI-Index-MC-r13				INTEGER (0..15)
	}																		OPTIONAL,	-- Need OR
	groupHoppingDisabled-r13				ENUMERATED {true}				OPTIONAL,	-- Need OR
	dmrs-WithOCC-Activated-r13				ENUMERATED {true}				OPTIONAL,	-- Need OR
	pusch-DMRS-r11							CHOICE {
		release									NULL,
		setup									SEQUENCE {
			nPUSCH-Identity-r13						INTEGER (0..509),
			nDMRS-CSH-Identity-r13					INTEGER (0..509)
		}
	}																		OPTIONAL,	-- Need ON
	uciOnPUSCH								CHOICE {
		release									NULL,
		setup									SEQUENCE {
			betaOffset-ACK-Index-SubframeSet2-r13			INTEGER (0..15),
			betaOffset2-ACK-Index-SubframeSet2-r13			INTEGER (0..15)	OPTIONAL,	-- Need OR
			betaOffset-RI-Index-SubframeSet2-r13			INTEGER (0..15),
			betaOffset-CQI-Index-SubframeSet2-r13			INTEGER (0..15),
			betaOffsetMC-r12						SEQUENCE {
				betaOffset-ACK-Index-MC-SubframeSet2-r13	INTEGER (0..15),
				betaOffset2-ACK-Index-MC-SubframeSet2-r13	INTEGER (0..15)	OPTIONAL,	-- Need OR
				betaOffset-RI-Index-MC-SubframeSet2-r13		INTEGER (0..15),
				betaOffset-CQI-Index-MC-SubframeSet2-r13	INTEGER (0..15)
			}																OPTIONAL	-- Need OR
		}
	}																		OPTIONAL,	-- Need ON
	pusch-HoppingConfig-r13					ENUMERATED {on}					OPTIONAL	-- Need OR
}

PUSCH-ConfigDedicated-v1430 ::=			SEQUENCE {
	ce-PUSCH-NB-MaxTBS-r14					ENUMERATED {on}					OPTIONAL,	-- Need OR
	ce-PUSCH-MaxBandwidth-r14				ENUMERATED {bw5}				OPTIONAL,	-- Need OR
	tdd-PUSCH-UpPTS-r14						TDD-PUSCH-UpPTS-r14				OPTIONAL,	-- Need ON
	ul-DMRS-IFDMA-r14						BOOLEAN,
	enable256QAM-r14						Enable256QAM-r14				OPTIONAL	-- Need ON
}

PUSCH-ConfigDedicatedSCell-r10 ::=		SEQUENCE {
	groupHoppingDisabled-r10				ENUMERATED {true}				OPTIONAL,	-- Need OR
	dmrs-WithOCC-Activated-r10				ENUMERATED {true}				OPTIONAL	-- Need OR
}

PUSCH-ConfigDedicatedSCell-v1430 ::=			SEQUENCE {
	enable256QAM-r14						Enable256QAM-r14				OPTIONAL	-- Need OR
}

TDD-PUSCH-UpPTS-r14 ::=					CHOICE {
	release									NULL,
	setup									SEQUENCE {
		symPUSCH-UpPTS-r14						ENUMERATED {sym1, sym2, sym3, sym4, sym5, sym6}																					OPTIONAL,	-- Need ON
		dmrs-LessUpPTS-Config-r14				ENUMERATED {true}			OPTIONAL	-- Need OR
	}
}

Enable256QAM-r14 ::=					CHOICE {
		release								NULL,
		setup								CHOICE {
			tpc-SubframeSet-Configured-r14		SEQUENCE {
					subframeSet1-DCI-Format0-r14										BOOLEAN,
					subframeSet1-DCI-Format4-r14										BOOLEAN,
					subframeSet2-DCI-Format0-r14										BOOLEAN,
					subframeSet2-DCI-Format4-r14										BOOLEAN
			},
			tpc-SubframeSet-NotConfigured-r14	SEQUENCE {
					dci-Format0-r14		BOOLEAN,
					dci-Format4-r14		BOOLEAN
			}
		}
}

PUSCH-EnhancementsConfig-r14 ::=		CHOICE {
	release							NULL,
	setup							SEQUENCE {
		pusch-HoppingOffsetPUSCH-Enh-r14			INTEGER (1..100)		OPTIONAL,	-- Need ON
		interval-ULHoppingPUSCH-Enh-r14			CHOICE {
			interval-FDD-PUSCH-Enh-r14				ENUMERATED {int1, int2, int4, int8},
			interval-TDD-PUSCH-Enh-r14				ENUMERATED {int1, int5, int10, int20}
		}																	OPTIONAL	-- Need ON
	}
}

UL-ReferenceSignalsPUSCH ::=		SEQUENCE {
	groupHoppingEnabled					BOOLEAN,
	groupAssignmentPUSCH				INTEGER (0..29),
	sequenceHoppingEnabled				BOOLEAN,
	cyclicShift							INTEGER (0..7)
}


RACH-ConfigCommon ::=		SEQUENCE {
	preambleInfo						SEQUENCE {
		numberOfRA-Preambles				ENUMERATED {
												n4, n8, n12, n16, n20, n24, n28,
												n32, n36, n40, n44, n48, n52, n56,
												n60, n64},
		preamblesGroupAConfig				SEQUENCE {
			sizeOfRA-PreamblesGroupA			ENUMERATED {
													n4, n8, n12, n16, n20, n24, n28,
													n32, n36, n40, n44, n48, n52, n56,
													n60},
			messageSizeGroupA						ENUMERATED {b56, b144, b208, b256},
			messagePowerOffsetGroupB			ENUMERATED {
													minusinfinity, dB0, dB5, dB8, dB10, dB12,
													dB15, dB18},
			...
		}			OPTIONAL													-- Need OP
	},
	powerRampingParameters				PowerRampingParameters,
	ra-SupervisionInfo					SEQUENCE {
		preambleTransMax					PreambleTransMax,
		ra-ResponseWindowSize				ENUMERATED {
												sf2, sf3, sf4, sf5, sf6, sf7,
												sf8, sf10},
		mac-ContentionResolutionTimer		ENUMERATED {
												sf8, sf16, sf24, sf32, sf40, sf48,
												sf56, sf64}
	},
	maxHARQ-Msg3Tx						INTEGER (1..8),
	...,
	[[	preambleTransMax-CE-r13			PreambleTransMax					OPTIONAL,	-- Need OR
		rach-CE-LevelInfoList-r13		RACH-CE-LevelInfoList-r13			OPTIONAL	-- Need OR
	]]
}

RACH-ConfigCommon-v1250 ::=		SEQUENCE {
	txFailParams-r12				SEQUENCE {
		connEstFailCount-r12					ENUMERATED {n1, n2, n3, n4},
		connEstFailOffsetValidity-r12			ENUMERATED {s30, s60, s120, s240,
														s300, s420, s600, s900},
		connEstFailOffset-r12					INTEGER (0..15)		OPTIONAL	-- Need OP
	}
}

RACH-ConfigCommonSCell-r11 ::=		SEQUENCE {
	powerRampingParameters-r11				PowerRampingParameters,
	ra-SupervisionInfo-r11					SEQUENCE {
		preambleTransMax-r11					PreambleTransMax
	},
	...
}

RACH-CE-LevelInfoList-r13 ::=	SEQUENCE (SIZE (1..maxCE-Level-r13)) OF RACH-CE-LevelInfo-r13

RACH-CE-LevelInfo-r13 ::=		SEQUENCE {
	preambleMappingInfo-r13				SEQUENCE {
		firstPreamble-r13					INTEGER(0..63),
		lastPreamble-r13					INTEGER(0..63)
	},
	ra-ResponseWindowSize-r13			ENUMERATED {sf20, sf50, sf80, sf120, sf180,
													sf240, sf320, sf400},

	mac-ContentionResolutionTimer-r13	ENUMERATED {sf80, sf100, sf120,
													sf160, sf200, sf240, sf480, sf960},
	rar-HoppingConfig-r13				ENUMERATED {on,off},
	...
}

PowerRampingParameters ::=			SEQUENCE {
	powerRampingStep					ENUMERATED {dB0, dB2,dB4, dB6},
	preambleInitialReceivedTargetPower	ENUMERATED {
											dBm-120, dBm-118, dBm-116, dBm-114, dBm-112,
											dBm-110, dBm-108, dBm-106, dBm-104, dBm-102,
											dBm-100, dBm-98, dBm-96, dBm-94,
											dBm-92, dBm-90}
}

PreambleTransMax ::=				ENUMERATED {
											n3, n4, n5, n6, n7,	n8, n10, n20, n50,
											n100, n200}


RACH-ConfigDedicated ::=		SEQUENCE {
	ra-PreambleIndex					INTEGER (0..63),
	ra-PRACH-MaskIndex					INTEGER (0..15)
}


RadioResourceConfigCommonSIB ::=	SEQUENCE {
	rach-ConfigCommon					RACH-ConfigCommon,
	bcch-Config						BCCH-Config,
	pcch-Config						PCCH-Config,
	prach-Config						PRACH-ConfigSIB,
	pdsch-ConfigCommon					PDSCH-ConfigCommon,
	pusch-ConfigCommon					PUSCH-ConfigCommon,
	pucch-ConfigCommon					PUCCH-ConfigCommon,
	soundingRS-UL-ConfigCommon			SoundingRS-UL-ConfigCommon,
	uplinkPowerControlCommon			UplinkPowerControlCommon,
	ul-CyclicPrefixLength				UL-CyclicPrefixLength,
	...,
	[[	uplinkPowerControlCommon-v1020	UplinkPowerControlCommon-v1020		OPTIONAL	-- Need OR
	]],
	[[	rach-ConfigCommon-v1250			RACH-ConfigCommon-v1250				OPTIONAL	-- Need OR
	]],
	[[	pusch-ConfigCommon-v1270		PUSCH-ConfigCommon-v1270			OPTIONAL	-- Need OR
	]],
	[[	bcch-Config-v1310				BCCH-Config-v1310					OPTIONAL,	-- Need OR
		pcch-Config-v1310				PCCH-Config-v1310					OPTIONAL,	-- Need OR
		freqHoppingParameters-r13		FreqHoppingParameters-r13			OPTIONAL,	-- Need OR
		pdsch-ConfigCommon-v1310		PDSCH-ConfigCommon-v1310			OPTIONAL,	-- Need OR
		pusch-ConfigCommon-v1310		PUSCH-ConfigCommon-v1310			OPTIONAL,	-- Need OR
		prach-ConfigCommon-v1310		PRACH-ConfigSIB-v1310				OPTIONAL,	-- Need OR
		pucch-ConfigCommon-v1310		PUCCH-ConfigCommon-v1310			OPTIONAL	-- Need OR
	]],
	[[	highSpeedConfig-r14				HighSpeedConfig-r14					OPTIONAL,	-- Need OR
		prach-Config-v1430				PRACH-Config-v1430					OPTIONAL,	-- Need OR
		pucch-ConfigCommon-v1430		PUCCH-ConfigCommon-v1430			OPTIONAL	-- Need OR
	]]
}

RadioResourceConfigCommon ::=		SEQUENCE {
	rach-ConfigCommon					RACH-ConfigCommon					OPTIONAL,	-- Need ON
	prach-Config						PRACH-Config,
	pdsch-ConfigCommon					PDSCH-ConfigCommon					OPTIONAL,	-- Need ON
	pusch-ConfigCommon					PUSCH-ConfigCommon,
	phich-Config						PHICH-Config						OPTIONAL,	-- Need ON
	pucch-ConfigCommon					PUCCH-ConfigCommon					OPTIONAL,	-- Need ON
	soundingRS-UL-ConfigCommon			SoundingRS-UL-ConfigCommon			OPTIONAL,	-- Need ON
	uplinkPowerControlCommon			UplinkPowerControlCommon			OPTIONAL,	-- Need ON
	antennaInfoCommon					AntennaInfoCommon					OPTIONAL,	-- Need ON
	p-Max								P-Max								OPTIONAL,	-- Need OP
	tdd-Config							TDD-Config							OPTIONAL,	-- Cond TDD
	ul-CyclicPrefixLength				UL-CyclicPrefixLength,
	...,
	[[	uplinkPowerControlCommon-v1020	UplinkPowerControlCommon-v1020		OPTIONAL	-- Need ON
	]],
	[[	tdd-Config-v1130				TDD-Config-v1130					OPTIONAL	-- Cond TDD3
	]],
	[[	pusch-ConfigCommon-v1270		PUSCH-ConfigCommon-v1270			OPTIONAL	-- Need OR
	]],
	[[
		prach-Config-v1310				PRACH-Config-v1310					OPTIONAL,	-- Need ON
		freqHoppingParameters-r13		FreqHoppingParameters-r13			OPTIONAL,	-- Need ON
		pdsch-ConfigCommon-v1310		PDSCH-ConfigCommon-v1310			OPTIONAL,	-- Need ON
		pucch-ConfigCommon-v1310		PUCCH-ConfigCommon-v1310			OPTIONAL,	-- Need ON
		pusch-ConfigCommon-v1310		PUSCH-ConfigCommon-v1310			OPTIONAL,	-- Need ON
		uplinkPowerControlCommon-v1310	UplinkPowerControlCommon-v1310		OPTIONAL	-- Need ON
	]],
	[[	highSpeedConfig-r14				HighSpeedConfig-r14					OPTIONAL,	-- Need OR
		prach-Config-v1430				PRACH-Config-v1430					OPTIONAL,	-- Need OR
		pucch-ConfigCommon-v1430		PUCCH-ConfigCommon-v1430			OPTIONAL,	-- Need OR
		tdd-Config-v1430				TDD-Config-v1430					OPTIONAL	-- Cond TDD3
	]],
	[[
		tdd-Config-v1450				TDD-Config-v1450					OPTIONAL	-- Cond TDD3
	]]
}

RadioResourceConfigCommonPSCell-r12 ::=	SEQUENCE {
	basicFields-r12						RadioResourceConfigCommonSCell-r10,
	pucch-ConfigCommon-r12				PUCCH-ConfigCommon,
	rach-ConfigCommon-r12				RACH-ConfigCommon,
	uplinkPowerControlCommonPSCell-r12	UplinkPowerControlCommonPSCell-r12,
	...,
	[[	uplinkPowerControlCommonPSCell-v1310
									UplinkPowerControlCommon-v1310		OPTIONAL	-- Need ON
	]]
}

RadioResourceConfigCommonPSCell-v12f0 ::=	SEQUENCE {
	basicFields-v12f0					RadioResourceConfigCommonSCell-v10l0
}

RadioResourceConfigCommonPSCell-v1440 ::=	SEQUENCE {
	basicFields-v1440					RadioResourceConfigCommonSCell-v1440
}

RadioResourceConfigCommonSCell-r10 ::=	SEQUENCE {
	-- DL configuration as well as configuration applicable for DL and UL
	nonUL-Configuration-r10					SEQUENCE {
		-- 1: Cell characteristics
		dl-Bandwidth-r10						ENUMERATED {n6, n15, n25, n50, n75, n100},
		-- 2: Physical configuration, general
		antennaInfoCommon-r10					AntennaInfoCommon,
		mbsfn-SubframeConfigList-r10			MBSFN-SubframeConfigList	OPTIONAL,	-- Need OR
		-- 3: Physical configuration, control
		phich-Config-r10						PHICH-Config,
		-- 4: Physical configuration, physical channels
		pdsch-ConfigCommon-r10					PDSCH-ConfigCommon,
		tdd-Config-r10							TDD-Config					OPTIONAL	-- Cond TDDSCell
	},
	-- UL configuration
	ul-Configuration-r10				SEQUENCE {
		ul-FreqInfo-r10						SEQUENCE {
			ul-CarrierFreq-r10					ARFCN-ValueEUTRA			OPTIONAL,	-- Need OP
			ul-Bandwidth-r10					ENUMERATED {n6, n15,
													n25, n50, n75, n100}	OPTIONAL,	-- Need OP
			additionalSpectrumEmissionSCell-r10		AdditionalSpectrumEmission
		},
		p-Max-r10							P-Max							OPTIONAL,	-- Need OP
		uplinkPowerControlCommonSCell-r10		UplinkPowerControlCommonSCell-r10,
		-- A special version of IE UplinkPowerControlCommon may be introduced
		-- 3: Physical configuration, control
		soundingRS-UL-ConfigCommon-r10		SoundingRS-UL-ConfigCommon,
		ul-CyclicPrefixLength-r10			UL-CyclicPrefixLength,
		-- 4: Physical configuration, physical channels
		prach-ConfigSCell-r10					PRACH-ConfigSCell-r10		OPTIONAL,	-- Cond TDD-OR-NoR11
		pusch-ConfigCommon-r10				PUSCH-ConfigCommon
	}																		OPTIONAL,	-- Need OR
	...,
	[[	ul-CarrierFreq-v1090				ARFCN-ValueEUTRA-v9e0			OPTIONAL	-- Need OP
	]],
	[[	rach-ConfigCommonSCell-r11			RACH-ConfigCommonSCell-r11		OPTIONAL,	-- Cond ULSCell
		prach-ConfigSCell-r11				PRACH-Config					OPTIONAL,	-- Cond UL
		tdd-Config-v1130					TDD-Config-v1130				OPTIONAL,	-- Cond TDD2
		uplinkPowerControlCommonSCell-v1130
								UplinkPowerControlCommonSCell-v1130			OPTIONAL	-- Cond UL
	]],
	[[	pusch-ConfigCommon-v1270		PUSCH-ConfigCommon-v1270			OPTIONAL	-- Need OR
	]],
	[[	pucch-ConfigCommon-r13				PUCCH-ConfigCommon		OPTIONAL,	-- Cond UL
		uplinkPowerControlCommonSCell-v1310
								UplinkPowerControlCommonSCell-v1310	OPTIONAL	-- Cond UL
	]],
	[[	highSpeedConfigSCell-r14		HighSpeedConfigSCell-r14			OPTIONAL,	-- Need OR
		prach-Config-v1430				PRACH-Config-v1430					OPTIONAL,	-- Cond UL
	ul-Configuration-r14				SEQUENCE {
		ul-FreqInfo-r14						SEQUENCE {
			ul-CarrierFreq-r14					ARFCN-ValueEUTRA-r9			OPTIONAL,	-- Need OP
			ul-Bandwidth-r14					ENUMERATED {n6, n15,
													n25, n50, n75, n100}	OPTIONAL,	-- Need OP
			additionalSpectrumEmissionSCell-r14		AdditionalSpectrumEmission
		},
		p-Max-r14							P-Max							OPTIONAL,	-- Need OP
		soundingRS-UL-ConfigCommon-r14		SoundingRS-UL-ConfigCommon,
		ul-CyclicPrefixLength-r14			UL-CyclicPrefixLength,
		prach-ConfigSCell-r14					PRACH-ConfigSCell-r10		OPTIONAL,	-- Cond TDD-OR-NoR11
		uplinkPowerControlCommonPUSCH-LessCell-v1430												UplinkPowerControlCommonPUSCH-LessCell-v1430	OPTIONAL	-- Need OR
}																	OPTIONAL,	-- Cond ULSRS
	harq-ReferenceConfig-r14					ENUMERATED {sa2,sa4,sa5}	OPTIONAL,		-- Need OR
	soundingRS-FlexibleTiming-r14   			ENUMERATED {true}			OPTIONAL		-- Need OR
	]],
	[[	mbsfn-SubframeConfigList-v1430		MBSFN-SubframeConfigList-v1430		OPTIONAL-- Need ON
	]]
}

RadioResourceConfigCommonSCell-v10l0 ::=	SEQUENCE {
	-- UL configuration
	ul-Configuration-v10l0				SEQUENCE {
		additionalSpectrumEmissionSCell-v10l0		AdditionalSpectrumEmission-v10l0
	}
}

RadioResourceConfigCommonSCell-v1440 ::=	SEQUENCE {
	ul-Configuration-v1440				SEQUENCE {
		ul-FreqInfo-v1440						SEQUENCE {
			additionalSpectrumEmissionSCell-v1440		AdditionalSpectrumEmission-v10l0
		}
	}
}

BCCH-Config ::=						SEQUENCE {
	modificationPeriodCoeff				ENUMERATED {n2, n4, n8, n16}
}

BCCH-Config-v1310 ::=				SEQUENCE {
	modificationPeriodCoeff-v1310		ENUMERATED {n64}
}

FreqHoppingParameters-r13 ::=		SEQUENCE {
	dummy			ENUMERATED {nb2, nb4}				OPTIONAL,
	dummy2			CHOICE {
		interval-FDD-r13						ENUMERATED {int1, int2, int4, int8},
		interval-TDD-r13						ENUMERATED {int1, int5, int10, int20}
	}																		OPTIONAL,
	dummy3			CHOICE {
		interval-FDD-r13						ENUMERATED {int2, int4, int8, int16},
		interval-TDD-r13						ENUMERATED { int5, int10, int20, int40}
	}																								OPTIONAL,
	interval-ULHoppingConfigCommonModeA-r13	CHOICE {
		interval-FDD-r13						ENUMERATED {int1, int2, int4, int8},
		interval-TDD-r13						ENUMERATED {int1, int5, int10, int20}
	}																		OPTIONAL,	-- Cond MP-A
	interval-ULHoppingConfigCommonModeB-r13	CHOICE {
		interval-FDD-r13						ENUMERATED {int2, int4, int8, int16},
		interval-TDD-r13						ENUMERATED { int5, int10, int20, int40}
	}																		OPTIONAL,	-- Cond MP-B
	dummy4				INTEGER (1..maxAvailNarrowBands-r13)			OPTIONAL
}

PCCH-Config ::=						SEQUENCE {
	defaultPagingCycle					ENUMERATED {
											rf32, rf64, rf128, rf256},
	nB									ENUMERATED {
											fourT, twoT, oneT, halfT, quarterT, oneEighthT,
											oneSixteenthT, oneThirtySecondT}
}

PCCH-Config-v1310 ::=				SEQUENCE {
	paging-narrowBands-r13				INTEGER (1..maxAvailNarrowBands-r13),
	mpdcch-NumRepetition-Paging-r13		ENUMERATED {r1, r2, r4, r8, r16, r32, r64, r128, r256},
	nB-v1310							ENUMERATED {one64thT, one128thT, one256thT}
																			OPTIONAL	-- Need OR
}

UL-CyclicPrefixLength ::=			ENUMERATED {len1, len2}

HighSpeedConfig-r14 ::=			SEQUENCE {
	highSpeedEnhancedMeasFlag-r14			ENUMERATED {true}				OPTIONAL,	-- Need OR
	highSpeedEnhancedDemodulationFlag-r14	ENUMERATED {true}				OPTIONAL	-- Need OR
}

HighSpeedConfigSCell-r14 ::=		SEQUENCE {
	highSpeedEnhancedDemodulationFlag-r14	ENUMERATED {true}				OPTIONAL	-- Need OR
}


RadioResourceConfigDedicated ::=		SEQUENCE {
	srb-ToAddModList					SRB-ToAddModList			OPTIONAL,		-- Cond HO-Conn
	drb-ToAddModList					DRB-ToAddModList			OPTIONAL,		-- Cond HO-toEUTRA
	drb-ToReleaseList					DRB-ToReleaseList			OPTIONAL,		-- Need ON
	mac-MainConfig						CHOICE {
			explicitValue					MAC-MainConfig,
			defaultValue					NULL
	}		OPTIONAL,																-- Cond HO-toEUTRA2
	sps-Config							SPS-Config					OPTIONAL,		-- Need ON
	physicalConfigDedicated				PhysicalConfigDedicated		OPTIONAL,		-- Need ON
	...,
	[[	rlf-TimersAndConstants-r9		RLF-TimersAndConstants-r9			OPTIONAL	-- Need ON
	]],
	[[	measSubframePatternPCell-r10	MeasSubframePatternPCell-r10		OPTIONAL	-- Need ON
	]],
	[[	neighCellsCRS-Info-r11			NeighCellsCRS-Info-r11				OPTIONAL	-- Need ON
	]],
	[[	naics-Info-r12				NAICS-AssistanceInfo-r12			OPTIONAL	-- Need ON
	]],
	[[	neighCellsCRS-Info-r13			NeighCellsCRS-Info-r13				OPTIONAL,	-- Cond CRSIM
		rlf-TimersAndConstants-r13		RLF-TimersAndConstants-r13			OPTIONAL	-- Need ON
	]],
	[[	sps-Config-v1430				SPS-Config-v1430					OPTIONAL	-- Cond SPS
	]]
}

RadioResourceConfigDedicated-v1370 ::=		SEQUENCE {
	physicalConfigDedicated-v1370		PhysicalConfigDedicated-v1370		OPTIONAL	-- Need ON
}

RadioResourceConfigDedicatedPSCell-r12 ::=		SEQUENCE {
	-- UE specific configuration extensions applicable for an PSCell
	physicalConfigDedicatedPSCell-r12		PhysicalConfigDedicated		OPTIONAL,	-- Need ON
	sps-Config-r12							SPS-Config					OPTIONAL,	-- Need ON
	naics-Info-r12							NAICS-AssistanceInfo-r12	OPTIONAL,	-- Need ON
	...,
	[[	neighCellsCRS-InfoPSCell-r13		NeighCellsCRS-Info-r13		OPTIONAL	-- Need ON
	]],
	[[	sps-Config-v1430				SPS-Config-v1430				OPTIONAL	-- Cond SPS2
	]]
}

RadioResourceConfigDedicatedPSCell-v1370 ::=		SEQUENCE {
	physicalConfigDedicatedPSCell-v1370		PhysicalConfigDedicated-v1370	OPTIONAL	-- Need ON
}

RadioResourceConfigDedicatedSCG-r12 ::=		SEQUENCE {
	drb-ToAddModListSCG-r12				DRB-ToAddModListSCG-r12			OPTIONAL,	-- Need ON
	mac-MainConfigSCG-r12				MAC-MainConfig					OPTIONAL,	-- Need ON
	rlf-TimersAndConstantsSCG-r12		RLF-TimersAndConstantsSCG-r12	OPTIONAL,	-- Need ON
	...
}

RadioResourceConfigDedicatedSCell-r10 ::=	SEQUENCE {
	-- UE specific configuration extensions applicable for an SCell
	physicalConfigDedicatedSCell-r10		PhysicalConfigDedicatedSCell-r10	OPTIONAL,	-- Need ON
	...,
	[[	mac-MainConfigSCell-r11			MAC-MainConfigSCell-r11			OPTIONAL	-- Cond SCellAdd
	]],
	[[	naics-Info-r12				NAICS-AssistanceInfo-r12		OPTIONAL	-- Need ON
	]],
	[[	neighCellsCRS-InfoSCell-r13			NeighCellsCRS-Info-r13		OPTIONAL	-- Need ON
	]],
	[[	physicalConfigDedicatedSCell-v1370	PhysicalConfigDedicatedSCell-v1370	OPTIONAL	-- Need ON
	]]
}

SRB-ToAddModList ::=				SEQUENCE (SIZE (1..2)) OF SRB-ToAddMod

SRB-ToAddMod ::=	SEQUENCE {
	srb-Identity						INTEGER (1..2),
	rlc-Config							CHOICE {
		explicitValue						RLC-Config,
		defaultValue						NULL
	}		OPTIONAL,																-- Cond Setup
	logicalChannelConfig				CHOICE {
		explicitValue						LogicalChannelConfig,
		defaultValue						NULL
	}		OPTIONAL,																-- Cond Setup
	...
}

DRB-ToAddModList ::=				SEQUENCE (SIZE (1..maxDRB)) OF DRB-ToAddMod

DRB-ToAddModListSCG-r12 ::=		SEQUENCE (SIZE (1..maxDRB)) OF DRB-ToAddModSCG-r12

DRB-ToAddMod ::=	SEQUENCE {
	eps-BearerIdentity					INTEGER (0..15)			OPTIONAL,		-- Cond DRB-Setup
	drb-Identity						DRB-Identity,
	pdcp-Config							PDCP-Config				OPTIONAL,		-- Cond PDCP
	rlc-Config							RLC-Config				OPTIONAL,		-- Cond SetupM
	logicalChannelIdentity				INTEGER (3..10)			OPTIONAL,		-- Cond DRB-SetupM
	logicalChannelConfig				LogicalChannelConfig	OPTIONAL,		-- Cond SetupM
	...,
	[[	drb-TypeChange-r12					ENUMERATED {toMCG}		OPTIONAL,		-- Need OP
		rlc-Config-v1250					RLC-Config-v1250		OPTIONAL		-- Need ON
	]],
	[[	rlc-Config-v1310					RLC-Config-v1310		OPTIONAL,		-- Need ON
		drb-TypeLWA-r13						BOOLEAN					OPTIONAL,		-- Need ON
		drb-TypeLWIP-r13					ENUMERATED {lwip, lwip-DL-only,
											lwip-UL-only, eutran}		OPTIONAL		-- Need ON
	]],
	[[	rlc-Config-v1430					RLC-Config-v1430		OPTIONAL,		-- Need ON
		lwip-UL-Aggregation-r14				BOOLEAN					OPTIONAL,		-- Cond LWIP
		lwip-DL-Aggregation-r14				BOOLEAN					OPTIONAL,		-- Cond LWIP
		lwa-WLAN-AC-r14			ENUMERATED {ac-bk, ac-be, ac-vi, ac-vo}	OPTIONAL	-- Cond UL-LWA
	]]
}

DRB-ToAddModSCG-r12 ::=	SEQUENCE {
	drb-Identity-r12					DRB-Identity,
	drb-Type-r12						CHOICE {
		split-r12							NULL,
		scg-r12								SEQUENCE {
			eps-BearerIdentity-r12				INTEGER (0..15)	OPTIONAL,	-- Cond DRB-Setup
			pdcp-Config-r12						PDCP-Config		OPTIONAL	-- Cond PDCP-S
		}
	}															OPTIONAL,	-- Cond SetupS2
	rlc-ConfigSCG-r12					RLC-Config				OPTIONAL,	-- Cond SetupS
	rlc-Config-v1250						RLC-Config-v1250			OPTIONAL,	-- Need ON
	logicalChannelIdentitySCG-r12		INTEGER (3..10)			OPTIONAL,	-- Cond DRB-SetupS
	logicalChannelConfigSCG-r12			LogicalChannelConfig	OPTIONAL,	-- Cond SetupS
	...,
	[[	rlc-Config-v1430					RLC-Config-v1430		OPTIONAL		-- Need ON
	]]
}

DRB-ToReleaseList ::=				SEQUENCE (SIZE (1..maxDRB)) OF DRB-Identity

MeasSubframePatternPCell-r10 ::=		CHOICE {
	release								NULL,
	setup							MeasSubframePattern-r10
}

NeighCellsCRS-Info-r11 ::=		CHOICE {
	release							NULL,
	setup							CRS-AssistanceInfoList-r11
}

CRS-AssistanceInfoList-r11 ::=	SEQUENCE (SIZE (1..maxCellReport)) OF CRS-AssistanceInfo-r11

CRS-AssistanceInfo-r11 ::= SEQUENCE {
	physCellId-r11						PhysCellId,
	antennaPortsCount-r11				ENUMERATED {an1, an2, an4, spare1},
	mbsfn-SubframeConfigList-r11		MBSFN-SubframeConfigList,
	...,
	[[	mbsfn-SubframeConfigList-v1430	MBSFN-SubframeConfigList-v1430		OPTIONAL	-- Need ON
	]]
}

NeighCellsCRS-Info-r13 ::=		CHOICE {
	release							NULL,
	setup							CRS-AssistanceInfoList-r13
}

CRS-AssistanceInfoList-r13 ::=	SEQUENCE (SIZE (1..maxCellReport)) OF CRS-AssistanceInfo-r13

CRS-AssistanceInfo-r13 ::= SEQUENCE {
	physCellId-r13						PhysCellId,
	antennaPortsCount-r13				ENUMERATED {an1, an2, an4, spare1},
	mbsfn-SubframeConfigList-r13		MBSFN-SubframeConfigList			OPTIONAL,	-- Need ON
	...,
	[[	mbsfn-SubframeConfigList-v1430	MBSFN-SubframeConfigList-v1430		OPTIONAL	-- Need ON
	]]
}

NAICS-AssistanceInfo-r12 ::=		CHOICE {
	release							NULL,
	setup							SEQUENCE {
		neighCellsToReleaseList-r12		NeighCellsToReleaseList-r12			OPTIONAL	,	-- Need ON
		neighCellsToAddModList-r12		NeighCellsToAddModList-r12			OPTIONAL,	-- Need ON
		servCellp-a-r12					P-a								OPTIONAL	-- Need ON
	}
}

NeighCellsToReleaseList-r12 ::=	SEQUENCE (SIZE (1..maxNeighCell-r12)) OF PhysCellId

NeighCellsToAddModList-r12 ::=	SEQUENCE (SIZE (1..maxNeighCell-r12)) OF NeighCellsInfo-r12

NeighCellsInfo-r12	::=		SEQUENCE {
	physCellId-r12					PhysCellId,
	p-b-r12						INTEGER (0..3),
	crs-PortsCount-r12				ENUMERATED {n1, n2, n4, spare},
	mbsfn-SubframeConfig-r12		MBSFN-SubframeConfigList				OPTIONAL,	-- Need ON
	p-aList-r12					SEQUENCE (SIZE (1..maxP-a-PerNeighCell-r12)) OF P-a,
	transmissionModeList-r12		BIT STRING (SIZE(8)),
	resAllocGranularity-r12			INTEGER (1..4),
	...
}
P-a ::= ENUMERATED {	dB-6, dB-4dot77, dB-3, dB-1dot77,
									dB0, dB1, dB2, dB3}


RCLWI-Configuration-r13 ::=			CHOICE {
	release								NULL,
	setup								SEQUENCE {
		rclwi-Config-r13					RCLWI-Config-r13
	}
}

RCLWI-Config-r13 ::=				SEQUENCE {
	command								CHOICE {
		steerToWLAN-r13						SEQUENCE {
			mobilityConfig-r13					WLAN-Id-List-r12
		},
		steerToLTE-r13						NULL
	},
	...
}


RLC-Config ::=				CHOICE {
	am									SEQUENCE {
		ul-AM-RLC							UL-AM-RLC,
		dl-AM-RLC							DL-AM-RLC
	},
	um-Bi-Directional					SEQUENCE {
		ul-UM-RLC							UL-UM-RLC,
		dl-UM-RLC							DL-UM-RLC
	},
	um-Uni-Directional-UL				SEQUENCE {
		ul-UM-RLC							UL-UM-RLC
	},
	um-Uni-Directional-DL				SEQUENCE {
		dl-UM-RLC							DL-UM-RLC
	},
	...
}

RLC-Config-v1250 ::=				SEQUENCE {
	ul-extended-RLC-LI-Field-r12			BOOLEAN,
	dl-extended-RLC-LI-Field-r12			BOOLEAN
}

RLC-Config-v1310 ::=				SEQUENCE {
	ul-extended-RLC-AM-SN-r13					BOOLEAN,
	dl-extended-RLC-AM-SN-r13					BOOLEAN,
	pollPDU-v1310								PollPDU-v1310		OPTIONAL	-- Need OR
}

RLC-Config-v1430 ::=				CHOICE {
	release								NULL,
	setup								SEQUENCE {
		pollByte-r14						PollByte-r14
	}
}

UL-AM-RLC ::=						SEQUENCE {
	t-PollRetransmit					T-PollRetransmit,
	pollPDU								PollPDU,
	pollByte							PollByte,
	maxRetxThreshold					ENUMERATED {
											t1, t2, t3, t4, t6, t8, t16, t32}
}

DL-AM-RLC ::=						SEQUENCE {
	t-Reordering						T-Reordering,
	t-StatusProhibit					T-StatusProhibit
}

UL-UM-RLC ::=						SEQUENCE {
	sn-FieldLength						SN-FieldLength
}

DL-UM-RLC ::=						SEQUENCE {
	sn-FieldLength						SN-FieldLength,
	t-Reordering						T-Reordering
}

SN-FieldLength ::=					ENUMERATED {size5, size10}

T-PollRetransmit ::=				ENUMERATED {
										ms5, ms10, ms15, ms20, ms25, ms30, ms35,
										ms40, ms45, ms50, ms55, ms60, ms65, ms70,
										ms75, ms80, ms85, ms90, ms95, ms100, ms105,
										ms110, ms115, ms120, ms125, ms130, ms135,
										ms140, ms145, ms150, ms155, ms160, ms165,
										ms170, ms175, ms180, ms185, ms190, ms195,
										ms200, ms205, ms210, ms215, ms220, ms225,
										ms230, ms235, ms240, ms245, ms250, ms300,
										ms350, ms400, ms450, ms500, ms800-v1310,
										ms1000-v1310, ms2000-v1310, ms4000-v1310,
										spare5, spare4, spare3, spare2, spare1}

PollPDU ::=							ENUMERATED {
										p4, p8, p16, p32, p64, p128, p256, pInfinity}

PollPDU-v1310 ::=					ENUMERATED {
										p512, p1024, p2048, p4096, p6144, p8192, p12288, p16384}

PollByte ::=						ENUMERATED {
										kB25, kB50, kB75, kB100, kB125, kB250, kB375,
										kB500, kB750, kB1000, kB1250, kB1500, kB2000,
										kB3000, kBinfinity, spare1}

PollByte-r14 ::=					ENUMERATED {
										kB1, kB2, kB5, kB8, kB10, kB15, kB3500,
										kB4000, kB4500, kB5000, kB5500, kB6000, kB6500,
										kB7000, kB7500, kB8000, kB9000, kB10000, kB11000, kB12000,
										kB13000, kB14000, kB15000, kB16000, kB17000, kB18000,
										kB19000, kB20000, kB25000, kB30000, kB35000, kB40000}

T-Reordering ::=					ENUMERATED {
										ms0, ms5, ms10, ms15, ms20, ms25, ms30, ms35,
										ms40, ms45, ms50, ms55, ms60, ms65, ms70,
										ms75, ms80, ms85, ms90, ms95, ms100, ms110,
										ms120, ms130, ms140, ms150, ms160, ms170,
										ms180, ms190, ms200, ms1600-v1310}

T-StatusProhibit ::=				ENUMERATED {
										ms0, ms5, ms10, ms15, ms20, ms25, ms30, ms35,
										ms40, ms45, ms50, ms55, ms60, ms65, ms70,
										ms75, ms80, ms85, ms90, ms95, ms100, ms105,
										ms110, ms115, ms120, ms125, ms130, ms135,
										ms140, ms145, ms150, ms155, ms160, ms165,
										ms170, ms175, ms180, ms185, ms190, ms195,
										ms200, ms205, ms210, ms215, ms220, ms225,
										ms230, ms235, ms240, ms245, ms250, ms300,
										ms350, ms400, ms450, ms500, ms800-v1310,
										ms1000-v1310, ms1200-v1310, ms1600-v1310, ms2000-v1310, ms2400-v1310, spare2,
										spare1}


RLF-TimersAndConstants-r9 ::=			CHOICE {
	release									NULL,
	setup									SEQUENCE {
		t301-r9								ENUMERATED {
												ms100, ms200, ms300, ms400, ms600, ms1000, ms1500,
												ms2000},
		t310-r9								ENUMERATED {
												ms0, ms50, ms100, ms200, ms500, ms1000, ms2000},
		n310-r9								ENUMERATED {
												n1, n2, n3, n4, n6, n8, n10, n20},
		t311-r9								ENUMERATED {
												ms1000, ms3000, ms5000, ms10000, ms15000,
												ms20000, ms30000},
		n311-r9								ENUMERATED {
												n1, n2, n3, n4, n5, n6, n8, n10},
		...
	}
}

RLF-TimersAndConstants-r13 ::=			CHOICE {
	release									NULL,
	setup									SEQUENCE {
		t301-v1310								ENUMERATED {
													ms2500, ms3000, ms3500, ms4000, ms5000,
													ms6000, ms8000, ms10000},
		...,
		[[	t310-v1330							ENUMERATED {ms4000, ms6000}	OPTIONAL	-- Need ON
		]]
	}
}

RLF-TimersAndConstantsSCG-r12 ::=			CHOICE {
	release								NULL,
	setup								SEQUENCE {
		t313-r12							ENUMERATED {
												ms0, ms50, ms100, ms200, ms500, ms1000, ms2000},
		n313-r12							ENUMERATED {
												n1, n2, n3, n4, n6, n8, n10, n20},
		n314-r12							ENUMERATED {
												n1, n2, n3, n4, n5, n6, n8, n10},
		...
	}
}


RN-SubframeConfig-r10 ::=		SEQUENCE {
	subframeConfigPattern-r10			CHOICE {
		subframeConfigPatternFDD-r10	BIT STRING (SIZE(8)),
		subframeConfigPatternTDD-r10	INTEGER (0..31)
	}																	OPTIONAL,	-- Need ON
	rpdcch-Config-r10				SEQUENCE {
		resourceAllocationType-r10		ENUMERATED {type0, type1, type2Localized, type2Distributed,
													spare4, spare3, spare2, spare1},
		resourceBlockAssignment-r10			CHOICE {
			type01-r10							CHOICE {
				nrb6-r10							BIT STRING (SIZE(6)),
				nrb15-r10							BIT STRING (SIZE(8)),
				nrb25-r10							BIT STRING (SIZE(13)),
				nrb50-r10							BIT STRING (SIZE(17)),
				nrb75-r10							BIT STRING (SIZE(19)),
				nrb100-r10							BIT STRING (SIZE(25))
			},
			type2-r10							CHOICE {
				nrb6-r10							BIT STRING (SIZE(5)),
				nrb15-r10							BIT STRING (SIZE(7)),
				nrb25-r10							BIT STRING (SIZE(9)),
				nrb50-r10							BIT STRING (SIZE(11)),
				nrb75-r10							BIT STRING (SIZE(12)),
				nrb100-r10							BIT STRING (SIZE(13))
			},
			...
		},
		demodulationRS-r10				CHOICE {
			interleaving-r10				ENUMERATED {crs},
			noInterleaving-r10				ENUMERATED {crs, dmrs}
		},
		pdsch-Start-r10					INTEGER (1..3),
		pucch-Config-r10				CHOICE {
			tdd								CHOICE {
				channelSelectionMultiplexingBundling	SEQUENCE {
					n1PUCCH-AN-List-r10			SEQUENCE (SIZE (1..4)) OF INTEGER (0..2047)
				},
				fallbackForFormat3				SEQUENCE {
					n1PUCCH-AN-P0-r10				INTEGER (0..2047),
					n1PUCCH-AN-P1-r10				INTEGER (0..2047)		OPTIONAL	-- Need OR
				}
			},
			fdd								SEQUENCE {
				n1PUCCH-AN-P0-r10				INTEGER (0..2047),
				n1PUCCH-AN-P1-r10				INTEGER (0..2047)			OPTIONAL	-- Need OR
			}
		},
		...
	}																	OPTIONAL,	-- Need ON
	...
}


SchedulingRequestConfig ::=		CHOICE {
	release								NULL,
	setup								SEQUENCE {
		sr-PUCCH-ResourceIndex				INTEGER (0..2047),
		sr-ConfigIndex						INTEGER (0..157),
		dsr-TransMax						ENUMERATED {
												n4, n8, n16, n32, n64, spare3, spare2, spare1}
	}
}

SchedulingRequestConfig-v1020 ::=	SEQUENCE {
	sr-PUCCH-ResourceIndexP1-r10		INTEGER (0..2047)			OPTIONAL		-- Need OR
}

SchedulingRequestConfigSCell-r13 ::=		CHOICE {
	release								NULL,
	setup								SEQUENCE {
		sr-PUCCH-ResourceIndex-r13			INTEGER (0..2047),
		sr-PUCCH-ResourceIndexP1-r13		INTEGER (0..2047)			OPTIONAL,		-- Need OR
		sr-ConfigIndex-r13					INTEGER (0..157),
		dsr-TransMax-r13					ENUMERATED {
												n4, n8, n16, n32, n64, spare3, spare2, spare1}
	}

}


SoundingRS-UL-ConfigCommon ::=		CHOICE {
	release								NULL,
	setup								SEQUENCE {
		srs-BandwidthConfig					ENUMERATED {bw0, bw1, bw2, bw3, bw4, bw5, bw6, bw7},
		srs-SubframeConfig					ENUMERATED {
												sc0, sc1, sc2, sc3, sc4, sc5, sc6, sc7,
												sc8, sc9, sc10, sc11, sc12, sc13, sc14, sc15},
		ackNackSRS-SimultaneousTransmission	BOOLEAN,
		srs-MaxUpPts						ENUMERATED {true}			OPTIONAL	-- Cond TDD
	}
}

SoundingRS-UL-ConfigDedicated ::=	CHOICE{
	release								NULL,
	setup								SEQUENCE {
		srs-Bandwidth						ENUMERATED {bw0, bw1, bw2, bw3},
		srs-HoppingBandwidth				ENUMERATED {hbw0, hbw1, hbw2, hbw3},
		freqDomainPosition					INTEGER (0..23),
		duration							BOOLEAN,
		srs-ConfigIndex						INTEGER (0..1023),
		transmissionComb					INTEGER (0..1),
		cyclicShift							ENUMERATED {cs0, cs1, cs2, cs3, cs4, cs5, cs6, cs7}
	}
}

SoundingRS-UL-ConfigDedicated-v1020 ::=	SEQUENCE {
	srs-AntennaPort-r10					SRS-AntennaPort
}

SoundingRS-UL-ConfigDedicated-v1310 ::=	CHOICE{
	release								NULL,
	setup								SEQUENCE {
		transmissionComb-v1310				INTEGER (2..3)				OPTIONAL,	-- Need OR
		cyclicShift-v1310					ENUMERATED {cs8, cs9, cs10, cs11}	OPTIONAL,	-- Need OR
		transmissionCombNum-r13				ENUMERATED {n2, n4}		OPTIONAL	-- Need OR
	}
}

SoundingRS-UL-ConfigDedicatedUpPTsExt-r13 ::=	CHOICE{
	release								NULL,
	setup								SEQUENCE {
		srs-UpPtsAdd-r13						ENUMERATED {sym2, sym4},
		srs-Bandwidth-r13					ENUMERATED {bw0, bw1, bw2, bw3},
		srs-HoppingBandwidth-r13			ENUMERATED {hbw0, hbw1, hbw2, hbw3},
		freqDomainPosition-r13				INTEGER (0..23),
		duration-r13						BOOLEAN,
		srs-ConfigIndex-r13					INTEGER (0..1023),
		transmissionComb-r13				INTEGER (0..3),
		cyclicShift-r13						ENUMERATED {cs0, cs1, cs2, cs3, cs4, cs5, cs6, cs7,
														cs8, cs9, cs10, cs11},
		srs-AntennaPort-r13					SRS-AntennaPort,
		transmissionCombNum-r13				ENUMERATED {n2, n4}
	}
}

SoundingRS-UL-ConfigDedicatedAperiodic-r10 ::=	CHOICE{
	release								NULL,
	setup								SEQUENCE {
		srs-ConfigIndexAp-r10				INTEGER (0..31),
		srs-ConfigApDCI-Format4-r10			SEQUENCE (SIZE (1..3)) OF SRS-ConfigAp-r10	OPTIONAL,--Need ON
		srs-ActivateAp-r10					CHOICE {
				release							NULL,
				setup							SEQUENCE {
					srs-ConfigApDCI-Format0-r10			SRS-ConfigAp-r10,
					srs-ConfigApDCI-Format1a2b2c-r10		SRS-ConfigAp-r10,
					...
				}
		}																	OPTIONAL	-- Need ON
	}
}

SoundingRS-UL-ConfigDedicatedAperiodic-v1310 ::=	CHOICE{
	release								NULL,
	setup								SEQUENCE {
		srs-ConfigApDCI-Format4-v1310		SEQUENCE (SIZE (1..3)) OF SRS-ConfigAp-v1310	OPTIONAL,--Need ON
		srs-ActivateAp-v1310				CHOICE {
				release							NULL,
				setup							SEQUENCE {
					srs-ConfigApDCI-Format0-v1310		SRS-ConfigAp-v1310	OPTIONAL,	-- Need ON
					srs-ConfigApDCI-Format1a2b2c-v1310	SRS-ConfigAp-v1310	OPTIONAL	-- Need ON
				}
		}																	OPTIONAL	-- Need ON
	}
}

SoundingRS-UL-ConfigDedicatedAperiodicUpPTsExt-r13 ::=	CHOICE{
	release								NULL,
	setup								SEQUENCE {
		srs-UpPtsAdd-r13					ENUMERATED {sym2, sym4},
		srs-ConfigIndexAp-r13				INTEGER (0..31),
		srs-ConfigApDCI-Format4-r13			SEQUENCE (SIZE (1..3)) OF SRS-ConfigAp-r13	OPTIONAL,--Need ON
		srs-ActivateAp-r13					CHOICE {
				release							NULL,
				setup							SEQUENCE {
					srs-ConfigApDCI-Format0-r13			SRS-ConfigAp-r13,
					srs-ConfigApDCI-Format1a2b2c-r13		SRS-ConfigAp-r13
				}
		}																	OPTIONAL	-- Need ON
	}
}

SoundingRS-UL-ConfigDedicatedAperiodic-v1430 ::=	CHOICE{
	release								NULL,
	setup								SEQUENCE {
		srs-SubframeIndication-r14			INTEGER (1..4)	OPTIONAL		-- Need ON
	}
}

SRS-ConfigAp-r10 ::= SEQUENCE {
	srs-AntennaPortAp-r10				SRS-AntennaPort,
	srs-BandwidthAp-r10					ENUMERATED {bw0, bw1, bw2, bw3},
	freqDomainPositionAp-r10			INTEGER (0..23),
	transmissionCombAp-r10				INTEGER (0..1),
	cyclicShiftAp-r10					ENUMERATED {cs0, cs1, cs2, cs3, cs4, cs5, cs6, cs7}
}

SRS-ConfigAp-v1310 ::= SEQUENCE {
	transmissionCombAp-v1310			INTEGER (2..3)						OPTIONAL,	-- Need OR
	cyclicShiftAp-v1310					ENUMERATED {cs8, cs9, cs10, cs11}	OPTIONAL,	-- Need OR
	transmissionCombNum-r13				ENUMERATED {n2, n4}			OPTIONAL	-- Need OR
}

SRS-ConfigAp-r13 ::= SEQUENCE {
	srs-AntennaPortAp-r13				SRS-AntennaPort,
	srs-BandwidthAp-r13					ENUMERATED {bw0, bw1, bw2, bw3},
	freqDomainPositionAp-r13			INTEGER (0..23),
	transmissionCombAp-r13				INTEGER (0..3),
	cyclicShiftAp-r13					ENUMERATED {cs0, cs1, cs2, cs3, cs4, cs5, cs6, cs7,
											cs8, cs9, cs10, cs11},
	transmissionCombNum-r13				ENUMERATED {n2, n4}
}

SRS-AntennaPort ::=					ENUMERATED {an1, an2, an4, spare1}


SPS-Config ::=	SEQUENCE {
	semiPersistSchedC-RNTI			C-RNTI					OPTIONAL,			-- Need OR
	sps-ConfigDL					SPS-ConfigDL			OPTIONAL,			-- Need ON
	sps-ConfigUL					SPS-ConfigUL			OPTIONAL			-- Need ON
}

SPS-Config-v1430 ::=	SEQUENCE {
	ul-SPS-V-RNTI-r14					C-RNTI					OPTIONAL,			-- Need OR
	sl-SPS-V-RNTI-r14					C-RNTI					OPTIONAL,			-- Need OR
	sps-ConfigUL-ToAddModList-r14		SPS-ConfigUL-ToAddModList-r14	OPTIONAL,	-- Need ON
	sps-ConfigUL-ToReleaseList-r14		SPS-ConfigUL-ToReleaseList-r14	OPTIONAL,	-- Need ON
	sps-ConfigSL-ToAddModList-r14		SPS-ConfigSL-ToAddModList-r14	OPTIONAL,	-- Need ON
	sps-ConfigSL-ToReleaseList-r14		SPS-ConfigSL-ToReleaseList-r14	OPTIONAL	-- Need ON
}

SPS-ConfigUL-ToAddModList-r14 ::= SEQUENCE (SIZE (1..maxConfigSPS-r14)) OF SPS-ConfigUL

SPS-ConfigUL-ToReleaseList-r14 ::= SEQUENCE (SIZE (1..maxConfigSPS-r14)) OF SPS-ConfigIndex-r14

SPS-ConfigSL-ToAddModList-r14 ::= SEQUENCE (SIZE (1..maxConfigSPS-r14)) OF SPS-ConfigSL-r14

SPS-ConfigSL-ToReleaseList-r14 ::= SEQUENCE (SIZE (1..maxConfigSPS-r14)) OF SPS-ConfigIndex-r14

SPS-ConfigDL ::=	CHOICE{
	release							NULL,
	setup							SEQUENCE {
		semiPersistSchedIntervalDL			ENUMERATED {
												sf10, sf20, sf32, sf40, sf64, sf80,
												sf128, sf160, sf320, sf640, spare6,
												spare5, spare4, spare3, spare2,
												spare1},
		numberOfConfSPS-Processes			INTEGER (1..8),
		n1PUCCH-AN-PersistentList			N1PUCCH-AN-PersistentList,
		...,
		[[	twoAntennaPortActivated-r10		CHOICE {
				release							NULL,
				setup							SEQUENCE {
					n1PUCCH-AN-PersistentListP1-r10	N1PUCCH-AN-PersistentList
				}
			}																OPTIONAL	-- Need ON
		]]
	}
}

SPS-ConfigUL ::=	CHOICE {
	release							NULL,
	setup							SEQUENCE {
		semiPersistSchedIntervalUL			ENUMERATED {
												sf10, sf20, sf32, sf40, sf64, sf80,
												sf128, sf160, sf320, sf640, sf1-v1430,
												sf2-v1430, sf3-v1430, sf4-v1430, sf5-v1430,
												spare1},
		implicitReleaseAfter				ENUMERATED {e2, e3, e4, e8},
		p0-Persistent						SEQUENCE {
			p0-NominalPUSCH-Persistent			INTEGER (-126..24),
			p0-UE-PUSCH-Persistent				INTEGER (-8..7)
		}		OPTIONAL,												-- Need OP
		twoIntervalsConfig					ENUMERATED {true}			OPTIONAL,	-- Cond TDD
		...,
		[[	p0-PersistentSubframeSet2-r12		CHOICE {
				release								NULL,
				setup								SEQUENCE {
					p0-NominalPUSCH-PersistentSubframeSet2-r12			INTEGER (-126..24),
					p0-UE-PUSCH-PersistentSubframeSet2-r12				INTEGER (-8..7)
				}
			}															OPTIONAL	-- Need ON
		]],
		[[	numberOfConfUlSPS-Processes-r13			INTEGER (1..8)		OPTIONAL	-- Need OR
		]],
		[[	fixedRV-NonAdaptive-r14					ENUMERATED {true}		OPTIONAL,	-- Need OR
			sps-ConfigIndex-r14						SPS-ConfigIndex-r14		OPTIONAL,	-- Need OR
			semiPersistSchedIntervalUL-v1430		ENUMERATED {
											sf50, sf100, sf200, sf300, sf400, sf500,
											sf600, sf700, sf800, sf900, sf1000, spare5,
											spare4, spare3, spare2, spare1}	OPTIONAL	-- Need OR

		]]
	}
}

SPS-ConfigSL-r14 ::=	SEQUENCE {
	sps-ConfigIndex-r14				SPS-ConfigIndex-r14,
	semiPersistSchedIntervalSL-r14	ENUMERATED {
										sf20, sf50, sf100, sf200, sf300, sf400,
										sf500, sf600, sf700, sf800, sf900, sf1000,
										spare4, spare3, spare2, spare1}
}

SPS-ConfigIndex-r14 ::=			INTEGER (1..maxConfigSPS-r14)

N1PUCCH-AN-PersistentList ::=		SEQUENCE (SIZE (1..4)) OF INTEGER (0..2047)


SRS-TPC-PDCCH-Config-r14 ::=					CHOICE {
	release								NULL,
	setup								SEQUENCE {
		srs-TPC-RNTI-r14									BIT STRING (SIZE (16)),
	startingBitOfFormat3B-r14							INTEGER (0..31),				fieldTypeFormat3B-r14								INTEGER (1..4),
		srs-CC-SetIndexlist-r14									SEQUENCE (SIZE(1..4)) OF SRS-CC-SetIndex-r14	OPTIONAL	-- Cond SRS-Trigger-TypeA

	}
}

SRS-CC-SetIndex-r14 ::=			SEQUENCE {
	cc-SetIndex-r14				INTEGER (0..3),
	cc-IndexInOneCC-Set-r14		INTEGER (0..7)
}


TDD-Config ::=						SEQUENCE {
	subframeAssignment					ENUMERATED {
											sa0, sa1, sa2, sa3, sa4, sa5, sa6},
	specialSubframePatterns				ENUMERATED {
											ssp0, ssp1, ssp2, ssp3, ssp4,ssp5, ssp6, ssp7,
											ssp8}
}

TDD-Config-v1130 ::=				SEQUENCE {
	specialSubframePatterns-v1130		ENUMERATED {ssp7,ssp9}
}

TDD-Config-v1430 ::=				SEQUENCE {
	specialSubframePatterns-v1430		ENUMERATED {ssp10}
}

TDD-Config-v1450 ::=				SEQUENCE {
	specialSubframePatterns-v1450		ENUMERATED {ssp10-CRS-LessDwPTS}
}

TDD-ConfigSL-r12 ::=		SEQUENCE {
	subframeAssignmentSL-r12				ENUMERATED {
											none, sa0, sa1, sa2, sa3, sa4, sa5, sa6}
}


TimeAlignmentTimer ::=					ENUMERATED {
												sf500, sf750, sf1280, sf1920, sf2560, sf5120,
												sf10240, infinity}

TPC-PDCCH-Config ::=					CHOICE {
	release								NULL,
	setup								SEQUENCE {
		tpc-RNTI							BIT STRING (SIZE (16)),
		tpc-Index							TPC-Index
	}
}

TPC-PDCCH-ConfigSCell-r13 ::=					CHOICE {
	release								NULL,
	setup								SEQUENCE {
		tpc-Index-PUCCH-SCell-r13		TPC-Index
	}
}

TPC-Index ::=							CHOICE {
	indexOfFormat3							INTEGER (1..15),
	indexOfFormat3A							INTEGER (1..31)
}


TunnelConfigLWIP-r13 ::= SEQUENCE {
	ip-Address-r13			IP-Address-r13,
	ike-Identity-r13			IKE-Identity-r13,
	...,
	[[	lwip-Counter-r13	INTEGER (0..65535)		OPTIONAL	-- Cond LWIP-Setup
	]]
}

IKE-Identity-r13 ::= SEQUENCE {
	idI-r13					OCTET STRING
}

IP-Address-r13 ::= CHOICE {
	ipv4-r13					BIT STRING (SIZE (32)),
	ipv6-r13					BIT STRING (SIZE (128))
}


UplinkPowerControlCommon ::=		SEQUENCE {
	p0-NominalPUSCH						INTEGER (-126..24),
	alpha								Alpha-r12,
	p0-NominalPUCCH						INTEGER (-127..-96),
	deltaFList-PUCCH					DeltaFList-PUCCH,
	deltaPreambleMsg3					INTEGER (-1..6)
}

UplinkPowerControlCommon-v1020 ::=	SEQUENCE {
	deltaF-PUCCH-Format3-r10				ENUMERATED {deltaF-1, deltaF0, deltaF1, deltaF2,
														deltaF3, deltaF4, deltaF5, deltaF6},
	deltaF-PUCCH-Format1bCS-r10				ENUMERATED {deltaF1, deltaF2, spare2, spare1}
}

UplinkPowerControlCommon-v1310 ::=	SEQUENCE {
	deltaF-PUCCH-Format4-r13			ENUMERATED {deltaF16, deltaF15, deltaF14,deltaF13, deltaF12,
										deltaF11, deltaF10, spare1}			OPTIONAL,	-- Need OR
	deltaF-PUCCH-Format5-13				ENUMERATED { deltaF13, deltaF12, deltaF11, deltaF10, deltaF9,
										deltaF8, deltaF7, spare1}				OPTIONAL	-- Need OR
}

UplinkPowerControlCommonPSCell-r12 ::=		SEQUENCE {
-- For uplink power control the additional/ missing fields are signalled (compared to SCell)
	deltaF-PUCCH-Format3-r12				ENUMERATED {deltaF-1, deltaF0, deltaF1, deltaF2,
														deltaF3, deltaF4, deltaF5, deltaF6},
	deltaF-PUCCH-Format1bCS-r12				ENUMERATED {deltaF1, deltaF2, spare2, spare1},
	p0-NominalPUCCH-r12						INTEGER (-127..-96),
	deltaFList-PUCCH-r12					DeltaFList-PUCCH
}


UplinkPowerControlCommonSCell-r10 ::=	SEQUENCE {
	p0-NominalPUSCH-r10					INTEGER (-126..24),
	alpha-r10							Alpha-r12
}

UplinkPowerControlCommonSCell-v1130 ::=	SEQUENCE {
	deltaPreambleMsg3-r11				INTEGER (-1..6)
}

UplinkPowerControlCommonSCell-v1310 ::=	SEQUENCE {
-- For uplink power control the additional/ missing fields are signalled (compared to SCell)
	p0-NominalPUCCH							INTEGER (-127..-96),
	deltaFList-PUCCH						DeltaFList-PUCCH,
	deltaF-PUCCH-Format3-r12				ENUMERATED {deltaF-1, deltaF0, deltaF1,
											deltaF2, deltaF3, deltaF4, deltaF5,
											deltaF6}						OPTIONAL,	-- Need OR
	deltaF-PUCCH-Format1bCS-r12				ENUMERATED {deltaF1, deltaF2,
											spare2, spare1}					OPTIONAL,	-- Need OR
	deltaF-PUCCH-Format4-r13					ENUMERATED {deltaF16, deltaF15, deltaF14,
												deltaF13, deltaF12, deltaF11, deltaF10,
												spare1}							OPTIONAL,	-- Need OR
	deltaF-PUCCH-Format5-13						ENUMERATED { deltaF13, deltaF12, deltaF11,
												deltaF10, deltaF9, deltaF8, deltaF7,
												spare1}							OPTIONAL	-- Need OR
}
UplinkPowerControlCommonPUSCH-LessCell-v1430 ::=	SEQUENCE {
	p0-Nominal-PeriodicSRS-r14						INTEGER (-126..24)		OPTIONAL,	-- Need OR
	p0-Nominal-AperiodicSRS-r14						INTEGER (-126..24)		OPTIONAL,	-- Need OR
	alpha-SRS-r14								Alpha-r12					OPTIONAL	-- Need OR
}

UplinkPowerControlDedicated ::=		SEQUENCE {
	p0-UE-PUSCH							INTEGER (-8..7),
	deltaMCS-Enabled					ENUMERATED {en0, en1},
	accumulationEnabled					BOOLEAN,
	p0-UE-PUCCH							INTEGER (-8..7),
	pSRS-Offset							INTEGER (0..15),
	filterCoefficient					FilterCoefficient					DEFAULT fc4
}

UplinkPowerControlDedicated-v1020 ::= SEQUENCE {
	deltaTxD-OffsetListPUCCH-r10		DeltaTxD-OffsetListPUCCH-r10		OPTIONAL,	-- Need OR
	pSRS-OffsetAp-r10					INTEGER (0..15)						OPTIONAL	-- Need OR
}

UplinkPowerControlDedicated-v1130 ::=		SEQUENCE {
	pSRS-Offset-v1130						INTEGER (16..31)				OPTIONAL,	-- Need OR
	pSRS-OffsetAp-v1130						INTEGER (16..31)				OPTIONAL,	-- Need OR
	deltaTxD-OffsetListPUCCH-v1130			DeltaTxD-OffsetListPUCCH-v1130	OPTIONAL	-- Need OR
}

UplinkPowerControlDedicated-v1250 ::=	SEQUENCE {
	set2PowerControlParameter		CHOICE {
		release							NULL,
		setup							SEQUENCE {
			tpc-SubframeSet-r12					BIT STRING (SIZE(10)),
			p0-NominalPUSCH-SubframeSet2-r12		INTEGER (-126..24),
			alpha-SubframeSet2-r12				Alpha-r12,
			p0-UE-PUSCH-SubframeSet2-r12			INTEGER (-8..7)
		}
	}
}

UplinkPUSCH-LessPowerControlDedicated-v1430 ::=		SEQUENCE {
	p0-UE-PeriodicSRS-r14						INTEGER (-8..7)			OPTIONAL,	-- Need OR
	p0-UE-AperiodicSRS-r14						INTEGER (-8..7)			OPTIONAL,	-- Need OR
	accumulationEnabled-r14						BOOLEAN
}

UplinkPowerControlDedicatedSCell-r10 ::=		SEQUENCE {
	p0-UE-PUSCH-r10						INTEGER (-8..7),
	deltaMCS-Enabled-r10					ENUMERATED {en0, en1},
	accumulationEnabled-r10				BOOLEAN,
	pSRS-Offset-r10						INTEGER (0..15),
	pSRS-OffsetAp-r10					INTEGER (0..15)					OPTIONAL,	-- Need OR
	filterCoefficient-r10				FilterCoefficient					DEFAULT fc4,
	pathlossReferenceLinking-r10		ENUMERATED {pCell, sCell}
}

UplinkPowerControlDedicatedSCell-v1310 ::=	SEQUENCE {
--Release 8
	p0-UE-PUCCH							INTEGER (-8..7),
--Release 10
	deltaTxD-OffsetListPUCCH-r10		DeltaTxD-OffsetListPUCCH-r10		OPTIONAL	-- Need OR
}

Alpha-r12 ::=						ENUMERATED {al0, al04, al05, al06, al07, al08, al09, al1}

DeltaFList-PUCCH ::=				SEQUENCE {
	deltaF-PUCCH-Format1				ENUMERATED {deltaF-2, deltaF0, deltaF2},
	deltaF-PUCCH-Format1b				ENUMERATED {deltaF1, deltaF3, deltaF5},
	deltaF-PUCCH-Format2				ENUMERATED {deltaF-2, deltaF0, deltaF1, deltaF2},
	deltaF-PUCCH-Format2a				ENUMERATED {deltaF-2, deltaF0, deltaF2},
	deltaF-PUCCH-Format2b				ENUMERATED {deltaF-2, deltaF0, deltaF2}
}

DeltaTxD-OffsetListPUCCH-r10 ::=	SEQUENCE {
	deltaTxD-OffsetPUCCH-Format1-r10		ENUMERATED {dB0, dB-2},
	deltaTxD-OffsetPUCCH-Format1a1b-r10		ENUMERATED {dB0, dB-2},
	deltaTxD-OffsetPUCCH-Format22a2b-r10	ENUMERATED {dB0, dB-2},
	deltaTxD-OffsetPUCCH-Format3-r10		ENUMERATED {dB0, dB-2},
	...

}

DeltaTxD-OffsetListPUCCH-v1130 ::=	SEQUENCE {
	deltaTxD-OffsetPUCCH-Format1bCS-r11		ENUMERATED {dB0, dB-1}
}


WLAN-Id-List-r13 ::=				SEQUENCE (SIZE (1..maxWLAN-Id-r13)) OF WLAN-Identifiers-r12


WLAN-MobilityConfig-r13 ::=		SEQUENCE {
	wlan-ToReleaseList-r13				WLAN-Id-List-r13			OPTIONAL,	-- Need ON
	wlan-ToAddList-r13					WLAN-Id-List-r13			OPTIONAL,	-- Need ON
	associationTimer-r13				ENUMERATED {s10, s30,
										s60, s120, s240}			OPTIONAL,	-- Need OR
	successReportRequested-r13			ENUMERATED {true}			OPTIONAL,	-- Need OR
	...,
	[[	wlan-SuspendConfig-r14			WLAN-SuspendConfig-r14		OPTIONAL	-- Need ON
	]]
}


NextHopChainingCount ::=					INTEGER (0..7)


SecurityAlgorithmConfig ::=			SEQUENCE {
	cipheringAlgorithm					CipheringAlgorithm-r12,
	integrityProtAlgorithm				ENUMERATED {
											eia0-v920, eia1, eia2, eia3-v1130, spare4, spare3,
											spare2, spare1, ...}
}

CipheringAlgorithm-r12 ::=				ENUMERATED {
											eea0, eea1, eea2, eea3-v1130, spare4, spare3,
											spare2, spare1, ...}


ShortMAC-I ::=						BIT STRING (SIZE (16))


AdditionalSpectrumEmission ::=		INTEGER (1..32)

AdditionalSpectrumEmission-v10l0 ::=	INTEGER (33..288)


ARFCN-ValueCDMA2000 ::=			INTEGER (0..2047)


ARFCN-ValueEUTRA ::=				INTEGER (0..maxEARFCN)

ARFCN-ValueEUTRA-v9e0 ::=			INTEGER (maxEARFCN-Plus1..maxEARFCN2)

ARFCN-ValueEUTRA-r9 ::=				INTEGER (0..maxEARFCN2)


ARFCN-ValueGERAN ::=			INTEGER (0..1023)


ARFCN-ValueUTRA ::=					INTEGER (0..16383)


BandclassCDMA2000 ::=					ENUMERATED {
											bc0, bc1, bc2, bc3, bc4, bc5, bc6, bc7, bc8,
											bc9, bc10, bc11, bc12, bc13, bc14, bc15, bc16,
											bc17, bc18-v9a0, bc19-v9a0, bc20-v9a0, bc21-v9a0,
											spare10, spare9, spare8, spare7, spare6, spare5, spare4,
											spare3, spare2, spare1, ...}


BandIndicatorGERAN ::=			ENUMERATED {dcs1800, pcs1900}


CarrierFreqCDMA2000 ::=			SEQUENCE {
	bandClass							BandclassCDMA2000,
	arfcn							ARFCN-ValueCDMA2000
}


CarrierFreqGERAN ::=			SEQUENCE {
	arfcn							ARFCN-ValueGERAN,
	bandIndicator					BandIndicatorGERAN
}


CarrierFreqsGERAN ::=			SEQUENCE {
	startingARFCN						ARFCN-ValueGERAN,
	bandIndicator						BandIndicatorGERAN,
	followingARFCNs						CHOICE {
		explicitListOfARFCNs				ExplicitListOfARFCNs,
		equallySpacedARFCNs					SEQUENCE {
			arfcn-Spacing						INTEGER (1..8),
			numberOfFollowingARFCNs				INTEGER (0..31)
		},
		variableBitMapOfARFCNs				OCTET STRING (SIZE (1..16))
	}
}

ExplicitListOfARFCNs ::=			SEQUENCE (SIZE (0..31)) OF ARFCN-ValueGERAN


CarrierFreqListMBMS-r11 ::=		SEQUENCE (SIZE (1..maxFreqMBMS-r11)) OF ARFCN-ValueEUTRA-r9


CDMA2000-Type ::=					ENUMERATED {type1XRTT, typeHRPD}


CellIdentity ::=					BIT STRING (SIZE (28))


CellIndexList ::=						SEQUENCE (SIZE (1..maxCellMeas)) OF CellIndex

CellIndex ::=							INTEGER (1..maxCellMeas)


CellReselectionPriority ::=				INTEGER (0..7)


CellSelectionInfoCE-r13 ::=		SEQUENCE {
	q-RxLevMinCE-r13				Q-RxLevMin,
	q-QualMinRSRQ-CE-r13			Q-QualMin-r9						OPTIONAL	-- Need OR
}


CellSelectionInfoCE1-r13 ::=		SEQUENCE {
	q-RxLevMinCE1-r13				Q-RxLevMin,
	q-QualMinRSRQ-CE1-r13			Q-QualMin-r9						OPTIONAL	-- Need OR
}

CellSelectionInfoCE1-v1360 ::=		SEQUENCE {
	delta-RxLevMinCE1-v1360					INTEGER (-8..-1)
}

CellReselectionSubPriority-r13 ::=			ENUMERATED {oDot2, oDot4, oDot6, oDot8}


CSFB-RegistrationParam1XRTT ::=		SEQUENCE {
	sid									BIT STRING (SIZE (15)),
	nid									BIT STRING (SIZE (16)),
	multipleSID							BOOLEAN,
	multipleNID							BOOLEAN,
	homeReg								BOOLEAN,
	foreignSIDReg						BOOLEAN,
	foreignNIDReg						BOOLEAN,
	parameterReg						BOOLEAN,
	powerUpReg							BOOLEAN,
	registrationPeriod					BIT STRING (SIZE (7)),
	registrationZone					BIT STRING (SIZE (12)),
	totalZone							BIT STRING (SIZE (3)),
	zoneTimer							BIT STRING (SIZE (3))
}

CSFB-RegistrationParam1XRTT-v920 ::=	SEQUENCE {
	powerDownReg-r9						ENUMERATED {true}
}


CellGlobalIdEUTRA ::=					SEQUENCE {
	plmn-Identity							PLMN-Identity,
	cellIdentity							CellIdentity
}


CellGlobalIdUTRA ::=					SEQUENCE {
	plmn-Identity							PLMN-Identity,
	cellIdentity							BIT STRING (SIZE (28))
}


CellGlobalIdGERAN ::=					SEQUENCE {
	plmn-Identity							PLMN-Identity,
	locationAreaCode						BIT STRING (SIZE (16)),
	cellIdentity						BIT STRING (SIZE (16))
}


CellGlobalIdCDMA2000 ::=				CHOICE {
	cellGlobalId1XRTT						BIT STRING (SIZE (47)),
	cellGlobalIdHRPD						BIT STRING (SIZE (128))
}


CellSelectionInfoNFreq-r13 ::=	SEQUENCE {
	-- Cell selection information as in SIB1
	q-RxLevMin-r13					Q-RxLevMin,
	q-RxLevMinOffset					INTEGER (1..8)			OPTIONAL,	-- Need OP
	-- Cell re-selection information as in SIB3
	q-Hyst-r13							ENUMERATED {
											dB0, dB1, dB2, dB3, dB4, dB5, dB6, dB8, dB10,
											dB12, dB14, dB16, dB18, dB20, dB22, dB24},
	q-RxLevMinReselection-r13			Q-RxLevMin,
	t-ReselectionEUTRA-r13				T-Reselection
}


CSG-Identity ::=					BIT STRING (SIZE (27))


FreqBandIndicator ::=					INTEGER (1..maxFBI)

FreqBandIndicator-v9e0 ::=				INTEGER (maxFBI-Plus1..maxFBI2)

FreqBandIndicator-r11 ::=				INTEGER (1..maxFBI2)


MobilityControlInfo ::=		SEQUENCE {
	targetPhysCellId					PhysCellId,
	carrierFreq							CarrierFreqEUTRA					OPTIONAL,	-- Cond HO-toEUTRA2
	carrierBandwidth					CarrierBandwidthEUTRA				OPTIONAL,	-- Cond HO-toEUTRA
	additionalSpectrumEmission			AdditionalSpectrumEmission			OPTIONAL,	-- Cond HO-toEUTRA
	t304								ENUMERATED {
											ms50, ms100, ms150, ms200, ms500, ms1000,
											ms2000, ms10000-v1310},
	newUE-Identity						C-RNTI,
	radioResourceConfigCommon			RadioResourceConfigCommon,
	rach-ConfigDedicated				RACH-ConfigDedicated				OPTIONAL,	-- Need OP
	...,
	[[	carrierFreq-v9e0				CarrierFreqEUTRA-v9e0				OPTIONAL	-- Need ON
	]],
	[[	drb-ContinueROHC-r11			ENUMERATED {true}					OPTIONAL	-- Cond HO
	]],
	[[	mobilityControlInfoV2X-r14	MobilityControlInfoV2X-r14				OPTIONAL,	-- Need ON
		handoverWithoutWT-Change-r14	ENUMERATED {keepLWA-Config, sendEndMarker}	OPTIONAL,	-- Cond HO
		makeBeforeBreak-r14				ENUMERATED {true}					OPTIONAL,	-- Need OR
		rach-Skip-r14					RACH-Skip-r14						OPTIONAL,	-- Need OR
		sameSFN-Indication-r14			ENUMERATED {true}					OPTIONAL	-- Cond HO-SFNsynced
	]],
	[[
		mib-RepetitionStatus-r14		BOOLEAN								OPTIONAL,	-- Need OR
		schedulingInfoSIB1-BR-r14		INTEGER (0..31)						OPTIONAL	-- Cond HO-SFNsynced
	]]
}

MobilityControlInfo-v10l0 ::=		SEQUENCE {
	additionalSpectrumEmission-v10l0	AdditionalSpectrumEmission-v10l0	OPTIONAL	-- Need ON
}

MobilityControlInfoSCG-r12 ::=		SEQUENCE {
	t307-r12							ENUMERATED {
											ms50, ms100, ms150, ms200, ms500, ms1000,
											ms2000, spare1},
	ue-IdentitySCG-r12					C-RNTI							OPTIONAL,	-- Cond SCGEst,
	rach-ConfigDedicated-r12			RACH-ConfigDedicated			OPTIONAL,	-- Need OP
	cipheringAlgorithmSCG-r12		CipheringAlgorithm-r12		OPTIONAL,	-- Need ON
	...,
	[[	makeBeforeBreakSCG-r14			ENUMERATED {true}				OPTIONAL,	-- Need OR
		rach-SkipSCG-r14				RACH-Skip-r14					OPTIONAL	-- Need OR
	]]
}

MobilityControlInfoV2X-r14 ::=	SEQUENCE {
	v2x-CommTxPoolExceptional-r14		SL-CommResourcePoolV2X-r14		OPTIONAL,		-- Need OR
	v2x-CommRxPool-r14					SL-CommRxPoolListV2X-r14		OPTIONAL,		-- Need OR
	v2x-CommSyncConfig-r14				SL-SyncConfigListV2X-r14		OPTIONAL,		-- Need OR
	cbr-MobilityTxConfigList-r14		SL-CBR-CommonTxConfigList-r14	OPTIONAL		-- Need OR
}

CarrierBandwidthEUTRA ::=			SEQUENCE {
	dl-Bandwidth						ENUMERATED {
												n6, n15, n25, n50, n75, n100, spare10,
												spare9, spare8, spare7, spare6, spare5,
												spare4, spare3, spare2, spare1},
	ul-Bandwidth						ENUMERATED {
												n6, n15, n25, n50, n75, n100, spare10,
												spare9, spare8, spare7, spare6, spare5,
												spare4, spare3, spare2, spare1}	OPTIONAL -- Need OP
}

CarrierFreqEUTRA ::=				SEQUENCE {
	dl-CarrierFreq						ARFCN-ValueEUTRA,
	ul-CarrierFreq						ARFCN-ValueEUTRA				OPTIONAL	-- Cond FDD
}

CarrierFreqEUTRA-v9e0 ::=			SEQUENCE {
	dl-CarrierFreq-v9e0					ARFCN-ValueEUTRA-r9,
	ul-CarrierFreq-v9e0					ARFCN-ValueEUTRA-r9			OPTIONAL	-- Cond FDD
}

RACH-Skip-r14 ::=					SEQUENCE {
	targetTA-r14					CHOICE {
		ta0-r14							NULL,
		mcg-PTAG-r14						NULL,
		scg-PTAG-r14						NULL,
		mcg-STAG-r14					STAG-Id-r11,
		scg-STAG-r14					STAG-Id-r11
	},
	ul-ConfigInfo-r14				SEQUENCE {
		numberOfConfUL-Processes-r14			INTEGER (1..8),
		ul-SchedInterval-r14			ENUMERATED {sf2, sf5, sf10},
		ul-StartSubframe-r14			INTEGER (0..9),
		ul-Grant-r14					BIT STRING (SIZE (16))
	}																OPTIONAL	-- Need OR
}


MobilityParametersCDMA2000 ::=			OCTET STRING


MobilityStateParameters ::=			SEQUENCE {
	t-Evaluation						ENUMERATED {
											s30, s60, s120, s180, s240, spare3, spare2, spare1},
	t-HystNormal						ENUMERATED {
											s30, s60, s120, s180, s240, spare3, spare2, spare1},
	n-CellChangeMedium					INTEGER (1..16),
	n-CellChangeHigh					INTEGER (1..16)
}


MultiBandInfoList ::=	SEQUENCE (SIZE (1..maxMultiBands)) OF FreqBandIndicator

MultiBandInfoList-v9e0 ::=	SEQUENCE (SIZE (1..maxMultiBands)) OF MultiBandInfo-v9e0

MultiBandInfoList-v10j0 ::=	SEQUENCE (SIZE (1..maxMultiBands)) OF NS-PmaxList-r10

MultiBandInfoList-v10l0 ::=	SEQUENCE (SIZE (1..maxMultiBands)) OF NS-PmaxList-v10l0

MultiBandInfoList-r11 ::=	SEQUENCE (SIZE (1..maxMultiBands)) OF FreqBandIndicator-r11

MultiBandInfo-v9e0 ::=		SEQUENCE {
	freqBandIndicator-v9e0				FreqBandIndicator-v9e0		OPTIONAL	-- Need OP
}


NS-PmaxList-r10 ::=				SEQUENCE (SIZE (1..maxNS-Pmax-r10)) OF NS-PmaxValue-r10

NS-PmaxList-v10l0 ::=			SEQUENCE (SIZE (1..maxNS-Pmax-r10)) OF NS-PmaxValue-v10l0

NS-PmaxValue-r10 ::=			SEQUENCE {
	additionalPmax-r10					P-Max							OPTIONAL,	-- Need OP
	additionalSpectrumEmission			AdditionalSpectrumEmission
}

NS-PmaxValue-v10l0 ::=			SEQUENCE {
	additionalSpectrumEmission-v10l0	AdditionalSpectrumEmission-v10l0	OPTIONAL	-- Need OP
}


PhysCellId ::=						INTEGER (0..503)


PhysCellIdRange ::=				SEQUENCE {
	start							PhysCellId,
	range							ENUMERATED {
										n4, n8, n12, n16, n24, n32, n48, n64, n84,
										n96, n128, n168, n252, n504, spare2,
										spare1}					OPTIONAL	-- Need OP
}


PhysCellIdRangeUTRA-FDDList-r9::=		SEQUENCE (SIZE (1..maxPhysCellIdRange-r9)) OF PhysCellIdRangeUTRA-FDD-r9

PhysCellIdRangeUTRA-FDD-r9 ::=			SEQUENCE {
		start-r9							PhysCellIdUTRA-FDD,
		range-r9							INTEGER (2..512)				OPTIONAL	-- Need OP
}


PhysCellIdCDMA2000 ::=			INTEGER (0..maxPNOffset)


PhysCellIdGERAN ::=				SEQUENCE {
	networkColourCode					BIT STRING (SIZE (3)),
	baseStationColourCode				BIT STRING (SIZE (3))
}


PhysCellIdUTRA-FDD ::=				INTEGER (0..511)


PhysCellIdUTRA-TDD ::=				INTEGER (0..127)


PLMN-Identity ::=					SEQUENCE {
	mcc									MCC					OPTIONAL,					-- Cond MCC
	mnc									MNC
}

MCC ::=								SEQUENCE (SIZE (3)) OF
											MCC-MNC-Digit

MNC ::=								SEQUENCE (SIZE (2..3)) OF
											MCC-MNC-Digit

MCC-MNC-Digit ::=					INTEGER (0..9)



PLMN-IdentityList3-r11 ::=				SEQUENCE (SIZE (1..16)) OF PLMN-Identity


PreRegistrationInfoHRPD ::=			SEQUENCE {
	preRegistrationAllowed				BOOLEAN,
	preRegistrationZoneId				PreRegistrationZoneIdHRPD	OPTIONAL, -- cond PreRegAllowed
	secondaryPreRegistrationZoneIdList	SecondaryPreRegistrationZoneIdListHRPD	OPTIONAL -- Need OR
}

SecondaryPreRegistrationZoneIdListHRPD ::=	SEQUENCE (SIZE (1..2)) OF PreRegistrationZoneIdHRPD

PreRegistrationZoneIdHRPD ::=			INTEGER (0..255)


Q-QualMin-r9 ::=					INTEGER (-34..-3)


Q-RxLevMin ::=						INTEGER (-70..-22)


Q-OffsetRange ::=						ENUMERATED {
												dB-24, dB-22, dB-20, dB-18, dB-16, dB-14,
												dB-12, dB-10, dB-8, dB-6, dB-5, dB-4, dB-3,
												dB-2, dB-1, dB0, dB1, dB2, dB3, dB4, dB5,
												dB6, dB8, dB10, dB12, dB14, dB16, dB18,
												dB20, dB22, dB24}


Q-OffsetRangeInterRAT ::=					INTEGER (-15..15)


ReselectionThreshold ::=				INTEGER (0..31)


ReselectionThresholdQ-r9 ::=			INTEGER (0..31)


SCellIndex-r10 ::=						INTEGER (1..7)
SCellIndex-r13 ::=						INTEGER (1..31)


ServCellIndex-r10 ::=					INTEGER (0..7)
ServCellIndex-r13 ::=				INTEGER (0..31)


SpeedStateScaleFactors ::=			SEQUENCE {
	sf-Medium							ENUMERATED {oDot25, oDot5, oDot75, lDot0},
	sf-High								ENUMERATED {oDot25, oDot5, oDot75, lDot0}
}

SystemInfoListGERAN ::=				SEQUENCE (SIZE (1..maxGERAN-SI)) OF
										OCTET STRING (SIZE (1..23))


SystemTimeInfoCDMA2000 ::=			SEQUENCE {
	cdma-EUTRA-Synchronisation			BOOLEAN,
	cdma-SystemTime						CHOICE {
		synchronousSystemTime				BIT STRING (SIZE (39)),
		asynchronousSystemTime				BIT STRING (SIZE (49))
	}
}


TrackingAreaCode ::=				BIT STRING (SIZE (16))


T-Reselection ::=					INTEGER (0..7)


T-ReselectionEUTRA-CE-r13 ::=				INTEGER (0..15)


AllowedMeasBandwidth ::=				ENUMERATED {mbw6, mbw15, mbw25, mbw50, mbw75, mbw100}


CSI-RSRP-Range-r12 ::=						INTEGER(0..97)


Hysteresis ::=							INTEGER (0..30)


LocationInfo-r10 ::=	SEQUENCE {
	locationCoordinates-r10					CHOICE {
		ellipsoid-Point-r10						OCTET STRING,
		ellipsoidPointWithAltitude-r10			OCTET STRING,
	...,
		ellipsoidPointWithUncertaintyCircle-r11					OCTET STRING,
		ellipsoidPointWithUncertaintyEllipse-r11				OCTET STRING,
		ellipsoidPointWithAltitudeAndUncertaintyEllipsoid-r11	OCTET STRING,
		ellipsoidArc-r11										OCTET STRING,
		polygon-r11												OCTET STRING
	},
	horizontalVelocity-r10					OCTET STRING				OPTIONAL,
	gnss-TOD-msec-r10						OCTET STRING				OPTIONAL,
	...
}


MBSFN-RSRQ-Range-r12 ::=				INTEGER(0..31)

MeasConfig ::=						SEQUENCE {
	-- Measurement objects
	measObjectToRemoveList				MeasObjectToRemoveList				OPTIONAL,	-- Need ON
	measObjectToAddModList				MeasObjectToAddModList				OPTIONAL,	-- Need ON
	-- Reporting configurations
	reportConfigToRemoveList			ReportConfigToRemoveList			OPTIONAL,	-- Need ON
	reportConfigToAddModList			ReportConfigToAddModList			OPTIONAL,	-- Need ON
	-- Measurement identities
	measIdToRemoveList					MeasIdToRemoveList					OPTIONAL,	-- Need ON
	measIdToAddModList					MeasIdToAddModList					OPTIONAL,	-- Need ON
	-- Other parameters
	quantityConfig						QuantityConfig						OPTIONAL,	-- Need ON
	measGapConfig						MeasGapConfig						OPTIONAL,	-- Need ON
	s-Measure							RSRP-Range							OPTIONAL,	-- Need ON
	preRegistrationInfoHRPD				PreRegistrationInfoHRPD				OPTIONAL,	-- Need OP
	speedStatePars			CHOICE {
		release								NULL,
		setup								SEQUENCE {
			mobilityStateParameters				MobilityStateParameters,
			timeToTrigger-SF					SpeedStateScaleFactors
		}
	}																		OPTIONAL,	-- Need ON
	...,
	[[	measObjectToAddModList-v9e0			MeasObjectToAddModList-v9e0		OPTIONAL	-- Need ON
	]],
	[[	allowInterruptions-r11				BOOLEAN							OPTIONAL	-- Need ON
	]],
	[[	measScaleFactor-r12			CHOICE {
			release						NULL,
			setup						MeasScaleFactor-r12
		}																OPTIONAL,	-- Need ON
		measIdToRemoveListExt-r12			MeasIdToRemoveListExt-r12		OPTIONAL,	-- Need ON
		measIdToAddModListExt-r12			MeasIdToAddModListExt-r12		OPTIONAL,	-- Need ON
		measRSRQ-OnAllSymbols-r12		BOOLEAN							OPTIONAL	-- Need ON
	]],
	[[
		measObjectToRemoveListExt-r13		MeasObjectToRemoveListExt-r13	OPTIONAL,	-- Need ON
		measObjectToAddModListExt-r13		MeasObjectToAddModListExt-r13	OPTIONAL,	-- Need ON
		measIdToAddModList-v1310			MeasIdToAddModList-v1310		OPTIONAL,	-- Need ON
		measIdToAddModListExt-v1310			MeasIdToAddModListExt-v1310		OPTIONAL	-- Need ON
	]],
	[[	measGapConfigPerCC-List-r14			MeasGapConfigPerCC-List-r14		OPTIONAL,	-- Need ON
		measGapSharingConfig-r14			MeasGapSharingConfig-r14		OPTIONAL	-- Need ON
	]]
}

MeasIdToRemoveList ::=				SEQUENCE (SIZE (1..maxMeasId)) OF MeasId

MeasIdToRemoveListExt-r12 ::=		SEQUENCE (SIZE (1..maxMeasId)) OF MeasId-v1250

MeasObjectToRemoveList ::=			SEQUENCE (SIZE (1..maxObjectId)) OF MeasObjectId

MeasObjectToRemoveListExt-r13 ::=	SEQUENCE (SIZE (1..maxObjectId)) OF MeasObjectId-v1310

ReportConfigToRemoveList ::=		SEQUENCE (SIZE (1..maxReportConfigId)) OF ReportConfigId


MeasDS-Config-r12 ::=			CHOICE {
	release							NULL,
	setup							SEQUENCE {
		dmtc-PeriodOffset-r12			CHOICE {
			ms40-r12						INTEGER(0..39),
			ms80-r12						INTEGER(0..79),
			ms160-r12						INTEGER(0..159),
			...
		},
		ds-OccasionDuration-r12		CHOICE {
			durationFDD-r12				INTEGER(1..maxDS-Duration-r12),
			durationTDD-r12				INTEGER(2..maxDS-Duration-r12)
		},
		measCSI-RS-ToRemoveList-r12	MeasCSI-RS-ToRemoveList-r12	OPTIONAL,	-- Need ON
		measCSI-RS-ToAddModList-r12	MeasCSI-RS-ToAddModList-r12	OPTIONAL,	-- Need ON
		...
	}
}

MeasCSI-RS-ToRemoveList-r12 ::=	SEQUENCE (SIZE (1..maxCSI-RS-Meas-r12)) OF MeasCSI-RS-Id-r12

MeasCSI-RS-ToAddModList-r12 ::=	SEQUENCE (SIZE (1..maxCSI-RS-Meas-r12)) OF MeasCSI-RS-Config-r12

MeasCSI-RS-Id-r12 ::=			INTEGER (1..maxCSI-RS-Meas-r12)

MeasCSI-RS-Config-r12 ::=		SEQUENCE {
	measCSI-RS-Id-r12				MeasCSI-RS-Id-r12,
	physCellId-r12					INTEGER (0..503),
	scramblingIdentity-r12			INTEGER (0..503),
	resourceConfig-r12				INTEGER (0..31),
	subframeOffset-r12				INTEGER (0..4),
	csi-RS-IndividualOffset-r12		Q-OffsetRange,
	...
}


MeasGapConfig ::=					CHOICE {
	release								NULL,
	setup								SEQUENCE {
		gapOffset							CHOICE {
				gp0									INTEGER (0..39),
				gp1									INTEGER (0..79),

				...,
				gp2-r14								INTEGER (0..39),
				gp3-r14								INTEGER (0..79),
				gp-ncsg0-r14						INTEGER (0..39),
				gp-ncsg1-r14						INTEGER (0..79),
				gp-ncsg2-r14						INTEGER (0..39),
				gp-ncsg3-r14						INTEGER (0..79),
				gp-nonUniform1-r14					INTEGER (0..1279),
				gp-nonUniform2-r14					INTEGER (0..2559),
				gp-nonUniform3-r14					INTEGER (0..5119),
				gp-nonUniform4-r14					INTEGER (0..10239)
		}
	}
}



MeasGapConfigPerCC-List-r14 ::=	CHOICE {
	release						NULL,
	setup						SEQUENCE {
		measGapConfigToRemoveList-r14	MeasGapConfigToRemoveList-r14	OPTIONAL,	-- Need ON
		measGapConfigToAddModList-r14	MeasGapConfigToAddModList-r14	OPTIONAL	-- Need ON
	}
}

MeasGapConfigToRemoveList-r14 ::=	SEQUENCE (SIZE (1..maxServCell-r13)) OF ServCellIndex-r13

MeasGapConfigToAddModList-r14 ::=	SEQUENCE (SIZE (1..maxServCell-r13)) OF MeasGapConfigPerCC-r14

MeasGapConfigPerCC-r14 ::=	SEQUENCE {
	servCellId-r14				ServCellIndex-r13,
	measGapConfigCC-r14			MeasGapConfig
}


MeasGapSharingConfig-r14 ::=			CHOICE {
	release								NULL,
	setup								SEQUENCE {
		measGapSharingScheme-r14				ENUMERATED {scheme00, scheme01, scheme10, scheme11}
	}
}


MeasId ::=							INTEGER (1..maxMeasId)

MeasId-v1250 ::=					INTEGER (maxMeasId-Plus1..maxMeasId-r12)


MeasIdToAddModList ::=				SEQUENCE (SIZE (1..maxMeasId)) OF MeasIdToAddMod

MeasIdToAddModList-v1310 ::=		SEQUENCE (SIZE (1..maxMeasId)) OF MeasIdToAddMod-v1310

MeasIdToAddModListExt-r12 ::=		SEQUENCE (SIZE (1..maxMeasId)) OF MeasIdToAddModExt-r12

MeasIdToAddModListExt-v1310 ::=		SEQUENCE (SIZE (1..maxMeasId)) OF MeasIdToAddMod-v1310

MeasIdToAddMod ::=	SEQUENCE {
	measId								MeasId,
	measObjectId						MeasObjectId,
	reportConfigId						ReportConfigId
}

MeasIdToAddModExt-r12 ::=	SEQUENCE {
	measId-v1250						MeasId-v1250,
	measObjectId-r12					MeasObjectId,
	reportConfigId-r12					ReportConfigId
}

MeasIdToAddMod-v1310 ::=	SEQUENCE {
	measObjectId-v1310			MeasObjectId-v1310		OPTIONAL
}


MeasObjectCDMA2000 ::=				SEQUENCE {
	cdma2000-Type						CDMA2000-Type,
	carrierFreq							CarrierFreqCDMA2000,
	searchWindowSize					INTEGER (0..15)						OPTIONAL,	-- Need ON
	offsetFreq							Q-OffsetRangeInterRAT				DEFAULT 0,
	cellsToRemoveList					CellIndexList						OPTIONAL,	-- Need ON
	cellsToAddModList					CellsToAddModListCDMA2000			OPTIONAL,	-- Need ON
	cellForWhichToReportCGI				PhysCellIdCDMA2000					OPTIONAL,	-- Need ON
	...
}

CellsToAddModListCDMA2000 ::=		SEQUENCE (SIZE (1..maxCellMeas)) OF CellsToAddModCDMA2000

CellsToAddModCDMA2000 ::=	SEQUENCE {
	cellIndex							INTEGER (1..maxCellMeas),
	physCellId							PhysCellIdCDMA2000
}


MeasObjectEUTRA ::=					SEQUENCE {
	carrierFreq							ARFCN-ValueEUTRA,
	allowedMeasBandwidth				AllowedMeasBandwidth,
	presenceAntennaPort1				PresenceAntennaPort1,
	neighCellConfig						NeighCellConfig,
	offsetFreq							Q-OffsetRange				DEFAULT dB0,
	-- Cell list
	cellsToRemoveList					CellIndexList				OPTIONAL,		-- Need ON
	cellsToAddModList					CellsToAddModList			OPTIONAL,		-- Need ON
	-- Black list
	blackCellsToRemoveList				CellIndexList				OPTIONAL,		-- Need ON
	blackCellsToAddModList				BlackCellsToAddModList		OPTIONAL,		-- Need ON
	cellForWhichToReportCGI				PhysCellId					OPTIONAL,		-- Need ON
	...,
	[[measCycleSCell-r10				MeasCycleSCell-r10		OPTIONAL,		-- Need ON
		measSubframePatternConfigNeigh-r10	MeasSubframePatternConfigNeigh-r10	OPTIONAL							-- Need ON
	]],
	[[widebandRSRQ-Meas-r11				BOOLEAN	OPTIONAL		-- Cond WB-RSRQ
	]],
	[[	altTTT-CellsToRemoveList-r12	CellIndexList				OPTIONAL,		-- Need ON
		altTTT-CellsToAddModList-r12	AltTTT-CellsToAddModList-r12	OPTIONAL,		-- Need ON
		t312-r12						CHOICE {
			release							NULL,
			setup							ENUMERATED {ms0, ms50, ms100, ms200,
											ms300, ms400, ms500, ms1000}
		}														OPTIONAL,		-- Need ON
		reducedMeasPerformance-r12		BOOLEAN					OPTIONAL,		-- Need ON
		measDS-Config-r12				MeasDS-Config-r12			OPTIONAL		-- Need ON
	]],
	[[
		whiteCellsToRemoveList-r13		CellIndexList				OPTIONAL,		-- Need ON
		whiteCellsToAddModList-r13		WhiteCellsToAddModList-r13	OPTIONAL,		-- Need ON
		rmtc-Config-r13				RMTC-Config-r13			OPTIONAL,		-- Need ON
		carrierFreq-r13					ARFCN-ValueEUTRA-v9e0		OPTIONAL			-- Need ON
	]],
	[[
		tx-ResourcePoolToRemoveList-r14	Tx-ResourcePoolMeasList-r14		OPTIONAL,	-- Need ON
		tx-ResourcePoolToAddList-r14	Tx-ResourcePoolMeasList-r14		OPTIONAL,	-- Need ON
		fembms-MixedCarrier-r14				BOOLEAN					OPTIONAL			-- Need ON
	]]
}

MeasObjectEUTRA-v9e0 ::=			SEQUENCE {
	carrierFreq-v9e0					ARFCN-ValueEUTRA-v9e0
}

CellsToAddModList ::=				SEQUENCE (SIZE (1..maxCellMeas)) OF CellsToAddMod

CellsToAddMod ::=	SEQUENCE {
	cellIndex							INTEGER (1..maxCellMeas),
	physCellId							PhysCellId,
	cellIndividualOffset				Q-OffsetRange
}

BlackCellsToAddModList ::=			SEQUENCE (SIZE (1..maxCellMeas)) OF BlackCellsToAddMod

BlackCellsToAddMod ::=	SEQUENCE {
	cellIndex							INTEGER (1..maxCellMeas),
	physCellIdRange						PhysCellIdRange
}

MeasCycleSCell-r10 ::=				ENUMERATED {sf160, sf256, sf320, sf512,
													sf640, sf1024, sf1280, spare1}

MeasSubframePatternConfigNeigh-r10 ::=	CHOICE {
	release									NULL,
	setup									SEQUENCE {
		measSubframePatternNeigh-r10			MeasSubframePattern-r10,
		measSubframeCellList-r10				MeasSubframeCellList-r10	OPTIONAL	-- Cond always
	}
}

MeasSubframeCellList-r10 ::=	SEQUENCE (SIZE (1..maxCellMeas)) OF PhysCellIdRange

AltTTT-CellsToAddModList-r12 ::=	SEQUENCE (SIZE (1..maxCellMeas)) OF AltTTT-CellsToAddMod-r12

AltTTT-CellsToAddMod-r12 ::=	SEQUENCE {
	cellIndex-r12							INTEGER (1..maxCellMeas),
	physCellIdRange-r12						PhysCellIdRange
}

WhiteCellsToAddModList-r13 ::=			SEQUENCE (SIZE (1..maxCellMeas)) OF WhiteCellsToAddMod-r13

WhiteCellsToAddMod-r13 ::=	SEQUENCE {
	cellIndex-r13							INTEGER (1..maxCellMeas),
	physCellIdRange-r13						PhysCellIdRange
}

RMTC-Config-r13 ::=	CHOICE {
	release								NULL,
	setup								SEQUENCE {
		rmtc-Period-r13					ENUMERATED {ms40, ms80, ms160, ms320, ms640},
		rmtc-SubframeOffset-r13			INTEGER(0..639)					OPTIONAL,		-- Need ON
		measDuration-r13				ENUMERATED {sym1, sym14, sym28, sym42, sym70},
		...
	}
}

Tx-ResourcePoolMeasList-r14 ::=	SEQUENCE (SIZE (1..maxSL-PoolToMeasure-r14)) OF SL-V2X-TxPoolReportIdentity-r14


MeasObjectGERAN ::=					SEQUENCE {
	carrierFreqs						CarrierFreqsGERAN,
	offsetFreq							Q-OffsetRangeInterRAT		DEFAULT 0,
	ncc-Permitted						BIT STRING(SIZE (8))		DEFAULT '11111111'B,
	cellForWhichToReportCGI				PhysCellIdGERAN				OPTIONAL,	-- Need ON
	...
}


MeasObjectId ::=					INTEGER (1..maxObjectId)

MeasObjectId-v1310 ::=			INTEGER (maxObjectId-Plus1-r13..maxObjectId-r13)

MeasObjectId-r13 ::=				INTEGER (1..maxObjectId-r13)


MeasObjectToAddModList ::=			SEQUENCE (SIZE (1..maxObjectId)) OF MeasObjectToAddMod

MeasObjectToAddModListExt-r13 ::=	SEQUENCE (SIZE (1..maxObjectId)) OF MeasObjectToAddModExt-r13

MeasObjectToAddModList-v9e0 ::=		SEQUENCE (SIZE (1..maxObjectId)) OF MeasObjectToAddMod-v9e0

MeasObjectToAddMod ::=	SEQUENCE {
	measObjectId						MeasObjectId,
	measObject							CHOICE {
		measObjectEUTRA						MeasObjectEUTRA,
		measObjectUTRA						MeasObjectUTRA,
		measObjectGERAN						MeasObjectGERAN,
		measObjectCDMA2000					MeasObjectCDMA2000,
		...,
		measObjectWLAN-r13					MeasObjectWLAN-r13
	}
}

MeasObjectToAddModExt-r13 ::=	SEQUENCE {
	measObjectId-r13					MeasObjectId-v1310,
	measObject-r13							CHOICE {
		measObjectEUTRA-r13						MeasObjectEUTRA,
		measObjectUTRA-r13						MeasObjectUTRA,
		measObjectGERAN-r13						MeasObjectGERAN,
		measObjectCDMA2000-r13					MeasObjectCDMA2000,
		...,
		measObjectWLAN-v1320					MeasObjectWLAN-r13
	}
}

MeasObjectToAddMod-v9e0 ::=	SEQUENCE {
	measObjectEUTRA-v9e0				MeasObjectEUTRA-v9e0		OPTIONAL	-- Cond eutra
}


MeasObjectUTRA ::=					SEQUENCE {
	carrierFreq							ARFCN-ValueUTRA,
	offsetFreq							Q-OffsetRangeInterRAT		DEFAULT 0,
	cellsToRemoveList					CellIndexList				OPTIONAL,			-- Need ON
	cellsToAddModList					CHOICE {
		cellsToAddModListUTRA-FDD			CellsToAddModListUTRA-FDD,
		cellsToAddModListUTRA-TDD			CellsToAddModListUTRA-TDD
	}																OPTIONAL,			-- Need ON
	cellForWhichToReportCGI				CHOICE {
		utra-FDD							PhysCellIdUTRA-FDD,
		utra-TDD							PhysCellIdUTRA-TDD
	}																OPTIONAL,	-- Need ON
	...,
	[[	csg-allowedReportingCells-v930			CSG-AllowedReportingCells-r9	OPTIONAL		-- Need ON
	]],
	[[	reducedMeasPerformance-r12				BOOLEAN			OPTIONAL		-- Need ON
	]]
}

CellsToAddModListUTRA-FDD ::=		SEQUENCE (SIZE (1..maxCellMeas)) OF CellsToAddModUTRA-FDD

CellsToAddModUTRA-FDD ::=	SEQUENCE {
	cellIndex							INTEGER (1..maxCellMeas),
	physCellId							PhysCellIdUTRA-FDD
}

CellsToAddModListUTRA-TDD ::=		SEQUENCE (SIZE (1..maxCellMeas)) OF CellsToAddModUTRA-TDD

CellsToAddModUTRA-TDD ::=	SEQUENCE {
	cellIndex							INTEGER (1..maxCellMeas),
	physCellId							PhysCellIdUTRA-TDD
}

CSG-AllowedReportingCells-r9 ::=		SEQUENCE {
	physCellIdRangeUTRA-FDDList-r9			PhysCellIdRangeUTRA-FDDList-r9	OPTIONAL	-- Need OR
}

MeasObjectWLAN-r13 ::=	SEQUENCE {
	carrierFreq-r13					CHOICE {
		bandIndicatorListWLAN-r13		SEQUENCE (SIZE (1..maxWLAN-Bands-r13)) OF WLAN-BandIndicator-r13,
		carrierInfoListWLAN-r13			SEQUENCE (SIZE (1..maxWLAN-CarrierInfo-r13)) OF WLAN-CarrierInfo-r13
	}		OPTIONAL,	-- Need ON
	wlan-ToAddModList-r13				WLAN-Id-List-r13			OPTIONAL,	-- Need ON
	wlan-ToRemoveList-r13				WLAN-Id-List-r13			OPTIONAL,	-- Need ON
	...
}

WLAN-BandIndicator-r13 ::=	ENUMERATED {band2dot4, band5, band60-v1430, spare5, spare4, spare3, spare2, spare1, ...}


MeasResults ::=						SEQUENCE {
	measId								MeasId,
	measResultPCell					SEQUENCE {
		rsrpResult							RSRP-Range,
		rsrqResult							RSRQ-Range
	},
	measResultNeighCells				CHOICE {
		measResultListEUTRA					MeasResultListEUTRA,
		measResultListUTRA					MeasResultListUTRA,
		measResultListGERAN					MeasResultListGERAN,
		measResultsCDMA2000					MeasResultsCDMA2000,
		...
	}																		OPTIONAL,
	...,
	[[	measResultForECID-r9				MeasResultForECID-r9			OPTIONAL
	]],
	[[	locationInfo-r10					LocationInfo-r10				OPTIONAL,
		measResultServFreqList-r10			MeasResultServFreqList-r10		OPTIONAL
	]],
	[[	measId-v1250						MeasId-v1250					OPTIONAL,
		measResultPCell-v1250				RSRQ-Range-v1250				OPTIONAL,
		measResultCSI-RS-List-r12			MeasResultCSI-RS-List-r12		OPTIONAL
	]],
	[[	measResultForRSSI-r13				MeasResultForRSSI-r13			OPTIONAL,
		measResultServFreqListExt-r13		MeasResultServFreqListExt-r13	OPTIONAL,
		measResultSSTD-r13					MeasResultSSTD-r13				OPTIONAL,
		measResultPCell-v1310				SEQUENCE {
			rs-sinr-Result-r13					RS-SINR-Range-r13
		}																	OPTIONAL,
		ul-PDCP-DelayResultList-r13			UL-PDCP-DelayResultList-r13		OPTIONAL,
		measResultListWLAN-r13				MeasResultListWLAN-r13			OPTIONAL
	]],
	[[	measResultPCell-v1360				RSRP-Range-v1360				OPTIONAL
	]],
	[[	measResultListCBR-r14				MeasResultListCBR-r14			OPTIONAL,
		measResultListWLAN-r14				MeasResultListWLAN-r14			OPTIONAL
	]]
}

MeasResultListEUTRA ::=				SEQUENCE (SIZE (1..maxCellReport)) OF MeasResultEUTRA

MeasResultEUTRA ::=	SEQUENCE {
	physCellId							PhysCellId,
	cgi-Info							SEQUENCE {
		cellGlobalId						CellGlobalIdEUTRA,
		trackingAreaCode					TrackingAreaCode,
		plmn-IdentityList					PLMN-IdentityList2				OPTIONAL
	}															OPTIONAL,
	measResult							SEQUENCE {
		rsrpResult							RSRP-Range						OPTIONAL,
		rsrqResult							RSRQ-Range						OPTIONAL,
		...,
		[[	additionalSI-Info-r9				AdditionalSI-Info-r9		OPTIONAL
		]],
		[[	primaryPLMN-Suitable-r12			ENUMERATED {true}			OPTIONAL,
			measResult-v1250					RSRQ-Range-v1250			OPTIONAL
		]],
		[[	rs-sinr-Result-r13					RS-SINR-Range-r13			OPTIONAL,
			cgi-Info-v1310						SEQUENCE {
				freqBandIndicator-r13				FreqBandIndicator-r11		OPTIONAL,
				multiBandInfoList-r13				MultiBandInfoList-r11		OPTIONAL,
				freqBandIndicatorPriority-r13		ENUMERATED {true}			OPTIONAL
			}																OPTIONAL
		]],
		[[
			measResult-v1360					RSRP-Range-v1360					OPTIONAL
		]]
	}
}

MeasResultServFreqList-r10 ::=	SEQUENCE (SIZE (1..maxServCell-r10)) OF MeasResultServFreq-r10

MeasResultServFreqListExt-r13 ::=	SEQUENCE (SIZE (1..maxServCell-r13)) OF MeasResultServFreq-r13

MeasResultServFreq-r10 ::=			SEQUENCE {
	servFreqId-r10						ServCellIndex-r10,
	measResultSCell-r10					SEQUENCE {
		rsrpResultSCell-r10					RSRP-Range,
		rsrqResultSCell-r10					RSRQ-Range
	}															OPTIONAL,
	measResultBestNeighCell-r10			SEQUENCE {
		physCellId-r10						PhysCellId,
		rsrpResultNCell-r10					RSRP-Range,
		rsrqResultNCell-r10					RSRQ-Range
	}															OPTIONAL,
	...,
	[[	measResultSCell-v1250				RSRQ-Range-v1250	OPTIONAL,
		measResultBestNeighCell-v1250		RSRQ-Range-v1250	OPTIONAL
	]],
	[[	measResultSCell-v1310				SEQUENCE {
			rs-sinr-Result-r13					RS-SINR-Range-r13
		}		OPTIONAL,
		measResultBestNeighCell-v1310		SEQUENCE {
			rs-sinr-Result-r13					RS-SINR-Range-r13
		}		OPTIONAL
	]]
}

MeasResultServFreq-r13 ::=			SEQUENCE {
	servFreqId-r13						ServCellIndex-r13,
	measResultSCell-r13					SEQUENCE {
		rsrpResultSCell-r13					RSRP-Range,
		rsrqResultSCell-r13					RSRQ-Range-r13,
		rs-sinr-Result-r13					RS-SINR-Range-r13	OPTIONAL
	}															OPTIONAL,
	measResultBestNeighCell-r13			SEQUENCE {
		physCellId-r13						PhysCellId,
		rsrpResultNCell-r13					RSRP-Range,
		rsrqResultNCell-r13					RSRQ-Range-r13,
		rs-sinr-Result-r13					RS-SINR-Range-r13	OPTIONAL
	}															OPTIONAL,
	...,
	[[	measResultBestNeighCell-v1360		SEQUENCE {
			rsrpResultNCell-v1360				RSRP-Range-v1360
		}														OPTIONAL
	]]
}

MeasResultCSI-RS-List-r12 ::=	SEQUENCE (SIZE (1..maxCellReport)) OF MeasResultCSI-RS-r12

MeasResultCSI-RS-r12 ::=		SEQUENCE {
	measCSI-RS-Id-r12				MeasCSI-RS-Id-r12,
	csi-RSRP-Result-r12				CSI-RSRP-Range-r12,
	...
}

MeasResultListUTRA ::=				SEQUENCE (SIZE (1..maxCellReport)) OF MeasResultUTRA

MeasResultUTRA ::=	SEQUENCE {
	physCellId							CHOICE {
		fdd									PhysCellIdUTRA-FDD,
		tdd									PhysCellIdUTRA-TDD
	},
	cgi-Info							SEQUENCE {
		cellGlobalId						CellGlobalIdUTRA,
		locationAreaCode					BIT STRING (SIZE (16))			OPTIONAL,
		routingAreaCode						BIT STRING (SIZE (8))			OPTIONAL,
		plmn-IdentityList					PLMN-IdentityList2				OPTIONAL
	}															OPTIONAL,
	measResult							SEQUENCE {
		utra-RSCP							INTEGER (-5..91)				OPTIONAL,
		utra-EcN0							INTEGER (0..49)					OPTIONAL,
		...,
		[[	additionalSI-Info-r9				AdditionalSI-Info-r9				OPTIONAL
		]],
		[[	primaryPLMN-Suitable-r12			ENUMERATED {true}			OPTIONAL
		]]
	}
}

MeasResultListGERAN ::=				SEQUENCE (SIZE (1..maxCellReport)) OF MeasResultGERAN

MeasResultGERAN ::=	SEQUENCE {
	carrierFreq							CarrierFreqGERAN,
	physCellId							PhysCellIdGERAN,
	cgi-Info							SEQUENCE {
		cellGlobalId						CellGlobalIdGERAN,
		routingAreaCode						BIT STRING (SIZE (8))			OPTIONAL
	}																		OPTIONAL,
	measResult							SEQUENCE {
		rssi								INTEGER (0..63),
		...
	}
}

MeasResultsCDMA2000 ::=				SEQUENCE {
	preRegistrationStatusHRPD			BOOLEAN,
	measResultListCDMA2000				MeasResultListCDMA2000
}

MeasResultListCDMA2000 ::=			SEQUENCE (SIZE (1..maxCellReport)) OF MeasResultCDMA2000

MeasResultCDMA2000 ::=	SEQUENCE {
	physCellId							PhysCellIdCDMA2000,
	cgi-Info							CellGlobalIdCDMA2000				OPTIONAL,
	measResult							SEQUENCE {
		pilotPnPhase						INTEGER	(0..32767)				OPTIONAL,
		pilotStrength						INTEGER (0..63),
		...
	}
}

MeasResultListWLAN-r13 ::=		SEQUENCE (SIZE (1..maxCellReport)) OF MeasResultWLAN-r13

MeasResultListWLAN-r14 ::=		SEQUENCE (SIZE (1..maxWLAN-Id-Report-r14)) OF MeasResultWLAN-r13

MeasResultWLAN-r13 ::=	SEQUENCE {
	wlan-Identifiers-r13					WLAN-Identifiers-r12,
	carrierInfoWLAN-r13						WLAN-CarrierInfo-r13	OPTIONAL,
	bandWLAN-r13							WLAN-BandIndicator-r13	OPTIONAL,
	rssiWLAN-r13							WLAN-RSSI-Range-r13,
	availableAdmissionCapacityWLAN-r13		INTEGER (0..31250)		OPTIONAL,
	backhaulDL-BandwidthWLAN-r13			WLAN-backhaulRate-r12	OPTIONAL,
	backhaulUL-BandwidthWLAN-r13			WLAN-backhaulRate-r12	OPTIONAL,
	channelUtilizationWLAN-r13				INTEGER (0..255)		OPTIONAL,
	stationCountWLAN-r13					INTEGER (0..65535)		OPTIONAL,
	connectedWLAN-r13						ENUMERATED {true}		OPTIONAL,
	...
}

MeasResultListCBR-r14 ::=			SEQUENCE (SIZE (1..maxCBR-Report-r14)) OF MeasResultCBR-r14

MeasResultCBR-r14 ::=	SEQUENCE {
	poolIdentity-r14		SL-V2X-TxPoolReportIdentity-r14,
	cbr-PSSCH-r14			SL-CBR-r14,
	cbr-PSCCH-r14			SL-CBR-r14				OPTIONAL
}

MeasResultForECID-r9 ::=		SEQUENCE {
	ue-RxTxTimeDiffResult-r9				INTEGER (0..4095),
	currentSFN-r9							BIT STRING (SIZE (10))
}

PLMN-IdentityList2 ::=				SEQUENCE (SIZE (1..5)) OF PLMN-Identity

AdditionalSI-Info-r9 ::=			SEQUENCE {
	csg-MemberStatus-r9				ENUMERATED {member}				OPTIONAL,
	csg-Identity-r9						CSG-Identity						OPTIONAL
}
MeasResultForRSSI-r13 ::=			SEQUENCE {
	rssi-Result-r13							RSSI-Range-r13,
	channelOccupancy-r13					INTEGER (0..100),
	...
}

UL-PDCP-DelayResultList-r13 ::=		SEQUENCE (SIZE (1..maxQCI-r13)) OF UL-PDCP-DelayResult-r13


UL-PDCP-DelayResult-r13 ::=			SEQUENCE {
	qci-Id-r13							ENUMERATED {qci1, qci2, qci3, qci4, spare4, spare3, spare2, spare1},
	excessDelay-r13						INTEGER (0..31),
	...
}


MeasResultSSTD-r13 ::=						SEQUENCE {
	sfn-OffsetResult-r13						INTEGER (0..1023),
	frameBoundaryOffsetResult-r13				INTEGER (-5..4),
	subframeBoundaryOffsetResult-r13			INTEGER (0..127)
}


MeasScaleFactor-r12 ::=			ENUMERATED {sf-EUTRA-cf1, sf-EUTRA-cf2}


QuantityConfig ::=					SEQUENCE {
	quantityConfigEUTRA					QuantityConfigEUTRA					OPTIONAL,	-- Need ON
	quantityConfigUTRA					QuantityConfigUTRA					OPTIONAL,	-- Need ON
	quantityConfigGERAN					QuantityConfigGERAN					OPTIONAL,	-- Need ON
	quantityConfigCDMA2000				QuantityConfigCDMA2000				OPTIONAL,	-- Need ON
	...,
	[[	quantityConfigUTRA-v1020		QuantityConfigUTRA-v1020			OPTIONAL	-- Need ON
	]],
	[[	quantityConfigEUTRA-v1250		QuantityConfigEUTRA-v1250			OPTIONAL	-- Need ON
	]],
	[[	quantityConfigEUTRA-v1310		QuantityConfigEUTRA-v1310			OPTIONAL,	-- Need ON
		quantityConfigWLAN-r13			QuantityConfigWLAN-r13				OPTIONAL	-- Need ON
	]]
}

QuantityConfigEUTRA ::=				SEQUENCE {
	filterCoefficientRSRP				FilterCoefficient					DEFAULT fc4,
	filterCoefficientRSRQ				FilterCoefficient					DEFAULT fc4
}

QuantityConfigEUTRA-v1250 ::=		SEQUENCE {
	filterCoefficientCSI-RSRP-r12		FilterCoefficient					OPTIONAL		-- Need OR
}

QuantityConfigEUTRA-v1310 ::=		SEQUENCE {
	filterCoefficientRS-SINR-r13		FilterCoefficient					DEFAULT fc4
}

QuantityConfigUTRA ::=				SEQUENCE {
	measQuantityUTRA-FDD				ENUMERATED {cpich-RSCP, cpich-EcN0},
	measQuantityUTRA-TDD				ENUMERATED {pccpch-RSCP},
	filterCoefficient					FilterCoefficient					DEFAULT fc4
}

QuantityConfigUTRA-v1020 ::=		SEQUENCE {
	filterCoefficient2-FDD-r10			FilterCoefficient					DEFAULT fc4
}

QuantityConfigGERAN ::=				SEQUENCE {
	measQuantityGERAN					ENUMERATED {rssi},
	filterCoefficient					FilterCoefficient					DEFAULT fc2
}

QuantityConfigCDMA2000 ::=			SEQUENCE {
	measQuantityCDMA2000				ENUMERATED {pilotStrength, pilotPnPhaseAndPilotStrength}
}

QuantityConfigWLAN-r13 ::=			SEQUENCE {
	measQuantityWLAN-r13				ENUMERATED {rssiWLAN},
	filterCoefficient-r13				FilterCoefficient					DEFAULT fc4
}


ReportConfigEUTRA ::=				SEQUENCE {
	triggerType							CHOICE {
		event								SEQUENCE {
			eventId								CHOICE {
				eventA1								SEQUENCE {
					a1-Threshold						ThresholdEUTRA
				},
				eventA2								SEQUENCE {
					a2-Threshold						ThresholdEUTRA
				},
				eventA3								SEQUENCE {
					a3-Offset							INTEGER (-30..30),
					reportOnLeave						BOOLEAN
				},
				eventA4								SEQUENCE {
					a4-Threshold						ThresholdEUTRA
				},
				eventA5								SEQUENCE {
					a5-Threshold1						ThresholdEUTRA,
					a5-Threshold2						ThresholdEUTRA
				},
				...,
				eventA6-r10							SEQUENCE {
					a6-Offset-r10						INTEGER (-30..30),
					a6-ReportOnLeave-r10				BOOLEAN
				},
				eventC1-r12							SEQUENCE {
					c1-Threshold-r12					ThresholdEUTRA-v1250,
					c1-ReportOnLeave-r12				BOOLEAN
				},
				eventC2-r12							SEQUENCE {
					c2-RefCSI-RS-r12					MeasCSI-RS-Id-r12,
					c2-Offset-r12						INTEGER (-30..30),
					c2-ReportOnLeave-r12				BOOLEAN
				},
				eventV1-r14							SEQUENCE {
					v1-Threshold-r14					SL-CBR-r14
				},
				eventV2-r14							SEQUENCE {
					v2-Threshold-r14					SL-CBR-r14
				}
			},
			hysteresis							Hysteresis,
			timeToTrigger						TimeToTrigger
		},
		periodical								SEQUENCE {
			purpose									ENUMERATED {
														reportStrongestCells, reportCGI}
		}
	},
	triggerQuantity						ENUMERATED {rsrp, rsrq},
	reportQuantity						ENUMERATED {sameAsTriggerQuantity, both},
	maxReportCells						INTEGER (1..maxCellReport),
	reportInterval						ReportInterval,
	reportAmount						ENUMERATED {r1, r2, r4, r8, r16, r32, r64, infinity},
	...,
	[[	si-RequestForHO-r9					ENUMERATED {setup}		OPTIONAL,	-- Cond reportCGI
		ue-RxTxTimeDiffPeriodical-r9		ENUMERATED {setup}		OPTIONAL	-- Need OR
	]],
	[[	includeLocationInfo-r10				ENUMERATED {true}		OPTIONAL,	-- Need OR
		reportAddNeighMeas-r10				ENUMERATED {setup}		OPTIONAL	-- Need OR
	]],
	[[	alternativeTimeToTrigger-r12		CHOICE {
			release								NULL,
			setup								TimeToTrigger
		}													OPTIONAL,	-- Need ON
		useT312-r12							BOOLEAN			OPTIONAL,	-- Need ON
		usePSCell-r12						BOOLEAN			OPTIONAL,	-- Need ON
		aN-Threshold1-v1250					RSRQ-RangeConfig-r12		OPTIONAL,	-- Need ON
		a5-Threshold2-v1250					RSRQ-RangeConfig-r12		OPTIONAL,	-- Need ON
		reportStrongestCSI-RSs-r12			BOOLEAN			OPTIONAL,	-- Need ON
		reportCRS-Meas-r12					BOOLEAN			OPTIONAL,	-- Need ON
		triggerQuantityCSI-RS-r12			BOOLEAN			OPTIONAL		-- Need ON
	]],
	[[	reportSSTD-Meas-r13					BOOLEAN			OPTIONAL,		-- Need ON
		rs-sinr-Config-r13					CHOICE {
			release								NULL,
			setup								SEQUENCE {
				triggerQuantity-v1310				ENUMERATED {sinr}		OPTIONAL,	-- Need ON
				aN-Threshold1-r13					RS-SINR-Range-r13		OPTIONAL,	-- Need ON
				a5-Threshold2-r13					RS-SINR-Range-r13		OPTIONAL,	-- Need ON
				reportQuantity-v1310				ENUMERATED {rsrpANDsinr, rsrqANDsinr, all}
			}
		}																OPTIONAL,	-- Need ON
		useWhiteCellList-r13				BOOLEAN						OPTIONAL,	-- Need ON
		measRSSI-ReportConfig-r13			MeasRSSI-ReportConfig-r13	OPTIONAL,	-- Need ON
		includeMultiBandInfo-r13			ENUMERATED {true}			OPTIONAL,	-- Cond reportCGI
		ul-DelayConfig-r13					UL-DelayConfig-r13			OPTIONAL	-- Need ON
	]],
	[[	ue-RxTxTimeDiffPeriodicalTDD-r13	BOOLEAN						OPTIONAL	-- Need ON
	]],
	[[
		purpose-v1430			ENUMERATED {reportLocation, sidelink, spare2, spare1}
															OPTIONAL	-- Need ON
	]]
}

RSRQ-RangeConfig-r12 ::=			CHOICE {
	release								NULL,
	setup								RSRQ-Range-v1250
}

ThresholdEUTRA ::=					CHOICE{
	threshold-RSRP						RSRP-Range,
	threshold-RSRQ						RSRQ-Range
}

ThresholdEUTRA-v1250 ::=			CSI-RSRP-Range-r12

MeasRSSI-ReportConfig-r13 ::=	SEQUENCE {
	channelOccupancyThreshold-r13			RSSI-Range-r13				OPTIONAL	-- Need OR
}


ReportConfigId ::=					INTEGER (1..maxReportConfigId)


ReportConfigInterRAT ::=			SEQUENCE {
	triggerType							CHOICE {
		event								SEQUENCE {
			eventId								CHOICE {
				eventB1								SEQUENCE {
					b1-Threshold						CHOICE {
						b1-ThresholdUTRA					ThresholdUTRA,
						b1-ThresholdGERAN					ThresholdGERAN,
						b1-ThresholdCDMA2000				ThresholdCDMA2000
					}
				},
				eventB2								SEQUENCE {
					b2-Threshold1						ThresholdEUTRA,
					b2-Threshold2						CHOICE {
						b2-Threshold2UTRA					ThresholdUTRA,
						b2-Threshold2GERAN					ThresholdGERAN,
						b2-Threshold2CDMA2000				ThresholdCDMA2000
					}
				},
				...,
				eventW1-r13						SEQUENCE {
					w1-Threshold-r13			WLAN-RSSI-Range-r13
				},
				eventW2-r13						SEQUENCE {
					w2-Threshold1-r13			WLAN-RSSI-Range-r13,
					w2-Threshold2-r13			WLAN-RSSI-Range-r13
				},
				eventW3-r13						SEQUENCE {
					w3-Threshold-r13			WLAN-RSSI-Range-r13
				}
			},
			hysteresis						Hysteresis,
			timeToTrigger					TimeToTrigger
		},
		periodical								SEQUENCE {
			purpose									ENUMERATED {
														reportStrongestCells,
														reportStrongestCellsForSON,
														reportCGI}
		}
	},
	maxReportCells						INTEGER (1..maxCellReport),
	reportInterval						ReportInterval,
	reportAmount						ENUMERATED {r1, r2, r4, r8, r16, r32, r64, infinity},
	...,
	[[	si-RequestForHO-r9					ENUMERATED {setup}		OPTIONAL	-- Cond reportCGI
	]],
	[[	reportQuantityUTRA-FDD-r10			ENUMERATED {both}		OPTIONAL	-- Need OR
	]],
	[[	includeLocationInfo-r11				BOOLEAN					OPTIONAL	-- Need ON
	]],
	[[	b2-Threshold1-v1250					CHOICE {
			release								NULL,
			setup								RSRQ-Range-v1250
		}															OPTIONAL	-- Need ON
	]],
	[[	reportQuantityWLAN-r13				ReportQuantityWLAN-r13	OPTIONAL	-- Need ON
	]],
	[[	reportAnyWLAN-r14					BOOLEAN					OPTIONAL	-- Need ON
	]]
}

ThresholdUTRA ::=					CHOICE{
	utra-RSCP							INTEGER (-5..91),
	utra-EcN0							INTEGER (0..49)
}

ThresholdGERAN ::=				INTEGER (0..63)

ThresholdCDMA2000 ::=			INTEGER (0..63)

ReportQuantityWLAN-r13 ::=		SEQUENCE {
	bandRequestWLAN-r13							ENUMERATED {true}	OPTIONAL,	-- Need OR
	carrierInfoRequestWLAN-r13					ENUMERATED {true}	OPTIONAL,	-- Need OR
	availableAdmissionCapacityRequestWLAN-r13	ENUMERATED {true}	OPTIONAL,	-- Need OR
	backhaulDL-BandwidthRequestWLAN-r13			ENUMERATED {true}	OPTIONAL,	-- Need OR
	backhaulUL-BandwidthRequestWLAN-r13			ENUMERATED {true}	OPTIONAL,	-- Need OR
	channelUtilizationRequestWLAN-r13			ENUMERATED {true}	OPTIONAL,	-- Need OR
	stationCountRequestWLAN-r13					ENUMERATED {true}	OPTIONAL,	-- Need OR
	...
}


ReportConfigToAddModList ::=		SEQUENCE (SIZE (1..maxReportConfigId)) OF ReportConfigToAddMod

ReportConfigToAddMod ::=	SEQUENCE {
	reportConfigId						ReportConfigId,
	reportConfig						CHOICE {
		reportConfigEUTRA					ReportConfigEUTRA,
		reportConfigInterRAT				ReportConfigInterRAT
	}
}



ReportInterval ::=					ENUMERATED {
										ms120, ms240, ms480, ms640, ms1024, ms2048, ms5120, ms10240,
										min1, min6, min12, min30, min60, spare3, spare2, spare1}


RSRP-Range ::=						INTEGER(0..97)

RSRP-Range-v1360 ::=					INTEGER(-17..-1)

RSRP-RangeSL-r12 ::=				INTEGER(0..13)

RSRP-RangeSL2-r12 ::=				INTEGER(0..7)

RSRP-RangeSL3-r12 ::=				INTEGER(0..11)

RSRP-RangeSL4-r13 ::=				INTEGER(0..49)


RSRQ-Range ::=						INTEGER(0..34)

RSRQ-Range-v1250 ::=				INTEGER(-30..46)

RSRQ-Range-r13 ::=				INTEGER(-30..46)


RSRQ-Type-r12 ::=					SEQUENCE {
	allSymbols-r12							BOOLEAN,
	wideBand-r12							BOOLEAN
}


RS-SINR-Range-r13 ::=						INTEGER(0..127)


RSSI-Range-r13 ::=						INTEGER(0..76)


TimeToTrigger ::=					ENUMERATED {
										ms0, ms40, ms64, ms80, ms100, ms128, ms160, ms256,
										ms320, ms480, ms512, ms640, ms1024, ms1280, ms2560,
										ms5120}


UL-DelayConfig-r13 ::=					CHOICE {
		release								NULL,
		setup								SEQUENCE {
			delayThreshold-r13							ENUMERATED {
												ms30, ms40, ms50, ms60, ms70, ms80,
												ms90,ms100, ms150, ms300, ms500, ms750, spare4,												spare3, spare2, spare1}
		}
}


WLAN-CarrierInfo-r13 ::=		SEQUENCE {
	operatingClass-r13		INTEGER (0..255)			OPTIONAL,	-- Need ON
	countryCode-r13			ENUMERATED {unitedStates, europe, japan, global, ...}	OPTIONAL,	-- Need ON
	channelNumbers-r13		WLAN-ChannelList-r13		OPTIONAL,	-- Need ON
	...
}

WLAN-ChannelList-r13 ::=	SEQUENCE (SIZE (1..maxWLAN-Channels-r13)) OF WLAN-Channel-r13

WLAN-Channel-r13 ::=	INTEGER(0..255)


WLAN-RSSI-Range-r13 ::=						INTEGER(0..141)


WLAN-Status-r13 ::=		ENUMERATED {successfulAssociation, failureWlanRadioLink, failureWlanUnavailable, failureTimeout}

WLAN-Status-v1430 ::=	ENUMERATED {suspended, resumed}


WLAN-SuspendConfig-r14 ::=	SEQUENCE {
	wlan-SuspendResumeAllowed-r14			BOOLEAN		OPTIONAL,	-- Need ON
	wlan-SuspendTriggersStatusReport-r14		BOOLEAN		OPTIONAL	-- Need ON
}


AbsoluteTimeInfo-r10 ::=				BIT STRING (SIZE (48))


AreaConfiguration-r10 ::=	CHOICE {
	cellGlobalIdList-r10			CellGlobalIdList-r10,
	trackingAreaCodeList-r10		TrackingAreaCodeList-r10
}

AreaConfiguration-v1130 ::=		SEQUENCE {
	trackingAreaCodeList-v1130		TrackingAreaCodeList-v1130
}

CellGlobalIdList-r10 ::=				SEQUENCE (SIZE (1..32)) OF CellGlobalIdEUTRA

TrackingAreaCodeList-r10 ::=			SEQUENCE (SIZE (1..8)) OF TrackingAreaCode

TrackingAreaCodeList-v1130 ::=	SEQUENCE {
	plmn-Identity-perTAC-List-r11			SEQUENCE (SIZE (1..8)) OF PLMN-Identity
}


BandCombinationList-r14 ::=	SEQUENCE (SIZE (1..maxBandComb-r13)) OF BandCombination-r14

BandCombination-r14 ::= SEQUENCE (SIZE (1..maxSimultaneousBands-r10)) OF BandIndication-r14

BandIndication-r14 ::=	SEQUENCE {
	bandEUTRA-r14					FreqBandIndicator-r11,
	ca-BandwidthClassDL-r14			CA-BandwidthClass-r10,
	ca-BandwidthClassUL-r14			CA-BandwidthClass-r10			OPTIONAL
}


C-RNTI ::=							BIT STRING (SIZE (16))


DedicatedInfoCDMA2000 ::=				OCTET STRING


DedicatedInfoNAS ::=		OCTET STRING


FilterCoefficient ::=					ENUMERATED {
											fc0, fc1, fc2, fc3, fc4, fc5,
											fc6, fc7, fc8, fc9, fc11, fc13,
											fc15, fc17, fc19, spare1, ...}


LoggingDuration-r10 ::=			ENUMERATED {
									min10, min20, min40, min60, min90, min120, spare2, spare1}


LoggingInterval-r10 ::=			ENUMERATED {
									ms1280, ms2560, ms5120, ms10240, ms20480,
									ms30720, ms40960, ms61440}


MeasSubframePattern-r10 ::= CHOICE {
	subframePatternFDD-r10				BIT STRING (SIZE (40)),
	subframePatternTDD-r10				CHOICE {
		subframeConfig1-5-r10					BIT STRING (SIZE (20)),
		subframeConfig0-r10						BIT STRING (SIZE (70)),
		subframeConfig6-r10						BIT STRING (SIZE (60)),
		...
	},
	...
}


MMEC ::=							BIT STRING (SIZE (8))


NeighCellConfig ::=			BIT STRING (SIZE (2))


OtherConfig-r9 ::= SEQUENCE	{
	reportProximityConfig-r9			ReportProximityConfig-r9		OPTIONAL,	-- Need ON
	...,
	[[	idc-Config-r11					IDC-Config-r11					OPTIONAL,	-- Need ON
		powerPrefIndicationConfig-r11	PowerPrefIndicationConfig-r11	OPTIONAL,	-- Need ON
		obtainLocationConfig-r11		ObtainLocationConfig-r11		OPTIONAL	-- Need ON
	]],
	[[	bw-PreferenceIndicationTimer-r14		ENUMERATED {s0, s0dot5, s1, s2, s5, s10, s20,
											s30, s60, s90, s120, s300, s600, spare3,
											spare2, spare1}			OPTIONAL,	-- Need OR
		sps-AssistanceInfoReport-r14		BOOLEAN			OPTIONAL,	-- Need ON
		delayBudgetReportingConfig-r14	CHOICE{
			release					NULL,
			setup					SEQUENCE{
				delayBudgetReportingProhibitTimer-r14	ENUMERATED {
																s0, s0dot4, s0dot8,
																s1dot6, s3, s6, s12, s30}
			}
		}																OPTIONAL,	-- Need ON
		rlm-ReportConfig-r14			CHOICE {
			release					NULL,
			setup					SEQUENCE{
				rlmReportTimer-r14				ENUMERATED {s0, s0dot5, s1, s2, s5, s10, s20, s30,
												s60, s90, s120, s300, s600, spare3, spare2, spare1},
				rlmReportRep-MPDCCH-r14			ENUMERATED {setup}		OPTIONAL	-- Need OR
			}
		}	OPTIONAL	-- Need ON
	]],
	[[	overheatingAssistanceConfig-r14	CHOICE{
			release					NULL,
			setup					SEQUENCE{
				overheatingIndicationProhibitTimer-r14	ENUMERATED {s0, s0dot5, s1, s2, s5, s10,
														s20, s30, s60, s90, s120, s300, s600,
														spare3, spare2, spare1}
			}
		}	OPTIONAL		-- Need ON
	]]
}

IDC-Config-r11 ::=				SEQUENCE {
	idc-Indication-r11					ENUMERATED {setup}				OPTIONAL,	-- Need OR
	autonomousDenialParameters-r11		SEQUENCE {
			autonomousDenialSubframes-r11			ENUMERATED {n2, n5, n10, n15,
														n20, n30, spare2, spare1},
			autonomousDenialValidity-r11			ENUMERATED {
														sf200, sf500, sf1000, sf2000,
														spare4, spare3, spare2, spare1}
	}		OPTIONAL,		-- Need OR
	...,
	[[	idc-Indication-UL-CA-r11			ENUMERATED {setup}		OPTIONAL	-- Cond idc-Ind
	]],
	[[	idc-HardwareSharingIndication-r13	ENUMERATED {setup}		OPTIONAL	-- Need OR
	]]
}

ObtainLocationConfig-r11 ::= SEQUENCE {
	obtainLocation-r11				ENUMERATED {setup}					OPTIONAL	-- Need OR
}

PowerPrefIndicationConfig-r11 ::= CHOICE{
	release					NULL,
	setup					SEQUENCE{
		powerPrefIndicationTimer-r11		ENUMERATED {s0, s0dot5, s1, s2, s5, s10, s20,
											s30, s60, s90, s120, s300, s600, spare3,
											spare2, spare1}
	}
}

ReportProximityConfig-r9 ::= SEQUENCE {
	proximityIndicationEUTRA-r9		ENUMERATED {enabled}			OPTIONAL,	-- Need OR
	proximityIndicationUTRA-r9		ENUMERATED {enabled}			OPTIONAL	-- Need OR
}


RAND-CDMA2000 ::=						BIT STRING (SIZE (32))


RAT-Type ::=						ENUMERATED {
										eutra, utra, geran-cs, geran-ps, cdma2000-1XRTT,
										spare3, spare2, spare1, ...}


ResumeIdentity-r13 ::=						BIT STRING (SIZE(40))


RRC-TransactionIdentifier ::=		INTEGER (0..3)


S-TMSI ::=							SEQUENCE {
	mmec								MMEC,
	m-TMSI								BIT STRING (SIZE (32))
}


TraceReference-r10 ::=			SEQUENCE {
	plmn-Identity-r10				PLMN-Identity,
	traceId-r10						OCTET STRING (SIZE (3))
}


UE-CapabilityRAT-ContainerList ::=SEQUENCE (SIZE (0..maxRAT-Capabilities)) OF UE-CapabilityRAT-Container

UE-CapabilityRAT-Container ::= SEQUENCE {
	rat-Type							RAT-Type,
	ueCapabilityRAT-Container			OCTET STRING
}


UE-EUTRA-Capability ::=			SEQUENCE {
	accessStratumRelease				AccessStratumRelease,
	ue-Category							INTEGER (1..5),
	pdcp-Parameters						PDCP-Parameters,
	phyLayerParameters					PhyLayerParameters,
	rf-Parameters						RF-Parameters,
	measParameters						MeasParameters,
	featureGroupIndicators				BIT STRING (SIZE (32))				OPTIONAL,
	interRAT-Parameters				SEQUENCE {
		utraFDD								IRAT-ParametersUTRA-FDD				OPTIONAL,
		utraTDD128							IRAT-ParametersUTRA-TDD128				OPTIONAL,
		utraTDD384							IRAT-ParametersUTRA-TDD384				OPTIONAL,
		utraTDD768							IRAT-ParametersUTRA-TDD768				OPTIONAL,
		geran								IRAT-ParametersGERAN					OPTIONAL,
		cdma2000-HRPD						IRAT-ParametersCDMA2000-HRPD			OPTIONAL,
		cdma2000-1xRTT						IRAT-ParametersCDMA2000-1XRTT			OPTIONAL
	},
	nonCriticalExtension				UE-EUTRA-Capability-v920-IEs		OPTIONAL
}

-- Late non critical extensions
UE-EUTRA-Capability-v9a0-IEs ::=	SEQUENCE {
	featureGroupIndRel9Add-r9			BIT STRING (SIZE (32))				OPTIONAL,
	fdd-Add-UE-EUTRA-Capabilities-r9	UE-EUTRA-CapabilityAddXDD-Mode-r9	OPTIONAL,
	tdd-Add-UE-EUTRA-Capabilities-r9	UE-EUTRA-CapabilityAddXDD-Mode-r9	OPTIONAL,
	nonCriticalExtension				UE-EUTRA-Capability-v9c0-IEs		OPTIONAL
}

UE-EUTRA-Capability-v9c0-IEs ::=		SEQUENCE {
	interRAT-ParametersUTRA-v9c0		IRAT-ParametersUTRA-v9c0		OPTIONAL,
	nonCriticalExtension				UE-EUTRA-Capability-v9d0-IEs	OPTIONAL
}

UE-EUTRA-Capability-v9d0-IEs ::=		SEQUENCE {
	phyLayerParameters-v9d0				PhyLayerParameters-v9d0			OPTIONAL,
	nonCriticalExtension				UE-EUTRA-Capability-v9e0-IEs	OPTIONAL
}

UE-EUTRA-Capability-v9e0-IEs ::=	SEQUENCE {
	rf-Parameters-v9e0					RF-Parameters-v9e0						OPTIONAL,
	nonCriticalExtension				UE-EUTRA-Capability-v9h0-IEs			OPTIONAL
}

UE-EUTRA-Capability-v9h0-IEs ::=	SEQUENCE {
	interRAT-ParametersUTRA-v9h0		IRAT-ParametersUTRA-v9h0			OPTIONAL,
	-- Following field is only to be used for late REL-9 extensions
	lateNonCriticalExtension			OCTET STRING							OPTIONAL,
	nonCriticalExtension				UE-EUTRA-Capability-v10c0-IEs			OPTIONAL
}

UE-EUTRA-Capability-v10c0-IEs ::=	SEQUENCE {
	otdoa-PositioningCapabilities-r10	OTDOA-PositioningCapabilities-r10		OPTIONAL,
	nonCriticalExtension				UE-EUTRA-Capability-v10f0-IEs			OPTIONAL
}

UE-EUTRA-Capability-v10f0-IEs ::=	SEQUENCE {
	rf-Parameters-v10f0					RF-Parameters-v10f0						OPTIONAL,
	nonCriticalExtension				UE-EUTRA-Capability-v10i0-IEs			OPTIONAL
}

UE-EUTRA-Capability-v10i0-IEs ::=	SEQUENCE {
	rf-Parameters-v10i0					RF-Parameters-v10i0						OPTIONAL,
	-- Following field is only to be used for late REL-10 extensions
	lateNonCriticalExtension			OCTET STRING (CONTAINING UE-EUTRA-Capability-v10j0-IEs)	OPTIONAL,
	nonCriticalExtension				UE-EUTRA-Capability-v11d0-IEs			OPTIONAL
}

UE-EUTRA-Capability-v10j0-IEs ::=	SEQUENCE {
	rf-Parameters-v10j0					RF-Parameters-v10j0						OPTIONAL,
	nonCriticalExtension				SEQUENCE {}								OPTIONAL
}

UE-EUTRA-Capability-v11d0-IEs ::=	SEQUENCE {
	rf-Parameters-v11d0					RF-Parameters-v11d0						OPTIONAL,
	otherParameters-v11d0				Other-Parameters-v11d0					OPTIONAL,
	nonCriticalExtension				UE-EUTRA-Capability-v11x0-IEs			OPTIONAL
}

UE-EUTRA-Capability-v11x0-IEs ::=	SEQUENCE {
	-- Following field is only to be used for late REL-11 extensions
	lateNonCriticalExtension			OCTET STRING								OPTIONAL,
	nonCriticalExtension				UE-EUTRA-Capability-v12b0-IEs				OPTIONAL
}

UE-EUTRA-Capability-v12b0-IEs ::= SEQUENCE {
	rf-Parameters-v12b0					RF-Parameters-v12b0						OPTIONAL,
	nonCriticalExtension				UE-EUTRA-Capability-v12x0-IEs			OPTIONAL
}

UE-EUTRA-Capability-v12x0-IEs ::= SEQUENCE {
	-- Following field is only to be used for late REL-12 extensions
	lateNonCriticalExtension			OCTET STRING							OPTIONAL,
	nonCriticalExtension				UE-EUTRA-Capability-v1370-IEs			OPTIONAL
}

UE-EUTRA-Capability-v1370-IEs ::= SEQUENCE {
	ce-Parameters-v1370					CE-Parameters-v1370						OPTIONAL,
	fdd-Add-UE-EUTRA-Capabilities-v1370	UE-EUTRA-CapabilityAddXDD-Mode-v1370	OPTIONAL,
	tdd-Add-UE-EUTRA-Capabilities-v1370	UE-EUTRA-CapabilityAddXDD-Mode-v1370	OPTIONAL,
	nonCriticalExtension				UE-EUTRA-Capability-v1380-IEs			OPTIONAL
}

UE-EUTRA-Capability-v1380-IEs ::= SEQUENCE {
	rf-Parameters-v1380					RF-Parameters-v1380						OPTIONAL,
	ce-Parameters-v1380					CE-Parameters-v1380,
	fdd-Add-UE-EUTRA-Capabilities-v1380	UE-EUTRA-CapabilityAddXDD-Mode-v1380,
	tdd-Add-UE-EUTRA-Capabilities-v1380	UE-EUTRA-CapabilityAddXDD-Mode-v1380,
	nonCriticalExtension				UE-EUTRA-Capability-v1390-IEs			OPTIONAL
}

UE-EUTRA-Capability-v1390-IEs ::= SEQUENCE {
	rf-Parameters-v1390					RF-Parameters-v1390						OPTIONAL,
	nonCriticalExtension				UE-EUTRA-Capability-v13x0-IEs 	OPTIONAL
}

UE-EUTRA-Capability-v13x0-IEs ::= SEQUENCE {
	-- Following field is only to be used for late REL-13 extensions
	lateNonCriticalExtension			OCTET STRING							OPTIONAL,
	nonCriticalExtension				UE-EUTRA-Capability-v1470-IEs		OPTIONAL
}

UE-EUTRA-Capability-v1470-IEs ::= SEQUENCE {
	mbms-Parameters-v1470				MBMS-Parameters-v1470			OPTIONAL,
	phyLayerParameters-v1470				PhyLayerParameters-v1470			OPTIONAL,
	rf-Parameters-v1470					RF-Parameters-v1470				OPTIONAL,
	-- Following field is only to be used for late REL-14 extensions
	nonCriticalExtension					SEQUENCE {}								OPTIONAL
}

-- Regular non critical extensions
UE-EUTRA-Capability-v920-IEs ::=		SEQUENCE {
	phyLayerParameters-v920					PhyLayerParameters-v920,
	interRAT-ParametersGERAN-v920			IRAT-ParametersGERAN-v920,
	interRAT-ParametersUTRA-v920			IRAT-ParametersUTRA-v920			OPTIONAL,
	interRAT-ParametersCDMA2000-v920		IRAT-ParametersCDMA2000-1XRTT-v920	OPTIONAL,
	deviceType-r9							ENUMERATED {noBenFromBatConsumpOpt}	OPTIONAL,
	csg-ProximityIndicationParameters-r9	CSG-ProximityIndicationParameters-r9,
	neighCellSI-AcquisitionParameters-r9	NeighCellSI-AcquisitionParameters-r9,
	son-Parameters-r9						SON-Parameters-r9,
	nonCriticalExtension					UE-EUTRA-Capability-v940-IEs		OPTIONAL
}

UE-EUTRA-Capability-v940-IEs ::=	SEQUENCE {
	lateNonCriticalExtension			OCTET STRING (CONTAINING UE-EUTRA-Capability-v9a0-IEs)
																			OPTIONAL,
	nonCriticalExtension				UE-EUTRA-Capability-v1020-IEs		OPTIONAL
}

UE-EUTRA-Capability-v1020-IEs ::=	SEQUENCE {
	ue-Category-v1020					INTEGER (6..8)							OPTIONAL,
	phyLayerParameters-v1020			PhyLayerParameters-v1020				OPTIONAL,
	rf-Parameters-v1020					RF-Parameters-v1020						OPTIONAL,
	measParameters-v1020				MeasParameters-v1020					OPTIONAL,
	featureGroupIndRel10-r10			BIT STRING (SIZE (32))					OPTIONAL,
	interRAT-ParametersCDMA2000-v1020	IRAT-ParametersCDMA2000-1XRTT-v1020		OPTIONAL,
	ue-BasedNetwPerfMeasParameters-r10	UE-BasedNetwPerfMeasParameters-r10		OPTIONAL,
	interRAT-ParametersUTRA-TDD-v1020	IRAT-ParametersUTRA-TDD-v1020			OPTIONAL,
	nonCriticalExtension				UE-EUTRA-Capability-v1060-IEs			OPTIONAL
}

UE-EUTRA-Capability-v1060-IEs ::=	SEQUENCE {
	fdd-Add-UE-EUTRA-Capabilities-v1060	UE-EUTRA-CapabilityAddXDD-Mode-v1060	OPTIONAL,
	tdd-Add-UE-EUTRA-Capabilities-v1060	UE-EUTRA-CapabilityAddXDD-Mode-v1060	OPTIONAL,
	rf-Parameters-v1060					RF-Parameters-v1060						OPTIONAL,
	nonCriticalExtension				UE-EUTRA-Capability-v1090-IEs			OPTIONAL
}

UE-EUTRA-Capability-v1090-IEs ::=	SEQUENCE {
	rf-Parameters-v1090					RF-Parameters-v1090						OPTIONAL,
	nonCriticalExtension				UE-EUTRA-Capability-v1130-IEs			OPTIONAL
}

UE-EUTRA-Capability-v1130-IEs ::=	SEQUENCE {
	pdcp-Parameters-v1130				PDCP-Parameters-v1130,
	phyLayerParameters-v1130			PhyLayerParameters-v1130				OPTIONAL,
	rf-Parameters-v1130					RF-Parameters-v1130,
	measParameters-v1130				MeasParameters-v1130,
	interRAT-ParametersCDMA2000-v1130	IRAT-ParametersCDMA2000-v1130,
	otherParameters-r11					Other-Parameters-r11,
	fdd-Add-UE-EUTRA-Capabilities-v1130	UE-EUTRA-CapabilityAddXDD-Mode-v1130	OPTIONAL,
	tdd-Add-UE-EUTRA-Capabilities-v1130	UE-EUTRA-CapabilityAddXDD-Mode-v1130	OPTIONAL,
	nonCriticalExtension				UE-EUTRA-Capability-v1170-IEs			OPTIONAL
}

UE-EUTRA-Capability-v1170-IEs ::=	SEQUENCE {
	phyLayerParameters-v1170			PhyLayerParameters-v1170				OPTIONAL,
	ue-Category-v1170					INTEGER (9..10)							OPTIONAL,
	nonCriticalExtension				UE-EUTRA-Capability-v1180-IEs			OPTIONAL
}

UE-EUTRA-Capability-v1180-IEs ::=	SEQUENCE {
	rf-Parameters-v1180					RF-Parameters-v1180						OPTIONAL,
	mbms-Parameters-r11					MBMS-Parameters-r11						OPTIONAL,
	fdd-Add-UE-EUTRA-Capabilities-v1180	UE-EUTRA-CapabilityAddXDD-Mode-v1180	OPTIONAL,
	tdd-Add-UE-EUTRA-Capabilities-v1180	UE-EUTRA-CapabilityAddXDD-Mode-v1180	OPTIONAL,
	nonCriticalExtension				UE-EUTRA-Capability-v11a0-IEs			OPTIONAL
}

UE-EUTRA-Capability-v11a0-IEs ::=	SEQUENCE {
	ue-Category-v11a0					INTEGER (11..12)						OPTIONAL,
	measParameters-v11a0				MeasParameters-v11a0					OPTIONAL,
	nonCriticalExtension				UE-EUTRA-Capability-v1250-IEs			OPTIONAL
}

UE-EUTRA-Capability-v1250-IEs ::=	SEQUENCE {
	phyLayerParameters-v1250			PhyLayerParameters-v1250				OPTIONAL,
	rf-Parameters-v1250					RF-Parameters-v1250						OPTIONAL,
	rlc-Parameters-r12					RLC-Parameters-r12						OPTIONAL,
	ue-BasedNetwPerfMeasParameters-v1250	UE-BasedNetwPerfMeasParameters-v1250	OPTIONAL,
	ue-CategoryDL-r12					INTEGER (0..14)							OPTIONAL,
	ue-CategoryUL-r12					INTEGER (0..13)							OPTIONAL,
	wlan-IW-Parameters-r12				WLAN-IW-Parameters-r12					OPTIONAL,
	measParameters-v1250				MeasParameters-v1250					OPTIONAL,
	dc-Parameters-r12					DC-Parameters-r12						OPTIONAL,
	mbms-Parameters-v1250				MBMS-Parameters-v1250					OPTIONAL,
	mac-Parameters-r12					MAC-Parameters-r12						OPTIONAL,
	fdd-Add-UE-EUTRA-Capabilities-v1250	UE-EUTRA-CapabilityAddXDD-Mode-v1250	OPTIONAL,
	tdd-Add-UE-EUTRA-Capabilities-v1250	UE-EUTRA-CapabilityAddXDD-Mode-v1250	OPTIONAL,
	sl-Parameters-r12				SL-Parameters-r12							OPTIONAL,
	nonCriticalExtension				UE-EUTRA-Capability-v1260-IEs			OPTIONAL
}

UE-EUTRA-Capability-v1260-IEs ::=	SEQUENCE {
	ue-CategoryDL-v1260					INTEGER (15..16)						OPTIONAL,
	nonCriticalExtension				UE-EUTRA-Capability-v1270-IEs			OPTIONAL
}

UE-EUTRA-Capability-v1270-IEs ::= SEQUENCE {
	rf-Parameters-v1270					RF-Parameters-v1270						OPTIONAL,
	nonCriticalExtension				UE-EUTRA-Capability-v1280-IEs			OPTIONAL
}

UE-EUTRA-Capability-v1280-IEs ::= SEQUENCE {
	phyLayerParameters-v1280			PhyLayerParameters-v1280				OPTIONAL,
	nonCriticalExtension				UE-EUTRA-Capability-v1310-IEs			OPTIONAL
}

UE-EUTRA-Capability-v1310-IEs ::= SEQUENCE {
	ue-CategoryDL-v1310				ENUMERATED {n17, m1}					OPTIONAL,
	ue-CategoryUL-v1310				ENUMERATED {n14, m1}					OPTIONAL,
	pdcp-Parameters-v1310				PDCP-Parameters-v1310,
	rlc-Parameters-v1310				RLC-Parameters-v1310,
	mac-Parameters-v1310				MAC-Parameters-v1310					OPTIONAL,
	phyLayerParameters-v1310			PhyLayerParameters-v1310				OPTIONAL,
	rf-Parameters-v1310					RF-Parameters-v1310						OPTIONAL,
	measParameters-v1310				MeasParameters-v1310					OPTIONAL,
	dc-Parameters-v1310					DC-Parameters-v1310						OPTIONAL,
	sl-Parameters-v1310					SL-Parameters-v1310						OPTIONAL,
	scptm-Parameters-r13				SCPTM-Parameters-r13					OPTIONAL,
	ce-Parameters-r13					CE-Parameters-r13						OPTIONAL,
	interRAT-ParametersWLAN-r13			IRAT-ParametersWLAN-r13,
	laa-Parameters-r13					LAA-Parameters-r13						OPTIONAL,
	lwa-Parameters-r13					LWA-Parameters-r13						OPTIONAL,
	wlan-IW-Parameters-v1310				WLAN-IW-Parameters-v1310,
	lwip-Parameters-r13					LWIP-Parameters-r13,
	fdd-Add-UE-EUTRA-Capabilities-v1310	UE-EUTRA-CapabilityAddXDD-Mode-v1310	OPTIONAL,
	tdd-Add-UE-EUTRA-Capabilities-v1310	UE-EUTRA-CapabilityAddXDD-Mode-v1310	OPTIONAL,
	nonCriticalExtension				UE-EUTRA-Capability-v1320-IEs			OPTIONAL
}

UE-EUTRA-Capability-v1320-IEs ::= SEQUENCE {
	ce-Parameters-v1320					CE-Parameters-v1320						OPTIONAL,
	phyLayerParameters-v1320			PhyLayerParameters-v1320				OPTIONAL,
	rf-Parameters-v1320					RF-Parameters-v1320						OPTIONAL,
	fdd-Add-UE-EUTRA-Capabilities-v1320	UE-EUTRA-CapabilityAddXDD-Mode-v1320	OPTIONAL,
	tdd-Add-UE-EUTRA-Capabilities-v1320	UE-EUTRA-CapabilityAddXDD-Mode-v1320	OPTIONAL,
	nonCriticalExtension				UE-EUTRA-Capability-v1330-IEs			OPTIONAL
}

UE-EUTRA-Capability-v1330-IEs ::= SEQUENCE {
	ue-CategoryDL-v1330					INTEGER (18..19)						OPTIONAL,
	phyLayerParameters-v1330			PhyLayerParameters-v1330				OPTIONAL,
	ue-CE-NeedULGaps-r13				ENUMERATED {true}						OPTIONAL,
	nonCriticalExtension				UE-EUTRA-Capability-v1340-IEs			OPTIONAL
}

UE-EUTRA-Capability-v1340-IEs ::= SEQUENCE {
	ue-CategoryUL-v1340				INTEGER (15)								OPTIONAL,
	nonCriticalExtension				UE-EUTRA-Capability-v1350-IEs			OPTIONAL
}

UE-EUTRA-Capability-v1350-IEs ::= SEQUENCE {
	ue-CategoryDL-v1350				ENUMERATED {oneBis}						OPTIONAL,
	ue-CategoryUL-v1350				ENUMERATED {oneBis}					OPTIONAL,
	ce-Parameters-v1350				CE-Parameters-v1350,
	nonCriticalExtension			UE-EUTRA-Capability-v1360-IEs			OPTIONAL
}

UE-EUTRA-Capability-v1360-IEs ::= SEQUENCE {
	other-Parameters-v1360		Other-Parameters-v1360					OPTIONAL,
	nonCriticalExtension		UE-EUTRA-Capability-v1430-IEs			OPTIONAL
}

UE-EUTRA-Capability-v1430-IEs ::= SEQUENCE {
	phyLayerParameters-v1430				PhyLayerParameters-v1430,
	ue-CategoryDL-v1430						ENUMERATED {m2}							OPTIONAL,
	ue-CategoryUL-v1430						ENUMERATED {n16, n17, n18, n19, n20, m2}	OPTIONAL,
	ue-CategoryUL-v1430b					ENUMERATED {n21}						OPTIONAL,
	mac-Parameters-v1430					MAC-Parameters-v1430					OPTIONAL,
	measParameters-v1430					MeasParameters-v1430					OPTIONAL,
	pdcp-Parameters-v1430					PDCP-Parameters-v1430					OPTIONAL,
	rlc-Parameters-v1430					RLC-Parameters-v1430,
	rf-Parameters-v1430						RF-Parameters-v1430						OPTIONAL,
	laa-Parameters-v1430					LAA-Parameters-v1430					OPTIONAL,
	lwa-Parameters-v1430					LWA-Parameters-v1430					OPTIONAL,
	lwip-Parameters-v1430					LWIP-Parameters-v1430					OPTIONAL,
	otherParameters-v1430					Other-Parameters-v1430,
	mmtel-Parameters-r14					MMTEL-Parameters-r14					OPTIONAL,
	mobilityParameters-r14					MobilityParameters-r14					OPTIONAL,
	ce-Parameters-v1430						CE-Parameters-v1430,
	fdd-Add-UE-EUTRA-Capabilities-v1430		UE-EUTRA-CapabilityAddXDD-Mode-v1430	OPTIONAL,
	tdd-Add-UE-EUTRA-Capabilities-v1430		UE-EUTRA-CapabilityAddXDD-Mode-v1430	OPTIONAL,
	mbms-Parameters-v1430					MBMS-Parameters-v1430					OPTIONAL,
	sl-Parameters-v1430						SL-Parameters-v1430						OPTIONAL,
	ue-BasedNetwPerfMeasParameters-v1430	UE-BasedNetwPerfMeasParameters-v1430	OPTIONAL,
	highSpeedEnhParameters-r14				HighSpeedEnhParameters-r14				OPTIONAL,
	nonCriticalExtension					UE-EUTRA-Capability-v1440-IEs			OPTIONAL
}

UE-EUTRA-Capability-v1440-IEs ::= SEQUENCE {
	lwa-Parameters-v1440				LWA-Parameters-v1440,
	mac-Parameters-v1440				MAC-Parameters-v1440,
	nonCriticalExtension				UE-EUTRA-Capability-v1450-IEs			OPTIONAL
}

UE-EUTRA-Capability-v1450-IEs ::= SEQUENCE {
	phyLayerParameters-v1450			PhyLayerParameters-v1450			OPTIONAL,
	rf-Parameters-v1450					RF-Parameters-v1450					OPTIONAL,
	otherParameters-v1450				OtherParameters-v1450,
	ue-CategoryDL-v1450					INTEGER (20)						OPTIONAL,
	nonCriticalExtension				UE-EUTRA-Capability-v1460-IEs		OPTIONAL
}

UE-EUTRA-Capability-v1460-IEs ::= SEQUENCE {
	ue-CategoryDL-v1460				INTEGER (21)						OPTIONAL,
	otherParameters-v1460			Other-Parameters-v1460,
	nonCriticalExtension			SEQUENCE {}							OPTIONAL
}

UE-EUTRA-CapabilityAddXDD-Mode-r9 ::=	SEQUENCE {
	phyLayerParameters-r9					PhyLayerParameters						OPTIONAL,
	featureGroupIndicators-r9				BIT STRING (SIZE (32))					OPTIONAL,
	featureGroupIndRel9Add-r9				BIT STRING (SIZE (32))					OPTIONAL,
	interRAT-ParametersGERAN-r9				IRAT-ParametersGERAN					OPTIONAL,
	interRAT-ParametersUTRA-r9				IRAT-ParametersUTRA-v920				OPTIONAL,
	interRAT-ParametersCDMA2000-r9			IRAT-ParametersCDMA2000-1XRTT-v920		OPTIONAL,
	neighCellSI-AcquisitionParameters-r9	NeighCellSI-AcquisitionParameters-r9	OPTIONAL,
	...
}

UE-EUTRA-CapabilityAddXDD-Mode-v1060 ::=	SEQUENCE {
	phyLayerParameters-v1060			PhyLayerParameters-v1020			OPTIONAL,
	featureGroupIndRel10-v1060			BIT STRING (SIZE (32))				OPTIONAL,
	interRAT-ParametersCDMA2000-v1060	IRAT-ParametersCDMA2000-1XRTT-v1020	OPTIONAL,
	interRAT-ParametersUTRA-TDD-v1060	IRAT-ParametersUTRA-TDD-v1020		OPTIONAL,
	...,
	[[	otdoa-PositioningCapabilities-r10	OTDOA-PositioningCapabilities-r10	OPTIONAL
	]]
}

UE-EUTRA-CapabilityAddXDD-Mode-v1130 ::=	SEQUENCE {
	phyLayerParameters-v1130			PhyLayerParameters-v1130			OPTIONAL,
	measParameters-v1130				MeasParameters-v1130				OPTIONAL,
	otherParameters-r11					Other-Parameters-r11				OPTIONAL,
	...
}

UE-EUTRA-CapabilityAddXDD-Mode-v1180 ::=	SEQUENCE {
	mbms-Parameters-r11					MBMS-Parameters-r11
}

UE-EUTRA-CapabilityAddXDD-Mode-v1250 ::=	SEQUENCE {
	phyLayerParameters-v1250			PhyLayerParameters-v1250			OPTIONAL,
	measParameters-v1250				MeasParameters-v1250				OPTIONAL
}

UE-EUTRA-CapabilityAddXDD-Mode-v1310 ::=	SEQUENCE {
	phyLayerParameters-v1310			PhyLayerParameters-v1310			OPTIONAL
}

UE-EUTRA-CapabilityAddXDD-Mode-v1320 ::=	SEQUENCE {
	phyLayerParameters-v1320			PhyLayerParameters-v1320			OPTIONAL,
	scptm-Parameters-r13				SCPTM-Parameters-r13				OPTIONAL
}

UE-EUTRA-CapabilityAddXDD-Mode-v1370 ::=	SEQUENCE {
	ce-Parameters-v1370					CE-Parameters-v1370					OPTIONAL
}

UE-EUTRA-CapabilityAddXDD-Mode-v1380 ::=	SEQUENCE {
	ce-Parameters-v1380					CE-Parameters-v1380
}

UE-EUTRA-CapabilityAddXDD-Mode-v1430 ::=	SEQUENCE {
	phyLayerParameters-v1430			PhyLayerParameters-v1430			OPTIONAL,
	mmtel-Parameters-r14				MMTEL-Parameters-r14				OPTIONAL
}

AccessStratumRelease ::=			ENUMERATED {
										rel8, rel9, rel10, rel11, rel12, rel13,
										rel14, spare1, ...}

MobilityParameters-r14 ::=			SEQUENCE {
	makeBeforeBreak-r14					ENUMERATED {supported}					OPTIONAL,
	rach-Less-r14						ENUMERATED {supported}					OPTIONAL
}

DC-Parameters-r12 ::=			SEQUENCE {
	drb-TypeSplit-r12						ENUMERATED {supported}			OPTIONAL,
	drb-TypeSCG-r12							ENUMERATED {supported}			OPTIONAL
}

DC-Parameters-v1310 ::=			SEQUENCE {
	pdcp-TransferSplitUL-r13				ENUMERATED {supported}			OPTIONAL,
	ue-SSTD-Meas-r13						ENUMERATED {supported}			OPTIONAL
}

MAC-Parameters-r12 ::=				SEQUENCE {
	logicalChannelSR-ProhibitTimer-r12	ENUMERATED {supported}				OPTIONAL,
	longDRX-Command-r12				ENUMERATED {supported}					OPTIONAL
}

MAC-Parameters-v1310 ::=				SEQUENCE {
	extendedMAC-LengthField-r13		ENUMERATED {supported}				OPTIONAL,
	extendedLongDRX-r13				ENUMERATED {supported}				OPTIONAL
}

MAC-Parameters-v1430 ::=				SEQUENCE {
	shortSPS-IntervalFDD-r14			ENUMERATED {supported}				OPTIONAL,
	shortSPS-IntervalTDD-r14			ENUMERATED {supported}				OPTIONAL,
	skipUplinkDynamic-r14				ENUMERATED {supported}				OPTIONAL,
	skipUplinkSPS-r14					ENUMERATED {supported}				OPTIONAL,
	multipleUplinkSPS-r14				ENUMERATED {supported}				OPTIONAL,
	dataInactMon-r14					ENUMERATED {supported}				OPTIONAL
}

MAC-Parameters-v1440 ::=				SEQUENCE {
	rai-Support-r14					ENUMERATED {supported}			OPTIONAL
}

RLC-Parameters-r12 ::=				SEQUENCE {
	extended-RLC-LI-Field-r12			ENUMERATED {supported}
}

RLC-Parameters-v1310 ::=				SEQUENCE {
	extendedRLC-SN-SO-Field-r13				ENUMERATED {supported}			OPTIONAL
}

RLC-Parameters-v1430 ::=				SEQUENCE {
	extendedPollByte-r14						ENUMERATED {supported}			OPTIONAL
}

PDCP-Parameters ::=				SEQUENCE {
	supportedROHC-Profiles				SEQUENCE {
		profile0x0001						BOOLEAN,
		profile0x0002						BOOLEAN,
		profile0x0003						BOOLEAN,
		profile0x0004						BOOLEAN,
		profile0x0006						BOOLEAN,
		profile0x0101						BOOLEAN,
		profile0x0102						BOOLEAN,
		profile0x0103						BOOLEAN,
		profile0x0104						BOOLEAN
	},
	maxNumberROHC-ContextSessions		ENUMERATED {
											cs2, cs4, cs8, cs12, cs16, cs24, cs32,
											cs48, cs64, cs128, cs256, cs512, cs1024,
											cs16384, spare2, spare1}				DEFAULT cs16,
	...
}

PDCP-Parameters-v1130 ::=		SEQUENCE {
	pdcp-SN-Extension-r11					ENUMERATED {supported}			OPTIONAL,
	supportRohcContextContinue-r11			ENUMERATED {supported}			OPTIONAL
}

PDCP-Parameters-v1310 ::=				SEQUENCE {
	pdcp-SN-Extension-18bits-r13			ENUMERATED {supported}	OPTIONAL
}

PDCP-Parameters-v1430 ::=				SEQUENCE {
	supportedUplinkOnlyROHC-Profiles-r14		SEQUENCE {
		profile0x0006-r14						BOOLEAN
	},
	maxNumberROHC-ContextSessions-r14		ENUMERATED {
											cs2, cs4, cs8, cs12, cs16, cs24, cs32,
											cs48, cs64, cs128, cs256, cs512, cs1024,
											cs16384, spare2, spare1}				DEFAULT cs16
}

PhyLayerParameters ::=				SEQUENCE {
	ue-TxAntennaSelectionSupported		BOOLEAN,
	ue-SpecificRefSigsSupported		BOOLEAN
}

PhyLayerParameters-v920 ::=		SEQUENCE {
	enhancedDualLayerFDD-r9			ENUMERATED {supported}			OPTIONAL,
	enhancedDualLayerTDD-r9			ENUMERATED {supported}			OPTIONAL
}

PhyLayerParameters-v9d0 ::=			SEQUENCE {
	tm5-FDD-r9						ENUMERATED {supported}			OPTIONAL,
	tm5-TDD-r9						ENUMERATED {supported}			OPTIONAL
}

PhyLayerParameters-v1020 ::=			SEQUENCE {
	twoAntennaPortsForPUCCH-r10				ENUMERATED {supported}					OPTIONAL,
	tm9-With-8Tx-FDD-r10					ENUMERATED {supported}					OPTIONAL,
	pmi-Disabling-r10						ENUMERATED {supported}					OPTIONAL,
	crossCarrierScheduling-r10				ENUMERATED {supported}					OPTIONAL,
	simultaneousPUCCH-PUSCH-r10				ENUMERATED {supported}					OPTIONAL,
	multiClusterPUSCH-WithinCC-r10			ENUMERATED {supported}					OPTIONAL,
	nonContiguousUL-RA-WithinCC-List-r10	NonContiguousUL-RA-WithinCC-List-r10	OPTIONAL
}

PhyLayerParameters-v1130 ::=			SEQUENCE {
	crs-InterfHandl-r11						ENUMERATED {supported}					OPTIONAL,
	ePDCCH-r11								ENUMERATED {supported}					OPTIONAL,
	multiACK-CSI-Reporting-r11				ENUMERATED {supported}					OPTIONAL,
	ss-CCH-InterfHandl-r11					ENUMERATED {supported}					OPTIONAL,
	tdd-SpecialSubframe-r11					ENUMERATED {supported}					OPTIONAL,
	txDiv-PUCCH1b-ChSelect-r11				ENUMERATED {supported}					OPTIONAL,
	ul-CoMP-r11								ENUMERATED {supported}					OPTIONAL
}

PhyLayerParameters-v1170 ::=			SEQUENCE {
	interBandTDD-CA-WithDifferentConfig-r11	BIT STRING (SIZE (2))			OPTIONAL
}

PhyLayerParameters-v1250 ::=			SEQUENCE {
	e-HARQ-Pattern-FDD-r12					ENUMERATED {supported}			OPTIONAL,
	enhanced-4TxCodebook-r12				ENUMERATED {supported}			OPTIONAL,
	tdd-FDD-CA-PCellDuplex-r12				BIT STRING (SIZE (2))			OPTIONAL,
	phy-TDD-ReConfig-TDD-PCell-r12			ENUMERATED {supported}			OPTIONAL,
	phy-TDD-ReConfig-FDD-PCell-r12			ENUMERATED {supported}			OPTIONAL,
	pusch-FeedbackMode-r12					ENUMERATED {supported}			OPTIONAL,
	pusch-SRS-PowerControl-SubframeSet-r12	ENUMERATED {supported}			OPTIONAL,
	csi-SubframeSet-r12						ENUMERATED {supported}			OPTIONAL,
	noResourceRestrictionForTTIBundling-r12	ENUMERATED {supported}			OPTIONAL,
	discoverySignalsInDeactSCell-r12		ENUMERATED {supported}			OPTIONAL,
	naics-Capability-List-r12				NAICS-Capability-List-r12		OPTIONAL
}

PhyLayerParameters-v1280 ::=			SEQUENCE {
	alternativeTBS-Indices-r12				ENUMERATED {supported}			OPTIONAL
}

PhyLayerParameters-v1310 ::=			SEQUENCE {
	aperiodicCSI-Reporting-r13				BIT STRING (SIZE (2))			OPTIONAL,
	codebook-HARQ-ACK-r13					BIT STRING (SIZE (2))			OPTIONAL,
	crossCarrierScheduling-B5C-r13			ENUMERATED {supported}			OPTIONAL,
	fdd-HARQ-TimingTDD-r13					ENUMERATED {supported}			OPTIONAL,
	maxNumberUpdatedCSI-Proc-r13			INTEGER(5..32)					OPTIONAL,
	pucch-Format4-r13						ENUMERATED {supported}			OPTIONAL,
	pucch-Format5-r13						ENUMERATED {supported}			OPTIONAL,
	pucch-SCell-r13							ENUMERATED {supported}			OPTIONAL,
	spatialBundling-HARQ-ACK-r13			ENUMERATED {supported}			OPTIONAL,
	supportedBlindDecoding-r13				SEQUENCE {
		maxNumberDecoding-r13					INTEGER(1..32)					OPTIONAL,
		pdcch-CandidateReductions-r13			ENUMERATED {supported}			OPTIONAL,
		skipMonitoringDCI-Format0-1A-r13		ENUMERATED {supported}			OPTIONAL
	}																		OPTIONAL,
	uci-PUSCH-Ext-r13						ENUMERATED {supported}			OPTIONAL,
	crs-InterfMitigationTM10-r13			ENUMERATED {supported}			OPTIONAL,
	pdsch-CollisionHandling-r13				ENUMERATED {supported}			OPTIONAL
}

PhyLayerParameters-v1320 ::=			SEQUENCE {
	mimo-UE-Parameters-r13					MIMO-UE-Parameters-r13			OPTIONAL
}

PhyLayerParameters-v1330 ::=			SEQUENCE {
	cch-InterfMitigation-RefRecTypeA-r13	ENUMERATED {supported}			OPTIONAL,
	cch-InterfMitigation-RefRecTypeB-r13	ENUMERATED {supported}			OPTIONAL,
	cch-InterfMitigation-MaxNumCCs-r13		INTEGER (1.. maxServCell-r13)	OPTIONAL,
	crs-InterfMitigationTM1toTM9-r13		INTEGER (1.. maxServCell-r13)	OPTIONAL
}

PhyLayerParameters-v1430 ::=			SEQUENCE {
	ce-PUSCH-NB-MaxTBS-r14					ENUMERATED {supported}			OPTIONAL,
	ce-PDSCH-PUSCH-MaxBandwidth-r14			ENUMERATED {bw5, bw20}			OPTIONAL,
	ce-HARQ-AckBundling-r14					ENUMERATED {supported}			OPTIONAL,
	ce-PDSCH-TenProcesses-r14				ENUMERATED {supported}			OPTIONAL,
	ce-RetuningSymbols-r14					ENUMERATED {n0, n1}				OPTIONAL,
	ce-PDSCH-PUSCH-Enhancement-r14			ENUMERATED {supported}			OPTIONAL,
	ce-SchedulingEnhancement-r14			ENUMERATED {supported}			OPTIONAL,
	ce-SRS-Enhancement-r14					ENUMERATED {supported}			OPTIONAL,
	ce-PUCCH-Enhancement-r14				ENUMERATED {supported}			OPTIONAL,
	ce-ClosedLoopTxAntennaSelection-r14		ENUMERATED {supported}			OPTIONAL,
	tdd-SpecialSubframe-r14					ENUMERATED {supported}			OPTIONAL,
	tdd-TTI-Bundling-r14					ENUMERATED {supported}			OPTIONAL,
	dmrs-LessUpPTS-r14						ENUMERATED {supported}			OPTIONAL,
	mimo-UE-Parameters-v1430				MIMO-UE-Parameters-v1430		OPTIONAL,
	alternativeTBS-Index-r14				ENUMERATED {supported}			OPTIONAL,
	feMBMS-Unicast-Parameters-r14			FeMBMS-Unicast-Parameters-r14	OPTIONAL
}

PhyLayerParameters-v1450 ::=			SEQUENCE {
	ce-SRS-EnhancementWithoutComb4-r14		ENUMERATED {supported}			OPTIONAL,
	crs-LessDwPTS-r14						ENUMERATED {supported}			OPTIONAL
}

PhyLayerParameters-v1470 ::=			SEQUENCE {
	mimo-UE-Parameters-v1470				MIMO-UE-Parameters-v1470			OPTIONAL,
	srs-UpPTS-6sym-r14					ENUMERATED {supported}			OPTIONAL
}

MIMO-UE-Parameters-r13 ::=				SEQUENCE {
	parametersTM9-r13						MIMO-UE-ParametersPerTM-r13		OPTIONAL,
	parametersTM10-r13						MIMO-UE-ParametersPerTM-r13		OPTIONAL,
	srs-EnhancementsTDD-r13					ENUMERATED {supported}			OPTIONAL,
	srs-Enhancements-r13					ENUMERATED {supported}			OPTIONAL,
	interferenceMeasRestriction-r13			ENUMERATED {supported}			OPTIONAL
}

MIMO-UE-Parameters-v1430 ::=			SEQUENCE {
	parametersTM9-v1430						MIMO-UE-ParametersPerTM-v1430	OPTIONAL,
	parametersTM10-v1430					MIMO-UE-ParametersPerTM-v1430	OPTIONAL
}

MIMO-UE-Parameters-v1470 ::=			SEQUENCE {
	parametersTM9-v1470					MIMO-UE-ParametersPerTM-v1470,
	parametersTM10-v1470					MIMO-UE-ParametersPerTM-v1470
}

MIMO-UE-ParametersPerTM-r13 ::=			SEQUENCE {
	nonPrecoded-r13							MIMO-NonPrecodedCapabilities-r13	OPTIONAL,
	beamformed-r13							MIMO-UE-BeamformedCapabilities-r13	OPTIONAL,
	channelMeasRestriction-r13				ENUMERATED {supported}				OPTIONAL,
	dmrs-Enhancements-r13					ENUMERATED {supported}				OPTIONAL,
	csi-RS-EnhancementsTDD-r13				ENUMERATED {supported}				OPTIONAL
}

MIMO-UE-ParametersPerTM-v1430 ::=		SEQUENCE {
	nzp-CSI-RS-AperiodicInfo-r14			SEQUENCE {
		nMaxProc-r14							INTEGER(5..32),
		nMaxResource-r14						ENUMERATED {ffs1, ffs2, ffs3, ffs4}
	}																			OPTIONAL,
	nzp-CSI-RS-PeriodicInfo-r14				SEQUENCE {
		nMaxResource-r14						ENUMERATED {ffs1, ffs2, ffs3, ffs4}
	}																			OPTIONAL,
	zp-CSI-RS-AperiodicInfo-r14					ENUMERATED {supported}			OPTIONAL,
	ul-dmrs-Enhancements-r14				ENUMERATED {supported}				OPTIONAL,
	densityReductionNP-r14					ENUMERATED {supported}				OPTIONAL,
	densityReductionBF-r14					ENUMERATED {supported}				OPTIONAL,
	hybridCSI-r14							ENUMERATED {supported}				OPTIONAL,
	semiOL-r14								ENUMERATED {supported}				OPTIONAL,
	csi-ReportingNP-r14						ENUMERATED {supported}				OPTIONAL,
	csi-ReportingAdvanced-r14				ENUMERATED {supported}				OPTIONAL
}

MIMO-UE-ParametersPerTM-v1470 ::=		SEQUENCE {
	csi-ReportingAdvancedMaxPorts-r14		ENUMERATED {n8, n12, n16, n20, n24, n28}	OPTIONAL
}

MIMO-CA-ParametersPerBoBC-r13 ::=		SEQUENCE {
	parametersTM9-r13						MIMO-CA-ParametersPerBoBCPerTM-r13		OPTIONAL,
	parametersTM10-r13						MIMO-CA-ParametersPerBoBCPerTM-r13		OPTIONAL
}

MIMO-CA-ParametersPerBoBC-v1430 ::=		SEQUENCE {
	parametersTM9-v1430						MIMO-CA-ParametersPerBoBCPerTM-v1430	OPTIONAL,
	parametersTM10-v1430					MIMO-CA-ParametersPerBoBCPerTM-v1430	OPTIONAL
}

MIMO-CA-ParametersPerBoBC-v1470 ::=		SEQUENCE {
	parametersTM9-v1470						MIMO-CA-ParametersPerBoBCPerTM-v1470	,
	parametersTM10-v1470						MIMO-CA-ParametersPerBoBCPerTM-v1470
}

MIMO-CA-ParametersPerBoBCPerTM-r13 ::=	SEQUENCE {
	nonPrecoded-r13							MIMO-NonPrecodedCapabilities-r13	OPTIONAL,
	beamformed-r13							MIMO-BeamformedCapabilityList-r13	OPTIONAL,
	dmrs-Enhancements-r13					ENUMERATED {different}				OPTIONAL
}

MIMO-CA-ParametersPerBoBCPerTM-v1430 ::=	SEQUENCE {
	csi-ReportingNP-r14						ENUMERATED {different}				OPTIONAL,
	csi-ReportingAdvanced-r14				ENUMERATED {different}				OPTIONAL
}

MIMO-CA-ParametersPerBoBCPerTM-v1470 ::=	SEQUENCE {
	csi-ReportingAdvancedMaxPorts-r14		ENUMERATED {n8, n12, n16, n20, n24, n28}	OPTIONAL
}

MIMO-NonPrecodedCapabilities-r13 ::=	SEQUENCE {
	config1-r13								ENUMERATED {supported}			OPTIONAL,
	config2-r13								ENUMERATED {supported}			OPTIONAL,
	config3-r13								ENUMERATED {supported}			OPTIONAL,
	config4-r13								ENUMERATED {supported}			OPTIONAL
}

MIMO-UE-BeamformedCapabilities-r13 ::=		SEQUENCE {
	altCodebook-r13							ENUMERATED {supported}			OPTIONAL,
	mimo-BeamformedCapabilities-r13			MIMO-BeamformedCapabilityList-r13
}

MIMO-BeamformedCapabilityList-r13 ::=		SEQUENCE (SIZE (1..maxCSI-Proc-r11)) OF MIMO-BeamformedCapabilities-r13

MIMO-BeamformedCapabilities-r13 ::=		SEQUENCE {
	k-Max-r13								INTEGER (1..8),
	n-MaxList-r13							BIT STRING (SIZE (1..7))		OPTIONAL
 }

NonContiguousUL-RA-WithinCC-List-r10 ::= SEQUENCE (SIZE (1..maxBands)) OF NonContiguousUL-RA-WithinCC-r10

NonContiguousUL-RA-WithinCC-r10 ::=		SEQUENCE {
	nonContiguousUL-RA-WithinCC-Info-r10	ENUMERATED {supported}					OPTIONAL
}

RF-Parameters ::=					SEQUENCE {
	supportedBandListEUTRA				SupportedBandListEUTRA
}

RF-Parameters-v9e0 ::=					SEQUENCE {
	supportedBandListEUTRA-v9e0				SupportedBandListEUTRA-v9e0				OPTIONAL
}

RF-Parameters-v1020 ::=				SEQUENCE {
	supportedBandCombination-r10			SupportedBandCombination-r10
}

RF-Parameters-v1060 ::=				SEQUENCE {
	supportedBandCombinationExt-r10			SupportedBandCombinationExt-r10
}

RF-Parameters-v1090 ::=					SEQUENCE {
	supportedBandCombination-v1090			SupportedBandCombination-v1090			OPTIONAL
}

RF-Parameters-v10f0 ::=					SEQUENCE {
	modifiedMPR-Behavior-r10					BIT STRING (SIZE (32))				OPTIONAL
}

RF-Parameters-v10i0 ::=					SEQUENCE {
	supportedBandCombination-v10i0			SupportedBandCombination-v10i0			OPTIONAL
}

RF-Parameters-v10j0 ::=					SEQUENCE {
	multiNS-Pmax-r10						ENUMERATED {supported}					OPTIONAL
}

RF-Parameters-v1130 ::=				SEQUENCE {
	supportedBandCombination-v1130			SupportedBandCombination-v1130			OPTIONAL
}

RF-Parameters-v1180 ::=				SEQUENCE {
	freqBandRetrieval-r11					ENUMERATED {supported}			OPTIONAL,
	requestedBands-r11						SEQUENCE (SIZE (1.. maxBands)) OF FreqBandIndicator-r11						OPTIONAL,
	supportedBandCombinationAdd-r11			SupportedBandCombinationAdd-r11		OPTIONAL
}

RF-Parameters-v11d0 ::=					SEQUENCE {
	supportedBandCombinationAdd-v11d0		SupportedBandCombinationAdd-v11d0		OPTIONAL
}

RF-Parameters-v1250 ::=				SEQUENCE {
	supportedBandListEUTRA-v1250				SupportedBandListEUTRA-v1250			OPTIONAL,
	supportedBandCombination-v1250			SupportedBandCombination-v1250			OPTIONAL,
	supportedBandCombinationAdd-v1250		SupportedBandCombinationAdd-v1250		OPTIONAL,
	freqBandPriorityAdjustment-r12			ENUMERATED {supported}					OPTIONAL
}

RF-Parameters-v1270 ::=				SEQUENCE {
	supportedBandCombination-v1270			SupportedBandCombination-v1270			OPTIONAL,
	supportedBandCombinationAdd-v1270		SupportedBandCombinationAdd-v1270		OPTIONAL
}

RF-Parameters-v1310 ::=				SEQUENCE {
	eNB-RequestedParameters-r13			SEQUENCE {
		reducedIntNonContCombRequested-r13	ENUMERATED {true}						OPTIONAL,
		requestedCCsDL-r13					INTEGER (2..32)							OPTIONAL,
		requestedCCsUL-r13					INTEGER (2..32)							OPTIONAL,
		skipFallbackCombRequested-r13		ENUMERATED {true}						OPTIONAL
	}																				OPTIONAL,
	maximumCCsRetrieval-r13					ENUMERATED {supported}					OPTIONAL,
	skipFallbackCombinations-r13			ENUMERATED {supported}					OPTIONAL,
	reducedIntNonContComb-r13				ENUMERATED {supported}					OPTIONAL,
	supportedBandListEUTRA-v1310			SupportedBandListEUTRA-v1310			OPTIONAL,
	supportedBandCombinationReduced-r13		SupportedBandCombinationReduced-r13		OPTIONAL
}

RF-Parameters-v1320 ::=				SEQUENCE {
	supportedBandListEUTRA-v1320			SupportedBandListEUTRA-v1320			OPTIONAL,
	supportedBandCombination-v1320			SupportedBandCombination-v1320			OPTIONAL,
	supportedBandCombinationAdd-v1320		SupportedBandCombinationAdd-v1320		OPTIONAL,
	supportedBandCombinationReduced-v1320	SupportedBandCombinationReduced-v1320	OPTIONAL
}

RF-Parameters-v1380 ::=				SEQUENCE {
	supportedBandCombination-v1380			SupportedBandCombination-v1380			OPTIONAL,
	supportedBandCombinationAdd-v1380		SupportedBandCombinationAdd-v1380		OPTIONAL,
	supportedBandCombinationReduced-v1380	SupportedBandCombinationReduced-v1380	OPTIONAL
}

RF-Parameters-v1390 ::=				SEQUENCE {
	supportedBandCombination-v1390			SupportedBandCombination-v1390			OPTIONAL,
	supportedBandCombinationAdd-v1390		SupportedBandCombinationAdd-v1390		OPTIONAL,
	supportedBandCombinationReduced-v1390	SupportedBandCombinationReduced-v1390	OPTIONAL
}

RF-Parameters-v12b0 ::=				SEQUENCE {
	maxLayersMIMO-Indication-r12			ENUMERATED {supported}					OPTIONAL
}

RF-Parameters-v1430 ::=				SEQUENCE {
	supportedBandCombination-v1430			SupportedBandCombination-v1430			OPTIONAL,
	supportedBandCombinationAdd-v1430		SupportedBandCombinationAdd-v1430		OPTIONAL,
	supportedBandCombinationReduced-v1430	SupportedBandCombinationReduced-v1430	OPTIONAL,
	eNB-RequestedParameters-v1430			SEQUENCE {
		requestedDiffFallbackCombList-r14		BandCombinationList-r14
	}																				OPTIONAL,
	diffFallbackCombReport-r14				ENUMERATED {supported}					OPTIONAL
}

RF-Parameters-v1450 ::=				SEQUENCE {
	supportedBandCombination-v1450			SupportedBandCombination-v1450			OPTIONAL,
	supportedBandCombinationAdd-v1450		SupportedBandCombinationAdd-v1450		OPTIONAL,
	supportedBandCombinationReduced-v1450	SupportedBandCombinationReduced-v1450	OPTIONAL
}

RF-Parameters-v1470 ::=				SEQUENCE {
	supportedBandCombination-v1470			SupportedBandCombination-v1470			OPTIONAL,
	supportedBandCombinationAdd-v1470		SupportedBandCombinationAdd-v1470		OPTIONAL,
	supportedBandCombinationReduced-v1470	SupportedBandCombinationReduced-v1470	OPTIONAL
}

SupportedBandCombination-r10 ::= SEQUENCE (SIZE (1..maxBandComb-r10)) OF BandCombinationParameters-r10

SupportedBandCombinationExt-r10 ::= SEQUENCE (SIZE (1..maxBandComb-r10)) OF BandCombinationParametersExt-r10

SupportedBandCombination-v1090 ::= SEQUENCE (SIZE (1..maxBandComb-r10)) OF BandCombinationParameters-v1090

SupportedBandCombination-v10i0 ::= SEQUENCE (SIZE (1..maxBandComb-r10)) OF BandCombinationParameters-v10i0

SupportedBandCombination-v1130 ::= SEQUENCE (SIZE (1..maxBandComb-r10)) OF BandCombinationParameters-v1130

SupportedBandCombination-v1250 ::= SEQUENCE (SIZE (1..maxBandComb-r10)) OF BandCombinationParameters-v1250

SupportedBandCombination-v1270 ::= SEQUENCE (SIZE (1..maxBandComb-r10)) OF BandCombinationParameters-v1270

SupportedBandCombination-v1320 ::= SEQUENCE (SIZE (1..maxBandComb-r10)) OF BandCombinationParameters-v1320

SupportedBandCombination-v1380 ::= SEQUENCE (SIZE (1..maxBandComb-r10)) OF BandCombinationParameters-v1380

SupportedBandCombination-v1390 ::= SEQUENCE (SIZE (1..maxBandComb-r10)) OF BandCombinationParameters-v1390

SupportedBandCombination-v1430 ::= SEQUENCE (SIZE (1..maxBandComb-r10)) OF BandCombinationParameters-v1430

SupportedBandCombination-v1450 ::= SEQUENCE (SIZE (1..maxBandComb-r10)) OF BandCombinationParameters-v1450

SupportedBandCombination-v1470 ::= SEQUENCE (SIZE (1..maxBandComb-r10)) OF BandCombinationParameters-v1470

SupportedBandCombinationAdd-r11 ::= SEQUENCE (SIZE (1..maxBandComb-r11)) OF BandCombinationParameters-r11

SupportedBandCombinationAdd-v11d0 ::= SEQUENCE (SIZE (1..maxBandComb-r11)) OF BandCombinationParameters-v10i0

SupportedBandCombinationAdd-v1250 ::= SEQUENCE (SIZE (1..maxBandComb-r11)) OF BandCombinationParameters-v1250

SupportedBandCombinationAdd-v1270 ::= SEQUENCE (SIZE (1..maxBandComb-r11)) OF BandCombinationParameters-v1270

SupportedBandCombinationAdd-v1320 ::= SEQUENCE (SIZE (1..maxBandComb-r11)) OF BandCombinationParameters-v1320

SupportedBandCombinationAdd-v1380 ::= SEQUENCE (SIZE (1..maxBandComb-r11)) OF BandCombinationParameters-v1380

SupportedBandCombinationAdd-v1390 ::= SEQUENCE (SIZE (1..maxBandComb-r11)) OF BandCombinationParameters-v1390

SupportedBandCombinationAdd-v1430 ::= SEQUENCE (SIZE (1..maxBandComb-r11)) OF BandCombinationParameters-v1430

SupportedBandCombinationAdd-v1450 ::= SEQUENCE (SIZE (1..maxBandComb-r11)) OF BandCombinationParameters-v1450

SupportedBandCombinationAdd-v1470 ::= SEQUENCE (SIZE (1..maxBandComb-r11)) OF BandCombinationParameters-v1470

SupportedBandCombinationReduced-r13 ::=	SEQUENCE (SIZE (1..maxBandComb-r13)) OF BandCombinationParameters-r13

SupportedBandCombinationReduced-v1320 ::=	SEQUENCE (SIZE (1..maxBandComb-r13)) OF BandCombinationParameters-v1320

SupportedBandCombinationReduced-v1380 ::=	SEQUENCE (SIZE (1..maxBandComb-r13)) OF BandCombinationParameters-v1380

SupportedBandCombinationReduced-v1390 ::=	SEQUENCE (SIZE (1..maxBandComb-r13)) OF BandCombinationParameters-v1390

SupportedBandCombinationReduced-v1430 ::=	SEQUENCE (SIZE (1..maxBandComb-r13)) OF BandCombinationParameters-v1430

SupportedBandCombinationReduced-v1450 ::=	SEQUENCE (SIZE (1..maxBandComb-r13)) OF BandCombinationParameters-v1450

SupportedBandCombinationReduced-v1470 ::=	SEQUENCE (SIZE (1..maxBandComb-r13)) OF BandCombinationParameters-v1470

BandCombinationParameters-r10 ::= SEQUENCE (SIZE (1..maxSimultaneousBands-r10)) OF BandParameters-r10

BandCombinationParametersExt-r10 ::= SEQUENCE {
	supportedBandwidthCombinationSet-r10	SupportedBandwidthCombinationSet-r10	OPTIONAL
}

BandCombinationParameters-v1090 ::= SEQUENCE (SIZE (1..maxSimultaneousBands-r10)) OF BandParameters-v1090

BandCombinationParameters-v10i0::= SEQUENCE {
	bandParameterList-v10i0			SEQUENCE (SIZE (1..maxSimultaneousBands-r10)) OF
			BandParameters-v10i0	OPTIONAL
}

BandCombinationParameters-v1130 ::=	SEQUENCE {
	multipleTimingAdvance-r11		ENUMERATED {supported}					OPTIONAL,
	simultaneousRx-Tx-r11			ENUMERATED {supported}					OPTIONAL,
	bandParameterList-r11			SEQUENCE (SIZE (1..maxSimultaneousBands-r10)) OF BandParameters-v1130	OPTIONAL,
	...
}

BandCombinationParameters-r11 ::=	SEQUENCE {
	bandParameterList-r11			SEQUENCE (SIZE (1..maxSimultaneousBands-r10)) OF
			BandParameters-r11,
	supportedBandwidthCombinationSet-r11	SupportedBandwidthCombinationSet-r10	OPTIONAL,
	multipleTimingAdvance-r11		ENUMERATED {supported}					OPTIONAL,
	simultaneousRx-Tx-r11			ENUMERATED {supported}					OPTIONAL,
	bandInfoEUTRA-r11				BandInfoEUTRA,
	...
}

BandCombinationParameters-v1250::= SEQUENCE {
	dc-Support-r12					SEQUENCE {
		asynchronous-r12				ENUMERATED {supported}			OPTIONAL,
		supportedCellGrouping-r12		CHOICE {
				threeEntries-r12				BIT STRING (SIZE(3)),
				fourEntries-r12					BIT STRING (SIZE(7)),
				fiveEntries-r12					BIT STRING (SIZE(15))
		}																OPTIONAL
	}																	OPTIONAL,
	supportedNAICS-2CRS-AP-r12		BIT STRING (SIZE (1..maxNAICS-Entries-r12))		OPTIONAL,
	commSupportedBandsPerBC-r12				BIT STRING (SIZE (1.. maxBands))		OPTIONAL,
	...
}

BandCombinationParameters-v1270 ::= SEQUENCE {
	bandParameterList-v1270			SEQUENCE (SIZE (1..maxSimultaneousBands-r10)) OF
			BandParameters-v1270		OPTIONAL
}

BandCombinationParameters-r13 ::=	SEQUENCE {
	differentFallbackSupported-r13	ENUMERATED {true}				OPTIONAL,
	bandParameterList-r13			SEQUENCE (SIZE (1..maxSimultaneousBands-r10)) OF BandParameters-r13,
	supportedBandwidthCombinationSet-r13	SupportedBandwidthCombinationSet-r10	OPTIONAL,
	multipleTimingAdvance-r13		ENUMERATED {supported}				OPTIONAL,
	simultaneousRx-Tx-r13			ENUMERATED {supported}				OPTIONAL,
	bandInfoEUTRA-r13				BandInfoEUTRA,
	dc-Support-r13					SEQUENCE {
		asynchronous-r13			ENUMERATED {supported}				OPTIONAL,
		supportedCellGrouping-r13		CHOICE {
				threeEntries-r13				BIT STRING (SIZE(3)),
				fourEntries-r13					BIT STRING (SIZE(7)),
				fiveEntries-r13					BIT STRING (SIZE(15))
		}																OPTIONAL
	}																	OPTIONAL,
	supportedNAICS-2CRS-AP-r13		BIT STRING (SIZE (1..maxNAICS-Entries-r12))	OPTIONAL,
	commSupportedBandsPerBC-r13		BIT STRING (SIZE (1.. maxBands))		OPTIONAL
}

BandCombinationParameters-v1320 ::= SEQUENCE {
	bandParameterList-v1320			SEQUENCE (SIZE (1..maxSimultaneousBands-r10)) OF
			BandParameters-v1320		OPTIONAL,
	additionalRx-Tx-PerformanceReq-r13		ENUMERATED {supported}					OPTIONAL
}

BandCombinationParameters-v1380 ::= SEQUENCE {
	bandParameterList-v1380		SEQUENCE (SIZE (1..maxSimultaneousBands-r10)) OF
			BandParameters-v1380		OPTIONAL
}

BandCombinationParameters-v1390 ::= SEQUENCE {
	ue-CA-PowerClass-N-r13			ENUMERATED {class2}				OPTIONAL
}

BandCombinationParameters-v1430 ::= SEQUENCE {
	bandParameterList-v1430			SEQUENCE (SIZE (1..maxSimultaneousBands-r10)) OF
			BandParameters-v1430		OPTIONAL,
	v2x-SupportedTxBandCombListPerBC-r14			BIT STRING (SIZE (1.. maxBandComb-r13))		OPTIONAL,
	v2x-SupportedRxBandCombListPerBC-r14			BIT STRING (SIZE (1.. maxBandComb-r13))		OPTIONAL
}

BandCombinationParameters-v1450 ::= SEQUENCE {
	bandParameterList-v1450			SEQUENCE (SIZE (1..maxSimultaneousBands-r10)) OF
			BandParameters-v1450		OPTIONAL
}

BandCombinationParameters-v1470 ::= SEQUENCE {
	bandParameterList-v1470			SEQUENCE (SIZE (1..maxSimultaneousBands-r10)) OF
			BandParameters-v1470		OPTIONAL,
	srs-MaxSimultaneousCCs-r14	INTEGER (1..31)				OPTIONAL
}

SupportedBandwidthCombinationSet-r10 ::=	BIT STRING (SIZE (1..maxBandwidthCombSet-r10))

BandParameters-r10 ::= SEQUENCE {
	bandEUTRA-r10					FreqBandIndicator,
	bandParametersUL-r10			BandParametersUL-r10					OPTIONAL,
	bandParametersDL-r10			BandParametersDL-r10					OPTIONAL
}

BandParameters-v1090 ::= SEQUENCE {
	bandEUTRA-v1090					FreqBandIndicator-v9e0					OPTIONAL,
	...
}

BandParameters-v10i0::= SEQUENCE {
	bandParametersDL-v10i0		SEQUENCE (SIZE (1..maxBandwidthClass-r10)) OF CA-MIMO-ParametersDL-v10i0
}

BandParameters-v1130 ::= SEQUENCE {
	supportedCSI-Proc-r11			ENUMERATED {n1, n3, n4}
}

BandParameters-r11 ::= SEQUENCE {
	bandEUTRA-r11					FreqBandIndicator-r11,
	bandParametersUL-r11			BandParametersUL-r10					OPTIONAL,
	bandParametersDL-r11			BandParametersDL-r10					OPTIONAL,
	supportedCSI-Proc-r11			ENUMERATED {n1, n3, n4}					OPTIONAL
}

BandParameters-v1270 ::= SEQUENCE {
	bandParametersDL-v1270			SEQUENCE (SIZE (1..maxBandwidthClass-r10)) OF CA-MIMO-ParametersDL-v1270
}

BandParameters-r13 ::= SEQUENCE {
	bandEUTRA-r13					FreqBandIndicator-r11,
	bandParametersUL-r13				BandParametersUL-r13				OPTIONAL,
	bandParametersDL-r13				BandParametersDL-r13				OPTIONAL,
	supportedCSI-Proc-r13			ENUMERATED {n1, n3, n4}			OPTIONAL
}

BandParameters-v1320 ::= SEQUENCE {
	bandParametersDL-v1320			MIMO-CA-ParametersPerBoBC-r13
}

BandParameters-v1380 ::=	SEQUENCE {
	txAntennaSwitchDL-r13			INTEGER (1..32)					OPTIONAL,
	txAntennaSwitchUL-r13			INTEGER (1..32)					OPTIONAL
}

BandParameters-v1430 ::= SEQUENCE {
	bandParametersDL-v1430			MIMO-CA-ParametersPerBoBC-v1430	OPTIONAL,
	ul-256QAM-r14						ENUMERATED {supported}		OPTIONAL,
	ul-256QAM-perCC-InfoList-r14		SEQUENCE (SIZE (2..maxServCell-r13)) OF UL-256QAM-perCC-Info-r14		OPTIONAL,
	retuningTimeInfoBandList-r14		SEQUENCE (SIZE (1..maxSimultaneousBands-r10)) OF
			RetuningTimeInfo-r14	OPTIONAL
}

BandParameters-v1450 ::= SEQUENCE {
	must-CapabilityPerBand-r14		MUST-Parameters-r14		OPTIONAL
}

BandParameters-v1470 ::= SEQUENCE {
	bandParametersDL-v1470			MIMO-CA-ParametersPerBoBC-v1470	OPTIONAL
}

V2X-BandParameters-r14 ::= SEQUENCE {
	v2x-FreqBandEUTRA-r14			FreqBandIndicator-r11,
	bandParametersTxSL-r14			BandParametersTxSL-r14				OPTIONAL,
	bandParametersRxSL-r14			BandParametersRxSL-r14				OPTIONAL
}

BandParametersTxSL-r14 ::= SEQUENCE {
	v2x-BandwidthClassTxSL-r14		V2X-BandwidthClassSL-r14,
	v2x-eNB-Scheduled-r14			ENUMERATED {supported}				OPTIONAL,
	v2x-HighPower-r14				ENUMERATED {supported}				OPTIONAL
}

BandParametersRxSL-r14 ::= SEQUENCE {
	v2x-BandwidthClassRxSL-r14		V2X-BandwidthClassSL-r14,
	v2x-HighReception-r14			ENUMERATED {supported}				OPTIONAL
}

V2X-BandwidthClassSL-r14 ::= SEQUENCE (SIZE (1..maxBandwidthClass-r10)) OF V2X-BandwidthClass-r14

UL-256QAM-perCC-Info-r14 ::= SEQUENCE {
	ul-256QAM-perCC-r14			ENUMERATED {supported}				OPTIONAL
}

BandParametersUL-r10 ::= SEQUENCE (SIZE (1..maxBandwidthClass-r10)) OF CA-MIMO-ParametersUL-r10

BandParametersUL-r13 ::= CA-MIMO-ParametersUL-r10

CA-MIMO-ParametersUL-r10 ::= SEQUENCE {
	ca-BandwidthClassUL-r10				CA-BandwidthClass-r10,
	supportedMIMO-CapabilityUL-r10		MIMO-CapabilityUL-r10				OPTIONAL
}

BandParametersDL-r10 ::= SEQUENCE (SIZE (1..maxBandwidthClass-r10)) OF CA-MIMO-ParametersDL-r10

BandParametersDL-r13 ::= CA-MIMO-ParametersDL-r13

CA-MIMO-ParametersDL-r10 ::= SEQUENCE {
	ca-BandwidthClassDL-r10				CA-BandwidthClass-r10,
	supportedMIMO-CapabilityDL-r10		MIMO-CapabilityDL-r10				OPTIONAL
}

CA-MIMO-ParametersDL-v10i0 ::= SEQUENCE {
	fourLayerTM3-TM4-r10				ENUMERATED {supported}				OPTIONAL
}

CA-MIMO-ParametersDL-v1270 ::= SEQUENCE {
	intraBandContiguousCC-InfoList-r12			SEQUENCE (SIZE (1..maxServCell-r10)) OF IntraBandContiguousCC-Info-r12
}

CA-MIMO-ParametersDL-r13 ::= SEQUENCE {
	ca-BandwidthClassDL-r13					CA-BandwidthClass-r10,
	supportedMIMO-CapabilityDL-r13			MIMO-CapabilityDL-r10				OPTIONAL,
	fourLayerTM3-TM4-r13						ENUMERATED {supported}				OPTIONAL,
	intraBandContiguousCC-InfoList-r13		SEQUENCE (SIZE (1..maxServCell-r13)) OF IntraBandContiguousCC-Info-r12
}

IntraBandContiguousCC-Info-r12 ::= SEQUENCE {
	fourLayerTM3-TM4-perCC-r12			ENUMERATED {supported}				OPTIONAL,
	supportedMIMO-CapabilityDL-r12		MIMO-CapabilityDL-r10				OPTIONAL,
	supportedCSI-Proc-r12				ENUMERATED {n1, n3, n4}				OPTIONAL
}

CA-BandwidthClass-r10 ::= ENUMERATED {a, b, c, d, e, f, ...}

V2X-BandwidthClass-r14 ::= ENUMERATED {a, b, c, d, e, f, ...}

MIMO-CapabilityUL-r10 ::= ENUMERATED {twoLayers, fourLayers}

MIMO-CapabilityDL-r10 ::= ENUMERATED {twoLayers, fourLayers, eightLayers}

MUST-Parameters-r14 ::= SEQUENCE {
	must-TM234-UpTo2Tx-r14						ENUMERATED {supported}		OPTIONAL,
	must-TM89-UpToOneInterferingLayer-r14		ENUMERATED {supported}		OPTIONAL,
	must-TM10-UpToOneInterferingLayer-r14		ENUMERATED {supported}		OPTIONAL,
	must-TM89-UpToThreeInterferingLayers-r14	ENUMERATED {supported}		OPTIONAL,
	must-TM10-UpToThreeInterferingLayers-r14	ENUMERATED {supported}		OPTIONAL
}

SupportedBandListEUTRA ::=			SEQUENCE (SIZE (1..maxBands)) OF SupportedBandEUTRA

SupportedBandListEUTRA-v9e0::=			SEQUENCE (SIZE (1..maxBands)) OF SupportedBandEUTRA-v9e0

SupportedBandListEUTRA-v1250 ::=		SEQUENCE (SIZE (1..maxBands)) OF SupportedBandEUTRA-v1250

SupportedBandListEUTRA-v1310 ::=		SEQUENCE (SIZE (1..maxBands)) OF SupportedBandEUTRA-v1310

SupportedBandListEUTRA-v1320 ::=		SEQUENCE (SIZE (1..maxBands)) OF SupportedBandEUTRA-v1320

SupportedBandEUTRA ::=				SEQUENCE {
	bandEUTRA							FreqBandIndicator,
	halfDuplex							BOOLEAN
}

SupportedBandEUTRA-v9e0 ::=		SEQUENCE {
	bandEUTRA-v9e0						FreqBandIndicator-v9e0		OPTIONAL
}

SupportedBandEUTRA-v1250 ::=		SEQUENCE {
	dl-256QAM-r12						ENUMERATED {supported}		OPTIONAL,
	ul-64QAM-r12						ENUMERATED {supported}		OPTIONAL
}

SupportedBandEUTRA-v1310 ::=		SEQUENCE {
	ue-PowerClass-5-r13			ENUMERATED {supported}		OPTIONAL
}
SupportedBandEUTRA-v1320 ::=		SEQUENCE {
	intraFreq-CE-NeedForGaps-r13				ENUMERATED {supported}				OPTIONAL,
	ue-PowerClass-N-r13			ENUMERATED {class1, class2, class4}		OPTIONAL
}

MeasParameters ::=					SEQUENCE {
	bandListEUTRA						BandListEUTRA
}

MeasParameters-v1020 ::=			SEQUENCE {
	bandCombinationListEUTRA-r10			BandCombinationListEUTRA-r10
}

MeasParameters-v1130 ::=			SEQUENCE {
	rsrqMeasWideband-r11			ENUMERATED {supported}					OPTIONAL
}

MeasParameters-v11a0 ::=			SEQUENCE {
	benefitsFromInterruption-r11			ENUMERATED {true}				OPTIONAL
}

MeasParameters-v1250 ::=			SEQUENCE {
	timerT312-r12						ENUMERATED {supported}		OPTIONAL,
	alternativeTimeToTrigger-r12		ENUMERATED {supported}		OPTIONAL,
	incMonEUTRA-r12						ENUMERATED {supported}		OPTIONAL,
	incMonUTRA-r12						ENUMERATED {supported}		OPTIONAL,
	extendedMaxMeasId-r12				ENUMERATED {supported}		OPTIONAL,
	extendedRSRQ-LowerRange-r12			ENUMERATED {supported}		OPTIONAL,
	rsrq-OnAllSymbols-r12				ENUMERATED {supported}		OPTIONAL,
	crs-DiscoverySignalsMeas-r12		ENUMERATED {supported}		OPTIONAL,
	csi-RS-DiscoverySignalsMeas-r12		ENUMERATED {supported}		OPTIONAL
}

MeasParameters-v1310 ::=			SEQUENCE {
	rs-SINR-Meas-r13						ENUMERATED {supported}		OPTIONAL,
	whiteCellList-r13						ENUMERATED {supported}		OPTIONAL,
	extendedMaxObjectId-r13					ENUMERATED {supported}		OPTIONAL,
	ul-PDCP-Delay-r13						ENUMERATED {supported}		OPTIONAL,
	extendedFreqPriorities-r13				ENUMERATED {supported}		OPTIONAL,
	multiBandInfoReport-r13					ENUMERATED {supported}		OPTIONAL,
	rssi-AndChannelOccupancyReporting-r13	ENUMERATED {supported}		OPTIONAL
}

MeasParameters-v1430 ::=			SEQUENCE {
	ceMeasurements-r14						ENUMERATED {supported}		OPTIONAL,
	ncsg-r14								ENUMERATED {supported}				OPTIONAL,
	shortMeasurementGap-r14					ENUMERATED {supported}				OPTIONAL,
	perServingCellMeasurementGap-r14		ENUMERATED {supported}				OPTIONAL,
	nonUniformGap-r14						ENUMERATED {supported}				OPTIONAL
}

BandListEUTRA ::=					SEQUENCE (SIZE (1..maxBands)) OF BandInfoEUTRA

BandCombinationListEUTRA-r10 ::=	SEQUENCE (SIZE (1..maxBandComb-r10)) OF BandInfoEUTRA

BandInfoEUTRA ::=					SEQUENCE {
	interFreqBandList					InterFreqBandList,
	interRAT-BandList					InterRAT-BandList		OPTIONAL
}

InterFreqBandList ::=				SEQUENCE (SIZE (1..maxBands)) OF InterFreqBandInfo

InterFreqBandInfo ::=				SEQUENCE {
	interFreqNeedForGaps				BOOLEAN
}

InterRAT-BandList ::=				SEQUENCE (SIZE (1..maxBands)) OF InterRAT-BandInfo

InterRAT-BandInfo ::=				SEQUENCE {
	interRAT-NeedForGaps				BOOLEAN
}

IRAT-ParametersUTRA-FDD ::=		SEQUENCE {
	supportedBandListUTRA-FDD			SupportedBandListUTRA-FDD
}

IRAT-ParametersUTRA-v920 ::=		SEQUENCE {
	e-RedirectionUTRA-r9				ENUMERATED {supported}
}

IRAT-ParametersUTRA-v9c0 ::=		SEQUENCE {
	voiceOverPS-HS-UTRA-FDD-r9						ENUMERATED {supported}		OPTIONAL,
	voiceOverPS-HS-UTRA-TDD128-r9					ENUMERATED {supported}		OPTIONAL,
	srvcc-FromUTRA-FDD-ToUTRA-FDD-r9				ENUMERATED {supported}		OPTIONAL,
	srvcc-FromUTRA-FDD-ToGERAN-r9					ENUMERATED {supported}		OPTIONAL,
	srvcc-FromUTRA-TDD128-ToUTRA-TDD128-r9			ENUMERATED {supported}		OPTIONAL,
	srvcc-FromUTRA-TDD128-ToGERAN-r9				ENUMERATED {supported}		OPTIONAL
}

IRAT-ParametersUTRA-v9h0 ::=		SEQUENCE {
	mfbi-UTRA-r9						ENUMERATED {supported}
}

SupportedBandListUTRA-FDD ::=		SEQUENCE (SIZE (1..maxBands)) OF SupportedBandUTRA-FDD

SupportedBandUTRA-FDD ::=			ENUMERATED {
										bandI, bandII, bandIII, bandIV, bandV, bandVI,
										bandVII, bandVIII, bandIX, bandX, bandXI,
										bandXII, bandXIII, bandXIV, bandXV, bandXVI, ...,
										bandXVII-8a0, bandXVIII-8a0, bandXIX-8a0, bandXX-8a0,
										bandXXI-8a0, bandXXII-8a0, bandXXIII-8a0, bandXXIV-8a0,
										bandXXV-8a0, bandXXVI-8a0, bandXXVII-8a0, bandXXVIII-8a0,
										bandXXIX-8a0, bandXXX-8a0, bandXXXI-8a0, bandXXXII-8a0}

IRAT-ParametersUTRA-TDD128 ::=		SEQUENCE {
	supportedBandListUTRA-TDD128		SupportedBandListUTRA-TDD128
}

SupportedBandListUTRA-TDD128 ::=	SEQUENCE (SIZE (1..maxBands)) OF SupportedBandUTRA-TDD128

SupportedBandUTRA-TDD128 ::=		ENUMERATED {
										a, b, c, d, e, f, g, h, i, j, k, l, m, n,
										o, p, ...}

IRAT-ParametersUTRA-TDD384 ::=		SEQUENCE {
	supportedBandListUTRA-TDD384		SupportedBandListUTRA-TDD384
}

SupportedBandListUTRA-TDD384 ::=	SEQUENCE (SIZE (1..maxBands)) OF SupportedBandUTRA-TDD384

SupportedBandUTRA-TDD384 ::=		ENUMERATED {
											a, b, c, d, e, f, g, h, i, j, k, l, m, n,
											o, p, ...}

IRAT-ParametersUTRA-TDD768 ::=		SEQUENCE {
	supportedBandListUTRA-TDD768		SupportedBandListUTRA-TDD768
}

SupportedBandListUTRA-TDD768 ::=	SEQUENCE (SIZE (1..maxBands)) OF SupportedBandUTRA-TDD768

SupportedBandUTRA-TDD768 ::=		ENUMERATED {
										a, b, c, d, e, f, g, h, i, j, k, l, m, n,
										o, p, ...}

IRAT-ParametersUTRA-TDD-v1020 ::=		SEQUENCE {
	e-RedirectionUTRA-TDD-r10				ENUMERATED {supported}
}

IRAT-ParametersGERAN ::=			SEQUENCE {
	supportedBandListGERAN				SupportedBandListGERAN,
	interRAT-PS-HO-ToGERAN				BOOLEAN
}

IRAT-ParametersGERAN-v920 ::=		SEQUENCE {
	dtm-r9								ENUMERATED {supported}			OPTIONAL,
	e-RedirectionGERAN-r9				ENUMERATED {supported}			OPTIONAL
}

SupportedBandListGERAN ::=			SEQUENCE (SIZE (1..maxBands)) OF SupportedBandGERAN

SupportedBandGERAN ::=				ENUMERATED {
										gsm450, gsm480, gsm710, gsm750, gsm810, gsm850,
										gsm900P, gsm900E, gsm900R, gsm1800, gsm1900,
										spare5, spare4, spare3, spare2, spare1, ...}

IRAT-ParametersCDMA2000-HRPD ::=	SEQUENCE {
	supportedBandListHRPD				SupportedBandListHRPD,
	tx-ConfigHRPD						ENUMERATED {single, dual},
	rx-ConfigHRPD						ENUMERATED {single, dual}
}

SupportedBandListHRPD ::=			SEQUENCE (SIZE (1..maxCDMA-BandClass)) OF BandclassCDMA2000

IRAT-ParametersCDMA2000-1XRTT ::=	SEQUENCE {
	supportedBandList1XRTT				SupportedBandList1XRTT,
	tx-Config1XRTT						ENUMERATED {single, dual},
	rx-Config1XRTT						ENUMERATED {single, dual}
}

IRAT-ParametersCDMA2000-1XRTT-v920 ::=	SEQUENCE {
	e-CSFB-1XRTT-r9						ENUMERATED {supported},
	e-CSFB-ConcPS-Mob1XRTT-r9			ENUMERATED {supported}			OPTIONAL
}

IRAT-ParametersCDMA2000-1XRTT-v1020 ::=	SEQUENCE {
	e-CSFB-dual-1XRTT-r10				ENUMERATED {supported}
}

IRAT-ParametersCDMA2000-v1130 ::=		SEQUENCE {
	cdma2000-NW-Sharing-r11					ENUMERATED {supported}		OPTIONAL
}

SupportedBandList1XRTT ::=			SEQUENCE (SIZE (1..maxCDMA-BandClass)) OF BandclassCDMA2000

IRAT-ParametersWLAN-r13 ::=		SEQUENCE {
	supportedBandListWLAN-r13		SEQUENCE (SIZE (1..maxWLAN-Bands-r13)) OF WLAN-BandIndicator-r13					OPTIONAL
}

CSG-ProximityIndicationParameters-r9 ::=	SEQUENCE {
	intraFreqProximityIndication-r9	ENUMERATED {supported}			OPTIONAL,
	interFreqProximityIndication-r9	ENUMERATED {supported}			OPTIONAL,
	utran-ProximityIndication-r9		ENUMERATED {supported}			OPTIONAL
}

NeighCellSI-AcquisitionParameters-r9 ::=	SEQUENCE {
	intraFreqSI-AcquisitionForHO-r9	ENUMERATED {supported}			OPTIONAL,
	interFreqSI-AcquisitionForHO-r9	ENUMERATED {supported}			OPTIONAL,
	utran-SI-AcquisitionForHO-r9		ENUMERATED {supported}			OPTIONAL
}

SON-Parameters-r9 ::=				SEQUENCE {
	rach-Report-r9						ENUMERATED {supported}			OPTIONAL
}

UE-BasedNetwPerfMeasParameters-r10 ::=	SEQUENCE {
	loggedMeasurementsIdle-r10				ENUMERATED {supported}		OPTIONAL,
	standaloneGNSS-Location-r10				ENUMERATED {supported}		OPTIONAL
}

UE-BasedNetwPerfMeasParameters-v1250 ::=	SEQUENCE {
	loggedMBSFNMeasurements-r12				ENUMERATED {supported}
}

UE-BasedNetwPerfMeasParameters-v1430 ::=	SEQUENCE {
	locationReport-r14						ENUMERATED {supported}		OPTIONAL
}

OTDOA-PositioningCapabilities-r10 ::=	SEQUENCE {
	otdoa-UE-Assisted-r10					ENUMERATED {supported},
	interFreqRSTD-Measurement-r10			ENUMERATED {supported}		OPTIONAL
}

Other-Parameters-r11 ::=				SEQUENCE {
	inDeviceCoexInd-r11						ENUMERATED {supported}		OPTIONAL,
	powerPrefInd-r11						ENUMERATED {supported}		OPTIONAL,
	ue-Rx-TxTimeDiffMeasurements-r11		ENUMERATED {supported}		OPTIONAL
}

Other-Parameters-v11d0 ::=				SEQUENCE {
	inDeviceCoexInd-UL-CA-r11				ENUMERATED {supported}		OPTIONAL
}

Other-Parameters-v1360 ::=	SEQUENCE {
	inDeviceCoexInd-HardwareSharingInd-r13		ENUMERATED {supported}		OPTIONAL
}

Other-Parameters-v1430 ::=			SEQUENCE {
	bwPrefInd-r14					ENUMERATED {supported}		OPTIONAL,
	rlm-ReportSupport-r14			ENUMERATED {supported}		OPTIONAL
}

OtherParameters-v1450 ::=	SEQUENCE {
	overheatingInd-r14				ENUMERATED {supported}		OPTIONAL
}

Other-Parameters-v1460 ::= SEQUENCE {
	nonCSG-SI-Reporting-r14			ENUMERATED {supported}		OPTIONAL
}

MBMS-Parameters-r11 ::=				SEQUENCE {
	mbms-SCell-r11							ENUMERATED {supported}		OPTIONAL,
	mbms-NonServingCell-r11					ENUMERATED {supported}		OPTIONAL
}

MBMS-Parameters-v1250 ::=				SEQUENCE {
	mbms-AsyncDC-r12						ENUMERATED {supported}		OPTIONAL
}

MBMS-Parameters-v1430 ::=				SEQUENCE {
	fembmsDedicatedCell-r14				ENUMERATED {supported}		OPTIONAL,
	fembmsMixedCell-r14					ENUMERATED {supported}		OPTIONAL,
	subcarrierSpacingMBMS-khz7dot5-r14	ENUMERATED {supported}		OPTIONAL,
	subcarrierSpacingMBMS-khz1dot25-r14	ENUMERATED {supported}		OPTIONAL
}

MBMS-Parameters-v1470 ::=		SEQUENCE {
	mbms-MaxBW-r14					CHOICE {
		implicitValue 					NULL,
		explicitValue 					INTEGER(2..20)
	},
	mbms-ScalingFactor1dot25-r14		ENUMERATED {n3, n6, n9, n12} 	OPTIONAL,
	mbms-ScalingFactor7dot5-r14		ENUMERATED {n1, n2, n3, n4}		OPTIONAL
}

FeMBMS-Unicast-Parameters-r14 ::=		SEQUENCE {
	unicast-fembmsMixedSCell-r14			ENUMERATED {supported}		OPTIONAL,
	emptyUnicastRegion-r14					ENUMERATED {supported}		OPTIONAL
}

SCPTM-Parameters-r13 ::=				SEQUENCE {
	scptm-ParallelReception-r13					ENUMERATED {supported}		OPTIONAL,
	scptm-SCell-r13								ENUMERATED {supported}		OPTIONAL,
	scptm-NonServingCell-r13					ENUMERATED {supported}		OPTIONAL,
	scptm-AsyncDC-r13							ENUMERATED {supported}		OPTIONAL
}

CE-Parameters-r13 ::=		SEQUENCE {
	ce-ModeA-r13						ENUMERATED {supported}				OPTIONAL,
	ce-ModeB-r13						ENUMERATED {supported}				OPTIONAL
}

CE-Parameters-v1320 ::=		SEQUENCE {
	intraFreqA3-CE-ModeA-r13				ENUMERATED {supported}				OPTIONAL,
	intraFreqA3-CE-ModeB-r13				ENUMERATED {supported}				OPTIONAL,
	intraFreqHO-CE-ModeA-r13				ENUMERATED {supported}				OPTIONAL,
	intraFreqHO-CE-ModeB-r13				ENUMERATED {supported}				OPTIONAL
}

CE-Parameters-v1350 ::=		SEQUENCE {
	unicastFrequencyHopping-r13				ENUMERATED {supported}				OPTIONAL
}

CE-Parameters-v1370 ::=		SEQUENCE {
	tm9-CE-ModeA-r13						ENUMERATED {supported}			OPTIONAL,
	tm9-CE-ModeB-r13						ENUMERATED {supported}			OPTIONAL
}

CE-Parameters-v1380 ::=		SEQUENCE {
	tm6-CE-ModeA-r13						ENUMERATED {supported}			OPTIONAL
}

CE-Parameters-v1430 ::=		SEQUENCE {
	ce-SwitchWithoutHO-r14					ENUMERATED {supported}				OPTIONAL
}

LAA-Parameters-r13 ::=				SEQUENCE {
	crossCarrierSchedulingLAA-DL-r13			ENUMERATED {supported}		OPTIONAL,
	csi-RS-DRS-RRM-MeasurementsLAA-r13			ENUMERATED {supported}		OPTIONAL,
	downlinkLAA-r13								ENUMERATED {supported}		OPTIONAL,
	endingDwPTS-r13								ENUMERATED {supported}		OPTIONAL,
	secondSlotStartingPosition-r13				ENUMERATED {supported}		OPTIONAL,
	tm9-LAA-r13									ENUMERATED {supported}		OPTIONAL,
	tm10-LAA-r13								ENUMERATED {supported}		OPTIONAL
}

LAA-Parameters-v1430 ::=				SEQUENCE {
	crossCarrierSchedulingLAA-UL-r14			ENUMERATED {supported}		OPTIONAL,
	uplinkLAA-r14								ENUMERATED {supported}		OPTIONAL,
	twoStepSchedulingTimingInfo-r14				ENUMERATED {nPlus1, nPlus2, nPlus3}	OPTIONAL,
	uss-BlindDecodingAdjustment-r14				ENUMERATED {supported}		OPTIONAL,
	uss-BlindDecodingReduction-r14				ENUMERATED {supported}		OPTIONAL,
	outOfSequenceGrantHandling-r14				ENUMERATED {supported}		OPTIONAL
}

WLAN-IW-Parameters-r12 ::=	SEQUENCE {
	wlan-IW-RAN-Rules-r12					ENUMERATED {supported}		OPTIONAL,
	wlan-IW-ANDSF-Policies-r12						ENUMERATED {supported}		OPTIONAL
}

LWA-Parameters-r13 ::=		SEQUENCE {
	lwa-r13						ENUMERATED {supported}		OPTIONAL,
	lwa-SplitBearer-r13			ENUMERATED {supported}		OPTIONAL,
	wlan-MAC-Address-r13		OCTET STRING (SIZE (6))		OPTIONAL,
	lwa-BufferSize-r13			ENUMERATED {supported}		OPTIONAL
}

LWA-Parameters-v1430 ::=		SEQUENCE {
	lwa-HO-WithoutWT-Change-r14			ENUMERATED {supported}		OPTIONAL,
	lwa-UL-r14							ENUMERATED {supported}		OPTIONAL,
	wlan-PeriodicMeas-r14				ENUMERATED {supported}		OPTIONAL,
	wlan-ReportAnyWLAN-r14				ENUMERATED {supported}		OPTIONAL,
	wlan-SupportedDataRate-r14			INTEGER (1..2048)			OPTIONAL
}

LWA-Parameters-v1440 ::=		SEQUENCE {
	lwa-RLC-UM-r14						ENUMERATED {supported}		OPTIONAL
}

WLAN-IW-Parameters-v1310 ::=	SEQUENCE {
	rclwi-r13										ENUMERATED {supported}		OPTIONAL
}

LWIP-Parameters-r13 ::=		SEQUENCE {
	lwip-r13					ENUMERATED {supported}				OPTIONAL
}

LWIP-Parameters-v1430 ::=		SEQUENCE {
	lwip-Aggregation-DL-r14					ENUMERATED {supported}				OPTIONAL,
	lwip-Aggregation-UL-r14					ENUMERATED {supported}				OPTIONAL
}

NAICS-Capability-List-r12 ::= SEQUENCE (SIZE (1..maxNAICS-Entries-r12)) OF NAICS-Capability-Entry-r12


NAICS-Capability-Entry-r12	::=	SEQUENCE {
	numberOfNAICS-CapableCC-r12				INTEGER(1..5),
	numberOfAggregatedPRB-r12				ENUMERATED {
												n50, n75, n100, n125, n150, n175,
												n200, n225, n250, n275, n300, n350,
												n400, n450, n500, spare},
	...
}

SL-Parameters-r12 ::=				SEQUENCE {
	commSimultaneousTx-r12					ENUMERATED {supported}		OPTIONAL,
	commSupportedBands-r12					FreqBandIndicatorListEUTRA-r12	OPTIONAL,
	discSupportedBands-r12					SupportedBandInfoList-r12	OPTIONAL,
	discScheduledResourceAlloc-r12			ENUMERATED {supported}		OPTIONAL,
	disc-UE-SelectedResourceAlloc-r12		ENUMERATED {supported}		OPTIONAL,
	disc-SLSS-r12							ENUMERATED {supported}		OPTIONAL,
	discSupportedProc-r12					ENUMERATED {n50, n400}		OPTIONAL
}

SL-Parameters-v1310 ::=				SEQUENCE {
	discSysInfoReporting-r13					ENUMERATED {supported}		OPTIONAL,
	commMultipleTx-r13							ENUMERATED {supported}		OPTIONAL,
	discInterFreqTx-r13							ENUMERATED {supported}		OPTIONAL,
	discPeriodicSLSS-r13						ENUMERATED {supported}		OPTIONAL
}

SL-Parameters-v1430 ::=				SEQUENCE {
	zoneBasedPoolSelection-r14				ENUMERATED {supported}				OPTIONAL,
	ue-AutonomousWithFullSensing-r14		ENUMERATED {supported}				OPTIONAL,
	ue-AutonomousWithPartialSensing-r14		ENUMERATED {supported}				OPTIONAL,
	sl-CongestionControl-r14				ENUMERATED {supported}				OPTIONAL,
	v2x-TxWithShortResvInterval-r14			ENUMERATED {supported}				OPTIONAL,
	v2x-numberTxRxTiming-r14				INTEGER(1..16)						OPTIONAL,
	v2x-nonAdjacentPSCCH-PSSCH-r14			ENUMERATED {supported}				OPTIONAL,
	slss-TxRx-r14							ENUMERATED {supported}				OPTIONAL,
	v2x-SupportedBandCombinationList-r14	V2X-SupportedBandCombination-r14	OPTIONAL
}

V2X-SupportedBandCombination-r14 ::=		SEQUENCE (SIZE (1..maxBandComb-r13)) OF V2X-BandCombinationParameters-r14

V2X-BandCombinationParameters-r14 ::=	SEQUENCE (SIZE (1.. maxSimultaneousBands-r10)) OF V2X-BandParameters-r14

SupportedBandInfoList-r12 ::=		SEQUENCE (SIZE (1..maxBands)) OF SupportedBandInfo-r12

SupportedBandInfo-r12 ::=			SEQUENCE {
	support-r12								ENUMERATED {supported}	OPTIONAL
}

FreqBandIndicatorListEUTRA-r12 ::=		SEQUENCE (SIZE (1..maxBands)) OF FreqBandIndicator-r11

MMTEL-Parameters-r14 ::=			SEQUENCE {
	delayBudgetReporting-r14					ENUMERATED {supported}		OPTIONAL,
	pusch-Enhancements-r14						ENUMERATED {supported}		OPTIONAL,
	recommendedBitRate-r14						ENUMERATED {supported}		OPTIONAL,
	recommendedBitRateQuery-r14					ENUMERATED {supported}		OPTIONAL
}

RetuningTimeInfo-r14 ::= SEQUENCE {
	retuningInfo				SEQUENCE {
		rf-RetuningTimeDL-r14			ENUMERATED {n0, n0dot5, n1, n1dot5, n2, n2dot5, n3,
													n3dot5, n4, n4dot5, n5, n5dot5, n6, n6dot5,
													n7, spare1}		OPTIONAL,
		rf-RetuningTimeUL-r14			ENUMERATED {n0, n0dot5, n1, n1dot5, n2, n2dot5, n3,
													n3dot5, n4, n4dot5, n5, n5dot5, n6, n6dot5,
													n7, spare1}		OPTIONAL
	}
}

HighSpeedEnhParameters-r14 ::= SEQUENCE {
	measurementEnhancements-r14		ENUMERATED {supported}		OPTIONAL,
	demodulationEnhancements-r14	ENUMERATED {supported}		OPTIONAL,
	prach-Enhancements-r14			ENUMERATED {supported}		OPTIONAL
}


UE-RadioPagingInfo-r12 ::=				SEQUENCE {
	ue-Category-v1250					INTEGER (0)			OPTIONAL,
	...,
	[[	ue-CategoryDL-v1310						ENUMERATED {m1}		OPTIONAL,
		ce-ModeA-r13							ENUMERATED {true}	OPTIONAL,
		ce-ModeB-r13							ENUMERATED {true}	OPTIONAL
	]]
}


UE-TimersAndConstants ::=			SEQUENCE {
	t300								ENUMERATED {
											ms100, ms200, ms300, ms400, ms600, ms1000, ms1500,
											ms2000},
	t301								ENUMERATED {
											ms100, ms200, ms300, ms400, ms600, ms1000, ms1500,
											ms2000},
	t310								ENUMERATED {
											ms0, ms50, ms100, ms200, ms500, ms1000, ms2000},
	n310								ENUMERATED {
											n1, n2, n3, n4, n6, n8, n10, n20},
	t311								ENUMERATED {
											ms1000, ms3000, ms5000, ms10000, ms15000,
											ms20000, ms30000},
	n311								ENUMERATED {
											n1, n2, n3, n4, n5, n6, n8, n10},
	...,
	[[	t300-v1310						ENUMERATED {
											ms2500, ms3000, ms3500, ms4000, ms5000, ms6000, ms8000,
											ms10000}		OPTIONAL,	-- Need OR
		t301-v1310						ENUMERATED {
											ms2500, ms3000, ms3500, ms4000, ms5000, ms6000, ms8000,
											ms10000}		OPTIONAL	-- Need OR
	]],
	[[	t310-v1330							ENUMERATED {ms4000, ms6000}
															OPTIONAL	-- Need OR
	]]
}


VisitedCellInfoList-r12 ::=	SEQUENCE (SIZE (1..maxCellHistory-r12)) OF VisitedCellInfo-r12

VisitedCellInfo-r12 ::=				SEQUENCE {
	visitedCellId-r12					CHOICE {
		cellGlobalId-r12						CellGlobalIdEUTRA,
		pci-arfcn-r12							SEQUENCE {
			physCellId-r12							PhysCellId,
			carrierFreq-r12							ARFCN-ValueEUTRA-r9
		}
	}																OPTIONAL,
	timeSpent-r12						INTEGER (0..4095),
	...
}


WLAN-OffloadConfig-r12 ::=				SEQUENCE {
	thresholdRSRP-r12						SEQUENCE {
		thresholdRSRP-Low-r12					RSRP-Range,
		thresholdRSRP-High-r12					RSRP-Range
	}																	OPTIONAL, -- Need OR
	thresholdRSRQ-r12						SEQUENCE {
		thresholdRSRQ-Low-r12					RSRQ-Range,
		thresholdRSRQ-High-r12					RSRQ-Range
	}																	OPTIONAL, -- Need OR
	thresholdRSRQ-OnAllSymbolsWithWB-r12	SEQUENCE {
		thresholdRSRQ-OnAllSymbolsWithWB-Low-r12			RSRQ-Range,
		thresholdRSRQ-OnAllSymbolsWithWB-High-r12			RSRQ-Range
	}																	OPTIONAL, -- Need OP
	thresholdRSRQ-OnAllSymbols-r12			SEQUENCE {
			thresholdRSRQ-OnAllSymbolsLow-r12					RSRQ-Range,
			thresholdRSRQ-OnAllSymbolsHigh-r12					RSRQ-Range
	}																	OPTIONAL, -- Need OP
	thresholdRSRQ-WB-r12					SEQUENCE {
		thresholdRSRQ-WB-Low-r12							RSRQ-Range,
		thresholdRSRQ-WB-High-r12							RSRQ-Range
	}																	OPTIONAL, -- Need OP

	thresholdChannelUtilization-r12			SEQUENCE {
		thresholdChannelUtilizationLow-r12		INTEGER (0..255),
		thresholdChannelUtilizationHigh-r12		INTEGER (0..255)
	}																	OPTIONAL, -- Need OR
	thresholdBackhaul-Bandwidth-r12			SEQUENCE {
		thresholdBackhaulDL-BandwidthLow-r12	WLAN-backhaulRate-r12,
		thresholdBackhaulDL-BandwidthHigh-r12	WLAN-backhaulRate-r12,
		thresholdBackhaulUL-BandwidthLow-r12	WLAN-backhaulRate-r12,
		thresholdBackhaulUL-BandwidthHigh-r12	WLAN-backhaulRate-r12
	}																	OPTIONAL, -- Need OR
	thresholdWLAN-RSSI-r12						SEQUENCE {
		thresholdWLAN-RSSI-Low-r12					INTEGER (0..255),
		thresholdWLAN-RSSI-High-r12					INTEGER (0..255)
	}																	OPTIONAL, -- Need OR
	offloadPreferenceIndicator-r12			BIT STRING (SIZE (16))		OPTIONAL, -- Need OR
	t-SteeringWLAN-r12						T-Reselection				OPTIONAL, -- Need OR
	...
}

WLAN-backhaulRate-r12 ::=					ENUMERATED
										{r0, r4, r8, r16, r32, r64, r128, r256, r512,
										r1024, r2048, r4096, r8192, r16384, r32768, r65536, r131072,
										r262144, r524288, r1048576, r2097152, r4194304, r8388608,
										r16777216, r33554432, r67108864, r134217728, r268435456,
										r536870912, r1073741824, r2147483648, r4294967296}


MBMS-NotificationConfig-r9 ::=				SEQUENCE {
	notificationRepetitionCoeff-r9		ENUMERATED {n2, n4},
	notificationOffset-r9				INTEGER (0..10),
	notificationSF-Index-r9				INTEGER (1..6)
}

MBMS-NotificationConfig-v1430 ::=				SEQUENCE {
	notificationSF-Index-v1430				INTEGER (7..10)
}


MBMS-ServiceList-r13 ::=			SEQUENCE (SIZE (0..maxMBMS-ServiceListPerUE-r13)) OF MBMS-ServiceInfo-r13

MBMS-ServiceInfo-r13 ::=				SEQUENCE	{
	tmgi-r13							TMGI-r9
}


MBSFN-AreaId-r12 ::=					INTEGER (0..255)


MBSFN-AreaInfoList-r9 ::=			SEQUENCE (SIZE(1..maxMBSFN-Area)) OF MBSFN-AreaInfo-r9

MBSFN-AreaInfo-r9 ::=				SEQUENCE {
	mbsfn-AreaId-r9						MBSFN-AreaId-r12,
	non-MBSFNregionLength				ENUMERATED {s1, s2},
	notificationIndicator-r9			INTEGER (0..7),
	mcch-Config-r9						SEQUENCE {
		mcch-RepetitionPeriod-r9		ENUMERATED {rf32, rf64, rf128, rf256},
		mcch-Offset-r9					INTEGER (0..10),
		mcch-ModificationPeriod-r9		ENUMERATED {rf512, rf1024},
		sf-AllocInfo-r9					BIT STRING (SIZE(6)),
		signallingMCS-r9				ENUMERATED {n2, n7, n13, n19}
	},
	...,
	[[	mcch-Config-r14				SEQUENCE {
			mcch-RepetitionPeriod-v1430		ENUMERATED {rf1, rf2, rf4, rf8,
										rf16 }		OPTIONAL,	-- Need OR
			mcch-ModificationPeriod-v1430	ENUMERATED {rf1, rf2, rf4, rf8, rf16, rf32, rf64, rf128,
											rf256, spare7}					OPTIONAL	-- Need OR
		}																	OPTIONAL,	-- Need OR
		subcarrierSpacingMBMS-r14		ENUMERATED {khz-7dot5, khz-1dot25}	OPTIONAL	-- Need OR
	]]
}


MBSFN-SubframeConfig ::=			SEQUENCE {
	radioframeAllocationPeriod			ENUMERATED {n1, n2, n4, n8, n16, n32},
	radioframeAllocationOffset			INTEGER (0..7),
	subframeAllocation					CHOICE {
		oneFrame							BIT STRING (SIZE(6)),
		fourFrames							BIT STRING (SIZE(24))
	}
}

MBSFN-SubframeConfig-v1430 ::=		SEQUENCE {
	subframeAllocation-v1430				CHOICE {
		oneFrame-v1430						BIT STRING (SIZE(2)),
		fourFrames-v1430					BIT STRING (SIZE(8))
	}
}


PMCH-InfoList-r9 ::=				SEQUENCE (SIZE (0..maxPMCH-PerMBSFN)) OF PMCH-Info-r9

PMCH-InfoListExt-r12 ::=			SEQUENCE (SIZE (0..maxPMCH-PerMBSFN)) OF PMCH-InfoExt-r12

PMCH-Info-r9 ::=					SEQUENCE {
	pmch-Config-r9						PMCH-Config-r9,
	mbms-SessionInfoList-r9			MBMS-SessionInfoList-r9,
	...
}

PMCH-InfoExt-r12 ::=				SEQUENCE {
	pmch-Config-r12						PMCH-Config-r12,
	mbms-SessionInfoList-r12			MBMS-SessionInfoList-r9,
	...
}

MBMS-SessionInfoList-r9 ::=		SEQUENCE (SIZE (0..maxSessionPerPMCH)) OF MBMS-SessionInfo-r9

MBMS-SessionInfo-r9 ::=			SEQUENCE {
	tmgi-r9								TMGI-r9,
	sessionId-r9						OCTET STRING (SIZE (1))		OPTIONAL,	-- Need OR
	logicalChannelIdentity-r9			INTEGER (0..maxSessionPerPMCH-1),
	...
}

PMCH-Config-r9 ::=					SEQUENCE {
	sf-AllocEnd-r9						INTEGER (0..1535),
	dataMCS-r9							INTEGER (0..28),
	mch-SchedulingPeriod-r9			ENUMERATED {
										rf8, rf16, rf32, rf64, rf128, rf256, rf512, rf1024},
	...
}

PMCH-Config-r12 ::=					SEQUENCE {
	sf-AllocEnd-r12						INTEGER (0..1535),
	dataMCS-r12							CHOICE {
		normal-r12							INTEGER (0..28),
		higerOrder-r12						INTEGER (0..27)
	},
	mch-SchedulingPeriod-r12		ENUMERATED {
										rf4, rf8, rf16, rf32, rf64, rf128, rf256, rf512, rf1024},
	...,
	[[	mch-SchedulingPeriod-v1430		ENUMERATED {rf1, rf2}			OPTIONAL	-- Need OR
	]]
}

TMGI-r9 ::=						SEQUENCE {
	plmn-Id-r9							CHOICE {
		plmn-Index-r9						INTEGER (1..maxPLMN-r11),
		explicitValue-r9					PLMN-Identity
	},
	serviceId-r9						OCTET STRING (SIZE (3))
}


SC-MTCH-InfoList-r13 ::=			SEQUENCE (SIZE (0..maxSC-MTCH-r13)) OF SC-MTCH-Info-r13

SC-MTCH-Info-r13 ::=				SEQUENCE	{
	mbmsSessionInfo-r13						MBMSSessionInfo-r13,
	g-RNTI-r13								BIT STRING(SIZE(16)),
	sc-mtch-schedulingInfo-r13				SC-MTCH-SchedulingInfo-r13			OPTIONAL,	-- Need OP
	sc-mtch-neighbourCell-r13				BIT STRING (SIZE(maxNeighCell-SCPTM-r13))	OPTIONAL,	-- Need OP
	...,
	[[	p-a-r13								ENUMERATED {
												dB-6, dB-4dot77, dB-3, dB-1dot77,
												dB0, dB1, dB2, dB3}		OPTIONAL	-- Need ON
	]]
}

MBMSSessionInfo-r13 ::=				SEQUENCE	{
	tmgi-r13								TMGI-r9,
	sessionId-r13							OCTET STRING (SIZE (1))		OPTIONAL	-- Need OR
}

SC-MTCH-SchedulingInfo-r13::=		SEQUENCE	{
	onDurationTimerSCPTM-r13				ENUMERATED {
												psf1, psf2, psf3, psf4, psf5, psf6,
												psf8, psf10, psf20, psf30, psf40,
												psf50, psf60, psf80, psf100,
												psf200},
	drx-InactivityTimerSCPTM-r13			ENUMERATED {
												psf0, psf1, psf2, psf4, psf8,
												psf10, psf20, psf40,
												psf80, psf160, ps320,
												psf640, psf960,
												psf1280, psf1920, psf2560},
	schedulingPeriodStartOffsetSCPTM-r13	CHOICE {
		sf10									INTEGER(0..9),
		sf20									INTEGER(0..19),
		sf32									INTEGER(0..31),
		sf40									INTEGER(0..39),
		sf64									INTEGER(0..63),
		sf80									INTEGER(0..79),
		sf128									INTEGER(0..127),
		sf160									INTEGER(0..159),
		sf256									INTEGER(0..255),
		sf320									INTEGER(0..319),
		sf512									INTEGER(0..511),
		sf640									INTEGER(0..639),
		sf1024									INTEGER(0..1023),
		sf2048									INTEGER(0..2048),
		sf4096									INTEGER(0..4096),
		sf8192									INTEGER(0..8192)
	},
	...
}


SC-MTCH-InfoList-BR-r14 ::=		SEQUENCE (SIZE (0..maxSC-MTCH-BR-r14)) OF SC-MTCH-Info-BR-r14

SC-MTCH-Info-BR-r14 ::=			SEQUENCE	{
	sc-mtch-CarrierFreq-r14					ARFCN-ValueEUTRA-r9,
	mbmsSessionInfo-r14						MBMSSessionInfo-r13,
	g-RNTI-r14								BIT STRING(SIZE(16)),
	sc-mtch-schedulingInfo-r14			SC-MTCH-SchedulingInfo-BR-r14				OPTIONAL,	-- Need OP
	sc-mtch-neighbourCell-r14				BIT STRING (SIZE(maxNeighCell-SCPTM-r13))	OPTIONAL,	-- Need OP
	mpdcch-Narrowband-SC-MTCH-r14				INTEGER (1.. maxAvailNarrowBands-r13),
	mpdcch-NumRepetition-SC-MTCH-r14			ENUMERATED {r1, r2, r4, r8, r16,
															r32, r64, r128, r256},
	mpdcch-StartSF-SC-MTCH-r14		CHOICE {
			fdd-r14								ENUMERATED {v1, v1dot5, v2, v2dot5, v4,
																v5, v8, v10},
			tdd-r14								ENUMERATED {v1, v2, v4, v5, v8, v10,
																v20}
	},
	mpdcch-PDSCH-HoppingConfig-SC-MTCH-r14		ENUMERATED {on, off},
	mpdcch-PDSCH-CEmodeConfig-SC-MTCH-r14		ENUMERATED {ce-ModeA, ce-ModeB},
	mpdcch-PDSCH-MaxBandwidth-SC-MTCH-r14		ENUMERATED {bw1dot4, bw5},
	mpdcch-Offset-SC-MTCH-r14					ENUMERATED {zero, oneEighth, oneQuarter,
															threeEighth, oneHalf, fiveEighth,
															threeQuarter, sevenEighth},

	p-a-r14										ENUMERATED { dB-6, dB-4dot77, dB-3,
															dB-1dot77, dB0, dB1, dB2,
															dB3}				OPTIONAL,--	Need OR
	...
}

SC-MTCH-SchedulingInfo-BR-r14::=	SEQUENCE	{
	onDurationTimerSCPTM-r14				ENUMERATED {
												psf300, psf400, psf500, psf600,
												psf800, psf1000, psf1200, psf1600},
	drx-InactivityTimerSCPTM-r14			ENUMERATED {
												psf0, psf1, psf2, psf4, psf8, psf16,
												psf32, psf64, psf128, psf256, ps512,
												psf1024, psf2048, psf4096, psf8192, psf16384},
	schedulingPeriodStartOffsetSCPTM-r14	CHOICE {
		sf10									INTEGER(0..9),
		sf20									INTEGER(0..19),
		sf32									INTEGER(0..31),
		sf40									INTEGER(0..39),
		sf64									INTEGER(0..63),
		sf80									INTEGER(0..79),
		sf128									INTEGER(0..127),
		sf160									INTEGER(0..159),
		sf256									INTEGER(0..255),
		sf320									INTEGER(0..319),
		sf512									INTEGER(0..511),
		sf640									INTEGER(0..639),
		sf1024									INTEGER(0..1023),
		sf2048									INTEGER(0..2047),
		sf4096									INTEGER(0..4095),
		sf8192									INTEGER(0..8191)
	},
	...
}


SCPTM-NeighbourCellList-r13 ::=		SEQUENCE (SIZE (1..maxNeighCell-SCPTM-r13)) OF PCI-ARFCN-r13

PCI-ARFCN-r13 ::=					SEQUENCE {
		physCellId-r13						PhysCellId,
		carrierFreq-r13						ARFCN-ValueEUTRA-r9		OPTIONAL
}


SL-AnchorCarrierFreqList-V2X-r14 ::= SEQUENCE (SIZE (1..maxFreqV2X-r14)) OF ARFCN-ValueEUTRA-r9


SL-CBR-CommonTxConfigList-r14 ::=	SEQUENCE {
	cbr-RangeCommonConfigList-r14	SEQUENCE (SIZE (1..maxSL-V2X-CBRConfig-r14)) OF SL-CBR-Levels-Config-r14,
	sl-CBR-PSSCH-TxConfigList-r14	SEQUENCE (SIZE (1..maxSL-V2X-TxConfig-r14)) OF SL-CBR-PSSCH-TxConfig-r14
}

SL-CBR-Levels-Config-r14 ::=		SEQUENCE (SIZE (1..maxCBR-Level-r14)) OF SL-CBR-r14


SL-CBR-PSSCH-TxConfig-r14 ::=		SEQUENCE {
	cr-Limit-r14					INTEGER(0..10000),
	tx-Parameters-r14				SL-PSSCH-TxParameters-r14
}

SL-CBR-r14 ::=						INTEGER(0..100)


SL-CBR-PPPP-TxConfigList-r14 ::=	SEQUENCE (SIZE (1..8)) OF SL-PPPP-TxConfigIndex-r14

SL-PPPP-TxConfigIndex-r14 ::=		SEQUENCE {
	priorityThreshold-r14			SL-Priority-r13,
	defaultTxConfigIndex-r14		INTEGER(0..maxCBR-Level-1-r14),
	cbr-ConfigIndex-r14				INTEGER(0..maxSL-V2X-CBRConfig-1-r14),
	tx-ConfigIndexList-r14			SEQUENCE (SIZE (1..maxCBR-Level-r14)) OF Tx-ConfigIndex-r14
}

Tx-ConfigIndex-r14 ::=				INTEGER(0..maxSL-V2X-TxConfig-1-r14)


SL-CommConfig-r12 ::=				SEQUENCE	{
	commTxResources-r12					CHOICE {
		release								NULL,
		setup								CHOICE {
			scheduled-r12					SEQUENCE {
				sl-RNTI-r12						C-RNTI,
				mac-MainConfig-r12				MAC-MainConfigSL-r12,
				sc-CommTxConfig-r12				SL-CommResourcePool-r12,
				mcs-r12							INTEGER (0..28)				OPTIONAL	-- Need OP
			},
			ue-Selected-r12					SEQUENCE {
				-- Pool for normal usage
				commTxPoolNormalDedicated-r12	SEQUENCE {
					poolToReleaseList-r12			SL-TxPoolToReleaseList-r12 OPTIONAL,	-- Need ON
					poolToAddModList-r12			SL-CommTxPoolToAddModList-r12 OPTIONAL	-- Need ON
				}
			}
		}
	}																		OPTIONAL,	-- Need ON
	...,
	[[	commTxResources-v1310						CHOICE {
			release								NULL,
			setup								CHOICE {
				scheduled-v1310						SEQUENCE {
					logicalChGroupInfoList-r13			LogicalChGroupInfoList-r13,
					multipleTx-r13						BOOLEAN
				},
				ue-Selected-v1310					SEQUENCE {
					commTxPoolNormalDedicatedExt-r13	SEQUENCE {
						poolToReleaseListExt-r13			SL-TxPoolToReleaseListExt-r13 OPTIONAL,	-- Need ON
						poolToAddModListExt-r13				SL-CommTxPoolToAddModListExt-r13	OPTIONAL	-- Need ON
					}
				}
			}
		}																OPTIONAL,	-- Need ON
		commTxAllowRelayDedicated-r13		BOOLEAN			OPTIONAL	-- Need ON
	]]
}

LogicalChGroupInfoList-r13 ::=		SEQUENCE (SIZE (1..maxLCG-r13)) OF SL-PriorityList-r13

SL-CommTxPoolToAddModList-r12 ::=		SEQUENCE (SIZE (1..maxSL-TxPool-r12)) OF SL-CommTxPoolToAddMod-r12

SL-CommTxPoolToAddModListExt-r13 ::=	SEQUENCE (SIZE (1..maxSL-TxPool-v1310)) OF SL-CommTxPoolToAddModExt-r13

SL-CommTxPoolToAddMod-r12 ::=		SEQUENCE	{
	poolIdentity-r12					SL-TxPoolIdentity-r12,
	pool-r12							SL-CommResourcePool-r12
}

SL-CommTxPoolToAddModExt-r13 ::=		SEQUENCE	{
	poolIdentity-v1310					SL-TxPoolIdentity-v1310,
	pool-r13							SL-CommResourcePool-r12
}

MAC-MainConfigSL-r12 ::=		SEQUENCE	{
	periodic-BSR-TimerSL					PeriodicBSR-Timer-r12		OPTIONAL,	-- Need ON
	retx-BSR-TimerSL						RetxBSR-Timer-r12
}


SL-CommTxPoolList-r12 ::=		SEQUENCE (SIZE (1..maxSL-TxPool-r12)) OF SL-CommResourcePool-r12

SL-CommTxPoolListExt-r13 ::=	SEQUENCE (SIZE (1..maxSL-TxPool-v1310)) OF SL-CommResourcePool-r12

SL-CommTxPoolListV2X-r14 ::=		SEQUENCE (SIZE (1..maxSL-V2X-TxPool-r14)) OF SL-CommResourcePoolV2X-r14

SL-CommRxPoolList-r12 ::=		SEQUENCE (SIZE (1..maxSL-RxPool-r12)) OF SL-CommResourcePool-r12

SL-CommRxPoolListV2X-r14 ::=		SEQUENCE (SIZE (1..maxSL-V2X-RxPool-r14)) OF SL-CommResourcePoolV2X-r14

SL-CommResourcePool-r12 ::=		SEQUENCE {
	sc-CP-Len-r12						SL-CP-Len-r12,
	sc-Period-r12						SL-PeriodComm-r12,
	sc-TF-ResourceConfig-r12			SL-TF-ResourceConfig-r12,
	data-CP-Len-r12						SL-CP-Len-r12,
	dataHoppingConfig-r12				SL-HoppingConfigComm-r12,
	ue-SelectedResourceConfig-r12			SEQUENCE {
		data-TF-ResourceConfig-r12				SL-TF-ResourceConfig-r12,
		trpt-Subset-r12						SL-TRPT-Subset-r12	OPTIONAL	-- Need OP
	}																OPTIONAL,	-- Need OR
	rxParametersNCell-r12				SEQUENCE {
		tdd-Config-r12					TDD-Config					OPTIONAL,	-- Need OP
		syncConfigIndex-r12			INTEGER (0..15)
	}																OPTIONAL,	-- Need OR
	txParameters-r12					SEQUENCE {
		sc-TxParameters-r12				SL-TxParameters-r12,
		dataTxParameters-r12			SL-TxParameters-r12
	}																OPTIONAL,	-- Cond Tx
	...,
	[[	priorityList-r13				SL-PriorityList-r13			OPTIONAL	-- Cond Tx
	]]

}

SL-CommResourcePoolV2X-r14 ::=		SEQUENCE {
	sl-OffsetIndicator-r14				SL-OffsetIndicator-r12		OPTIONAL,	-- Need OR
	sl-Subframe-r14						SubframeBitmapSL-r14,
	adjacencyPSCCH-PSSCH-r14			BOOLEAN,
	sizeSubchannel-r14					ENUMERATED {
										n4, n5, n6, n8, n9, n10, n12, n15, n16, n18, n20, n25, n30,
										n48, n50, n72, n75, n96, n100, spare13, spare12, spare11,
										spare10, spare9, spare8, spare7, spare6, spare5, spare4,
										spare3, spare2, spare1},
	numSubchannel-r14					ENUMERATED {n1, n3, n5, n8, n10, n15, n20, spare1},
	startRB-Subchannel-r14				INTEGER (0..99),
	startRB-PSCCH-Pool-r14				INTEGER (0..99)				OPTIONAL,	-- Need OR
	rxParametersNCell-r14				SEQUENCE {
		tdd-Config-r14					TDD-Config					OPTIONAL,	-- Need OP
		syncConfigIndex-r14				INTEGER (0..15)
	}																OPTIONAL,	-- Need OR
	dataTxParameters-r14				SL-TxParameters-r12			OPTIONAL,	-- Cond Tx
	zoneID-r14							INTEGER (0..7)				OPTIONAL,	-- Need OR
	threshS-RSSI-CBR-r14					INTEGER (0..45)				OPTIONAL,	-- Need OR
	poolReportId-r14					SL-V2X-TxPoolReportIdentity-r14		OPTIONAL,	-- Need OR
	cbr-pssch-TxConfigList-r14			SL-CBR-PPPP-TxConfigList-r14	OPTIONAL,	-- Need OR
	resourceSelectionConfigP2X-r14		SL-P2X-ResourceSelectionConfig-r14	OPTIONAL,	-- Cond P2X
	syncAllowed-r14						SL-SyncAllowed-r14				OPTIONAL,	-- Need OR
	restrictResourceReservationPeriod-r14	SL-RestrictResourceReservationPeriodList-r14	OPTIONAL,	-- Need OR
	...
}

SL-TRPT-Subset-r12 ::=			BIT STRING (SIZE (3..5))

SL-V2X-TxPoolReportIdentity-r14::=		INTEGER (1..maxSL-PoolToMeasure-r14)


SL-CommTxPoolSensingConfig-r14 ::=		SEQUENCE {
	pssch-TxConfigList-r14					SL-PSSCH-TxConfigList-r14,
	thresPSSCH-RSRP-List-r14				SL-ThresPSSCH-RSRP-List-r14,
	restrictResourceReservationPeriod-r14	SL-RestrictResourceReservationPeriodList-r14	OPTIONAL,	-- Need OR
	probResourceKeep-r14				ENUMERATED {v0, v0dot2, v0dot4, v0dot6, v0dot8,
													spare3,spare2, spare1},
	p2x-SensingConfig-r14					SEQUENCE {
		minNumCandidateSF-r14				INTEGER (1..13),
		gapCandidateSensing-r14				BIT STRING (SIZE (10))
	}		OPTIONAL,	-- Need OR
	sl-ReselectAfter-r14				ENUMERATED {n1, n2, n3, n4, n5, n6, n7, n8, n9,
												spare7, spare6, spare5, spare4, spare3, spare2,
												spare1}				OPTIONAL		-- Need OR
}


SL-CP-Len-r12 ::=				ENUMERATED {normal, extended}


SL-DiscConfig-r12 ::=					SEQUENCE {
	discTxResources-r12						CHOICE {
		release								NULL,
		setup								CHOICE {
			scheduled-r12					SEQUENCE {
				discTxConfig-r12					SL-DiscResourcePool-r12	OPTIONAL, -- Need ON
				discTF-IndexList-r12				SL-TF-IndexPairList-r12	OPTIONAL, -- Need ON
				discHoppingConfig-r12				SL-HoppingConfigDisc-r12
														OPTIONAL	-- Need ON
			},
			ue-Selected-r12					SEQUENCE {
				discTxPoolDedicated-r12			SEQUENCE {
					poolToReleaseList-r12			SL-TxPoolToReleaseList-r12 OPTIONAL,	-- Need ON
					poolToAddModList-r12			SL-DiscTxPoolToAddModList-r12 OPTIONAL	-- Need ON
				}													OPTIONAL	-- Need ON
			}
		}
	}																OPTIONAL,	-- Need ON
	...,
	[[	discTF-IndexList-v1260				CHOICE {
			release								NULL,
			setup								SEQUENCE {
				discTF-IndexList-r12b				SL-TF-IndexPairList-r12b
			}
		}															OPTIONAL	-- Need ON
	]],
	[[	discTxResourcesPS-r13			CHOICE {
			release								NULL,
			setup								CHOICE {
				scheduled-r13						SL-DiscTxConfigScheduled-r13,
				ue-Selected-r13						SEQUENCE {
					discTxPoolPS-Dedicated-r13			SL-DiscTxPoolDedicated-r13
				}
			}
		}															OPTIONAL,	-- Need ON
		discTxInterFreqInfo-r13			CHOICE {
			release								NULL,
			setup								SEQUENCE {
				discTxCarrierFreq-r13				ARFCN-ValueEUTRA-r9			OPTIONAL,	-- Need OR
				discTxRefCarrierDedicated-r13		SL-DiscTxRefCarrierDedicated-r13	OPTIONAL,	-- Need OR
				discTxInfoInterFreqListAdd-r13			SL-DiscTxInfoInterFreqListAdd-r13	OPTIONAL	-- Need ON
			}
		}															OPTIONAL,	-- Need ON
		gapRequestsAllowedDedicated-r13		BOOLEAN			OPTIONAL,	-- Need ON
		discRxGapConfig-r13					CHOICE {
			release								NULL,
			setup								SL-GapConfig-r13
		}															OPTIONAL,	-- Need ON
		discTxGapConfig-r13					CHOICE {
			release								NULL,
			setup								SL-GapConfig-r13
		}															OPTIONAL,	-- Need ON
		discSysInfoToReportConfig-r13		CHOICE {
			release								NULL,
			setup								SL-DiscSysInfoToReportFreqList-r13
		}															OPTIONAL	-- Need ON
	]]
}

SL-DiscSysInfoToReportFreqList-r13 ::= SEQUENCE (SIZE (1..maxFreq)) OF ARFCN-ValueEUTRA-r9

SL-DiscTxInfoInterFreqListAdd-r13 ::=	SEQUENCE {
	discTxFreqToAddModList-r13				SEQUENCE (SIZE (1..maxFreq)) OF SL-DiscTxResourceInfoPerFreq-r13	OPTIONAL,	-- Need ON
	discTxFreqToReleaseList-r13				SEQUENCE (SIZE (1..maxFreq)) OF ARFCN-ValueEUTRA-r9	OPTIONAL,	-- Need ON
	...
}

SL-DiscTxResourceInfoPerFreq-r13 ::=	SEQUENCE	{
	discTxCarrierFreq-r13					ARFCN-ValueEUTRA-r9,
	discTxResources-r13						SL-DiscTxResource-r13	OPTIONAL,	-- Need OR
	discTxResourcesPS-r13					SL-DiscTxResource-r13	OPTIONAL,	-- Need OR
	discTxRefCarrierDedicated-r13			SL-DiscTxRefCarrierDedicated-r13	OPTIONAL,	-- Need OR
	discCellSelectionInfo-r13					CellSelectionInfoNFreq-r13			OPTIONAL,	-- Need OR
	...
}

SL-DiscTxResource-r13 ::=				CHOICE {
	release								NULL,
	setup								CHOICE {
		scheduled-r13					SL-DiscTxConfigScheduled-r13,
		ue-Selected-r13					SL-DiscTxPoolDedicated-r13
	}
}

SL-DiscTxPoolToAddModList-r12 ::=		SEQUENCE (SIZE (1..maxSL-TxPool-r12)) OF SL-DiscTxPoolToAddMod-r12

SL-DiscTxPoolToAddMod-r12 ::=		SEQUENCE	{
	poolIdentity-r12					SL-TxPoolIdentity-r12,
	pool-r12							SL-DiscResourcePool-r12
}

SL-DiscTxConfigScheduled-r13 ::=			SEQUENCE {
	discTxConfig-r13					SL-DiscResourcePool-r12	OPTIONAL, -- Need ON
	discTF-IndexList-r13				SL-TF-IndexPairList-r12b	OPTIONAL, -- Need ON
	discHoppingConfig-r13				SL-HoppingConfigDisc-r12	OPTIONAL,-- Need ON
	...
}

SL-DiscTxPoolDedicated-r13 ::=			SEQUENCE {
	poolToReleaseList-r13			SL-TxPoolToReleaseList-r12 OPTIONAL,	-- Need ON
	poolToAddModList-r13			SL-DiscTxPoolToAddModList-r12 OPTIONAL	-- Need ON
}

SL-TF-IndexPairList-r12 ::=		SEQUENCE (SIZE (1..maxSL-TF-IndexPair-r12)) OF SL-TF-IndexPair-r12

SL-TF-IndexPair-r12 ::=		SEQUENCE	{
	discSF-Index-r12					INTEGER (1.. 200)		OPTIONAL,	-- Need ON
	discPRB-Index-r12					INTEGER (1.. 50)		OPTIONAL	-- Need ON
}

SL-TF-IndexPairList-r12b ::=		SEQUENCE (SIZE (1..maxSL-TF-IndexPair-r12)) OF SL-TF-IndexPair-r12b

SL-TF-IndexPair-r12b ::=		SEQUENCE	{
	discSF-Index-r12b					INTEGER (0..209)		OPTIONAL,	-- Need ON
	discPRB-Index-r12b					INTEGER (0..49)			OPTIONAL	-- Need ON
}

SL-DiscTxRefCarrierDedicated-r13 ::=	CHOICE {
	pCell								NULL,
	sCell								SCellIndex-r10
}


SL-DiscTxPoolList-r12 ::=		SEQUENCE (SIZE (1..maxSL-TxPool-r12)) OF SL-DiscResourcePool-r12

SL-DiscRxPoolList-r12 ::=		SEQUENCE (SIZE (1..maxSL-RxPool-r12)) OF SL-DiscResourcePool-r12

SL-DiscResourcePool-r12 ::=		SEQUENCE	{
	cp-Len-r12						SL-CP-Len-r12,
	discPeriod-r12				ENUMERATED {rf32, rf64, rf128,
											rf256, rf512, rf1024, rf16-v1310, spare},
	numRetx-r12					INTEGER (0..3),
	numRepetition-r12				INTEGER (1..50),
	tf-ResourceConfig-r12			SL-TF-ResourceConfig-r12,
	txParameters-r12				SEQUENCE {
		txParametersGeneral-r12		SL-TxParameters-r12,
		ue-SelectedResourceConfig-r12	SEQUENCE {
			poolSelection-r12				CHOICE {
				rsrpBased-r12					SL-PoolSelectionConfig-r12,
				random-r12						NULL
			},
			txProbability-r12			ENUMERATED {p25, p50, p75, p100}
		}															OPTIONAL	-- Need OR
	}																OPTIONAL,	-- Cond Tx
	rxParameters-r12				SEQUENCE {
		tdd-Config-r12					TDD-Config					OPTIONAL,	-- Need OR
		syncConfigIndex-r12			INTEGER (0..15)
	}																OPTIONAL,	-- Need OR
	...,
	[[	discPeriod-v1310				CHOICE {
			release								NULL,
			setup								ENUMERATED {rf4, rf6, rf7, rf8,
													rf12, rf14, rf24, rf28}
			}														OPTIONAL,	-- Need ON
		rxParamsAddNeighFreq-r13		CHOICE {
			release							NULL,
			setup							SEQUENCE {
				physCellId-r13					PhysCellIdList-r13
			}
		}															OPTIONAL,	-- Need ON
		txParamsAddNeighFreq-r13		CHOICE {
			release							NULL,
			setup							SEQUENCE {
				physCellId-r13					PhysCellIdList-r13,
				p-Max							P-Max					OPTIONAL,	-- Need OP
				tdd-Config-r13					TDD-Config				OPTIONAL,	-- Cond TDD-OR
				tdd-Config-v1130				TDD-Config-v1130		OPTIONAL,	-- Cond TDD-OR
				freqInfo							SEQUENCE {
					ul-CarrierFreq						ARFCN-ValueEUTRA	OPTIONAL,	-- Need OP
					ul-Bandwidth						ENUMERATED {n6, n15, n25, n50, n75, n100}
																			OPTIONAL,	-- Need OP
				additionalSpectrumEmission			AdditionalSpectrumEmission
				},
				referenceSignalPower				INTEGER (-60..50),
				syncConfigIndex-r13				INTEGER (0..15)			OPTIONAL	-- Need OR
			}
		}															OPTIONAL	-- Need ON
	]],
	[[	txParamsAddNeighFreq-v1370		CHOICE {
			release							NULL,
			setup							SEQUENCE {
				freqInfo-v1370					SEQUENCE {
					additionalSpectrumEmission-v1370		AdditionalSpectrumEmission-v10l0
				}
			}
		}															OPTIONAL	-- Need ON
	]]
}

PhysCellIdList-r13	::=		SEQUENCE (SIZE (1.. maxSL-DiscCells-r13)) OF PhysCellId

SL-PoolSelectionConfig-r12 ::=		SEQUENCE {
	threshLow-r12							RSRP-RangeSL2-r12,
	threshHigh-r12							RSRP-RangeSL2-r12
}


SL-DiscSysInfoReport-r13 ::=	SEQUENCE {
	plmn-IdentityList-r13			PLMN-IdentityList			OPTIONAL,
	cellIdentity-13					CellIdentity				OPTIONAL,
	carrierFreqInfo-13				ARFCN-ValueEUTRA-r9			OPTIONAL,
	discRxResources-r13				SL-DiscRxPoolList-r12		OPTIONAL,
	discTxPoolCommon-r13			SL-DiscTxPoolList-r12		OPTIONAL,
	discTxPowerInfo-r13				SL-DiscTxPowerInfoList-r12	OPTIONAL,
	discSyncConfig-r13				SL-SyncConfigNFreq-r13		OPTIONAL,
	discCellSelectionInfo-r13		SEQUENCE {
		q-RxLevMin-r13					Q-RxLevMin,
		q-RxLevMinOffset-r13			INTEGER (1..8)			OPTIONAL
	}															OPTIONAL,
	cellReselectionInfo-r13			SEQUENCE {
		q-Hyst-r13						ENUMERATED {
												dB0, dB1, dB2, dB3, dB4, dB5, dB6, dB8, dB10,
												dB12, dB14, dB16, dB18, dB20, dB22, dB24},
		q-RxLevMin-r13					Q-RxLevMin,
		t-ReselectionEUTRA-r13			T-Reselection
	}															OPTIONAL,
	tdd-Config-r13					TDD-Config					OPTIONAL,
	freqInfo-r13					SEQUENCE {
		ul-CarrierFreq-r13				ARFCN-ValueEUTRA				OPTIONAL,
		ul-Bandwidth-r13				ENUMERATED {n6, n15, n25, n50, n75, n100}
																		OPTIONAL,
		additionalSpectrumEmission-r13	AdditionalSpectrumEmission		OPTIONAL
	}																OPTIONAL,
	p-Max-r13						P-Max	OPTIONAL,
	referenceSignalPower-r13		INTEGER (-60..50)	OPTIONAL,
	...,
	[[
	freqInfo-v1370					SEQUENCE {
		additionalSpectrumEmission-v1370	AdditionalSpectrumEmission-v10l0
	}																OPTIONAL
	]]
}


SL-DiscTxPowerInfoList-r12 ::=	SEQUENCE (SIZE (maxSL-DiscPowerClass-r12)) OF SL-DiscTxPowerInfo-r12

SL-DiscTxPowerInfo-r12 ::=				SEQUENCE	{
	discMaxTxPower-r12							P-Max,
	...
}


SL-GapConfig-r13 ::=				SEQUENCE {
	gapPatternList-r13				SL-GapPatternList-r13
}

SL-GapPatternList-r13 ::=	SEQUENCE (SIZE (1..maxSL-GP-r13)) OF SL-GapPattern-r13

SL-GapPattern-r13 ::=				SEQUENCE {
	gapPeriod-r13						ENUMERATED {sf40, sf60, sf70, sf80, sf120, sf140, sf160,
											sf240, sf280, sf320, sf640, sf1280, sf2560, sf5120,
											sf10240},
	gapOffset-r12						SL-OffsetIndicator-r12,
	gapSubframeBitmap-r13				BIT STRING (SIZE (1..10240)),
	...
}


SL-GapRequest-r13 ::=				SEQUENCE (SIZE (1..maxFreq)) OF SL-GapFreqInfo-r13

SL-GapFreqInfo-r13 ::=				SEQUENCE {
	carrierFreq-r13					ARFCN-ValueEUTRA-r9					OPTIONAL,
	gapPatternList-r13				SL-GapPatternList-r13
}


SL-HoppingConfigComm-r12 ::=		SEQUENCE	{
	hoppingParameter-r12				INTEGER (0..504),
	numSubbands-r12						ENUMERATED {ns1, ns2, ns4},
	rb-Offset-r12						INTEGER (0..110)
}

SL-HoppingConfigDisc-r12 ::=	SEQUENCE	{
	a-r12									INTEGER (1..200),
	b-r12									INTEGER (1..10),
	c-r12									ENUMERATED {n1, n5}
}


SL-InterFreqInfoListV2X-r14 ::=	SEQUENCE (SIZE (0..maxFreqV2X-1-r14)) OF SL-InterFreqInfoV2X-r14

SL-InterFreqInfoV2X-r14 ::=		SEQUENCE {
	plmn-IdentityList-r14				PLMN-IdentityList			OPTIONAL,		-- Need OP
	v2x-CommCarrierFreq-r14			ARFCN-ValueEUTRA-r9,
	sl-MaxTxPower-r14					P-Max				OPTIONAL,		-- Need OR
	sl-Bandwidth-r14					ENUMERATED {n6, n15, n25, n50, n75, n100}	OPTIONAL,	-- Need OR
	v2x-SchedulingPool-r14				SL-CommResourcePoolV2X-r14				OPTIONAL,	-- Need OR
	v2x-UE-ConfigList-r14		SL-V2X-UE-ConfigList-r14	OPTIONAL,	-- Need OR
	...,
	[[	additionalSpectrumEmissionV2X-r14		CHOICE {
			additionalSpectrumEmission-r14			AdditionalSpectrumEmission,
			additionalSpectrumEmission-v1440		AdditionalSpectrumEmission-v10l0
		}				OPTIONAL		-- Need ON
	]]
}


SL-V2X-UE-ConfigList-r14 ::=	SEQUENCE (SIZE (1.. maxCellIntra)) OF SL-V2X-InterFreqUE-Config-r14

SL-V2X-InterFreqUE-Config-r14 ::=		SEQUENCE {
	physCellIdList-r14					PhysCellIdList-r13					OPTIONAL,	-- Need OR
	typeTxSync-r14						SL-TypeTxSync-r14					OPTIONAL,	-- Need OR
	v2x-SyncConfig-r14					SL-SyncConfigListNFreqV2X-r14		OPTIONAL,	-- Need OR
	v2x-CommRxPool-r14					SL-CommRxPoolListV2X-r14				OPTIONAL,	-- Need OR
	v2x-CommTxPoolNormal-r14				SL-CommTxPoolListV2X-r14				OPTIONAL,	-- Need OR
	p2x-CommTxPoolNormal-r14				SL-CommTxPoolListV2X-r14				OPTIONAL,	-- Need OR
	v2x-CommTxPoolExceptional-r14		SL-CommResourcePoolV2X-r14			OPTIONAL,	-- Need OR
	v2x-ResourceSelectionConfig-r14		SL-CommTxPoolSensingConfig-r14		OPTIONAL,	-- Need OR
	zoneConfig-r14						SL-ZoneConfig-r14					OPTIONAL,	-- Need OR
	offsetDFN-r14						INTEGER (0..1000)					OPTIONAL,	-- Need OR
	...
}


SL-OffsetIndicator-r12 ::=			CHOICE {
	small-r12								INTEGER (0..319),
	large-r12								INTEGER (0..10239)
}

SL-OffsetIndicatorSync-r12 ::=			INTEGER (0..39)

SL-OffsetIndicatorSync-v1430 ::=		INTEGER (40..159)

SL-OffsetIndicatorSync-r14 ::=			INTEGER (0..159)


SL-P2X-ResourceSelectionConfig-r14 ::=			SEQUENCE {
	partialSensing-r14				ENUMERATED {true}				OPTIONAL,	-- Need OR
	randomSelection-r14				ENUMERATED {true}				OPTIONAL	-- Need OR
}


SL-PeriodComm-r12 ::=					ENUMERATED {sf40, sf60, sf70, sf80, sf120, sf140,
												sf160, sf240, sf280, sf320, spare6, spare5,
												spare4, spare3, spare2, spare}


SL-PriorityList-r13 ::=		SEQUENCE (SIZE (1..maxSL-Prio-r13)) OF SL-Priority-r13

SL-Priority-r13 ::=			INTEGER (1..8)


SL-PSSCH-TxConfigList-r14 ::=	SEQUENCE (SIZE (1..maxPSSCH-TxConfig-r14)) OF SL-PSSCH-TxConfig-r14

SL-PSSCH-TxConfig-r14 ::=		SEQUENCE {
	typeTxSync-r14				SL-TypeTxSync-r14		OPTIONAL,	-- Need OR
	thresUE-Speed-r14			ENUMERATED {kmph60, kmph80, kmph100, kmph120,
								kmph140, kmph160, kmph180, kmph200},
	parametersAboveThres-r14	SL-PSSCH-TxParameters-r14,
	parametersBelowThres-r14	SL-PSSCH-TxParameters-r14,
	...
}

SL-PSSCH-TxParameters-r14 ::=		SEQUENCE {
	minMCS-PSSCH-r14			INTEGER (0..31),
	maxMCS-PSSCH-r14			INTEGER (0..31),
	minSubChannel-NumberPSSCH-r14		INTEGER (1..20),
	maxSubchannel-NumberPSSCH-r14		INTEGER (1..20),
	allowedRetxNumberPSSCH-r14	ENUMERATED {n0, n1, both, spare1},
	maxTxPower-r14				SL-TxPower-r14				OPTIONAL			-- Cond CBR
}


SL-RestrictResourceReservationPeriodList-r14 ::=	SEQUENCE (SIZE (1..maxReservationPeriod-r14)) OF SL-RestrictResourceReservationPeriod-r14

SL-RestrictResourceReservationPeriod-r14 ::=		ENUMERATED {v0dot2, v0dot5, v1, v2, v3, v4, v5, v6, v7, v8, v9, v10, spare4,spare3, spare2, spare1}


SLSSID-r12 ::=					INTEGER (0..167)


SL-SyncAllowed-r14 ::=		SEQUENCE {
	gnss-Sync-r14						ENUMERATED {true}				OPTIONAL,	-- Need OR
	enb-Sync-r14						ENUMERATED {true}				OPTIONAL,	-- Need OR
	ue-Sync-r14							ENUMERATED {true}				OPTIONAL	-- Need OR
}


SL-SyncConfigList-r12 ::=		SEQUENCE (SIZE (1..maxSL-SyncConfig-r12)) OF SL-SyncConfig-r12

SL-SyncConfigListV2X-r14 ::=	SEQUENCE (SIZE (1.. maxSL-V2X-SyncConfig-r14)) OF SL-SyncConfig-r12

SL-SyncConfig-r12 ::=					SEQUENCE {
	syncCP-Len-r12							SL-CP-Len-r12,
	syncOffsetIndicator-r12				SL-OffsetIndicatorSync-r12,
	slssid-r12								SLSSID-r12,
	txParameters-r12							SEQUENCE {
		syncTxParameters-r12					SL-TxParameters-r12,
		syncTxThreshIC-r12						RSRP-RangeSL-r12,
		syncInfoReserved-r12						BIT STRING (SIZE (19))	OPTIONAL	-- Need OR
	}																	OPTIONAL,	-- Need OR
	rxParamsNCell-r12						SEQUENCE {
		physCellId-r12							PhysCellId,
		discSyncWindow-r12				ENUMERATED {w1, w2}
	}																	OPTIONAL,	-- Need OR
	...,
	[[	syncTxPeriodic-r13					ENUMERATED {true}			OPTIONAL	-- Need OR
	]],
	[[	syncOffsetIndicator-v1430		SL-OffsetIndicatorSync-v1430		OPTIONAL,	-- Need OR
		gnss-Sync-r14					ENUMERATED {true}				OPTIONAL	-- Need OR
	]],
	[[	syncOffsetIndicator2-r14		SL-OffsetIndicatorSync-r14	OPTIONAL,	-- Need OR
		syncOffsetIndicator3-r14		SL-OffsetIndicatorSync-r14	OPTIONAL		-- Need OR
	]]
}

SL-SyncConfigListNFreq-r13 ::=		SEQUENCE (SIZE (1..maxSL-SyncConfig-r12)) OF SL-SyncConfigNFreq-r13

SL-SyncConfigListNFreqV2X-r14 ::=		SEQUENCE (SIZE (1..maxSL-V2X-SyncConfig-r14)) OF SL-SyncConfigNFreq-r13

SL-SyncConfigNFreq-r13 ::=			SEQUENCE {
	asyncParameters-r13					SEQUENCE {
		syncCP-Len-r13						SL-CP-Len-r12,
		syncOffsetIndicator-r13				SL-OffsetIndicatorSync-r12,
		slssid-r13							SLSSID-r12
	}																OPTIONAL,	-- Need OR
	txParameters-r13					SEQUENCE {
		syncTxParameters-r13				SL-TxParameters-r12,
		syncTxThreshIC-r13					RSRP-RangeSL-r12,
		syncInfoReserved-r13					BIT STRING (SIZE (19))	OPTIONAL,	-- Need OR
		syncTxPeriodic-r13					ENUMERATED {true}		OPTIONAL	-- Need OR
	}																OPTIONAL,	-- Need OR
	rxParameters-r13					SEQUENCE {
		discSyncWindow-r13					ENUMERATED {w1, w2}
	}																	OPTIONAL,	-- Need OR
	...,
	[[	syncOffsetIndicator-v1430		SL-OffsetIndicatorSync-v1430	OPTIONAL,	-- Need OR
		gnss-Sync-r14					ENUMERATED {true}				OPTIONAL	-- Need OR
	]],
	[[	syncOffsetIndicator2-r14		SL-OffsetIndicatorSync-r14	OPTIONAL,	-- Need OR
		syncOffsetIndicator3-r14		SL-OffsetIndicatorSync-r14	OPTIONAL		-- Need OR
	]]
}


SL-TF-ResourceConfig-r12 ::=		SEQUENCE	{
	prb-Num-r12							INTEGER (1..100),
	prb-Start-r12						INTEGER (0..99),
	prb-End-r12							INTEGER (0..99),
	offsetIndicator-r12					SL-OffsetIndicator-r12,
	subframeBitmap-r12					SubframeBitmapSL-r12
}

SubframeBitmapSL-r12 ::=		CHOICE {
	bs4-r12									BIT STRING (SIZE (4)),
	bs8-r12									BIT STRING (SIZE (8)),
	bs12-r12								BIT STRING (SIZE (12)),
	bs16-r12								BIT STRING (SIZE (16)),
	bs30-r12								BIT STRING (SIZE (30)),
	bs40-r12								BIT STRING (SIZE (40)),
	bs42-r12								BIT STRING (SIZE (42))
}

SubframeBitmapSL-r14 ::=		CHOICE {
	bs10-r14								BIT STRING (SIZE (10)),
	bs16-r14								BIT STRING (SIZE (16)),
	bs20-r14								BIT STRING (SIZE (20)),
	bs30-r14								BIT STRING (SIZE (30)),
	bs40-r14								BIT STRING (SIZE (40)),
	bs50-r14								BIT STRING (SIZE (50)),
	bs60-r14								BIT STRING (SIZE (60)),
	bs100-r14								BIT STRING (SIZE (100))
}


SL-TxPower-r14 ::=		CHOICE {
	minusinfinity-r14				NULL,
	txPower-r14						INTEGER (-41..31)
}


SL-TypeTxSync-r14 ::=		ENUMERATED {gnss, enb, ue}


SL-ThresPSSCH-RSRP-List-r14 ::=	SEQUENCE (SIZE (64)) OF SL-ThresPSSCH-RSRP-r14

SL-ThresPSSCH-RSRP-r14 ::=		INTEGER (0..66)


SL-TxParameters-r12 ::=				SEQUENCE	{
	alpha-r12								Alpha-r12,
	p0-r12									P0-SL-r12
}

P0-SL-r12 ::=							INTEGER (-126..31)


SL-TxPoolIdentity-r12 ::=			INTEGER (1.. maxSL-TxPool-r12)

SL-TxPoolIdentity-v1310 ::=		INTEGER (maxSL-TxPool-r12Plus1-r13.. maxSL-TxPool-r13)

SL-V2X-TxPoolIdentity-r14 ::=		INTEGER (1.. maxSL-V2X-TxPool-r14)


SL-TxPoolToReleaseList-r12 ::=	SEQUENCE (SIZE (1..maxSL-TxPool-r12)) OF SL-TxPoolIdentity-r12

SL-TxPoolToReleaseListExt-r13 ::=	SEQUENCE (SIZE (1..maxSL-TxPool-v1310)) OF SL-TxPoolIdentity-v1310


SL-V2X-ConfigDedicated-r14 ::=				SEQUENCE	{
	commTxResources-r14					CHOICE {
		release								NULL,
		setup								CHOICE {
			scheduled-r14					SEQUENCE {
				sl-V-RNTI-r14			C-RNTI,
				mac-MainConfig-r14				MAC-MainConfigSL-r12,
				v2x-SchedulingPool-r14			SL-CommResourcePoolV2X-r14	OPTIONAL,	-- Need ON
				mcs-r14							INTEGER (0..31)				OPTIONAL,	-- Need OR
				logicalChGroupInfoList-r14		LogicalChGroupInfoList-r13
			},
			ue-Selected-r14					SEQUENCE {
				-- Pool for normal usage
				v2x-CommTxPoolNormalDedicated-r14	SEQUENCE {
					poolToReleaseList-r14	SL-TxPoolToReleaseListV2X-r14	OPTIONAL,	-- Need ON
					poolToAddModList-r14		SL-TxPoolToAddModListV2X-r14		OPTIONAL,	-- Need ON
					v2x-CommTxPoolSensingConfig-r14		SL-CommTxPoolSensingConfig-r14
																			OPTIONAL	-- Need ON
				}
			}
		}
	}																		OPTIONAL,	-- Need ON
	v2x-InterFreqInfoList-r14			SL-InterFreqInfoListV2X-r14			OPTIONAL,	-- Need ON
	thresSL-TxPrioritization-r14			SL-Priority-r13						OPTIONAL,	-- Need OR
	typeTxSync-r14						SL-TypeTxSync-r14					OPTIONAL,	-- Need OR
	cbr-DedicatedTxConfigList-r14		SL-CBR-CommonTxConfigList-r14	OPTIONAL,	-- Need OR
	...
}

SL-TxPoolToAddModListV2X-r14 ::=		SEQUENCE (SIZE (1.. maxSL-V2X-TxPool-r14)) OF SL-TxPoolToAddMod-r14

SL-TxPoolToAddMod-r14 ::=   SEQUENCE	{
	poolIdentity-r14					SL-V2X-TxPoolIdentity-r14,
	pool-r14							SL-CommResourcePoolV2X-r14
}

SL-TxPoolToReleaseListV2X-r14 ::=	SEQUENCE (SIZE (1.. maxSL-V2X-TxPool-r14)) OF SL-V2X-TxPoolIdentity-r14


SL-ZoneConfig-r14 ::=		SEQUENCE {
	zoneLength-r14	ENUMERATED { m5, m10, m20, m50, m100, m200, m500, spare1},
	zoneWidth-r14	ENUMERATED { m5, m10, m20, m50, m100, m200, m500, spare1},
	zoneIdLongiMod-r14	INTEGER (1..4),
	zoneIdLatiMod-r14	INTEGER (1..4)
}


maxACDC-Cat-r13				INTEGER ::=	16	-- Maximum number of ACDC categories (per PLMN)
maxAvailNarrowBands-r13		INTEGER ::=	16	-- Maximum number of narrowbands
maxBandComb-r10				INTEGER ::=	128	-- Maximum number of band combinations.
maxBandComb-r11				INTEGER ::=	256	-- Maximum number of additional band combinations.
maxBandComb-r13				INTEGER ::=	384 -- Maximum number of band combinations in Rel-13
maxBands					INTEGER ::= 64	-- Maximum number of bands listed in EUTRA UE caps
maxBandwidthClass-r10		INTEGER ::=	16	-- Maximum number of supported CA BW classes per band
maxBandwidthCombSet-r10		INTEGER ::=	32	-- Maximum number of bandwidth combination sets per
											-- supported band combination
maxCBR-Level-r14			INTEGER ::= 16	-- Maximum number of CBR levels
maxCBR-Level-1-r14			INTEGER ::= 15
maxCBR-Report-r14			INTEGER ::= 72	-- Maximum number of CBR results in a report
maxCDMA-BandClass			INTEGER ::= 32	-- Maximum value of the CDMA band classes
maxCE-Level-r13				INTEGER ::=	4	-- Maximum number of CE levels
maxCellBlack				INTEGER ::= 16	-- Maximum number of blacklisted physical cell identity
											-- ranges listed in SIB type 4 and 5
maxCellHistory-r12			INTEGER ::= 16	-- Maximum number of visited EUTRA cells reported
maxCellInfoGERAN-r9		INTEGER ::=	32	-- Maximum number of GERAN cells for which system in-
											-- formation can be provided as redirection assistance
maxCellInfoUTRA-r9			INTEGER ::=	16	-- Maximum number of UTRA cells for which system
											-- information can be provided as redirection
											-- assistance
maxCombIDC-r11				INTEGER ::= 128	-- Maximum number of reported UL CA combinations
maxCSI-IM-r11				INTEGER ::= 3	-- Maximum number of CSI-IM configurations
											-- (per carrier frequency)
maxCSI-IM-r12				INTEGER ::= 4	-- Maximum number of CSI-IM configurations
											-- (per carrier frequency)
minCSI-IM-r13				INTEGER ::= 5	-- Minimum number of CSI IM configurations from which
											-- REL-13 extension is used
maxCSI-IM-r13				INTEGER ::= 24	-- Maximum number of CSI-IM configurations
											-- (per carrier frequency)
maxCSI-IM-v1310				INTEGER ::= 20	-- Maximum number of additional CSI-IM configurations
											--  (per carrier frequency)
maxCSI-Proc-r11				INTEGER ::= 4	-- Maximum number of CSI processes (per carrier
											--  frequency)
maxCSI-RS-NZP-r11			INTEGER ::= 3	-- Maximum number of CSI RS resource
											--  configurations using non-zero Tx power
											--  (per carrier frequency)
minCSI-RS-NZP-r13			INTEGER ::= 4	-- Minimum number of CSI RS resource from which
											-- REL-13 extension is used
maxCSI-RS-NZP-r13			INTEGER ::= 24	-- Maximum number of CSI RS resource
											--  configurations using non-zero Tx power
											--  (per carrier frequency)
maxCSI-RS-NZP-v1310			INTEGER ::= 21	-- Maximum number of additional CSI RS resource
											--  configurations using non-zero Tx power
											--  (per carrier frequency)
maxCSI-RS-ZP-r11			INTEGER ::= 4	-- Maximum number of CSI RS resource
											--  configurations using zero Tx power(per carrier
											--  frequency)
maxCQI-ProcExt-r11			INTEGER ::= 3	-- Maximum number of additional periodic CQI
											-- configurations (per carrier frequency)
maxFreqUTRA-TDD-r10			INTEGER ::=	6	-- Maximum number of UTRA TDD carrier frequencies for
											-- which system information can be provided as
											-- redirection assistance
maxCellInter				INTEGER ::= 16	-- Maximum number of neighbouring inter-frequency
											-- cells listed in SIB type 5
maxCellIntra				INTEGER ::= 16	-- Maximum number of neighbouring intra-frequency
											-- cells listed in SIB type 4
maxCellListGERAN			INTEGER ::= 3	-- Maximum number of lists of GERAN cells
maxCellMeas					INTEGER ::= 32	-- Maximum number of entries in each of the
											-- cell lists in a measurement object
maxCellReport				INTEGER ::= 8	-- Maximum number of reported cells/CSI-RS resources
maxConfigSPS-r14			INTEGER ::= 8	-- Maximum number of simultaneous SPS configurations
maxCSI-RS-Meas-r12			INTEGER ::= 96	-- Maximum number of entries in the CSI-RS list
											-- in a measurement object
maxDRB						INTEGER ::= 11	-- Maximum number of Data Radio Bearers
maxDS-Duration-r12			INTEGER ::= 5	-- Maximum number of subframes in a discovery signals
											-- occasion
maxDS-ZTP-CSI-RS-r12		INTEGER ::= 5	-- Maximum number of zero transmission power CSI-RS for
											-- a serving cell concerning discovery signals
maxEARFCN					INTEGER ::= 65535	-- Maximum value of EUTRA carrier frequency
maxEARFCN-Plus1				INTEGER ::= 65536	-- Lowest value extended EARFCN range
maxEARFCN2					INTEGER ::= 262143	-- Highest value extended EARFCN range
maxEPDCCH-Set-r11			INTEGER ::= 2	-- Maximum number of EPDCCH sets
maxFBI						INTEGER ::= 64	-- Maximum value of fequency band indicator
maxFBI-Plus1					INTEGER ::= 65	-- Lowest value extended FBI range
maxFBI2						INTEGER ::= 256	-- Highest value extended FBI range
maxFreq						INTEGER ::= 8	-- Maximum number of carrier frequencies
maxFreqIDC-r11				INTEGER ::= 32	-- Maximum number of carrier frequencies that are
											-- affected by the IDC problems
maxFreqMBMS-r11				INTEGER ::= 5	-- Maximum number of carrier frequencies for which an
											-- MBMS capable UE may indicate an interest
maxFreqV2X-r14				INTEGER ::= 8	-- Maximum number of carrier frequencies for which V2X
											-- sidelink communication can be configured
maxFreqV2X-1-r14				INTEGER ::= 7	-- Highest index of frequencies
maxGERAN-SI					INTEGER ::= 10	-- Maximum number of GERAN SI blocks that can be
											-- provided as part of NACC information
maxGNFG						INTEGER ::= 16	-- Maximum number of GERAN neighbour freq groups
maxLCG-r13					INTEGER ::= 4	-- Maximum number of logical channel groups
maxLogMeasReport-r10		INTEGER ::= 520	-- Maximum number of logged measurement entries
											--  that can be reported by the UE in one message
maxMBSFN-Allocations		INTEGER ::= 8	-- Maximum number of MBSFN frame allocations with
											-- different offset
maxMBSFN-Area				INTEGER ::= 8
maxMBSFN-Area-1				INTEGER ::= 7
maxMBMS-ServiceListPerUE-r13	INTEGER ::= 15	-- Maximum number of services which the UE can
										-- include in the MBMS interest indication
maxMeasId					INTEGER ::= 32
maxMeasId-Plus1			INTEGER ::= 33
maxMeasId-r12				INTEGER ::= 64
maxMultiBands				INTEGER ::= 8	-- Maximum number of additional frequency bands
											-- that a cell belongs to
maxNS-Pmax-r10				INTEGER ::= 8	-- Maximum number of NS and P-Max values per band
maxNAICS-Entries-r12			INTEGER ::= 8	-- Maximum number of supported NAICS combination(s)
maxNeighCell-r12				INTEGER ::= 8	-- Maximum number of neighbouring cells in NAICS
											-- configuration (per carrier frequency)
maxNeighCell-SCPTM-r13		INTEGER ::=	8	-- Maximum number of SCPTM neighbour cells
maxObjectId					INTEGER ::= 32
maxObjectId-Plus1-r13		INTEGER ::= 33
maxObjectId-r13				INTEGER ::= 64
maxP-a-PerNeighCell-r12		INTEGER ::= 3	-- Maximum number of power offsets for a neighbour cell
											-- in NAICS configuration
maxPageRec					INTEGER ::= 16	--
maxPhysCellIdRange-r9		INTEGER ::= 4	-- Maximum number of physical cell identity ranges
maxPLMN-r11					INTEGER ::=	6	-- Maximum number of PLMNs
maxPLMN-1-r14				INTEGER ::=	5	-- Maximum number of PLMNs minus one
maxPNOffset					INTEGER ::=	511	-- Maximum number of CDMA2000 PNOffsets
maxPMCH-PerMBSFN			INTEGER ::= 15
maxPSSCH-TxConfig-r14		INTEGER ::= 16	-- Maximum number of PSSCH TX configurations
maxQCI-r13					INTEGER ::= 6	-- Maximum number of QCIs
maxRAT-Capabilities			INTEGER ::= 8	-- Maximum number of interworking RATs (incl EUTRA)
maxRE-MapQCL-r11			INTEGER ::= 4	-- Maximum number of PDSCH RE Mapping configurations
											--  (per carrier frequency)
maxReportConfigId			INTEGER ::= 32
maxReservationPeriod-r14	INTEGER ::= 16	-- Maximum number of resource reservation periodicities
											--  for sidelink V2X communication
maxRSTD-Freq-r10			INTEGER ::= 3	-- Maximum number of frequency layers for RSTD
											-- measurement
maxSAI-MBMS-r11				INTEGER ::= 64	-- Maximum number of MBMS service area identities
											-- broadcast per carrier frequency
maxSCell-r10				INTEGER ::= 4	-- Maximum number of SCells
maxSCell-r13				INTEGER ::= 31	-- Highest value of extended number range of SCells
maxSC-MTCH-r13				INTEGER ::= 1023	-- Maximum number of SC-MTCHs in one cell
maxSC-MTCH-BR-r14			INTEGER ::= 128	-- Maximum number of SC-MTCHs in one cell for feMTC
maxSL-CommRxPoolNFreq-r13	INTEGER ::= 32	-- Maximum number of individual sidelink communication
											-- Rx resource pools on neighbouring freq
maxSL-CommRxPoolPreconf-v1310	INTEGER ::= 12	-- Maximum number of additional preconfigured
												-- sidelink communication Rx resource pool entries
maxSL-TxPool-r12Plus1-r13	INTEGER ::= 5	-- First additional individual sidelink
												-- Tx resource pool
maxSL-TxPool-v1310			INTEGER ::= 4	-- Maximum number of additional sidelink
												-- Tx resource pool entries
maxSL-TxPool-r13			INTEGER ::= 8	-- Maximum number of individual sidelink
												-- Tx resource pools
maxSL-CommTxPoolPreconf-v1310	INTEGER ::= 7	-- Maximum number of additional preconfigured
												-- sidelink Tx resource pool entries
maxSL-Dest-r12			INTEGER ::= 16			-- Maximum number of sidelink destinations
maxSL-DiscCells-r13		INTEGER ::= 16			-- Maximum number of cells with similar sidelink
												-- configurations
maxSL-DiscPowerClass-r12	INTEGER ::= 3		-- Maximum number of sidelink power classes
maxSL-DiscRxPoolPreconf-r13		INTEGER ::= 16	-- Maximum number of preconfigured sidelink
												-- discovery Rx resource pool entries
maxSL-DiscSysInfoReportFreq-r13	INTEGER ::= 8	-- Maximum number of frequencies to include in a
												-- SidelinkUEInformation for SI reporting
maxSL-DiscTxPoolPreconf-r13		INTEGER ::= 4	-- Maximum number of preconfigured sidelink
												-- discovery Tx resource pool entries
maxSL-GP-r13			INTEGER ::= 8	-- Maximum number of gap patterns that can be requested
										-- for a frequency or assigned
maxSL-PoolToMeasure-r14	INTEGER ::= 72	-- Maximum number of TX resource pools for CBR
												-- measurement and report
maxSL-Prio-r13			INTEGER ::= 8	-- Maximum number of entries in sidelink priority list
maxSL-RxPool-r12			INTEGER ::= 16	-- Maximum number of individual sidelink Rx resource pools
maxSL-SyncConfig-r12		INTEGER ::= 16	-- Maximum number of sidelink Sync configurations
maxSL-TF-IndexPair-r12	INTEGER ::= 64	-- Maximum number of sidelink Time Freq resource index
											--  pairs
maxSL-TxPool-r12			INTEGER ::= 4	-- Maximum number of individual sidelink Tx resource pools
maxSL-V2X-RxPool-r14		INTEGER ::= 16	-- Maximum number of RX resource pools for
												-- V2X sidelink communication
maxSL-V2X-RxPoolPreconf-r14	INTEGER ::= 16		-- Maximum number of RX resource pools for
												-- V2X sidelink communication
maxSL-V2X-TxPool-r14		INTEGER ::= 8	-- Maximum number of TX resource pools for
												-- V2X sidelink communication
maxSL-V2X-TxPoolPreconf-r14	INTEGER ::= 8		-- Maximum number of TX resource pools for
												-- V2X sidelink communication
maxSL-V2X-SyncConfig-r14	INTEGER ::= 16	-- Maximum number of sidelink Sync configurations
												-- for V2X sidelink communication
maxSL-V2X-CBRConfig-r14		INTEGER ::= 4	-- Maximum number of CBR range configurations
												-- for V2X sidelink communication congestion
												-- control
maxSL-V2X-CBRConfig-1-r14	INTEGER ::= 3
maxSL-V2X-TxConfig-r14		INTEGER ::= 64	-- Maximum number of TX parameter configurations
												-- for V2X sidelink communication congestion
												-- control
maxSL-V2X-TxConfig-1-r14	INTEGER ::= 63
maxSL-V2X-CBRConfig2-r14		INTEGER ::= 8	-- Maximum number of CBR range configurations in
												-- pre-configuration for V2X sidelink
												-- communication congestion control
maxSL-V2X-CBRConfig2-1-r14	INTEGER ::= 7
maxSL-V2X-TxConfig2-r14		INTEGER ::= 128	-- Maximum number of TX parameter
												-- configurations in pre-configuration for V2X
												-- sidelink communication congestion control
maxSL-V2X-TxConfig2-1-r14	INTEGER ::= 127
maxSTAG-r11					INTEGER ::= 3	-- Maximum number of STAGs
maxServCell-r10				INTEGER ::= 5	-- Maximum number of Serving cells
maxServCell-r13				INTEGER ::= 32	-- Highest value of extended number range of Serving cells
maxServiceCount			INTEGER ::= 16	-- Maximum number of MBMS services that can be included
											--  in an MBMS counting request and response
maxServiceCount-1			INTEGER ::= 15
maxSessionPerPMCH			INTEGER ::= 29
maxSessionPerPMCH-1			INTEGER ::= 28
maxSIB						INTEGER ::= 32	-- Maximum number of SIBs
maxSIB-1					INTEGER ::= 31
maxSI-Message				INTEGER ::= 32	-- Maximum number of SI messages
maxSimultaneousBands-r10	INTEGER ::= 64	-- Maximum number of simultaneously aggregated bands
maxSubframePatternIDC-r11	INTEGER ::= 8	-- Maximum number of subframe reservation patterns
											-- that the UE can simultaneously recommend to the
											-- E-UTRAN for use.
maxTrafficPattern-r14		INTEGER ::= 8	-- Maximum number of periodical traffic patterns
											-- that the UE can simultaneously report to the
											-- E-UTRAN.
maxUTRA-FDD-Carrier			INTEGER ::= 16	-- Maximum number of UTRA FDD carrier frequencies
maxUTRA-TDD-Carrier			INTEGER ::= 16	-- Maximum number of UTRA TDD carrier frequencies
maxWLAN-Id-r12				INTEGER ::=	16	-- Maximum number of WLAN identifiers
maxWLAN-Bands-r13			INTEGER ::= 8	-- Maximum number of WLAN bands
maxWLAN-Id-r13				INTEGER ::= 32	-- Maximum number of WLAN identifiers
maxWLAN-Channels-r13		INTEGER ::= 16	-- maximum number of WLAN channels used in
											-- WLAN-CarrierInfo
maxWLAN-CarrierInfo-r13	INTEGER ::= 8	-- Maximum number of WLAN Carrier Information
maxWLAN-Id-Report-r14		INTEGER ::= 32	-- Maximum number of WLAN IDs to report


END


PC5-RRC-Definitions DEFINITIONS AUTOMATIC TAGS ::=

BEGIN

IMPORTS
	TDD-ConfigSL-r12
FROM EUTRA-RRC-Definitions;


SBCCH-SL-BCH-Message ::= SEQUENCE {
	message					SBCCH-SL-BCH-MessageType
}

SBCCH-SL-BCH-MessageType ::=						MasterInformationBlock-SL


SBCCH-SL-BCH-Message-V2X-r14 ::= SEQUENCE {
	message					SBCCH-SL-BCH-MessageType-V2X-r14
}

SBCCH-SL-BCH-MessageType-V2X-r14 ::=				MasterInformationBlock-SL-V2X-r14


MasterInformationBlock-SL ::=		SEQUENCE {
	sl-Bandwidth-r12					ENUMERATED {
											n6, n15, n25, n50, n75, n100},
	tdd-ConfigSL-r12					TDD-ConfigSL-r12,
	directFrameNumber-r12				BIT STRING (SIZE (10)),
	directSubframeNumber-r12			INTEGER (0..9),
	inCoverage-r12						BOOLEAN,
	reserved-r12						BIT STRING (SIZE (19))
}



MasterInformationBlock-SL-V2X-r14 ::=		SEQUENCE {
	sl-Bandwidth-r14					ENUMERATED {
											n6, n15, n25, n50, n75, n100},
	tdd-ConfigSL-r14					TDD-ConfigSL-r12,
	directFrameNumber-r14				BIT STRING (SIZE (10)),
	directSubframeNumber-r14			INTEGER (0..9),
	inCoverage-r14						BOOLEAN,
	reserved-r14						BIT STRING (SIZE (27))
}



END


NBIOT-RRC-Definitions DEFINITIONS AUTOMATIC TAGS ::=

BEGIN

IMPORTS
	RRCConnectionReestablishmentReject,
	SecurityModeCommand,
	SecurityModeComplete,
	SecurityModeFailure,
	AdditionalSpectrumEmission,
	ARFCN-ValueEUTRA-r9,
	CellIdentity,
	DedicatedInfoNAS,
	DRB-Identity,
	InitialUE-Identity,
	IntraFreqBlackCellList,
	IntraFreqNeighCellList,
	maxBands,
	maxCellBlack,
	maxCellInter,
	maxFBI2,
	maxFreq,
	maxMultiBands,
	maxPageRec,
	maxPLMN-r11,
	maxSAI-MBMS-r11,
	maxSIB,
	maxSIB-1,
	MBMS-SAI-r11,
	MBMS-SAI-List-r11,
	MBMSSessionInfo-r13,
	NextHopChainingCount,
	PagingUE-Identity,
	PLMN-Identity,
	P-Max,
	PowerRampingParameters,
	PreambleTransMax,
	PhysCellId,
	Q-OffsetRange,
	Q-QualMin-r9,
	Q-RxLevMin,
	ReestabUE-Identity,
	RegisteredMME,
	ReselectionThreshold,
	ResumeIdentity-r13,
	RRC-TransactionIdentifier,
	RSRP-Range,
	ShortMAC-I,
	S-TMSI,
	SystemInformationBlockType16-r11,
	SystemInfoValueTagSI-r13,
	T-Reordering,
	TimeAlignmentTimer,
	TMGI-r9,
	TrackingAreaCode,
	DataInactivityTimer-r14

FROM EUTRA-RRC-Definitions;


BCCH-BCH-Message-NB ::= SEQUENCE {
	message					BCCH-BCH-MessageType-NB
}


BCCH-BCH-MessageType-NB::=	MasterInformationBlock-NB



BCCH-DL-SCH-Message-NB ::= SEQUENCE {
	message					BCCH-DL-SCH-MessageType-NB
}

BCCH-DL-SCH-MessageType-NB ::= CHOICE {
	c1						CHOICE {
		systemInformation-r13				SystemInformation-NB,
		systemInformationBlockType1-r13		SystemInformationBlockType1-NB
	},
	messageClassExtension	SEQUENCE {}
}


PCCH-Message-NB ::= SEQUENCE {
	message					PCCH-MessageType-NB
}

PCCH-MessageType-NB ::= CHOICE {
	c1						CHOICE {
		paging-r13							Paging-NB
	},
	messageClassExtension	SEQUENCE {}
}


DL-CCCH-Message-NB ::= SEQUENCE {
	message					DL-CCCH-MessageType-NB
}

DL-CCCH-MessageType-NB ::= CHOICE {
	c1						CHOICE {
		rrcConnectionReestablishment-r13		RRCConnectionReestablishment-NB,
		rrcConnectionReestablishmentReject-r13	RRCConnectionReestablishmentReject,
		rrcConnectionReject-r13					RRCConnectionReject-NB,
		rrcConnectionSetup-r13					RRCConnectionSetup-NB,
		spare4 NULL, spare3 NULL, spare2 NULL, spare1 NULL
	},
	messageClassExtension	SEQUENCE {}
}


DL-DCCH-Message-NB ::= SEQUENCE {
	message					DL-DCCH-MessageType-NB
}

DL-DCCH-MessageType-NB ::= CHOICE {
	c1						CHOICE {
		dlInformationTransfer-r13				DLInformationTransfer-NB,
		rrcConnectionReconfiguration-r13		RRCConnectionReconfiguration-NB,
		rrcConnectionRelease-r13				RRCConnectionRelease-NB,
		securityModeCommand-r13					SecurityModeCommand,
		ueCapabilityEnquiry-r13					UECapabilityEnquiry-NB,
		rrcConnectionResume-r13					RRCConnectionResume-NB,
		spare2 NULL, spare1 NULL
	},
	messageClassExtension	SEQUENCE {}
}



UL-CCCH-Message-NB ::= SEQUENCE {
	message					UL-CCCH-MessageType-NB
}

UL-CCCH-MessageType-NB ::= CHOICE {
	c1						CHOICE {
		rrcConnectionReestablishmentRequest-r13	RRCConnectionReestablishmentRequest-NB,
		rrcConnectionRequest-r13				RRCConnectionRequest-NB,
		rrcConnectionResumeRequest-r13			RRCConnectionResumeRequest-NB,
		spare1 NULL
	},
	messageClassExtension	SEQUENCE {}
}


SC-MCCH-Message-NB ::= SEQUENCE {
	message					SC-MCCH-MessageType-NB
}


SC-MCCH-MessageType-NB ::= CHOICE {
	c1						CHOICE {
		scptmConfiguration-r14						SCPTMConfiguration-NB-r14
	},
	messageClassExtension	SEQUENCE {}
}


UL-DCCH-Message-NB ::= SEQUENCE {
	message					UL-DCCH-MessageType-NB
}

UL-DCCH-MessageType-NB ::= CHOICE {
	c1						CHOICE {
		rrcConnectionReconfigurationComplete-r13	RRCConnectionReconfigurationComplete-NB,
		rrcConnectionReestablishmentComplete-r13	RRCConnectionReestablishmentComplete-NB,
		rrcConnectionSetupComplete-r13				RRCConnectionSetupComplete-NB,
		securityModeComplete-r13					SecurityModeComplete,
		securityModeFailure-r13						SecurityModeFailure,
		ueCapabilityInformation-r13					UECapabilityInformation-NB,
		ulInformationTransfer-r13					ULInformationTransfer-NB,
		rrcConnectionResumeComplete-r13				RRCConnectionResumeComplete-NB,
		spare8 NULL, spare7 NULL,
		spare6 NULL, spare5 NULL, spare4 NULL,
		spare3 NULL, spare2 NULL, spare1 NULL
	},
	messageClassExtension	SEQUENCE {}
}


DLInformationTransfer-NB ::=	SEQUENCE {
	rrc-TransactionIdentifier			RRC-TransactionIdentifier,
	criticalExtensions					CHOICE {
		c1									CHOICE {
			dlInformationTransfer-r13		DLInformationTransfer-NB-r13-IEs,
			spare1 NULL
		},
		criticalExtensionsFuture			SEQUENCE {}
	}
}

DLInformationTransfer-NB-r13-IEs ::=	SEQUENCE {
	dedicatedInfoNAS-r13					DedicatedInfoNAS,
	lateNonCriticalExtension				OCTET STRING					OPTIONAL,
	nonCriticalExtension					SEQUENCE {}						OPTIONAL
}


MasterInformationBlock-NB ::=	SEQUENCE {
	systemFrameNumber-MSB-r13		BIT STRING (SIZE (4)),
	hyperSFN-LSB-r13				BIT STRING (SIZE (2)),
	schedulingInfoSIB1-r13			INTEGER (0..15),
	systemInfoValueTag-r13			INTEGER (0..31),
	ab-Enabled-r13					BOOLEAN,
	operationModeInfo-r13			CHOICE {
		inband-SamePCI-r13				Inband-SamePCI-NB-r13,
		inband-DifferentPCI-r13			Inband-DifferentPCI-NB-r13,
		guardband-r13					Guardband-NB-r13,
		standalone-r13					Standalone-NB-r13
	},
	spare							BIT STRING (SIZE (11))
}

ChannelRasterOffset-NB-r13 ::= ENUMERATED {khz-7dot5, khz-2dot5, khz2dot5, khz7dot5}

Guardband-NB-r13 ::=			SEQUENCE {
	rasterOffset-r13				ChannelRasterOffset-NB-r13,
	spare							BIT STRING (SIZE (3))
}

Inband-SamePCI-NB-r13 ::=		SEQUENCE {
	eutra-CRS-SequenceInfo-r13		INTEGER (0..31)
}

Inband-DifferentPCI-NB-r13 ::=	SEQUENCE {
	eutra-NumCRS-Ports-r13			ENUMERATED {same, four},
	rasterOffset-r13				ChannelRasterOffset-NB-r13,
	spare							BIT STRING (SIZE (2))
}

Standalone-NB-r13 ::=			SEQUENCE {
	spare							BIT STRING (SIZE (5))
}


Paging-NB ::=						SEQUENCE {
	pagingRecordList-r13				PagingRecordList-NB-r13		OPTIONAL,	-- Need ON
	systemInfoModification-r13			ENUMERATED {true}				OPTIONAL,	-- Need ON
	systemInfoModification-eDRX-r13		ENUMERATED {true}				OPTIONAL,	-- Need ON
	nonCriticalExtension				SEQUENCE {}						OPTIONAL
}

PagingRecordList-NB-r13 ::=			SEQUENCE (SIZE (1..maxPageRec)) OF PagingRecord-NB-r13

PagingRecord-NB-r13 ::=				SEQUENCE {
	ue-Identity-r13						PagingUE-Identity,
	...
}


RRCConnectionReconfiguration-NB ::=	SEQUENCE {
	rrc-TransactionIdentifier				RRC-TransactionIdentifier,
	criticalExtensions						CHOICE {
		c1										CHOICE{
			rrcConnectionReconfiguration-r13		RRCConnectionReconfiguration-NB-r13-IEs,
			spare1 NULL
		},
		criticalExtensionsFuture			SEQUENCE {}
	}
}

RRCConnectionReconfiguration-NB-r13-IEs ::= SEQUENCE {
	dedicatedInfoNASList-r13			SEQUENCE (SIZE(1..maxDRB-NB-r13)) OF
													DedicatedInfoNAS		OPTIONAL,	-- Need ON
	radioResourceConfigDedicated-r13	RadioResourceConfigDedicated-NB-r13	OPTIONAL,	-- Need ON
	fullConfig-r13						ENUMERATED {true}					OPTIONAL,	-- Cond Reestab
	lateNonCriticalExtension			OCTET STRING						OPTIONAL,
	nonCriticalExtension				SEQUENCE {}	OPTIONAL
}


RRCConnectionReconfigurationComplete-NB ::= SEQUENCE {
	rrc-TransactionIdentifier				RRC-TransactionIdentifier,
	criticalExtensions						CHOICE {
		rrcConnectionReconfigurationComplete-r13	RRCConnectionReconfigurationComplete-NB-r13-IEs,
		criticalExtensionsFuture					SEQUENCE {}
	}
}

RRCConnectionReconfigurationComplete-NB-r13-IEs ::= SEQUENCE {
	lateNonCriticalExtension			OCTET STRING					OPTIONAL,
	nonCriticalExtension				SEQUENCE {}						OPTIONAL
}



RRCConnectionReestablishment-NB ::=	SEQUENCE {
	rrc-TransactionIdentifier			RRC-TransactionIdentifier,
	criticalExtensions					CHOICE {
		c1									CHOICE{
			rrcConnectionReestablishment-r13	RRCConnectionReestablishment-NB-r13-IEs,
			spare1	NULL
		},
		criticalExtensionsFuture			SEQUENCE {}
	}
}

RRCConnectionReestablishment-NB-r13-IEs ::= SEQUENCE {
	radioResourceConfigDedicated-r13			RadioResourceConfigDedicated-NB-r13,
	nextHopChainingCount-r13					NextHopChainingCount,
	lateNonCriticalExtension					OCTET STRING						OPTIONAL,
	nonCriticalExtension						RRCConnectionReestablishment-NB-v1430-IEs	OPTIONAL
}

RRCConnectionReestablishment-NB-v1430-IEs ::=	SEQUENCE {
	dl-NAS-MAC							BIT STRING (SIZE (16))	OPTIONAL,	-- Cond Reestablish-CP
	nonCriticalExtension				SEQUENCE {}				OPTIONAL
}


RRCConnectionReestablishmentComplete-NB ::= SEQUENCE {
	rrc-TransactionIdentifier				RRC-TransactionIdentifier,
	criticalExtensions						CHOICE {
		rrcConnectionReestablishmentComplete-r13	RRCConnectionReestablishmentComplete-NB-r13-IEs,
		criticalExtensionsFuture					SEQUENCE {}
	}
}

RRCConnectionReestablishmentComplete-NB-r13-IEs ::= SEQUENCE {
	lateNonCriticalExtension			OCTET STRING					OPTIONAL,
	nonCriticalExtension				RRCConnectionReestablishmentComplete-NB-v1470-IEs	OPTIONAL
}

RRCConnectionReestablishmentComplete-NB-v1470-IEs ::= SEQUENCE {
	measResultServCell-r14				MeasResultServCell-NB-r14		OPTIONAL,
	nonCriticalExtension				SEQUENCE {}						OPTIONAL
}


RRCConnectionReestablishmentRequest-NB ::= SEQUENCE {
	criticalExtensions					CHOICE {
		rrcConnectionReestablishmentRequest-r13
											RRCConnectionReestablishmentRequest-NB-r13-IEs,
		later								CHOICE {
			rrcConnectionReestablishmentRequest-r14
											RRCConnectionReestablishmentRequest-NB-r14-IEs,
			criticalExtensionsFuture		SEQUENCE {}
		}
	}
}

RRCConnectionReestablishmentRequest-NB-r13-IEs ::= SEQUENCE {
	ue-Identity-r13						ReestabUE-Identity,
	reestablishmentCause-r13			ReestablishmentCause-NB-r13,
	cqi-NPDCCH-r14						CQI-NPDCCH-NB-r14,
	earlyContentionResolution-r14		BOOLEAN,
	spare								BIT STRING (SIZE (20))
}

RRCConnectionReestablishmentRequest-NB-r14-IEs ::= SEQUENCE {
	ue-Identity-r14						ReestabUE-Identity-CP-NB-r14,
	reestablishmentCause-r14			ReestablishmentCause-NB-r13,
	cqi-NPDCCH-r14						CQI-NPDCCH-Short-NB-r14,
	earlyContentionResolution-r14		BOOLEAN,
	spare								BIT STRING (SIZE (1))
}

ReestablishmentCause-NB-r13 ::=			ENUMERATED {
											reconfigurationFailure, otherFailure,
											spare2, spare1}

ReestabUE-Identity-CP-NB-r14 ::=		SEQUENCE {
	s-TMSI-r14								S-TMSI,
	ul-NAS-MAC-r14							BIT STRING (SIZE (16)),
	ul-NAS-Count-r14						BIT STRING (SIZE (5))
}


RRCConnectionReject-NB ::=				SEQUENCE {
	criticalExtensions					CHOICE {
		c1									CHOICE {
			rrcConnectionReject-r13				RRCConnectionReject-NB-r13-IEs,
			spare1 NULL
		},
		criticalExtensionsFuture			SEQUENCE {}
	}
}

RRCConnectionReject-NB-r13-IEs ::=		SEQUENCE {
	extendedWaitTime-r13					INTEGER (1..1800),
	rrc-SuspendIndication-r13				ENUMERATED {true}			OPTIONAL,	-- Need ON
	lateNonCriticalExtension				OCTET STRING				OPTIONAL,
	nonCriticalExtension					SEQUENCE {}					OPTIONAL
}


RRCConnectionRelease-NB ::=		SEQUENCE {
	rrc-TransactionIdentifier			RRC-TransactionIdentifier,
	criticalExtensions					CHOICE {
		c1									CHOICE {
			rrcConnectionRelease-r13			RRCConnectionRelease-NB-r13-IEs,
			spare1 NULL
		},
		criticalExtensionsFuture			SEQUENCE {}
	}
}

RRCConnectionRelease-NB-r13-IEs ::=	SEQUENCE {
	releaseCause-r13					ReleaseCause-NB-r13,
	resumeIdentity-r13					ResumeIdentity-r13				OPTIONAL,	-- Need OR
	extendedWaitTime-r13				INTEGER (1..1800)				OPTIONAL,	-- Need ON
	redirectedCarrierInfo-r13			RedirectedCarrierInfo-NB-r13	OPTIONAL,	-- Need ON
	lateNonCriticalExtension			OCTET STRING					OPTIONAL,
	nonCriticalExtension				RRCConnectionRelease-NB-v1430-IEs		OPTIONAL
}

RRCConnectionRelease-NB-v1430-IEs ::=	SEQUENCE {
	redirectedCarrierInfo-v1430			RedirectedCarrierInfo-NB-v1430	OPTIONAL,	-- Cond Redirection
	extendedWaitTime-CPdata-r14		INTEGER (1..1800)	OPTIONAL,	-- Cond NoExtendedWaitTime
	nonCriticalExtension				SEQUENCE {}						OPTIONAL
}

ReleaseCause-NB-r13 ::=					ENUMERATED {loadBalancingTAUrequired, other,
													rrc-Suspend, spare1}
RedirectedCarrierInfo-NB-r13::=			CarrierFreq-NB-r13

RedirectedCarrierInfo-NB-v1430	::=		SEQUENCE {
	redirectedCarrierOffsetDedicated-r14	ENUMERATED{
												dB1, dB2, dB3, dB4, dB5, dB6, dB8, dB10,
												dB12, dB14, dB16, dB18, dB20, dB22, dB24, dB26},
	t322-r14								ENUMERATED{
												min5, min10, min20, min30, min60, min120, min180,
												spare1}
}


RRCConnectionRequest-NB ::=		SEQUENCE {
	criticalExtensions					CHOICE {
		rrcConnectionRequest-r13			RRCConnectionRequest-NB-r13-IEs,
		criticalExtensionsFuture			SEQUENCE {}
	}
}

RRCConnectionRequest-NB-r13-IEs ::=		SEQUENCE {
	ue-Identity-r13							InitialUE-Identity,
	establishmentCause-r13					EstablishmentCause-NB-r13,
	multiToneSupport-r13					ENUMERATED {true}				OPTIONAL,
	multiCarrierSupport-r13					ENUMERATED {true}				OPTIONAL,
	earlyContentionResolution-r14			BOOLEAN,
	cqi-NPDCCH-r14							CQI-NPDCCH-NB-r14,
	spare									BIT STRING (SIZE (17))
}


RRCConnectionResume-NB ::=		SEQUENCE {
	rrc-TransactionIdentifier			RRC-TransactionIdentifier,
	criticalExtensions					CHOICE {
		c1									CHOICE {
			rrcConnectionResume-r13				RRCConnectionResume-NB-r13-IEs,
			spare1								NULL
		},
		criticalExtensionsFuture			SEQUENCE {}
	}
}

RRCConnectionResume-NB-r13-IEs ::=		SEQUENCE {
	radioResourceConfigDedicated-r13		RadioResourceConfigDedicated-NB-r13	OPTIONAL,		-- Need ON
	nextHopChainingCount-r13				NextHopChainingCount,
	drb-ContinueROHC-r13					ENUMERATED {true}				OPTIONAL,	-- Need OP
	lateNonCriticalExtension				OCTET STRING					OPTIONAL,
	nonCriticalExtension					SEQUENCE {}						OPTIONAL
}


RRCConnectionResumeComplete-NB ::= SEQUENCE {
	rrc-TransactionIdentifier				RRC-TransactionIdentifier,
	criticalExtensions							CHOICE {
		rrcConnectionResumeComplete-r13				RRCConnectionResumeComplete-NB-r13-IEs,
		criticalExtensionsFuture					SEQUENCE {}
	}
}

RRCConnectionResumeComplete-NB-r13-IEs ::= SEQUENCE {
	selectedPLMN-Identity-r13					INTEGER (1..maxPLMN-r11)	OPTIONAL,
	dedicatedInfoNAS-r13						DedicatedInfoNAS	OPTIONAL,
	lateNonCriticalExtension					OCTET STRING					OPTIONAL,
	nonCriticalExtension						RRCConnectionResumeComplete-NB-v1470-IEs	OPTIONAL
}

RRCConnectionResumeComplete-NB-v1470-IEs ::= SEQUENCE {
	measResultServCell-r14						MeasResultServCell-NB-r14	OPTIONAL,
	nonCriticalExtension						SEQUENCE {}					OPTIONAL
}


RRCConnectionResumeRequest-NB ::=	SEQUENCE {
	criticalExtensions						CHOICE {
		rrcConnectionResumeRequest-r13			RRCConnectionResumeRequest-NB-r13-IEs,
		criticalExtensionsFuture				SEQUENCE {}
	}
}

RRCConnectionResumeRequest-NB-r13-IEs ::=	SEQUENCE {
	resumeID-r13								ResumeIdentity-r13,
	shortResumeMAC-I-r13						ShortMAC-I,
	resumeCause-r13								EstablishmentCause-NB-r13,
	earlyContentionResolution-r14				BOOLEAN,
	cqi-NPDCCH-r14								CQI-NPDCCH-NB-r14,
	spare										BIT STRING (SIZE (4))
}


RRCConnectionSetup-NB ::=		SEQUENCE {
	rrc-TransactionIdentifier			RRC-TransactionIdentifier,
	criticalExtensions					CHOICE {
		c1									CHOICE {
			rrcConnectionSetup-r13				RRCConnectionSetup-NB-r13-IEs,
			spare1 NULL
		},
		criticalExtensionsFuture			SEQUENCE {}
	}
}

RRCConnectionSetup-NB-r13-IEs ::=		SEQUENCE {
	radioResourceConfigDedicated-r13		RadioResourceConfigDedicated-NB-r13,
	lateNonCriticalExtension				OCTET STRING						OPTIONAL,
	nonCriticalExtension					SEQUENCE {}							OPTIONAL
}


RRCConnectionSetupComplete-NB ::=	SEQUENCE {
	rrc-TransactionIdentifier				RRC-TransactionIdentifier,
	criticalExtensions						CHOICE{
			rrcConnectionSetupComplete-r13		RRCConnectionSetupComplete-NB-r13-IEs,
			criticalExtensionsFuture			SEQUENCE {}
	}
}

RRCConnectionSetupComplete-NB-r13-IEs ::= SEQUENCE {
	selectedPLMN-Identity-r13				INTEGER (1..maxPLMN-r11),
	s-TMSI-r13								S-TMSI							OPTIONAL,
	registeredMME-r13						RegisteredMME					OPTIONAL,
	dedicatedInfoNAS-r13					DedicatedInfoNAS,
	attachWithoutPDN-Connectivity-r13		ENUMERATED {true}				OPTIONAL,
	up-CIoT-EPS-Optimisation-r13			ENUMERATED {true}				OPTIONAL,
	lateNonCriticalExtension				OCTET STRING					OPTIONAL,
	nonCriticalExtension					RRCConnectionSetupComplete-NB-v1430-IEs	OPTIONAL
}

RRCConnectionSetupComplete-NB-v1430-IEs ::= SEQUENCE {
	gummei-Type-r14							ENUMERATED { mapped}	OPTIONAL,
	dcn-ID-r14								INTEGER (0..65535)			OPTIONAL,
	nonCriticalExtension					RRCConnectionSetupComplete-NB-v1470-IEs OPTIONAL
}

RRCConnectionSetupComplete-NB-v1470-IEs ::= SEQUENCE {
	measResultServCell-r14						MeasResultServCell-NB-r14	OPTIONAL,
	nonCriticalExtension						SEQUENCE {}					OPTIONAL
}


SCPTMConfiguration-NB-r14 ::=	SEQUENCE {
	sc-mtch-InfoList-r14			SC-MTCH-InfoList-NB-r14,
	scptm-NeighbourCellList-r14		SCPTM-NeighbourCellList-NB-r14		OPTIONAL,	-- Need OP
	lateNonCriticalExtension		OCTET STRING						OPTIONAL,
	nonCriticalExtension			SEQUENCE {}							OPTIONAL
}


SystemInformation-NB ::=		SEQUENCE {
	criticalExtensions					CHOICE {
		systemInformation-r13				SystemInformation-NB-r13-IEs,
		criticalExtensionsFuture			SEQUENCE {}
	}
}
SystemInformation-NB-r13-IEs ::=	SEQUENCE {
	sib-TypeAndInfo-r13					SEQUENCE (SIZE (1..maxSIB)) OF CHOICE {
		sib2-r13							SystemInformationBlockType2-NB-r13,
		sib3-r13							SystemInformationBlockType3-NB-r13,
		sib4-r13							SystemInformationBlockType4-NB-r13,
		sib5-r13							SystemInformationBlockType5-NB-r13,
		sib14-r13							SystemInformationBlockType14-NB-r13,
		sib16-r13							SystemInformationBlockType16-NB-r13,
		...,
		sib15-v1430							SystemInformationBlockType15-NB-r14,
		sib20-v1430							SystemInformationBlockType20-NB-r14,
		sib22-v1430							SystemInformationBlockType22-NB-r14
	},
	lateNonCriticalExtension			OCTET STRING						OPTIONAL,
	nonCriticalExtension				SEQUENCE {}							OPTIONAL
}


SystemInformationBlockType1-NB ::=	SEQUENCE {
	hyperSFN-MSB-r13					BIT STRING (SIZE (8)),
	cellAccessRelatedInfo-r13			SEQUENCE {
		plmn-IdentityList-r13				PLMN-IdentityList-NB-r13,
		trackingAreaCode-r13				TrackingAreaCode,
		cellIdentity-r13					CellIdentity,
		cellBarred-r13						ENUMERATED {barred, notBarred},
		intraFreqReselection-r13			ENUMERATED {allowed, notAllowed}
	},
	cellSelectionInfo-r13				SEQUENCE {
		q-RxLevMin-r13						Q-RxLevMin,
		q-QualMin-r13						Q-QualMin-r9
	},
	p-Max-r13							P-Max					OPTIONAL,	-- Need OP
	freqBandIndicator-r13				FreqBandIndicator-NB-r13,
	freqBandInfo-r13					NS-PmaxList-NB-r13				OPTIONAL,	-- Need OR
	multiBandInfoList-r13				MultiBandInfoList-NB-r13		OPTIONAL,	-- Need OR
	downlinkBitmap-r13					DL-Bitmap-NB-r13				OPTIONAL,	-- Need OP,
	eutraControlRegionSize-r13			ENUMERATED {n1, n2, n3}			OPTIONAL,	-- Cond inband
	nrs-CRS-PowerOffset-r13				ENUMERATED {dB-6,      dB-4dot77, dB-3,
													dB-1dot77, dB0,       dB1,
													dB1dot23,  dB2,       dB3,
													dB4,       dB4dot23,  dB5,
													dB6,       dB7,       dB8,
													dB9}		OPTIONAL,	-- Cond inband-SamePCI
	schedulingInfoList-r13				SchedulingInfoList-NB-r13,
	si-WindowLength-r13					ENUMERATED {ms160,  ms320,  ms480,	ms640,
													ms960,	ms1280, ms1600, spare1},
	si-RadioFrameOffset-r13				INTEGER (1..15)		OPTIONAL,	-- Need OP
	systemInfoValueTagList-r13			SystemInfoValueTagList-NB-r13	OPTIONAL,	-- Need OR
	lateNonCriticalExtension			OCTET STRING					OPTIONAL,
	nonCriticalExtension				SystemInformationBlockType1-NB-v1350	OPTIONAL
}

SystemInformationBlockType1-NB-v1350 ::=	SEQUENCE {
	cellSelectionInfo-v1350				CellSelectionInfo-NB-v1350	OPTIONAL,	-- Cond Qrxlevmin
	nonCriticalExtension				SystemInformationBlockType1-NB-v1430	OPTIONAL
}

SystemInformationBlockType1-NB-v1430 ::=	SEQUENCE {
	cellSelectionInfo-v1430				CellSelectionInfo-NB-v1430		OPTIONAL,	-- Need OR
	nonCriticalExtension				SystemInformationBlockType1-NB-v1450					OPTIONAL
}

SystemInformationBlockType1-NB-v1450 ::= SEQUENCE {
	nrs-CRS-PowerOffset-v1450				ENUMERATED {dB-6,  dB-4dot77, dB-3,
													dB-1dot77, dB0,       dB1,
													dB1dot23,  dB2,       dB3,
													dB4,       dB4dot23,  dB5,
													dB6,       dB7,       dB8,
													dB9}		OPTIONAL,	-- Cond inband-SamePCI-ExceptAnchor
	nonCriticalExtension				SEQUENCE {}					OPTIONAL
}

PLMN-IdentityList-NB-r13 ::=		SEQUENCE (SIZE (1..maxPLMN-r11)) OF PLMN-IdentityInfo-NB-r13

PLMN-IdentityInfo-NB-r13 ::=		SEQUENCE {
	plmn-Identity-r13						PLMN-Identity,
	cellReservedForOperatorUse-r13			ENUMERATED {reserved, notReserved},
	attachWithoutPDN-Connectivity-r13		ENUMERATED {true}	OPTIONAL	-- Need OP
}

SchedulingInfoList-NB-r13 ::= SEQUENCE (SIZE (1..maxSI-Message-NB-r13)) OF SchedulingInfo-NB-r13

SchedulingInfo-NB-r13::=		SEQUENCE {
	si-Periodicity-r13				ENUMERATED {rf64, rf128, rf256, rf512,
												rf1024, rf2048, rf4096, spare},
	si-RepetitionPattern-r13		ENUMERATED {every2ndRF, every4thRF, every8thRF, every16thRF},
	sib-MappingInfo-r13				SIB-MappingInfo-NB-r13,
	si-TB-r13						ENUMERATED {b56, b120, b208, b256, b328, b440, b552, b680}
}

SystemInfoValueTagList-NB-r13 ::=	SEQUENCE (SIZE (1.. maxSI-Message-NB-r13)) OF
										SystemInfoValueTagSI-r13

SIB-MappingInfo-NB-r13 ::=			SEQUENCE (SIZE (0..maxSIB-1)) OF SIB-Type-NB-r13

SIB-Type-NB-r13 ::=					ENUMERATED {
										sibType3-NB-r13, sibType4-NB-r13, sibType5-NB-r13,
										sibType14-NB-r13, sibType16-NB-r13, sibType15-NB-r14,
										sibType20-NB-r14, sibType22-NB-r14}

CellSelectionInfo-NB-v1350 ::=		SEQUENCE {
	delta-RxLevMin-v1350				INTEGER (-8..-1)
}

CellSelectionInfo-NB-v1430 ::=		SEQUENCE {
	powerClass14dBm-Offset-r14			ENUMERATED {dB-6, dB-3, dB3, dB6, dB9, dB12}	OPTIONAL,	--	Need OP
	ce-authorisationOffset-r14			ENUMERATED {dB5, dB10, dB15, dB20, dB25, dB30, dB35}	OPTIONAL	--	Need OP
}


UECapabilityEnquiry-NB ::=	SEQUENCE {
	rrc-TransactionIdentifier			RRC-TransactionIdentifier,
	criticalExtensions					CHOICE {
		c1									CHOICE {
			ueCapabilityEnquiry-r13				UECapabilityEnquiry-NB-r13-IEs,
			spare1								NULL
		},
		criticalExtensionsFuture			SEQUENCE {}
	}
}

UECapabilityEnquiry-NB-r13-IEs ::=	SEQUENCE {
	lateNonCriticalExtension			OCTET STRING						OPTIONAL,
	nonCriticalExtension				SEQUENCE {}							OPTIONAL
}


UECapabilityInformation-NB ::=	SEQUENCE {
	rrc-TransactionIdentifier			RRC-TransactionIdentifier,
	criticalExtensions					CHOICE{
			ueCapabilityInformation-r13		UECapabilityInformation-NB-r13-IEs,
			criticalExtensionsFuture		SEQUENCE {}
	}
}

UECapabilityInformation-NB-r13-IEs ::=	SEQUENCE {
	ue-Capability-r13						UE-Capability-NB-r13,
	ue-RadioPagingInfo-r13					UE-RadioPagingInfo-NB-r13,
	lateNonCriticalExtension				OCTET STRING						OPTIONAL,
	nonCriticalExtension					UECapabilityInformation-NB-Ext-r14-IEs							OPTIONAL
}

UECapabilityInformation-NB-Ext-r14-IEs ::=	SEQUENCE {
	ue-Capability-ContainerExt-r14			OCTET STRING (CONTAINING UE-Capability-NB-Ext-r14-IEs),
	nonCriticalExtension					SEQUENCE {}							OPTIONAL
}


ULInformationTransfer-NB ::=	SEQUENCE {
	criticalExtensions					CHOICE {
			ulInformationTransfer-r13		ULInformationTransfer-NB-r13-IEs,
			criticalExtensionsFuture		SEQUENCE {}
	}
}

ULInformationTransfer-NB-r13-IEs ::=	SEQUENCE {
	dedicatedInfoNAS-r13					DedicatedInfoNAS,
	lateNonCriticalExtension				OCTET STRING					OPTIONAL,
	nonCriticalExtension					SEQUENCE {}						OPTIONAL
}


SystemInformationBlockType2-NB-r13 ::=	SEQUENCE {
	radioResourceConfigCommon-r13			RadioResourceConfigCommonSIB-NB-r13,
	ue-TimersAndConstants-r13				UE-TimersAndConstants-NB-r13,
	freqInfo-r13							SEQUENCE {
		ul-CarrierFreq-r13						CarrierFreq-NB-r13			OPTIONAL,	-- Need OP
		additionalSpectrumEmission-r13			AdditionalSpectrumEmission
	},
	timeAlignmentTimerCommon-r13			TimeAlignmentTimer,
	multiBandInfoList-r13	SEQUENCE (SIZE (1..maxMultiBands)) OF AdditionalSpectrumEmission		OPTIONAL,	-- Need OR
	lateNonCriticalExtension				OCTET STRING					OPTIONAL,
	...,
	[[	cp-Reestablishment-r14				ENUMERATED {true}				OPTIONAL		-- Need OP
	]],
	[[	servingCellMeasInfo-r14				ENUMERATED {true} 				OPTIONAL,		-- Need OR
		cqi-Reporting-r14					ENUMERATED {true} 				OPTIONAL		-- Need OR
	]]
}


SystemInformationBlockType3-NB-r13 ::=	SEQUENCE {
	cellReselectionInfoCommon-r13			SEQUENCE {
		q-Hyst-r13								ENUMERATED {
													dB0, dB1, dB2, dB3, dB4, dB5, dB6, dB8, dB10,
													dB12, dB14, dB16, dB18, dB20, dB22, dB24
													}
	},
	cellReselectionServingFreqInfo-r13		SEQUENCE {
		s-NonIntraSearch-r13					ReselectionThreshold
	},
	intraFreqCellReselectionInfo-r13		SEQUENCE {
		q-RxLevMin-r13							Q-RxLevMin,
		q-QualMin-r13							Q-QualMin-r9			OPTIONAL,	-- Need OP
		p-Max-r13								P-Max					OPTIONAL,	-- Need OP
		s-IntraSearchP-r13						ReselectionThreshold,
		t-Reselection-r13						T-Reselection-NB-r13
	},
	freqBandInfo-r13						NS-PmaxList-NB-r13				OPTIONAL,	-- Need OR
	multiBandInfoList-r13					SEQUENCE (SIZE (1..maxMultiBands)) OF
												NS-PmaxList-NB-r13			OPTIONAL,	-- Need OR
	lateNonCriticalExtension					OCTET STRING				OPTIONAL,
	...,
	[[	intraFreqCellReselectionInfo-v1350	IntraFreqCellReselectionInfo-NB-v1350 OPTIONAL	-- Cond Qrxlevmin
	]],
	[[	intraFreqCellReselectionInfo-v1360	IntraFreqCellReselectionInfo-NB-v1360 OPTIONAL	-- Need OR
	]],
	[[	intraFreqCellReselectionInfo-v1430	IntraFreqCellReselectionInfo-NB-v1430 OPTIONAL	-- Need OR
	]],
	[[	cellReselectionInfoCommon-v1450		CellReselectionInfoCommon-NB-v1450	OPTIONAL	-- Need OR
	]]
}

IntraFreqCellReselectionInfo-NB-v1350 ::=	SEQUENCE {
	delta-RxLevMin-v1350						INTEGER (-8..-1)
}

IntraFreqCellReselectionInfo-NB-v1360 ::=	SEQUENCE {
	s-IntraSearchP-v1360							ReselectionThreshold-NB-v1360
}

IntraFreqCellReselectionInfo-NB-v1430 ::=	SEQUENCE {
	powerClass14dBm-Offset-r14		ENUMERATED {dB-6, dB-3, dB3, dB6, dB9, dB12}	OPTIONAL,	-- Need OP
	ce-AuthorisationOffset-r14		ENUMERATED {dB5, dB10, dB15, dB20, dB25, dB30, dB35}	OPTIONAL	-- Need OP
}

CellReselectionInfoCommon-NB-v1450 ::=	SEQUENCE {
	s-SearchDeltaP-r14					ENUMERATED {dB6, dB9, dB12, dB15}
}


SystemInformationBlockType4-NB-r13 ::=		SEQUENCE {
	intraFreqNeighCellList-r13			IntraFreqNeighCellList	OPTIONAL,	-- Need OR
	intraFreqBlackCellList-r13			IntraFreqBlackCellList	OPTIONAL,	-- Need OR
	lateNonCriticalExtension			OCTET STRING			OPTIONAL,
	...
}



SystemInformationBlockType5-NB-r13 ::=	SEQUENCE {
	interFreqCarrierFreqList-r13			InterFreqCarrierFreqList-NB-r13,
	t-Reselection-r13						T-Reselection-NB-r13,
	lateNonCriticalExtension				OCTET STRING					OPTIONAL,
	...,
	[[	scptm-FreqOffset-r14				INTEGER (1..8)					OPTIONAL	-- Need OP
	]]
}


InterFreqCarrierFreqList-NB-r13 ::=		SEQUENCE (SIZE (1..maxFreq)) OF InterFreqCarrierFreqInfo-NB-r13


InterFreqCarrierFreqInfo-NB-r13 ::=	SEQUENCE {
	dl-CarrierFreq-r13					CarrierFreq-NB-r13,
	q-RxLevMin-r13						Q-RxLevMin,
	q-QualMin-r13						Q-QualMin-r9					OPTIONAL,		-- Need OP
	p-Max-r13							P-Max							OPTIONAL,		-- Need OP
	q-OffsetFreq-r13					Q-OffsetRange					DEFAULT dB0,
	interFreqNeighCellList-r13			InterFreqNeighCellList-NB-r13	OPTIONAL,		-- Need OR
	interFreqBlackCellList-r13			InterFreqBlackCellList-NB-r13	OPTIONAL,		-- Need OR
	multiBandInfoList-r13				MultiBandInfoList-NB-r13		OPTIONAL,		-- Need OR
	...,
	[[	delta-RxLevMin-v1350			INTEGER (-8..-1)		OPTIONAL	-- Cond Qrxlevmin
	]],
	[[	powerClass14dBm-Offset-r14		ENUMERATED {dB-6, dB-3, dB3, dB6, dB9, dB12}
OPTIONAL,	--	Need OP
		ce-AuthorisationOffset-r14		ENUMERATED {dB5, dB10, dB15, dB20, dB25, dB30, dB35}	OPTIONAL	-- Need OP
	]]
}

InterFreqNeighCellList-NB-r13 ::=		SEQUENCE (SIZE (1..maxCellInter)) OF PhysCellId


InterFreqBlackCellList-NB-r13 ::=		SEQUENCE (SIZE (1..maxCellBlack)) OF PhysCellId



SystemInformationBlockType14-NB-r13 ::=	SEQUENCE {
	ab-Param-r13					CHOICE {
		ab-Common-r13					AB-Config-NB-r13,
		ab-PerPLMN-List-r13				SEQUENCE (SIZE (1..maxPLMN-r11)) OF AB-ConfigPLMN-NB-r13
	}															OPTIONAL, -- Need OR
	lateNonCriticalExtension		OCTET STRING				OPTIONAL,
	...
}

AB-ConfigPLMN-NB-r13 ::=	SEQUENCE {
	ab-Config-r13					AB-Config-NB-r13			OPTIONAL -- Need OR
}

AB-Config-NB-r13 ::=		SEQUENCE {
	ab-Category-r13					ENUMERATED {a, b, c},
	ab-BarringBitmap-r13			BIT STRING (SIZE(10)),
	ab-BarringForExceptionData-r13	ENUMERATED {true}			OPTIONAL,	-- Need OP
	ab-BarringForSpecialAC-r13		BIT STRING (SIZE(5))
}


SystemInformationBlockType15-NB-r14 ::=	SEQUENCE {
	mbms-SAI-IntraFreq-r14					MBMS-SAI-List-r11				OPTIONAL,	-- Need OR
	mbms-SAI-InterFreqList-r14				MBMS-SAI-InterFreqList-NB-r14	OPTIONAL,	-- Need OR
	lateNonCriticalExtension				OCTET STRING					OPTIONAL,
	...
}

MBMS-SAI-InterFreqList-NB-r14 ::=		SEQUENCE (SIZE (1..maxFreq)) OF MBMS-SAI-InterFreq-NB-r14

MBMS-SAI-InterFreq-NB-r14 ::=			SEQUENCE {
	dl-CarrierFreq-r14						CarrierFreq-NB-r13,
	mbms-SAI-List-r14						MBMS-SAI-List-r11,
	multiBandInfoList-r14					AdditionalBandInfoList-NB-r14	OPTIONAL	-- Need OR
}


SystemInformationBlockType16-NB-r13 ::= SystemInformationBlockType16-r11


SystemInformationBlockType20-NB-r14 ::=	SEQUENCE {
	npdcch-SC-MCCH-Config-r14				NPDCCH-SC-MCCH-Config-NB-r14,
	sc-mcch-CarrierConfig-r14				CHOICE {
		dl-CarrierConfig-r14					DL-CarrierConfigCommon-NB-r14,
		dl-CarrierIndex-r14						INTEGER (0.. maxNonAnchorCarriers-NB-r14)
	},
	sc-mcch-RepetitionPeriod-r14			ENUMERATED {rf32, rf128, rf512, rf1024,
														rf2048, rf4096, rf8192, rf16384},
	sc-mcch-Offset-r14						INTEGER (0..10),
	sc-mcch-ModificationPeriod-r14			ENUMERATED { rf32, rf128, rf256, rf512, rf1024,
													rf2048, rf4096, rf8192, rf16384, rf32768,
													rf65536, rf131072, rf262144, rf524288,
													rf1048576, spare1},
	sc-mcch-SchedulingInfo-r14				SC-MCCH-SchedulingInfo-NB-r14		OPTIONAL,	-- Need OP
	lateNonCriticalExtension				OCTET STRING						OPTIONAL,
	...
}

NPDCCH-SC-MCCH-Config-NB-r14 ::=	SEQUENCE {
	npdcch-NumRepetitions-SC-MCCH-r14		ENUMERATED {r1, r2, r4, r8, r16,
														r32, r64, r128, r256,
														r512, r1024, r2048},
	npdcch-StartSF-SC-MCCH-r14				ENUMERATED {v1dot5, v2, v4, v8,
														v16, v32, v48, v64},
	npdcch-Offset-SC-MCCH-r14				ENUMERATED {zero, oneEighth, oneQuarter,
														threeEighth, oneHalf, fiveEighth,
														threeQuarter, sevenEighth}
}

SC-MCCH-SchedulingInfo-NB-r14::=	SEQUENCE	{
	onDurationTimerSCPTM-r14					ENUMERATED {
													pp1, pp2, pp3, pp4,
													pp8, pp16, pp32, spare},
	drx-InactivityTimerSCPTM-r14				ENUMERATED {
													pp0, pp1, pp2, pp3,
													pp4, pp8, pp16, pp32},
	schedulingPeriodStartOffsetSCPTM-r14		CHOICE {
		sf10										INTEGER(0..9),
		sf20										INTEGER(0..19),
		sf32										INTEGER(0..31),
		sf40										INTEGER(0..39),
		sf64										INTEGER(0..63),
		sf80										INTEGER(0..79),
		sf128										INTEGER(0..127),
		sf160										INTEGER(0..159),
		sf256										INTEGER(0..255),
		sf320										INTEGER(0..319),
		sf512										INTEGER(0..511),
		sf640										INTEGER(0..639),
		sf1024										INTEGER(0..1023),
		sf2048										INTEGER(0..2047),
		sf4096										INTEGER(0..4095),
		sf8192										INTEGER(0..8191)
	},
	...
}


SystemInformationBlockType22-NB-r14 ::=	SEQUENCE {
	dl-ConfigList-r14 					DL-ConfigCommonList-NB-r14	OPTIONAL,	-- Need OR
	ul-ConfigList-r14 					UL-ConfigCommonList-NB-r14	OPTIONAL,	-- Need OR
	pagingWeightAnchor-r14				PagingWeight-NB-r14			OPTIONAL,	-- Cond pcch-config
	nprach-ProbabilityAnchorList-r14	NPRACH-ProbabilityAnchorList-NB-r14	OPTIONAL,	-- Cond nprach-config
	lateNonCriticalExtension			OCTET STRING					OPTIONAL,
	...
}

DL-ConfigCommonList-NB-r14 ::=		SEQUENCE (SIZE (1.. maxNonAnchorCarriers-NB-r14)) OF
											DL-ConfigCommon-NB-r14

UL-ConfigCommonList-NB-r14 ::=		SEQUENCE (SIZE (1.. maxNonAnchorCarriers-NB-r14)) OF
											UL-ConfigCommon-NB-r14


DL-ConfigCommon-NB-r14 ::=			SEQUENCE {
	dl-CarrierConfig-r14				DL-CarrierConfigCommon-NB-r14,
	pcch-Config-r14 					PCCH-Config-NB-r14			OPTIONAL, -- Need OR
	...
}

PCCH-Config-NB-r14 ::=				SEQUENCE {
	npdcch-NumRepetitionPaging-r14		ENUMERATED {
											r1, r2, r4, r8, r16, r32, r64, r128,
											r256, r512, r1024, r2048,
											spare4, spare3, spare2, spare1} OPTIONAL, -- Need OP
	pagingWeight-r14						PagingWeight-NB-r14	DEFAULT w1,
	...
}

PagingWeight-NB-r14	::=			ENUMERATED {w1, w2, w3, w4, w5, w6, w7, w8,
												w9, w10, w11, w12, w13, w14, w15, w16}

UL-ConfigCommon-NB-r14 ::=			SEQUENCE {
	ul-CarrierFreq-r14					CarrierFreq-NB-r13,
	nprach-ParametersList-r14 			NPRACH-ParametersList-NB-r14	OPTIONAL, -- Need OR
	...
}

NPRACH-ParametersList-NB-r14 ::=		SEQUENCE (SIZE (1.. maxNPRACH-Resources-NB-r13)) OF
											NPRACH-Parameters-NB-r14


NPRACH-Parameters-NB-r14 ::=			SEQUENCE {
	nprach-Parameters-r14					SEQUENCE {
		nprach-Periodicity-r14					ENUMERATED {ms40, ms80, ms160, ms240,
															ms320, ms640, ms1280, ms2560}
													OPTIONAL,	-- NEED OP
		nprach-StartTime-r14					ENUMERATED {ms8, ms16, ms32, ms64,
															ms128, ms256, ms512, ms1024}
													OPTIONAL,	-- NEED OP
		nprach-SubcarrierOffset-r14				ENUMERATED {n0, n12, n24, n36, n2, n18, n34, spare1}
													OPTIONAL,	-- NEED OP
		nprach-NumSubcarriers-r14				ENUMERATED {n12, n24, n36, n48}
													OPTIONAL,	-- NEED OP
		nprach-SubcarrierMSG3-RangeStart-r14	ENUMERATED {zero, oneThird, twoThird, one}
													OPTIONAL,	-- NEED OP
		npdcch-NumRepetitions-RA-r14			ENUMERATED {r1, r2, r4, r8, r16, r32, r64, r128,
															r256, r512, r1024, r2048,
															spare4, spare3, spare2, spare1}
													OPTIONAL,	-- NEED OP
		npdcch-StartSF-CSS-RA-r14				ENUMERATED {v1dot5, v2, v4, v8, v16, v32, v48, v64}
														OPTIONAL,	-- NEED OP
		npdcch-Offset-RA-r14					ENUMERATED {zero, oneEighth, oneFourth, threeEighth}
													OPTIONAL,	-- NEED OP
		nprach-NumCBRA-StartSubcarriers-r14		ENUMERATED {n8, n10, n11, n12, n20, n22, n23, n24,
															n32, n34, n35, n36, n40, n44, n46, n48}
													OPTIONAL,	-- NEED OP
		npdcch-CarrierIndex-r14					INTEGER (1..maxNonAnchorCarriers-NB-r14)
													OPTIONAL,	-- Need OP
		...
	}	OPTIONAL	-- Need OR
}

NPRACH-ProbabilityAnchorList-NB-r14 ::=	SEQUENCE (SIZE (1.. maxNPRACH-Resources-NB-r13)) OF
												NPRACH-ProbabilityAnchor-NB-r14

NPRACH-ProbabilityAnchor-NB-r14 ::=		SEQUENCE {
	nprach-ProbabilityAnchor-r14			ENUMERATED {
												zero, oneSixteenth, oneFifteenth, oneFourteenth,
												oneThirteenth, oneTwelfth, oneEleventh, oneTenth,
												oneNinth, oneEighth, oneSeventh, oneSixth,
												oneFifth, oneFourth, oneThird, oneHalf}
														OPTIONAL	-- Need OP
}


CarrierConfigDedicated-NB-r13 ::=		SEQUENCE {
	dl-CarrierConfig-r13		DL-CarrierConfigDedicated-NB-r13,
	ul-CarrierConfig-r13		UL-CarrierConfigDedicated-NB-r13
}

DL-CarrierConfigDedicated-NB-r13 ::=	SEQUENCE {
	dl-CarrierFreq-r13						CarrierFreq-NB-r13,
	downlinkBitmapNonAnchor-r13				CHOICE {
		useNoBitmap-r13							NULL,
		useAnchorBitmap-r13						NULL,
		explicitBitmapConfiguration-r13			DL-Bitmap-NB-r13,
		spare									NULL
	}		OPTIONAL,	-- Need ON
	dl-GapNonAnchor-r13						CHOICE {
		useNoGap-r13							NULL,
		useAnchorGapConfig-r13					NULL,
		explicitGapConfiguration-r13			DL-GapConfig-NB-r13,
		spare									NULL
	}		OPTIONAL,	-- Need ON
	inbandCarrierInfo-r13					SEQUENCE {
		samePCI-Indicator-r13					CHOICE	{
			samePCI-r13								SEQUENCE {
				indexToMidPRB-r13						INTEGER (-55..54)
			},
			differentPCI-r13						SEQUENCE {
				eutra-NumCRS-Ports-r13					ENUMERATED {same, four}
			}
		}							OPTIONAL,		-- Cond anchor-guardband
		eutraControlRegionSize-r13				ENUMERATED {n1, n2, n3}
	}								OPTIONAL,		-- Cond non-anchor-inband
	...,
	[[	nrs-PowerOffsetNonAnchor-v1330		ENUMERATED {dB-12, dB-10, dB-8, dB-6,
														dB-4, dB-2, dB0, dB3}
									OPTIONAL	-- Need ON
	]]
}

UL-CarrierConfigDedicated-NB-r13 ::=	SEQUENCE {
	ul-CarrierFreq-r13			CarrierFreq-NB-r13		OPTIONAL,	-- Need OP
	...
}


CarrierFreq-NB-r13 ::=		SEQUENCE {
	carrierFreq-r13				ARFCN-ValueEUTRA-r9,
	carrierFreqOffset-r13		ENUMERATED {
									v-10, v-9, v-8,	v-7, v-6, v-5, v-4, v-3, v-2, v-1, v-0dot5,
									 v0,  v1,	v2,	v3,  v4,  v5,	v6,  v7,  v8,  v9
									}	OPTIONAL	-- Need ON
}


DL-Bitmap-NB-r13 ::=			CHOICE {
	subframePattern10-r13			BIT STRING (SIZE (10)),
	subframePattern40-r13			BIT STRING (SIZE (40))
}


DL-CarrierConfigCommon-NB-r14 ::=	SEQUENCE {
	dl-CarrierFreq-r14					CarrierFreq-NB-r13,
	downlinkBitmapNonAnchor-r14			CHOICE {
		useNoBitmap-r14						NULL,
		useAnchorBitmap-r14					NULL,
		explicitBitmapConfiguration-r14		DL-Bitmap-NB-r13
	},
	dl-GapNonAnchor-r14					CHOICE {
		useNoGap-r14						NULL,
		useAnchorGapConfig-r14				NULL,
		explicitGapConfiguration-r14		DL-GapConfig-NB-r13
	},
	inbandCarrierInfo-r14				SEQUENCE {
		samePCI-Indicator-r14				CHOICE	{
			samePCI-r14							SEQUENCE {
				indexToMidPRB-r14					INTEGER (-55..54)
			},
			differentPCI-r14					SEQUENCE {
				eutra-NumCRS-Ports-r14				ENUMERATED {same, four}
			}
		}	OPTIONAL,		-- Cond anchor-guardband
		eutraControlRegionSize-r14			ENUMERATED {n1, n2, n3}
	}	OPTIONAL,		-- Cond non-anchor-inband
	nrs-PowerOffsetNonAnchor-r14		ENUMERATED {dB-12, dB-10, dB-8, dB-6,
													dB-4, dB-2, dB0, dB3}	DEFAULT dB0,
	...
}



DL-GapConfig-NB-r13	::=		SEQUENCE {
	dl-GapThreshold-r13			ENUMERATED {n32, n64, n128, n256},
	dl-GapPeriodicity-r13		ENUMERATED {sf64, sf128, sf256, sf512},
	dl-GapDurationCoeff-r13		ENUMERATED {oneEighth, oneFourth, threeEighth, oneHalf}
}


LogicalChannelConfig-NB-r13 ::=		SEQUENCE {
	priority-r13						INTEGER (1..16)			OPTIONAL,		-- Cond UL
	logicalChannelSR-Prohibit-r13		BOOLEAN					OPTIONAL,		-- Need ON
	...
}


MAC-MainConfig-NB-r13 ::=			SEQUENCE {
	ul-SCH-Config-r13					SEQUENCE {
		periodicBSR-Timer-r13				PeriodicBSR-Timer-NB-r13		OPTIONAL,	-- Need ON
		retxBSR-Timer-r13					RetxBSR-Timer-NB-r13
	}																	OPTIONAL,	-- Need ON
	drx-Config-r13						DRX-Config-NB-r13				OPTIONAL,	-- Need ON
	timeAlignmentTimerDedicated-r13		TimeAlignmentTimer,
	logicalChannelSR-Config-r13			CHOICE {
		release								NULL,
		setup								SEQUENCE {
			logicalChannelSR-ProhibitTimer-r13	ENUMERATED {
													pp2, pp8, pp32, pp128, pp512,
													pp1024, pp2048, spare}
		}
	}																	OPTIONAL,	-- Need ON
	...,
	[[	rai-Activation-r14						ENUMERATED {true}			OPTIONAL,	-- Need OR
		dataInactivityTimerConfig-r14	CHOICE {
			release								NULL,
			setup								SEQUENCE {
				dataInactivityTimer-r14				DataInactivityTimer-r14
			}
		}																OPTIONAL	-- Need ON
	]],
	[[	drx-Cycle-v1430					ENUMERATED {
									sf1280, sf2560, sf5120, sf10240}	OPTIONAL	-- Need ON
	]],
	[[	ra-CFRA-Config-r14		ENUMERATED {true}			OPTIONAL		-- Need ON
	]]
}

PeriodicBSR-Timer-NB-r13 ::=		ENUMERATED {
										pp2, pp4, pp8, pp16, pp64, pp128, infinity, spare}

RetxBSR-Timer-NB-r13 ::=			ENUMERATED {
										pp4, pp16, pp64, pp128, pp256, pp512, infinity, spare}

DRX-Config-NB-r13 ::=				CHOICE {
	release								NULL,
	setup								SEQUENCE {
		onDurationTimer-r13					ENUMERATED {
												pp1, pp2, pp3, pp4, pp8, pp16, pp32, spare},
		drx-InactivityTimer-r13				ENUMERATED {
												pp0, pp1, pp2, pp3, pp4, pp8, pp16, pp32},
		drx-RetransmissionTimer-r13			ENUMERATED {
												pp0, pp1, pp2, pp4, pp6, pp8, pp16, pp24,
												pp33, spare7, spare6, spare5,
												spare4, spare3, spare2, spare1},
		drx-Cycle-r13						ENUMERATED {
												sf256, sf512, sf1024, sf1536, sf2048, sf3072,
												sf4096, sf4608, sf6144, sf7680, sf8192, sf9216,
												spare4, spare3, spare2, spare1},
		drx-StartOffset-r13					INTEGER (0..255),
		drx-ULRetransmissionTimer-r13		ENUMERATED {
												pp0, pp1, pp2, pp4, pp6, pp8, pp16, pp24,
												pp33, pp40, pp64, pp80, pp96,
												pp112, pp128, pp160, pp320}
	}
}



NPDCCH-ConfigDedicated-NB-r13 ::=	SEQUENCE {
	npdcch-NumRepetitions-r13			ENUMERATED {r1, r2, r4, r8, r16, r32, r64, r128,
													r256, r512, r1024, r2048,
													spare4, spare3, spare2, spare1},
	npdcch-StartSF-USS-r13				ENUMERATED {v1dot5, v2, v4, v8, v16, v32, v48, v64},
	npdcch-Offset-USS-r13				ENUMERATED {zero, oneEighth, oneFourth, threeEighth}
}



NPDSCH-ConfigCommon-NB-r13 ::=	SEQUENCE {
	nrs-Power-r13					INTEGER (-60..50)
}


NPRACH-ConfigSIB-NB-r13 ::=			SEQUENCE {
	nprach-CP-Length-r13				ENUMERATED {us66dot7, us266dot7},
	rsrp-ThresholdsPrachInfoList-r13	RSRP-ThresholdsNPRACH-InfoList-NB-r13	OPTIONAL,	-- need OR
	nprach-ParametersList-r13		NPRACH-ParametersList-NB-r13
}

NPRACH-ConfigSIB-NB-v1330 ::=		SEQUENCE {
	nprach-ParametersList-v1330			NPRACH-ParametersList-NB-v1330
}

NPRACH-ConfigSIB-NB-v1450 ::=		SEQUENCE {
	maxNumPreambleAttemptCE-r14			ENUMERATED {n3, n4, n5, n6, n7, n8, n10, spare1}
}

NPRACH-ParametersList-NB-r13 ::=	SEQUENCE (SIZE (1.. maxNPRACH-Resources-NB-r13)) OF NPRACH-Parameters-NB-r13

NPRACH-ParametersList-NB-v1330 ::=	SEQUENCE (SIZE (1.. maxNPRACH-Resources-NB-r13)) OF NPRACH-Parameters-NB-v1330

NPRACH-Parameters-NB-r13::=			SEQUENCE {
	nprach-Periodicity-r13					ENUMERATED {ms40, ms80, ms160, ms240,
														ms320, ms640, ms1280, ms2560},
	nprach-StartTime-r13					ENUMERATED {ms8, ms16, ms32, ms64,
														ms128, ms256, ms512, ms1024},
	nprach-SubcarrierOffset-r13				ENUMERATED {n0, n12, n24, n36, n2, n18, n34, spare1},
	nprach-NumSubcarriers-r13				ENUMERATED {n12, n24, n36, n48},
	nprach-SubcarrierMSG3-RangeStart-r13	ENUMERATED {zero, oneThird, twoThird, one},
	maxNumPreambleAttemptCE-r13				ENUMERATED {n3, n4, n5, n6, n7, n8, n10, spare1},
	numRepetitionsPerPreambleAttempt-r13	ENUMERATED {n1, n2, n4, n8, n16, n32, n64, n128},
	npdcch-NumRepetitions-RA-r13			ENUMERATED {r1, r2, r4, r8, r16, r32, r64, r128,
														r256, r512, r1024, r2048,
														spare4, spare3, spare2, spare1},
	npdcch-StartSF-CSS-RA-r13				ENUMERATED {v1dot5, v2, v4, v8, v16, v32, v48, v64},
	npdcch-Offset-RA-r13					ENUMERATED {zero, oneEighth, oneFourth, threeEighth}
}

NPRACH-Parameters-NB-v1330 ::=		SEQUENCE {
	nprach-NumCBRA-StartSubcarriers-r13		ENUMERATED {n8, n10, n11, n12, n20, n22, n23, n24,
														n32, n34, n35, n36, n40, n44, n46, n48}
}

RSRP-ThresholdsNPRACH-InfoList-NB-r13 ::= SEQUENCE (SIZE(1..2)) OF RSRP-Range


NPUSCH-ConfigCommon-NB-r13 ::=		SEQUENCE {
	ack-NACK-NumRepetitions-Msg4-r13	SEQUENCE (SIZE(1.. maxNPRACH-Resources-NB-r13)) OF
														ACK-NACK-NumRepetitions-NB-r13,
	srs-SubframeConfig-r13				ENUMERATED {
											sc0, sc1, sc2, sc3, sc4, sc5, sc6, sc7,
											sc8, sc9, sc10, sc11, sc12, sc13, sc14, sc15
											}							OPTIONAL,	-- Need OR
	dmrs-Config-r13						SEQUENCE {
		threeTone-BaseSequence-r13			INTEGER (0..12)			OPTIONAL,	-- Need OP
		threeTone-CyclicShift-r13			INTEGER (0..2),
		sixTone-BaseSequence-r13			INTEGER (0..14)			OPTIONAL,	-- Need OP
		sixTone-CyclicShift-r13				INTEGER (0..3),
		twelveTone-BaseSequence-r13			INTEGER (0..30)			OPTIONAL	-- Need OP
	}		OPTIONAL,	-- Need OR
	ul-ReferenceSignalsNPUSCH-r13		UL-ReferenceSignalsNPUSCH-NB-r13
}

UL-ReferenceSignalsNPUSCH-NB-r13 ::=	SEQUENCE {
	groupHoppingEnabled-r13					BOOLEAN,
	groupAssignmentNPUSCH-r13				INTEGER (0..29)
}

NPUSCH-ConfigDedicated-NB-r13 ::=	SEQUENCE {
	ack-NACK-NumRepetitions-r13			ACK-NACK-NumRepetitions-NB-r13	OPTIONAL,	-- Need ON
	npusch-AllSymbols-r13				BOOLEAN							OPTIONAL,	-- Cond SRS
	groupHoppingDisabled-r13			ENUMERATED {true}				OPTIONAL	-- Need OR
}

ACK-NACK-NumRepetitions-NB-r13	::=	ENUMERATED {r1, r2, r4, r8, r16, r32, r64, r128}



PDCP-Config-NB-r13 ::=		SEQUENCE {
	discardTimer-r13			ENUMERATED {
									ms5120, ms10240, ms20480, ms40960,
									ms81920, infinity, spare2, spare1
									}	OPTIONAL,			-- Cond Setup
	headerCompression-r13		CHOICE {
		notUsed						NULL,
		rohc						SEQUENCE {
			maxCID-r13					INTEGER (1..16383)				DEFAULT 15,
			profiles-r13				SEQUENCE {
				profile0x0002				BOOLEAN,
				profile0x0003				BOOLEAN,
				profile0x0004				BOOLEAN,
				profile0x0006				BOOLEAN,
				profile0x0102				BOOLEAN,
				profile0x0103				BOOLEAN,
				profile0x0104				BOOLEAN
			},
			...
		}
	},
	...
}


PhysicalConfigDedicated-NB-r13 ::=	SEQUENCE {
	carrierConfigDedicated-r13			CarrierConfigDedicated-NB-r13		OPTIONAL,	-- Need ON
	npdcch-ConfigDedicated-r13			NPDCCH-ConfigDedicated-NB-r13		OPTIONAL,	-- Need ON
	npusch-ConfigDedicated-r13			NPUSCH-ConfigDedicated-NB-r13		OPTIONAL,	-- Need ON
	uplinkPowerControlDedicated-r13		UplinkPowerControlDedicated-NB-r13	OPTIONAL,	-- Need ON
	...,
	[[	twoHARQ-ProcessesConfig-r14		ENUMERATED {true}	OPTIONAL	-- Need OR
	]],
	[[	interferenceRandomisationConfig-r14	ENUMERATED {true}	OPTIONAL	-- Need OR
	]]
}


RACH-ConfigCommon-NB-r13 ::=		SEQUENCE {
	preambleTransMax-CE-r13				PreambleTransMax,
	powerRampingParameters-r13			PowerRampingParameters,
	rach-InfoList-r13					RACH-InfoList-NB-r13,
	connEstFailOffset-r13				INTEGER (0..15)					OPTIONAL,	-- Need OP
	...,
	[[	powerRampingParameters-v1450	PowerRampingParameters-NB-v1450	OPTIONAL	-- Need OR
	]]
}

RACH-InfoList-NB-r13 ::=	SEQUENCE (SIZE (1.. maxNPRACH-Resources-NB-r13)) OF RACH-Info-NB-r13

RACH-Info-NB-r13	::=		SEQUENCE {
	ra-ResponseWindowSize-r13			ENUMERATED {
											pp2, pp3, pp4, pp5, pp6, pp7, pp8, pp10},
	mac-ContentionResolutionTimer-r13	ENUMERATED {
											pp1, pp2, pp3, pp4, pp8, pp16, pp32, pp64}
}

PowerRampingParameters-NB-v1450  ::=		SEQUENCE {
	preambleInitialReceivedTargetPower-v1450		ENUMERATED {
													dBm-130, dBm-128, dBm-126, dBm-124, dBm-122,
													dBm-88, dBm-86, dBm-84,dBm-82, dBm-80}
													OPTIONAL,	-- Need OR
	powerRampingParametersCE1-r14				SEQUENCE {
		powerRampingStepCE1-r14						ENUMERATED {dB0, dB2, dB4, dB6},
		preambleInitialReceivedTargetPowerCE1-r14	ENUMERATED {
													dBm-130, dBm-128, dBm-126, dBm-124, dBm-122,
													dBm-120, dBm-118, dBm-116, dBm-114, dBm-112,
													dBm-110, dBm-108, dBm-106, dBm-104, dBm-102,
													dBm-100, dBm-98, dBm-96, dBm-94, dBm-92,
													dBm-90, dBm-88, dBm-86, dBm-84,	dBm-82, dBm-80}
	} OPTIONAL	-- Need OR
}


RadioResourceConfigCommonSIB-NB-r13 ::=	SEQUENCE {
	rach-ConfigCommon-r13					RACH-ConfigCommon-NB-r13,
	bcch-Config-r13						BCCH-Config-NB-r13,
	pcch-Config-r13						PCCH-Config-NB-r13,
	nprach-Config-r13						NPRACH-ConfigSIB-NB-r13,
	npdsch-ConfigCommon-r13					NPDSCH-ConfigCommon-NB-r13,
	npusch-ConfigCommon-r13					NPUSCH-ConfigCommon-NB-r13,
	dl-Gap-r13								DL-GapConfig-NB-r13			OPTIONAL,		-- Need OP
	uplinkPowerControlCommon-r13			UplinkPowerControlCommon-NB-r13,
	...,
	[[	nprach-Config-v1330					NPRACH-ConfigSIB-NB-v1330	OPTIONAL		-- Need OR
	]],
	[[	nprach-Config-v1450					NPRACH-ConfigSIB-NB-v1450	OPTIONAL		-- Cond EnhPowerControl
	]]
}

BCCH-Config-NB-r13 ::=					SEQUENCE {
	modificationPeriodCoeff-r13				ENUMERATED {n16, n32, n64, n128}
}


PCCH-Config-NB-r13 ::=					SEQUENCE {
	defaultPagingCycle-r13					ENUMERATED {rf128, rf256, rf512, rf1024},
	nB-r13									ENUMERATED {
												fourT, twoT, oneT, halfT, quarterT, one8thT,
												one16thT, one32ndT, one64thT,
												one128thT, one256thT, one512thT, one1024thT,
												spare3, spare2, spare1},
	npdcch-NumRepetitionPaging-r13			ENUMERATED {
												r1, r2, r4, r8, r16, r32, r64, r128,
												r256, r512, r1024, r2048,
												spare4, spare3, spare2, spare1}
}


RadioResourceConfigDedicated-NB-r13 ::=	SEQUENCE {
	srb-ToAddModList-r13					SRB-ToAddModList-NB-r13			OPTIONAL,	-- Need ON
	drb-ToAddModList-r13					DRB-ToAddModList-NB-r13			OPTIONAL,	-- Need ON
	drb-ToReleaseList-r13					DRB-ToReleaseList-NB-r13		OPTIONAL,	-- Need ON
	mac-MainConfig-r13						CHOICE {
		explicitValue-r13						MAC-MainConfig-NB-r13,
		defaultValue-r13						NULL
	}																		OPTIONAL,	-- Need ON
	physicalConfigDedicated-r13				PhysicalConfigDedicated-NB-r13	OPTIONAL,	-- Need ON
	rlf-TimersAndConstants-r13				RLF-TimersAndConstants-NB-r13	OPTIONAL,	-- Need ON
	...
}

SRB-ToAddModList-NB-r13 ::=			SEQUENCE (SIZE (1)) OF SRB-ToAddMod-NB-r13

SRB-ToAddMod-NB-r13 ::=				SEQUENCE {
	rlc-Config-r13						CHOICE {
		explicitValue						RLC-Config-NB-r13,
		defaultValue						NULL
	}		OPTIONAL,															-- Cond Setup
	logicalChannelConfig-r13			CHOICE {
		explicitValue						LogicalChannelConfig-NB-r13,
		defaultValue						NULL
	}		OPTIONAL,															-- Cond Setup
	...,
	[[	rlc-Config-v1430				RLC-Config-NB-v1430			OPTIONAL	-- Need ON
	]]
}

DRB-ToAddModList-NB-r13 ::=			SEQUENCE (SIZE (1..maxDRB-NB-r13)) OF DRB-ToAddMod-NB-r13

DRB-ToAddMod-NB-r13 ::=				SEQUENCE {
	eps-BearerIdentity-r13				INTEGER (0..15)				OPTIONAL,	-- Cond DRB-Setup
	drb-Identity-r13					DRB-Identity,
	pdcp-Config-r13						PDCP-Config-NB-r13			OPTIONAL,	-- Cond Setup
	rlc-Config-r13						RLC-Config-NB-r13			OPTIONAL,	-- Cond Setup
	logicalChannelIdentity-r13			INTEGER (3..10)				OPTIONAL,	-- Cond DRB-Setup
	logicalChannelConfig-r13			LogicalChannelConfig-NB-r13	OPTIONAL,	-- Cond Setup
	...,
	[[	rlc-Config-v1430				RLC-Config-NB-v1430			OPTIONAL	-- Need ON
	]]
}

DRB-ToReleaseList-NB-r13 ::=		SEQUENCE (SIZE (1..maxDRB-NB-r13)) OF DRB-Identity


RLC-Config-NB-r13 ::=	CHOICE	{
	am						SEQUENCE {
		ul-AM-RLC-r13				UL-AM-RLC-NB-r13,
		dl-AM-RLC-r13				DL-AM-RLC-NB-r13
	},
	...
}

RLC-Config-NB-v1430 ::=	SEQUENCE {
	t-Reordering-r14			T-Reordering		OPTIONAL		-- Cond twoHARQ
}

UL-AM-RLC-NB-r13 ::=		SEQUENCE {
	t-PollRetransmit-r13		T-PollRetransmit-NB-r13,
	maxRetxThreshold-r13		ENUMERATED {t1, t2, t3, t4, t6, t8, t16, t32}
}

DL-AM-RLC-NB-r13 ::=		SEQUENCE {
	enableStatusReportSN-Gap-r13	ENUMERATED {true}	OPTIONAL
}

T-PollRetransmit-NB-r13 ::=	ENUMERATED {
									ms250,	ms500,	ms1000,	ms2000,	ms3000,	ms4000,
									ms6000, ms10000, ms15000, ms25000, ms40000, ms60000,
									ms90000, ms120000, ms180000, spare1}




RLF-TimersAndConstants-NB-r13 ::=	CHOICE {
	release								NULL,
	setup								SEQUENCE {
		t301-r13							ENUMERATED {
												ms2500, ms4000, ms6000, ms10000,
												ms15000, ms25000, ms40000, ms60000},
		t310-r13							ENUMERATED {
												ms0, ms200, ms500, ms1000, ms2000, ms4000, ms8000},
		n310-r13							ENUMERATED {
												n1, n2, n3, n4, n6, n8, n10, n20},
		t311-r13							ENUMERATED {
												ms1000, ms3000, ms5000, ms10000, ms15000,
												ms20000, ms30000},
		n311-r13							ENUMERATED {
												n1, n2, n3, n4, n5, n6, n8, n10},
		...,
		[[ t311-v1350						ENUMERATED {
												ms40000, ms60000, ms90000, ms120000}
														OPTIONAL	-- Need OR
		]]
	}
}



UplinkPowerControlCommon-NB-r13 ::=	SEQUENCE {
	p0-NominalNPUSCH-r13				INTEGER (-126..24),
	alpha-r13							ENUMERATED {al0, al04, al05, al06, al07, al08, al09, al1},
	deltaPreambleMsg3-r13				INTEGER (-1..6)
}

UplinkPowerControlDedicated-NB-r13 ::=	SEQUENCE {
	p0-UE-NPUSCH-r13						INTEGER (-8..7)
}


AdditionalBandInfoList-NB-r14 ::=	SEQUENCE (SIZE (1..maxMultiBands)) OF FreqBandIndicator-NB-r13


FreqBandIndicator-NB-r13 ::=			INTEGER (1.. maxFBI2)


MultiBandInfoList-NB-r13 ::=	SEQUENCE (SIZE (1..maxMultiBands)) OF MultiBandInfo-NB-r13

MultiBandInfo-NB-r13 ::=		SEQUENCE {
	freqBandIndicator-r13			FreqBandIndicator-NB-r13		OPTIONAL,	-- Need OR
	freqBandInfo-r13				NS-PmaxList-NB-r13				OPTIONAL	-- Need OR
}


NS-PmaxList-NB-r13 ::=			SEQUENCE (SIZE (1..maxNS-Pmax-NB-r13)) OF NS-PmaxValue-NB-r13

NS-PmaxValue-NB-r13 ::=			SEQUENCE {
	additionalPmax-r13				P-Max						OPTIONAL,	-- Need OR
	additionalSpectrumEmission-r13	AdditionalSpectrumEmission
}


ReselectionThreshold-NB-v1360 ::=			INTEGER (32..63)


T-Reselection-NB-r13 ::=		ENUMERATED {s0, s3, s6, s9, s12, s15, s18, s21}


CQI-NPDCCH-NB-r14 ::=	ENUMERATED {
							noMeasurements, candidateRep-A, candidateRep-B, candidateRep-C,
							candidateRep-D, candidateRep-E, candidateRep-F, candidateRep-G,
							candidateRep-H, candidateRep-I, candidateRep-J, candidateRep-K,
							candidateRep-L}


CQI-NPDCCH-Short-NB-r14 ::=	ENUMERATED {
								noMeasurements, candidateRep-1, candidateRep-2, candidateRep-3}


MeasResultServCell-NB-r14 ::=	SEQUENCE {
	nrsrpResult-r14					NRSRP-Range-NB-r14,
	nrsrqResult-r14					NRSRQ-Range-NB-r14
}


NRSRP-Range-NB-r14 ::=				INTEGER(0..113)


NRSRQ-Range-NB-r14 ::=				INTEGER(-30..46)


EstablishmentCause-NB-r13 ::=			ENUMERATED {
											mt-Access, mo-Signalling, mo-Data, mo-ExceptionData,
											delayTolerantAccess-v1330, spare3, spare2, spare1}


UE-Capability-NB-r13 ::=		SEQUENCE {
	accessStratumRelease-r13		AccessStratumRelease-NB-r13,
	ue-Category-NB-r13				ENUMERATED {nb1}					OPTIONAL,
	multipleDRB-r13					ENUMERATED {supported}				OPTIONAL,
	pdcp-Parameters-r13				PDCP-Parameters-NB-r13				OPTIONAL,
	phyLayerParameters-r13			PhyLayerParameters-NB-r13,
	rf-Parameters-r13				RF-Parameters-NB-r13,
	dummy							SEQUENCE {}							OPTIONAL
}

UE-Capability-NB-Ext-r14-IEs ::=		SEQUENCE {
	ue-Category-NB-r14					ENUMERATED {nb2}				OPTIONAL,
	mac-Parameters-r14					MAC-Parameters-NB-r14			OPTIONAL,
	phyLayerParameters-v1430			PhyLayerParameters-NB-v1430		OPTIONAL,
	rf-Parameters-v1430					RF-Parameters-NB-v1430,
	nonCriticalExtension				UE-Capability-NB-v1440-IEs		OPTIONAL
}

UE-Capability-NB-v1440-IEs ::=		SEQUENCE {
	phyLayerParameters-v1440			PhyLayerParameters-NB-v1440		OPTIONAL,
	nonCriticalExtension				SEQUENCE {}						OPTIONAL
}

AccessStratumRelease-NB-r13 ::=		ENUMERATED {rel13, rel14, spare6, spare5, spare4, spare3, spare2, spare1, ...}

PDCP-Parameters-NB-r13		::= SEQUENCE {
	supportedROHC-Profiles-r13			SEQUENCE {
		profile0x0002						BOOLEAN,
		profile0x0003						BOOLEAN,
		profile0x0004						BOOLEAN,
		profile0x0006						BOOLEAN,
		profile0x0102						BOOLEAN,
		profile0x0103						BOOLEAN,
		profile0x0104						BOOLEAN
	},
	maxNumberROHC-ContextSessions-r13	ENUMERATED {cs2, cs4, cs8, cs12}	DEFAULT cs2,
	...
}

MAC-Parameters-NB-r14		::=		SEQUENCE {
	dataInactMon-r14					ENUMERATED {supported}					OPTIONAL,
	rai-Support-r14						ENUMERATED {supported}				OPTIONAL
}

PhyLayerParameters-NB-r13	::=		SEQUENCE {
	multiTone-r13						ENUMERATED {supported}			OPTIONAL,
	multiCarrier-r13						ENUMERATED {supported}			OPTIONAL
	}

PhyLayerParameters-NB-v1430	::=		SEQUENCE {
	multiCarrier-NPRACH-r14				ENUMERATED {supported}			OPTIONAL,
	twoHARQ-Processes-r14				ENUMERATED {supported}			OPTIONAL
}

PhyLayerParameters-NB-v1440	::=		SEQUENCE {
	interferenceRandomisation-r14		ENUMERATED {supported}			OPTIONAL
}

RF-Parameters-NB-r13	::=			SEQUENCE {
	supportedBandList-r13				SupportedBandList-NB-r13,
	multiNS-Pmax-r13					ENUMERATED {supported}		OPTIONAL
}

RF-Parameters-NB-v1430 ::=			SEQUENCE {
	powerClassNB-14dBm-r14				ENUMERATED {supported}		OPTIONAL
}

SupportedBandList-NB-r13 ::=		SEQUENCE (SIZE (1..maxBands)) OF SupportedBand-NB-r13

SupportedBand-NB-r13	::=			SEQUENCE {
	band-r13							FreqBandIndicator-NB-r13,
	powerClassNB-20dBm-r13				ENUMERATED {supported}		OPTIONAL
}


UE-RadioPagingInfo-NB-r13 ::=		SEQUENCE {
	ue-Category-NB-r13				ENUMERATED {nb1}			OPTIONAL,
	...,
	[[ multiCarrierPaging-r14		ENUMERATED {true}			OPTIONAL
	]]
}


UE-TimersAndConstants-NB-r13 ::=	SEQUENCE {
	t300-r13							ENUMERATED {
											ms2500, ms4000, ms6000, ms10000,
											ms15000, ms25000, ms40000, ms60000},
	t301-r13							ENUMERATED {
											ms2500, ms4000, ms6000, ms10000,
											ms15000, ms25000, ms40000, ms60000},
	t310-r13							ENUMERATED {
											ms0, ms200, ms500, ms1000, ms2000, ms4000, ms8000},
	n310-r13							ENUMERATED {
											n1, n2, n3, n4, n6, n8, n10, n20},
	t311-r13							ENUMERATED {
											ms1000, ms3000, ms5000, ms10000, ms15000,
											ms20000, ms30000},
	n311-r13							ENUMERATED {
											n1, n2, n3, n4, n5, n6, n8, n10},
	...,
	[[ t311-v1350						ENUMERATED {
											ms40000, ms60000, ms90000, ms120000}
														OPTIONAL	-- Need OR
	]]
}


SC-MTCH-InfoList-NB-r14 ::=			SEQUENCE (SIZE (0.. maxSC-MTCH-NB-r14)) OF SC-MTCH-Info-NB-r14

SC-MTCH-Info-NB-r14 ::=				SEQUENCE	{
	sc-mtch-CarrierConfig-r14			CHOICE {
		dl-CarrierConfig-r14					DL-CarrierConfigCommon-NB-r14,
		dl-CarrierIndex-r14					INTEGER (0.. maxNonAnchorCarriers-NB-r14)
	},
	mbmsSessionInfo-r14					MBMSSessionInfo-r13,
	g-RNTI-r14							BIT STRING(SIZE(16)),
	sc-mtch-SchedulingInfo-r14			SC-MTCH-SchedulingInfo-NB-r14		OPTIONAL,	-- Need OP
	sc-mtch-NeighbourCell-r14			BIT STRING (SIZE(maxNeighCell-SCPTM-NB-r14))	OPTIONAL,	-- Need OP
	npdcch-NPDSCH-MaxTBS-SC-MTCH-r14		ENUMERATED {n680, n2536},
	npdcch-NumRepetitions-SC-MTCH-r14	ENUMERATED {r1, r2, r4, r8, r16,
													r32, r64, r128, r256,
													r512, r1024, r2048, spare4,
													spare3, spare2, spare1},
	npdcch-StartSF-SC-MTCH-r14			ENUMERATED {v1dot5, v2, v4, v8,
													v16, v32, v48, v64},
	npdcch-Offset-SC-MTCH-r14			ENUMERATED {zero, oneEighth, oneQuarter,
													threeEighth, oneHalf, fiveEighth,
													threeQuarter, sevenEighth},
	...
}

SC-MTCH-SchedulingInfo-NB-r14 ::=		SEQUENCE	{
	onDurationTimerSCPTM-r14				ENUMERATED {
												pp1, pp2, pp3, pp4,
												pp8, pp16, pp32, spare},
	drx-InactivityTimerSCPTM-r14			ENUMERATED {
												pp0, pp1, pp2, pp3,
												pp4, pp8, pp16, pp32},
	schedulingPeriodStartOffsetSCPTM-r14	CHOICE {
		sf10									INTEGER(0..9),
		sf20									INTEGER(0..19),
		sf32									INTEGER(0..31),
		sf40									INTEGER(0..39),
		sf64									INTEGER(0..63),
		sf80									INTEGER(0..79),
		sf128									INTEGER(0..127),
		sf160									INTEGER(0..159),
		sf256									INTEGER(0..255),
		sf320									INTEGER(0..319),
		sf512									INTEGER(0..511),
		sf640									INTEGER(0..639),
		sf1024									INTEGER(0..1023),
		sf2048									INTEGER(0..2047),
		sf4096									INTEGER(0..4095),
		sf8192									INTEGER(0..8191)
	},
	...
}


SCPTM-NeighbourCellList-NB-r14 ::=	SEQUENCE (SIZE (1..maxNeighCell-SCPTM-NB-r14)) OF PCI-ARFCN-NB-r14

PCI-ARFCN-NB-r14 ::=				SEQUENCE {
	physCellId-r14						PhysCellId,
	carrierFreq-r14						CarrierFreq-NB-r13		OPTIONAL	-- Need OP
}


maxNPRACH-Resources-NB-r13	INTEGER ::=	3	-- Maximum number of NPRACH resources for NB-IoT
maxNonAnchorCarriers-NB-r14	INTEGER ::= 15	-- Maximum number of non-anchor carriers for NB-IoT
maxDRB-NB-r13				INTEGER ::= 2	-- Maximum number of Data Radio Bearers for NB-IoT
maxNeighCell-SCPTM-NB-r14	INTEGER ::= 8	-- Maximum number of SCPTM neighbour cells
maxNS-Pmax-NB-r13			INTEGER ::= 4	-- Maximum number of NS and P-Max values per band
maxSC-MTCH-NB-r14			INTEGER ::= 64	-- Maximum number of SC-MTCHs in one cell for NB-IoT
maxSI-Message-NB-r13		INTEGER ::= 8	-- Maximum number of SI messages for NB-IoT


END


EUTRA-UE-Variables DEFINITIONS AUTOMATIC TAGS ::=

BEGIN

IMPORTS
	AbsoluteTimeInfo-r10,
	AreaConfiguration-r10,
	AreaConfiguration-v1130,
	CarrierFreqGERAN,
	CellIdentity,
	ConnEstFailReport-r11,
	SpeedStateScaleFactors,
	C-RNTI,
	LoggingDuration-r10,
	LoggingInterval-r10,
	LogMeasInfo-r10,
	MeasCSI-RS-Id-r12,
	MeasId,
	MeasId-v1250,
	MeasIdToAddModList,
	MeasIdToAddModListExt-r12,
	MeasIdToAddModList-v1310,
	MeasIdToAddModListExt-v1310,
	MeasObjectToAddModList,
	MeasObjectToAddModList-v9e0,
	MeasObjectToAddModListExt-r13,
	MeasScaleFactor-r12,
	MobilityStateParameters,
	NeighCellConfig,
	PhysCellId,
	PhysCellIdCDMA2000,
	PhysCellIdGERAN,
	PhysCellIdUTRA-FDD,
	PhysCellIdUTRA-TDD,
	PLMN-Identity,
	PLMN-IdentityList3-r11,
	QuantityConfig,
	ReportConfigToAddModList,
	RLF-Report-r9,
	TargetMBSFN-AreaList-r12,
	TraceReference-r10,
	Tx-ResourcePoolMeasList-r14,
	VisitedCellInfoList-r12,
	maxCellMeas,
	maxCSI-RS-Meas-r12,
	maxMeasId,
	maxMeasId-r12,
	UL-DelayConfig-r13,
	WLAN-CarrierInfo-r13,
	WLAN-Identifiers-r12,
	WLAN-Id-List-r13,
	WLAN-Status-r13,
	WLAN-Status-v1430,
	WLAN-SuspendConfig-r14

FROM EUTRA-RRC-Definitions;


VarConnEstFailReport-r11 ::=		SEQUENCE {
	connEstFailReport-r11				ConnEstFailReport-r11,
	plmn-Identity-r11					PLMN-Identity
}


VarLogMeasConfig-r10 ::=				SEQUENCE {
	areaConfiguration-r10			AreaConfiguration-r10		OPTIONAL,
	loggingDuration-r10				LoggingDuration-r10,
	loggingInterval-r10				LoggingInterval-r10
}

VarLogMeasConfig-r11 ::=		SEQUENCE {
	areaConfiguration-r10			AreaConfiguration-r10		OPTIONAL,
	areaConfiguration-v1130			AreaConfiguration-v1130		OPTIONAL,
	loggingDuration-r10				LoggingDuration-r10,
	loggingInterval-r10				LoggingInterval-r10
}

VarLogMeasConfig-r12 ::=		SEQUENCE {
	areaConfiguration-r10			AreaConfiguration-r10		OPTIONAL,
	areaConfiguration-v1130			AreaConfiguration-v1130		OPTIONAL,
	loggingDuration-r10				LoggingDuration-r10,
	loggingInterval-r10				LoggingInterval-r10,
	targetMBSFN-AreaList-r12		TargetMBSFN-AreaList-r12	OPTIONAL
}


VarLogMeasReport-r10 ::=				SEQUENCE {
	traceReference-r10					TraceReference-r10,
	traceRecordingSessionRef-r10			OCTET STRING (SIZE (2)),
	tce-Id-r10							OCTET STRING (SIZE (1)),
	plmn-Identity-r10					PLMN-Identity,
	absoluteTimeInfo-r10				AbsoluteTimeInfo-r10,
	logMeasInfoList-r10					LogMeasInfoList2-r10
}

VarLogMeasReport-r11 ::=			SEQUENCE {
	traceReference-r10					TraceReference-r10,
	traceRecordingSessionRef-r10		OCTET STRING (SIZE (2)),
	tce-Id-r10							OCTET STRING (SIZE (1)),
	plmn-IdentityList-r11				PLMN-IdentityList3-r11,
	absoluteTimeInfo-r10				AbsoluteTimeInfo-r10,
	logMeasInfoList-r10					LogMeasInfoList2-r10
}

LogMeasInfoList2-r10 ::=				SEQUENCE (SIZE (1..maxLogMeas-r10)) OF LogMeasInfo-r10


VarMeasConfig ::=					SEQUENCE {
	-- Measurement identities
	measIdList							MeasIdToAddModList					OPTIONAL,
	measIdListExt-r12					MeasIdToAddModListExt-r12			OPTIONAL,
	measIdList-v1310						MeasIdToAddModList-v1310				OPTIONAL,
	measIdListExt-v1310					MeasIdToAddModListExt-v1310			OPTIONAL,
	-- Measurement objects
	measObjectList						MeasObjectToAddModList				OPTIONAL,
	measObjectListExt-r13				MeasObjectToAddModListExt-r13		OPTIONAL,
	measObjectList-v9i0					MeasObjectToAddModList-v9e0			OPTIONAL,
	-- Reporting configurations
	reportConfigList					ReportConfigToAddModList			OPTIONAL,
	-- Other parameters
	quantityConfig						QuantityConfig						OPTIONAL,
	measScaleFactor-r12					MeasScaleFactor-r12					OPTIONAL,
	s-Measure							INTEGER (-140..-44)					OPTIONAL,
	speedStatePars						CHOICE {
		release								NULL,
		setup								SEQUENCE {
			mobilityStateParameters				MobilityStateParameters,
			timeToTrigger-SF					SpeedStateScaleFactors
		}
	}																		OPTIONAL,
	allowInterruptions-r11			BOOLEAN								OPTIONAL
}


VarMeasReportList ::=				SEQUENCE (SIZE (1..maxMeasId)) OF VarMeasReport
VarMeasReportList-r12 ::=			SEQUENCE (SIZE (1..maxMeasId-r12)) OF VarMeasReport

VarMeasReport ::=					SEQUENCE {
	-- List of measurement that have been triggered
	measId								MeasId,
	measId-v1250						MeasId-v1250					OPTIONAL,
	cellsTriggeredList					CellsTriggeredList				OPTIONAL,
	csi-RS-TriggeredList-r12			CSI-RS-TriggeredList-r12		OPTIONAL,
	poolsTriggeredList-r14				Tx-ResourcePoolMeasList-r14	OPTIONAL,
	numberOfReportsSent					INTEGER
}

CellsTriggeredList ::=				SEQUENCE (SIZE (1..maxCellMeas)) OF CHOICE {
	physCellIdEUTRA							PhysCellId,
	physCellIdUTRA							CHOICE {
		fdd										PhysCellIdUTRA-FDD,
		tdd										PhysCellIdUTRA-TDD
	},
	physCellIdGERAN							SEQUENCE {
		carrierFreq								CarrierFreqGERAN,
		physCellId								PhysCellIdGERAN
	},
	physCellIdCDMA2000						PhysCellIdCDMA2000,
	wlan-Identifiers-r13					WLAN-Identifiers-r12
}

CSI-RS-TriggeredList-r12 ::=		SEQUENCE (SIZE (1..maxCSI-RS-Meas-r12)) OF MeasCSI-RS-Id-r12

VarMobilityHistoryReport-r12 ::=	VisitedCellInfoList-r12


VarRLF-Report-r10 ::=				SEQUENCE {
	rlf-Report-r10							RLF-Report-r9,
	plmn-Identity-r10						PLMN-Identity
}

VarRLF-Report-r11 ::=				SEQUENCE {
	rlf-Report-r10						RLF-Report-r9,
	plmn-IdentityList-r11				PLMN-IdentityList3-r11
}


VarShortMAC-Input ::=					SEQUENCE {
	cellIdentity							CellIdentity,
	physCellId								PhysCellId,
	c-RNTI									C-RNTI
}


VarShortResumeMAC-Input-r13 ::=		SEQUENCE {
	cellIdentity-r13						CellIdentity,
	physCellId-r13							PhysCellId,
	c-RNTI-r13								C-RNTI,
	resumeDiscriminator-r13					BIT STRING(SIZE(1))
}


VarWLAN-MobilityConfig ::=					SEQUENCE {
	wlan-MobilitySet-r13					WLAN-Id-List-r13			OPTIONAL,
	successReportRequested					ENUMERATED {true}			OPTIONAL,
	wlan-SuspendConfig-r14					WLAN-SuspendConfig-r14		OPTIONAL
}


VarWLAN-Status-r13 ::=				SEQUENCE {
	status-r13								WLAN-Status-r13,
	status-r14								WLAN-Status-v1430	OPTIONAL
}


maxLogMeas-r10				INTEGER ::= 4060-- Maximum number of logged measurement entries
											--  that can be stored by the UE


END


NBIOT-UE-Variables DEFINITIONS AUTOMATIC TAGS ::=

BEGIN

IMPORTS
	VarShortMAC-Input,
	VarShortResumeMAC-Input-r13

FROM EUTRA-UE-Variables;

VarShortMAC-Input-NB-r13		::=	VarShortMAC-Input

VarShortResumeMAC-Input-NB-r13	::=	VarShortResumeMAC-Input-r13


END


EUTRA-Sidelink-Preconf DEFINITIONS AUTOMATIC TAGS ::=

BEGIN

IMPORTS
	AdditionalSpectrumEmission,
	AdditionalSpectrumEmission-v10l0,
	ARFCN-ValueEUTRA-r9,
	FilterCoefficient,
	maxCBR-Level-r14,
	maxCBR-Level-1-r14,
	maxFreq,
	maxFreqV2X-r14,
	maxSL-TxPool-r12,
	maxSL-CommRxPoolPreconf-v1310,
	maxSL-CommTxPoolPreconf-v1310,
	maxSL-DiscRxPoolPreconf-r13,
	maxSL-DiscTxPoolPreconf-r13,
	maxSL-V2X-CBRConfig2-r14,
	maxSL-V2X-CBRConfig2-1-r14,
	maxSL-V2X-RxPoolPreconf-r14,
	maxSL-V2X-TxConfig2-r14,
	maxSL-V2X-TxConfig2-1-r14,
	maxSL-V2X-TxPoolPreconf-r14,
	P-Max,
	ReselectionInfoRelay-r13,
	SL-AnchorCarrierFreqList-V2X-r14,
	SL-CBR-Levels-Config-r14,
	SL-CBR-PSSCH-TxConfig-r14,
	SL-CommTxPoolSensingConfig-r14,
	SL-CP-Len-r12,
	SL-HoppingConfigComm-r12,
	SL-OffsetIndicator-r12,
	SL-OffsetIndicatorSync-r12,
	SL-OffsetIndicatorSync-v1430,
	SL-PeriodComm-r12,
	RSRP-RangeSL3-r12,
	SL-PriorityList-r13,
	SL-TF-ResourceConfig-r12,
	SL-TRPT-Subset-r12,
	SL-TxParameters-r12,
	SL-ZoneConfig-r14,
	P0-SL-r12,
	TDD-ConfigSL-r12,
	SubframeBitmapSL-r14,
	SL-P2X-ResourceSelectionConfig-r14,
	SL-RestrictResourceReservationPeriodList-r14,
	SL-SyncAllowed-r14,
	SL-OffsetIndicatorSync-r14,
	SL-Priority-r13
FROM EUTRA-RRC-Definitions;


SL-Preconfiguration-r12 ::=		SEQUENCE {
	preconfigGeneral-r12				SL-PreconfigGeneral-r12,
	preconfigSync-r12					SL-PreconfigSync-r12,
	preconfigComm-r12					SL-PreconfigCommPoolList4-r12,
	...,
	[[	preconfigComm-v1310				SEQUENCE {
			commRxPoolList-r13			SL-PreconfigCommRxPoolList-r13,
			commTxPoolList-r13			SL-PreconfigCommTxPoolList-r13		OPTIONAL
		}																		OPTIONAL,
		preconfigDisc-r13				SEQUENCE {
			discRxPoolList-r13				SL-PreconfigDiscRxPoolList-r13,
			discTxPoolList-r13				SL-PreconfigDiscTxPoolList-r13		OPTIONAL
		}																		OPTIONAL,
		preconfigRelay-r13				SL-PreconfigRelay-r13				OPTIONAL
	]]

}

SL-PreconfigGeneral-r12 ::=		SEQUENCE {
	-- PDCP configuration
	rohc-Profiles-r12					SEQUENCE {
		profile0x0001-r12						BOOLEAN,
		profile0x0002-r12						BOOLEAN,
		profile0x0004-r12						BOOLEAN,
		profile0x0006-r12						BOOLEAN,
		profile0x0101-r12						BOOLEAN,
		profile0x0102-r12						BOOLEAN,
		profile0x0104-r12						BOOLEAN
	},
	-- Physical configuration
	carrierFreq-r12						ARFCN-ValueEUTRA-r9,
	maxTxPower-r12						P-Max,
	additionalSpectrumEmission-r12		AdditionalSpectrumEmission,
	sl-bandwidth-r12					ENUMERATED {n6, n15, n25, n50, n75, n100},
	tdd-ConfigSL-r12					TDD-ConfigSL-r12,
	reserved-r12						BIT STRING (SIZE (19)),
	...,
	[[	additionalSpectrumEmission-v1440		AdditionalSpectrumEmission-v10l0		OPTIONAL
	]]
}

SL-PreconfigSync-r12 ::=	SEQUENCE {
	syncCP-Len-r12						SL-CP-Len-r12,
	syncOffsetIndicator1-r12			SL-OffsetIndicatorSync-r12,
	syncOffsetIndicator2-r12			SL-OffsetIndicatorSync-r12,
	syncTxParameters-r12				P0-SL-r12,
	syncTxThreshOoC-r12					RSRP-RangeSL3-r12,
	filterCoefficient-r12				FilterCoefficient,
	syncRefMinHyst-r12					ENUMERATED {dB0, dB3, dB6, dB9, dB12},
	syncRefDiffHyst-r12					ENUMERATED {dB0, dB3, dB6, dB9, dB12, dBinf},
	...,
	[[	syncTxPeriodic-r13					ENUMERATED {true}			OPTIONAL
	]]
}

SL-PreconfigCommPoolList4-r12 ::=	SEQUENCE (SIZE (1..maxSL-TxPool-r12)) OF SL-PreconfigCommPool-r12

SL-PreconfigCommRxPoolList-r13 ::=	SEQUENCE (SIZE (1..maxSL-CommRxPoolPreconf-v1310)) OF SL-PreconfigCommPool-r12

SL-PreconfigCommTxPoolList-r13 ::=	SEQUENCE (SIZE (1..maxSL-CommTxPoolPreconf-v1310)) OF SL-PreconfigCommPool-r12

SL-PreconfigCommPool-r12 ::=		SEQUENCE {
-- This IE is same as SL-CommResourcePool with rxParametersNCell absent
	sc-CP-Len-r12						SL-CP-Len-r12,
	sc-Period-r12						SL-PeriodComm-r12,
	sc-TF-ResourceConfig-r12			SL-TF-ResourceConfig-r12,
	sc-TxParameters-r12					P0-SL-r12,
	data-CP-Len-r12						SL-CP-Len-r12,
	data-TF-ResourceConfig-r12			SL-TF-ResourceConfig-r12,
	dataHoppingConfig-r12				SL-HoppingConfigComm-r12,
	dataTxParameters-r12				P0-SL-r12,
	trpt-Subset-r12						SL-TRPT-Subset-r12,
	...,
	[[	priorityList-r13				SL-PriorityList-r13			OPTIONAL	-- For Tx
	]]
}

SL-PreconfigDiscRxPoolList-r13 ::=	SEQUENCE (SIZE (1..maxSL-DiscRxPoolPreconf-r13)) OF SL-PreconfigDiscPool-r13

SL-PreconfigDiscTxPoolList-r13 ::=	SEQUENCE (SIZE (1..maxSL-DiscTxPoolPreconf-r13)) OF SL-PreconfigDiscPool-r13

SL-PreconfigDiscPool-r13 ::=		SEQUENCE {
-- This IE is same as SL-DiscResourcePool with rxParameters absent
	cp-Len-r13						SL-CP-Len-r12,
	discPeriod-r13				ENUMERATED {rf4, rf6, rf7, rf8, rf12, rf14, rf16, rf24, rf28,
										rf32, rf64, rf128, rf256, rf512, rf1024, spare},
	numRetx-r13					INTEGER (0..3),
	numRepetition-r13				INTEGER (1..50),
	tf-ResourceConfig-r13			SL-TF-ResourceConfig-r12,
	txParameters-r13				SEQUENCE {
		txParametersGeneral-r13		P0-SL-r12,
		txProbability-r13			ENUMERATED {p25, p50, p75, p100}
	}																OPTIONAL,
	...
}

SL-PreconfigRelay-r13 ::=	SEQUENCE {
	reselectionInfoOoC-r13			ReselectionInfoRelay-r13
}


SL-V2X-Preconfiguration-r14 ::=	SEQUENCE {
	v2x-PreconfigFreqList-r14		SL-V2X-PreconfigFreqList-r14,
	anchorCarrierFreqList-r14		SL-AnchorCarrierFreqList-V2X-r14				OPTIONAL,
	cbr-PreconfigList-r14			SL-CBR-PreconfigTxConfigList-r14				OPTIONAL,
	...
}

SL-CBR-PreconfigTxConfigList-r14 ::=	SEQUENCE {
	cbr-RangeCommonConfigList-r14	SEQUENCE (SIZE (1..maxSL-V2X-CBRConfig2-r14)) OF SL-CBR-Levels-Config-r14,
	sl-CBR-PSSCH-TxConfigList-r14	SEQUENCE (SIZE (1..maxSL-V2X-TxConfig2-r14)) OF SL-CBR-PSSCH-TxConfig-r14
}

SL-V2X-PreconfigFreqList-r14 ::=	SEQUENCE (SIZE (1..maxFreqV2X-r14)) OF SL-V2X-PreconfigFreqInfo-r14

SL-V2X-PreconfigFreqInfo-r14 ::=		SEQUENCE {
	v2x-CommPreconfigGeneral-r14		SL-PreconfigGeneral-r12,
	v2x-CommPreconfigSync-r14			SL-PreconfigV2X-Sync-r14				OPTIONAL,
	v2x-CommRxPoolList-r14				SL-PreconfigV2X-RxPoolList-r14,
	v2x-CommTxPoolList-r14				SL-PreconfigV2X-TxPoolList-r14,
	p2x-CommTxPoolList-r14				SL-PreconfigV2X-TxPoolList-r14,
	v2x-ResourceSelectionConfig-r14			SL-CommTxPoolSensingConfig-r14			OPTIONAL,
	zoneConfig-r14						SL-ZoneConfig-r14						OPTIONAL,
	syncPriority-r14					ENUMERATED {gnss, enb},
	thresSL-TxPrioritization-r14		SL-Priority-r13						OPTIONAL,
	offsetDFN-r14						INTEGER (0..1000)					OPTIONAL,
	...
}

SL-PreconfigV2X-RxPoolList-r14 ::=	SEQUENCE (SIZE (1..maxSL-V2X-RxPoolPreconf-r14)) OF SL-V2X-PreconfigCommPool-r14

SL-PreconfigV2X-TxPoolList-r14 ::=	SEQUENCE (SIZE (1..maxSL-V2X-TxPoolPreconf-r14)) OF SL-V2X-PreconfigCommPool-r14

SL-V2X-PreconfigCommPool-r14 ::=		SEQUENCE {
-- This IE is same as SL-CommResourcePoolV2X with rxParametersNCell absent
	sl-OffsetIndicator-r14				SL-OffsetIndicator-r12		OPTIONAL,
	sl-Subframe-r14						SubframeBitmapSL-r14,
	adjacencyPSCCH-PSSCH-r14			BOOLEAN,
	sizeSubchannel-r14					ENUMERATED {
										n4, n5, n6, n8, n9, n10, n12, n15, n16, n18, n20, n25, n30,
										n48, n50, n72, n75, n96, n100, spare13, spare12, spare11,
										spare10, spare9, spare8, spare7, spare6, spare5, spare4,
										spare3, spare2, spare1},
	numSubchannel-r14					ENUMERATED {n1, n3, n5, n8, n10, n15, n20, spare1},
	startRB-Subchannel-r14				INTEGER (0..99),
	startRB-PSCCH-Pool-r14				INTEGER (0..99)				OPTIONAL,
	dataTxParameters-r14				P0-SL-r12,
	zoneID-r14							INTEGER (0..7)				OPTIONAL,
	threshS-RSSI-CBR-r14					INTEGER (0..45)				OPTIONAL,
	cbr-pssch-TxConfigList-r14			SL-CBR-PPPP-TxPreconfigList-r14	OPTIONAL,
	resourceSelectionConfigP2X-r14		SL-P2X-ResourceSelectionConfig-r14	OPTIONAL,
	syncAllowed-r14						SL-SyncAllowed-r14				OPTIONAL,
	restrictResourceReservationPeriod-r14	SL-RestrictResourceReservationPeriodList-r14	OPTIONAL,	-- Need OR
	...
}

SL-PreconfigV2X-Sync-r14 ::=	SEQUENCE {
	syncOffsetIndicators-r14			SL-V2X-SyncOffsetIndicators-r14,
	syncTxParameters-r14				P0-SL-r12,
	syncTxThreshOoC-r14					RSRP-RangeSL3-r12,
	filterCoefficient-r14				FilterCoefficient,
	syncRefMinHyst-r14					ENUMERATED {dB0, dB3, dB6, dB9, dB12},
	syncRefDiffHyst-r14					ENUMERATED {dB0, dB3, dB6, dB9, dB12, dBinf},
	...
}

SL-V2X-SyncOffsetIndicators-r14 ::=	SEQUENCE {
	syncOffsetIndicator1-r14			SL-OffsetIndicatorSync-r14,
	syncOffsetIndicator2-r14			SL-OffsetIndicatorSync-r14,
	syncOffsetIndicator3-r14			SL-OffsetIndicatorSync-r14			OPTIONAL
}

SL-CBR-PPPP-TxPreconfigList-r14 ::=	SEQUENCE (SIZE (1..8)) OF SL-PPPP-TxPreconfigIndex-r14

SL-PPPP-TxPreconfigIndex-r14 ::=	SEQUENCE {
	priorityThreshold-r14			SL-Priority-r13,
	defaultTxConfigIndex-r14		INTEGER(0..maxCBR-Level-1-r14),
	cbr-ConfigIndex-r14				INTEGER(0..maxSL-V2X-CBRConfig2-1-r14),
	tx-ConfigIndexList-r14			SEQUENCE (SIZE (1..maxCBR-Level-r14)) OF Tx-PreconfigIndex-r14
}

Tx-PreconfigIndex-r14 ::=			INTEGER(0..maxSL-V2X-TxConfig2-1-r14)

END


EUTRA-InterNodeDefinitions DEFINITIONS AUTOMATIC TAGS ::=

BEGIN

IMPORTS
	AntennaInfoCommon,
	AntennaInfoDedicated-v10i0,
	ARFCN-ValueEUTRA,
	ARFCN-ValueEUTRA-v9e0,
	ARFCN-ValueEUTRA-r9,
	CellIdentity,
	C-RNTI,
	DL-DCCH-Message,
	DRB-Identity,
	DRB-ToReleaseList,
	FreqBandIndicator-r11,
	InDeviceCoexIndication-r11,
	LWA-Config-r13,
	MasterInformationBlock,
	maxBands,
	maxFreq,
	maxDRB,
	maxSCell-r10,
	maxSCell-r13,
	maxServCell-r10,
	maxServCell-r13,
	MBMSInterestIndication-r11,
	MeasConfig,
	MeasGapConfig,
	MeasGapConfigPerCC-List-r14,
	MeasResultForRSSI-r13,
	MeasResultListWLAN-r13,
	OtherConfig-r9,
	PhysCellId,
	P-Max,
	PowerCoordinationInfo-r12,
	SidelinkUEInformation-r12,
	SL-CommConfig-r12,
	SL-DiscConfig-r12,
	RadioResourceConfigDedicated,
	RCLWI-Configuration-r13,
	RSRP-Range,
	RSRQ-Range,
	RSRQ-Range-v1250,
	RS-SINR-Range-r13,
	SCellToAddModList-r10,
	SCellToAddModListExt-r13,
	SCG-ConfigPartSCG-r12,
	SecurityAlgorithmConfig,
	SCellIndex-r10,
	SCellIndex-r13,
	SCellToReleaseList-r10,
	SCellToReleaseListExt-r13,
	ServCellIndex-r10,
	ServCellIndex-r13,
	ShortMAC-I,
	MeasResultSSTD-r13,
	SL-V2X-ConfigDedicated-r14,
	SystemInformationBlockType1,
	SystemInformationBlockType1-v890-IEs,
	SystemInformationBlockType2,
	UEAssistanceInformation-r11,
	UECapabilityInformation,
	UE-CapabilityRAT-ContainerList,
	UE-RadioPagingInfo-r12,
	WLANConnectionStatusReport-r13,
	WLAN-OffloadConfig-r12
FROM EUTRA-RRC-Definitions;


HandoverCommand ::=					SEQUENCE {
	criticalExtensions					CHOICE {
		c1									CHOICE{
			handoverCommand-r8					HandoverCommand-r8-IEs,
			spare7 NULL,
			spare6 NULL, spare5 NULL, spare4 NULL,
			spare3 NULL, spare2 NULL, spare1 NULL
		},
		criticalExtensionsFuture			SEQUENCE {}
	}
}

HandoverCommand-r8-IEs ::=			SEQUENCE {
	handoverCommandMessage				OCTET STRING (CONTAINING DL-DCCH-Message),
	nonCriticalExtension				SEQUENCE {}							OPTIONAL
}


HandoverPreparationInformation ::=	SEQUENCE {
	criticalExtensions					CHOICE {
		c1									CHOICE{
			handoverPreparationInformation-r8	HandoverPreparationInformation-r8-IEs,
			spare7 NULL,
			spare6 NULL, spare5 NULL, spare4 NULL,
			spare3 NULL, spare2 NULL, spare1 NULL
		},
		criticalExtensionsFuture			SEQUENCE {}
	}
}

HandoverPreparationInformation-r8-IEs ::= SEQUENCE {
	ue-RadioAccessCapabilityInfo		UE-CapabilityRAT-ContainerList,
	as-Config							AS-Config					OPTIONAL,		-- Cond HO
	rrm-Config							RRM-Config					OPTIONAL,
	as-Context							AS-Context				OPTIONAL,		-- Cond HO
	nonCriticalExtension				HandoverPreparationInformation-v920-IEs		OPTIONAL
}

HandoverPreparationInformation-v920-IEs	::= SEQUENCE {
	ue-ConfigRelease-r9					ENUMERATED {
										rel9, rel10, rel11, rel12, v10j0, v11e0,
										v1280, rel13, ..., rel14}			OPTIONAL,	-- Cond HO2
	nonCriticalExtension				HandoverPreparationInformation-v9d0-IEs		OPTIONAL
}

HandoverPreparationInformation-v9d0-IEs	::= SEQUENCE {
	lateNonCriticalExtension			OCTET STRING (CONTAINING HandoverPreparationInformation-v9j0-IEs)	OPTIONAL,
	nonCriticalExtension				HandoverPreparationInformation-v9e0-IEs			OPTIONAL
}

-- Late non-critical extensions:
HandoverPreparationInformation-v9j0-IEs ::= SEQUENCE {
	-- Following field is only for pre REL-10 late non-critical extensions
	lateNonCriticalExtension			OCTET STRING					OPTIONAL,
	nonCriticalExtension				HandoverPreparationInformation-v10j0-IEs		OPTIONAL
}

HandoverPreparationInformation-v10j0-IEs ::= SEQUENCE {
	as-Config-v10j0						AS-Config-v10j0			OPTIONAL,
	-- Following field is only for late non-critical extensions from REL-10
	nonCriticalExtension				SEQUENCE {}				OPTIONAL
}

-- Regular non-critical extensions:
HandoverPreparationInformation-v9e0-IEs	::= SEQUENCE {
	as-Config-v9e0						AS-Config-v9e0					OPTIONAL,	-- Cond HO2
	nonCriticalExtension				HandoverPreparationInformation-v1130-IEs		OPTIONAL
}

HandoverPreparationInformation-v1130-IEs	::= SEQUENCE {
	as-Context-v1130					AS-Context-v1130				OPTIONAL,	-- Cond HO2
	nonCriticalExtension				HandoverPreparationInformation-v1250-IEs						OPTIONAL
}

HandoverPreparationInformation-v1250-IEs ::= SEQUENCE {
	ue-SupportedEARFCN-r12				ARFCN-ValueEUTRA-r9				OPTIONAL,	-- Cond HO3
	as-Config-v1250					AS-Config-v1250				OPTIONAL,	-- Cond HO2
	nonCriticalExtension				HandoverPreparationInformation-v1320-IEs						OPTIONAL
}

HandoverPreparationInformation-v1320-IEs ::= SEQUENCE {
	as-Config-v1320						AS-Config-v1320					OPTIONAL,	-- Cond HO2
	as-Context-v1320					AS-Context-v1320				OPTIONAL,	-- Cond HO2
	nonCriticalExtension				HandoverPreparationInformation-v1430-IEs						OPTIONAL
}

HandoverPreparationInformation-v1430-IEs ::= SEQUENCE {
	as-Config-v1430					AS-Config-v1430						OPTIONAL,	-- Cond HO2
	makeBeforeBreakReq-r14			ENUMERATED {true}				OPTIONAL,	-- Cond HO2
	nonCriticalExtension			SEQUENCE {}							OPTIONAL
}


SCG-Config-r12 ::=					SEQUENCE {
	criticalExtensions					CHOICE {
		c1									CHOICE{
			scg-Config-r12					SCG-Config-r12-IEs,
			spare7 NULL,
			spare6 NULL, spare5 NULL, spare4 NULL,
			spare3 NULL, spare2 NULL, spare1 NULL
		},
		criticalExtensionsFuture			SEQUENCE {}
	}
}

SCG-Config-r12-IEs ::=				SEQUENCE {
	scg-RadioConfig-r12					SCG-ConfigPartSCG-r12				OPTIONAL,
	nonCriticalExtension				SEQUENCE {}							OPTIONAL
}


SCG-ConfigInfo-r12 ::=					SEQUENCE {
	criticalExtensions					CHOICE {
		c1									CHOICE{
			scg-ConfigInfo-r12					SCG-ConfigInfo-r12-IEs,
			spare7 NULL,
			spare6 NULL, spare5 NULL, spare4 NULL,
			spare3 NULL, spare2 NULL, spare1 NULL
		},
		criticalExtensionsFuture			SEQUENCE {}
	}
}

SCG-ConfigInfo-r12-IEs ::=			SEQUENCE {
	radioResourceConfigDedMCG-r12	RadioResourceConfigDedicated		OPTIONAL,
	sCellToAddModListMCG-r12		SCellToAddModList-r10				OPTIONAL,
	measGapConfig-r12				MeasGapConfig						OPTIONAL,
	powerCoordinationInfo-r12		PowerCoordinationInfo-r12			OPTIONAL,
	scg-RadioConfig-r12				SCG-ConfigPartSCG-r12				OPTIONAL,
	eutra-CapabilityInfo-r12		OCTET STRING (CONTAINING UECapabilityInformation)	OPTIONAL,
	scg-ConfigRestrictInfo-r12		SCG-ConfigRestrictInfo-r12			OPTIONAL,
	mbmsInterestIndication-r12		OCTET STRING (CONTAINING
										MBMSInterestIndication-r11)		OPTIONAL,
	measResultServCellListSCG-r12	MeasResultServCellListSCG-r12		OPTIONAL,
	drb-ToAddModListSCG-r12			DRB-InfoListSCG-r12					OPTIONAL,
	drb-ToReleaseListSCG-r12		DRB-ToReleaseList					OPTIONAL,
	sCellToAddModListSCG-r12		SCellToAddModListSCG-r12			OPTIONAL,
	sCellToReleaseListSCG-r12		SCellToReleaseList-r10				OPTIONAL,
	p-Max-r12							P-Max								OPTIONAL,
	nonCriticalExtension			SCG-ConfigInfo-v1310-IEs			OPTIONAL
}

SCG-ConfigInfo-v1310-IEs ::=		SEQUENCE {
	measResultSSTD-r13				MeasResultSSTD-r13					OPTIONAL,	sCellToAddModListMCG-Ext-r13		SCellToAddModListExt-r13			OPTIONAL,
	measResultServCellListSCG-Ext-r13	MeasResultServCellListSCG-Ext-r13	OPTIONAL,
	sCellToAddModListSCG-Ext-r13		SCellToAddModListSCG-Ext-r13			OPTIONAL,
	sCellToReleaseListSCG-Ext-r13	SCellToReleaseListExt-r13			OPTIONAL,
	nonCriticalExtension			SCG-ConfigInfo-v1330-IEs			OPTIONAL
}

SCG-ConfigInfo-v1330-IEs ::=		SEQUENCE {
	measResultListRSSI-SCG-r13		MeasResultListRSSI-SCG-r13			OPTIONAL,
	nonCriticalExtension			SCG-ConfigInfo-v1430-IEs							OPTIONAL
}

SCG-ConfigInfo-v1430-IEs ::=		SEQUENCE {
	makeBeforeBreakSCG-Req-r14		ENUMERATED {true}					OPTIONAL,
	measGapConfigPerCC-List		MeasGapConfigPerCC-List-r14			OPTIONAL,
	nonCriticalExtension			SEQUENCE {}							OPTIONAL
}

DRB-InfoListSCG-r12 ::=				SEQUENCE (SIZE (1..maxDRB)) OF DRB-InfoSCG-r12

DRB-InfoSCG-r12 ::=				SEQUENCE {
	eps-BearerIdentity-r12			INTEGER (0..15)				OPTIONAL,	-- Cond DRB-Setup
	drb-Identity-r12				DRB-Identity,
	drb-Type-r12					ENUMERATED {split, scg}		OPTIONAL,	-- Cond DRB-Setup
	...
}

SCellToAddModListSCG-r12 ::=	SEQUENCE (SIZE (1..maxSCell-r10)) OF Cell-ToAddMod-r12

SCellToAddModListSCG-Ext-r13 ::=	SEQUENCE (SIZE (1..maxSCell-r13)) OF Cell-ToAddMod-r12

Cell-ToAddMod-r12 ::=				SEQUENCE {
	sCellIndex-r12						SCellIndex-r10,
	cellIdentification-r12				SEQUENCE {
		physCellId-r12						PhysCellId,
		dl-CarrierFreq-r12					ARFCN-ValueEUTRA-r9
	}																OPTIONAL,	-- Cond SCellAdd
	measResultCellToAdd-r12				SEQUENCE {
		rsrpResult-r12						RSRP-Range,
		rsrqResult-r12						RSRQ-Range
	}																OPTIONAL,	-- Cond SCellAdd2
	...,
	[[		sCellIndex-r13					SCellIndex-r13				OPTIONAL,
		measResultCellToAdd-v1310			SEQUENCE {
			rs-sinr-Result-r13					RS-SINR-Range-r13
		}															OPTIONAL	-- Cond SCellAdd2
	]]
}

MeasResultServCellListSCG-r12 ::=	SEQUENCE (SIZE (1..maxServCell-r10)) OF MeasResultServCellSCG-r12

MeasResultServCellListSCG-Ext-r13 ::=	SEQUENCE (SIZE (1..maxServCell-r13)) OF MeasResultServCellSCG-r12

MeasResultServCellSCG-r12 ::=			SEQUENCE {
	servCellId-r12						ServCellIndex-r10,
	measResultSCell-r12					SEQUENCE {
		rsrpResultSCell-r12					RSRP-Range,
		rsrqResultSCell-r12					RSRQ-Range
	},
	...,
	[[		servCellId-r13						ServCellIndex-r13		OPTIONAL,
		measResultSCell-v1310				SEQUENCE {
			rs-sinr-ResultSCell-r13				RS-SINR-Range-r13
		}															OPTIONAL
	]]
}

MeasResultListRSSI-SCG-r13 ::=	SEQUENCE (SIZE (1..maxServCell-r13)) OF MeasResultRSSI-SCG-r13

MeasResultRSSI-SCG-r13 ::=			SEQUENCE {
	servCellId-r13						ServCellIndex-r13,
	measResultForRSSI-r13				MeasResultForRSSI-r13
}

SCG-ConfigRestrictInfo-r12 ::=		SEQUENCE {
	maxSCH-TB-BitsDL-r12				INTEGER (1..100),
	maxSCH-TB-BitsUL-r12				INTEGER (1..100)
}


UEPagingCoverageInformation ::= SEQUENCE {
	criticalExtensions					CHOICE {
		c1									CHOICE{
			uePagingCoverageInformation-r13			UEPagingCoverageInformation-r13-IEs,
			spare7 NULL,
			spare6 NULL, spare5 NULL, spare4 NULL,
			spare3 NULL, spare2 NULL, spare1 NULL
		},
		criticalExtensionsFuture			SEQUENCE {}
	}
}

UEPagingCoverageInformation-r13-IEs ::= SEQUENCE {
	mpdcch-NumRepetition-r13				INTEGER (1..256)	OPTIONAL,
	nonCriticalExtension					SEQUENCE {}		OPTIONAL
}


UERadioAccessCapabilityInformation ::= SEQUENCE {
	criticalExtensions					CHOICE {
		c1									CHOICE{
			ueRadioAccessCapabilityInformation-r8
												UERadioAccessCapabilityInformation-r8-IEs,
			spare7 NULL,
			spare6 NULL, spare5 NULL, spare4 NULL,
			spare3 NULL, spare2 NULL, spare1 NULL
		},
		criticalExtensionsFuture			SEQUENCE {}
	}
}

UERadioAccessCapabilityInformation-r8-IEs ::= SEQUENCE {
	ue-RadioAccessCapabilityInfo		OCTET STRING (CONTAINING UECapabilityInformation),
	nonCriticalExtension				SEQUENCE {}							OPTIONAL
}


UERadioPagingInformation ::= SEQUENCE {
	criticalExtensions					CHOICE {
		c1									CHOICE{
			ueRadioPagingInformation-r12			UERadioPagingInformation-r12-IEs,
			spare7 NULL,
			spare6 NULL, spare5 NULL, spare4 NULL,
			spare3 NULL, spare2 NULL, spare1 NULL
		},
		criticalExtensionsFuture			SEQUENCE {}
	}
}

UERadioPagingInformation-r12-IEs ::= SEQUENCE {
	ue-RadioPagingInfo-r12				OCTET STRING (CONTAINING UE-RadioPagingInfo-r12),
	nonCriticalExtension				UERadioPagingInformation-v1310-IEs			OPTIONAL
}

UERadioPagingInformation-v1310-IEs ::= SEQUENCE {
	supportedBandListEUTRAForPaging-r13		SEQUENCE (SIZE (1..maxBands)) OF FreqBandIndicator-r11 OPTIONAL,
	nonCriticalExtension					SEQUENCE {}								OPTIONAL

}


AS-Config ::=				SEQUENCE {
	sourceMeasConfig					MeasConfig,
	sourceRadioResourceConfig			RadioResourceConfigDedicated,
	sourceSecurityAlgorithmConfig		SecurityAlgorithmConfig,
	sourceUE-Identity					C-RNTI,
	sourceMasterInformationBlock		MasterInformationBlock,
	sourceSystemInformationBlockType1	SystemInformationBlockType1(WITH COMPONENTS
											{..., nonCriticalExtension ABSENT}),
	sourceSystemInformationBlockType2	SystemInformationBlockType2,
	antennaInfoCommon					AntennaInfoCommon,
	sourceDl-CarrierFreq				ARFCN-ValueEUTRA,
	...,
	[[	sourceSystemInformationBlockType1Ext	OCTET STRING (CONTAINING
												SystemInformationBlockType1-v890-IEs)	OPTIONAL,
		sourceOtherConfig-r9				OtherConfig-r9
	-- sourceOtherConfig-r9 should have been optional. A target eNB compliant with this transfer
	-- syntax should support receiving an AS-Config not including this extension addition group
	-- e.g. from a legacy source eNB
	]],
	[[	sourceSCellConfigList-r10			SCellToAddModList-r10			OPTIONAL
	]],
	[[	sourceConfigSCG-r12					SCG-Config-r12		OPTIONAL
	]]
}

AS-Config-v9e0 ::=				SEQUENCE {
	sourceDl-CarrierFreq-v9e0		ARFCN-ValueEUTRA-v9e0
}

AS-Config-v10j0 ::=				SEQUENCE {
	antennaInfoDedicatedPCell-v10i0		AntennaInfoDedicated-v10i0			OPTIONAL
}

AS-Config-v1250 ::=				SEQUENCE {
	sourceWlan-OffloadConfig-r12		WLAN-OffloadConfig-r12				OPTIONAL,
	sourceSL-CommConfig-r12				SL-CommConfig-r12					OPTIONAL,
	sourceSL-DiscConfig-r12				SL-DiscConfig-r12					OPTIONAL
}

AS-Config-v1320 ::=				SEQUENCE {
	sourceSCellConfigList-r13			SCellToAddModListExt-r13			OPTIONAL,
	sourceRCLWI-Configuration-r13		RCLWI-Configuration-r13				OPTIONAL
}

AS-Config-v1430 ::=				SEQUENCE {
	sourceSL-V2X-CommConfig-r14			SL-V2X-ConfigDedicated-r14					OPTIONAL,
	sourceLWA-Config-r14				LWA-Config-r13						OPTIONAL,
	sourceWLAN-MeasResult-r14			MeasResultListWLAN-r13				OPTIONAL
}


AS-Context ::=							SEQUENCE {
	reestablishmentInfo						ReestablishmentInfo			OPTIONAL	-- Cond HO
}

AS-Context-v1130 ::=					SEQUENCE {
	idc-Indication-r11						OCTET STRING (CONTAINING
											InDeviceCoexIndication-r11)	OPTIONAL,	-- Cond HO2
	mbmsInterestIndication-r11				OCTET STRING (CONTAINING
											MBMSInterestIndication-r11)	OPTIONAL,	-- Cond HO2
	powerPrefIndication-r11					OCTET STRING (CONTAINING
											UEAssistanceInformation-r11)	OPTIONAL,	-- Cond HO2
	...,
	[[	sidelinkUEInformation-r12				OCTET STRING (CONTAINING
												SidelinkUEInformation-r12)	OPTIONAL	-- Cond HO2
	]]
}

AS-Context-v1320 ::=					SEQUENCE {
	wlanConnectionStatusReport-r13			OCTET STRING (CONTAINING
											WLANConnectionStatusReport-r13)	OPTIONAL	-- Cond HO2
}


ReestablishmentInfo ::=				SEQUENCE {
	sourcePhysCellId					PhysCellId,
	targetCellShortMAC-I				ShortMAC-I,
	additionalReestabInfoList			AdditionalReestabInfoList				OPTIONAL,
	...
}

AdditionalReestabInfoList ::=		SEQUENCE ( SIZE (1..maxReestabInfo) ) OF AdditionalReestabInfo

AdditionalReestabInfo ::=	SEQUENCE{
	cellIdentity						CellIdentity,
	key-eNodeB-Star					Key-eNodeB-Star,
	shortMAC-I							ShortMAC-I
}

Key-eNodeB-Star ::=					BIT STRING (SIZE (256))


RRM-Config ::=				SEQUENCE {
	ue-InactiveTime				ENUMERATED {
									s1, s2, s3, s5, s7, s10, s15, s20,
									s25, s30, s40, s50, min1, min1s20c, min1s40,
									min2, min2s30, min3, min3s30, min4, min5, min6,
									min7, min8, min9, min10, min12, min14, min17, min20,
									min24, min28, min33, min38, min44, min50, hr1,
									hr1min30, hr2, hr2min30, hr3, hr3min30, hr4, hr5, hr6,
									hr8, hr10, hr13, hr16, hr20, day1, day1hr12, day2,
									day2hr12, day3, day4, day5, day7, day10, day14, day19,
									day24, day30, dayMoreThan30}		OPTIONAL,
	...,
	[[	candidateCellInfoList-r10	CandidateCellInfoList-r10		OPTIONAL
	]]
}

CandidateCellInfoList-r10 ::=	SEQUENCE (SIZE (1..maxFreq)) OF CandidateCellInfo-r10

CandidateCellInfo-r10 ::=		SEQUENCE {
	-- cellIdentification
	physCellId-r10					PhysCellId,
	dl-CarrierFreq-r10				ARFCN-ValueEUTRA,
	-- available measurement results
	rsrpResult-r10					RSRP-Range			OPTIONAL,
	rsrqResult-r10					RSRQ-Range			OPTIONAL,
	...,
	[[	dl-CarrierFreq-v1090			ARFCN-ValueEUTRA-v9e0		OPTIONAL
	]],
	[[	rsrqResult-v1250				RSRQ-Range-v1250			OPTIONAL
	]],
	[[	rs-sinr-Result-r13				RS-SINR-Range-r13			OPTIONAL
	]]
}


maxReestabInfo				INTEGER ::= 32	-- Maximum number of KeNB* and shortMAC-I forwarded
											-- at handover for re-establishment preparation


END


NBIOT-InterNodeDefinitions DEFINITIONS AUTOMATIC TAGS ::=

BEGIN

IMPORTS
	C-RNTI,
	PhysCellId,
	SecurityAlgorithmConfig,
	ShortMAC-I
FROM EUTRA-RRC-Definitions

	AdditionalReestabInfoList
FROM EUTRA-InterNodeDefinitions

	CarrierFreq-NB-r13,
	RadioResourceConfigDedicated-NB-r13,
	UECapabilityInformation-NB,
	UE-Capability-NB-r13,
	UE-Capability-NB-Ext-r14-IEs,
	UE-RadioPagingInfo-NB-r13
FROM NBIOT-RRC-Definitions;


HandoverPreparationInformation-NB ::=	SEQUENCE {
	criticalExtensions						CHOICE {
		c1										CHOICE{
			handoverPreparationInformation-r13		HandoverPreparationInformation-NB-IEs,
			spare3 NULL, spare2 NULL, spare1 NULL
		},
		criticalExtensionsFuture			SEQUENCE {}
	}
}

HandoverPreparationInformation-NB-IEs ::= SEQUENCE {
	ue-RadioAccessCapabilityInfo-r13		UE-Capability-NB-r13,
	as-Config-r13							AS-Config-NB,
	rrm-Config-r13							RRM-Config-NB					OPTIONAL,
	as-Context-r13							AS-Context-NB					OPTIONAL,
	nonCriticalExtension					HandoverPreparationInformation-NB-v1380-IEs					OPTIONAL
}

HandoverPreparationInformation-NB-v1380-IEs ::= SEQUENCE {
	lateNonCriticalExtension			OCTET STRING						OPTIONAL,
	nonCriticalExtension				HandoverPreparationInformation-NB-Ext-r14-IEs	OPTIONAL
}

HandoverPreparationInformation-NB-Ext-r14-IEs ::= SEQUENCE {
	ue-RadioAccessCapabilityInfoExt-r14		OCTET STRING (CONTAINING UE-Capability-NB-Ext-r14-IEs)	OPTIONAL,
	nonCriticalExtension					SEQUENCE {}						OPTIONAL
}


UEPagingCoverageInformation-NB ::= SEQUENCE {
	criticalExtensions					CHOICE {
		c1									CHOICE{
			uePagingCoverageInformation-r13			UEPagingCoverageInformation-NB-IEs,
			spare3 NULL, spare2 NULL, spare1 NULL
		},
		criticalExtensionsFuture			SEQUENCE {}
	}
}

UEPagingCoverageInformation-NB-IEs ::= SEQUENCE {
--	the possible value(s) can differ from those sent on Uu
	npdcch-NumRepetitionPaging-r13			INTEGER (1..2048)	OPTIONAL,
	nonCriticalExtension					SEQUENCE {}		OPTIONAL
}


UERadioAccessCapabilityInformation-NB ::= SEQUENCE {
	criticalExtensions						CHOICE {
		c1										CHOICE{
			ueRadioAccessCapabilityInformation-r13
													UERadioAccessCapabilityInformation-NB-IEs,
			spare3 NULL, spare2 NULL, spare1 NULL
		},
		criticalExtensionsFuture				SEQUENCE {}
	}
}

UERadioAccessCapabilityInformation-NB-IEs ::= SEQUENCE {
	ue-RadioAccessCapabilityInfo-r13			OCTET STRING (CONTAINING UE-Capability-NB-r13),
	nonCriticalExtension						UERadioAccessCapabilityInformation-NB-v1380-IEs	OPTIONAL
}

UERadioAccessCapabilityInformation-NB-v1380-IEs ::= SEQUENCE {
	lateNonCriticalExtension				OCTET STRING					OPTIONAL,
	nonCriticalExtension					UERadioAccessCapabilityInformation-NB-r14-IEs				OPTIONAL
}

UERadioAccessCapabilityInformation-NB-r14-IEs ::= SEQUENCE {
	ue-RadioAccessCapabilityInfo-r14		OCTET STRING (CONTAINING UECapabilityInformation-NB)	OPTIONAL,
	nonCriticalExtension					SEQUENCE {}						OPTIONAL
}


UERadioPagingInformation-NB ::= SEQUENCE {
	criticalExtensions					CHOICE {
		c1									CHOICE{
			ueRadioPagingInformation-r13			UERadioPagingInformation-NB-IEs,
			spare3 NULL, spare2 NULL, spare1 NULL
		},
		criticalExtensionsFuture			SEQUENCE {}
	}
}

UERadioPagingInformation-NB-IEs ::= SEQUENCE {
	ue-RadioPagingInfo-r13				OCTET STRING (CONTAINING UE-RadioPagingInfo-NB-r13),
	nonCriticalExtension				SEQUENCE {}									OPTIONAL
}


AS-Config-NB ::=					SEQUENCE {
	sourceRadioResourceConfig-r13			RadioResourceConfigDedicated-NB-r13,
	sourceSecurityAlgorithmConfig-r13		SecurityAlgorithmConfig,
	sourceUE-Identity-r13					C-RNTI,
	sourceDl-CarrierFreq-r13				CarrierFreq-NB-r13,
	...
}


AS-Context-NB ::=						SEQUENCE {
	reestablishmentInfo-r13					ReestablishmentInfo-NB			OPTIONAL,
	...
}


ReestablishmentInfo-NB ::=			SEQUENCE {
	sourcePhysCellId-r13					PhysCellId,
	targetCellShortMAC-I-r13				ShortMAC-I,
	additionalReestabInfoList-r13			AdditionalReestabInfoList				OPTIONAL,
	...
}




RRM-Config-NB ::=				SEQUENCE {
	ue-InactiveTime				ENUMERATED {
									s1, s2, s3, s5, s7, s10, s15, s20,
									s25, s30, s40, s50, min1, min1s20, min1s40,
									min2, min2s30, min3, min3s30, min4, min5, min6,
									min7, min8, min9, min10, min12, min14, min17, min20,
									min24, min28, min33, min38, min44, min50, hr1,
									hr1min30, hr2, hr2min30, hr3, hr3min30, hr4, hr5, hr6,
									hr8, hr10, hr13, hr16, hr20, day1, day1hr12, day2,
									day2hr12, day3, day4, day5, day7, day10, day14, day19,
									day24, day30, dayMoreThan30}		OPTIONAL,
	...
}


END


